{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["ILS O&E","ILS O&E in Archicad","legende"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":2,"defined_names":460,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ILS O&E","index":0,"n_rows":1828,"n_cols":37,"rows_kept":1828,"cut":false,"hidden":false,"merged":[[1765,3,1765,14],[1795,3,1795,14],[3,3,3,14],[1581,3,1581,14],[1608,3,1608,14],[1636,3,1636,14],[1663,3,1663,14],[1690,3,1690,14],[1766,3,1766,14],[1528,3,1528,14],[1554,3,1554,14],[19,3,19,14],[4,3,4,11],[18,3,18,14],[1796,3,1796,14],[13,3,13,5],[1609,3,1609,14],[1637,3,1637,14],[1664,3,1664,14],[1691,3,1691,14],[1733,3,1733,14],[1310,3,1310,14],[898,3,898,14],[966,3,966,14],[367,3,367,14],[270,3,270,14],[1425,3,1425,14],[1451,3,1451,14],[1503,3,1503,14],[1529,3,1529,14],[1555,3,1555,14],[1582,3,1582,14],[815,3,815,14],[816,3,816,14],[808,3,808,14],[1105,3,1105,14],[1502,3,1502,14],[1732,3,1732,14],[1266,15,1267,15],[1267,3,1267,14],[1477,3,1477,14],[1309,15,1310,15],[1346,3,1346,14],[1372,3,1372,14],[1399,3,1399,14],[1266,3,1266,14],[1309,3,1309,14],[1345,3,1345,14],[1371,3,1371,14],[1398,3,1398,14],[1424,3,1424,14],[1450,3,1450,14],[1476,3,1476,14],[1142,15,1143,15],[1143,3,1143,14],[1181,3,1181,14],[1180,15,1181,15],[1225,15,1226,15],[1226,3,1226,14],[1142,3,1142,14],[1180,3,1180,14],[1225,3,1225,14],[815,15,816,15],[809,3,809,14],[1036,15,1037,15],[1037,3,1037,14],[1105,15,1106,15],[1106,3,1106,14],[893,3,893,14],[810,3,810,14],[812,3,812,14],[814,3,814,14],[890,3,890,14],[894,3,894,14],[896,3,896,14],[965,3,965,14],[1003,3,1003,14],[1036,3,1036,14],[965,15,966,15],[1004,3,1004,14],[1003,15,1004,15],[891,3,891,14],[895,3,895,14],[897,3,897,14],[811,3,811,14],[813,3,813,14],[658,15,659,15],[659,3,659,14],[696,15,697,15],[697,3,697,14],[748,3,748,14],[747,15,748,15],[658,3,658,14],[696,3,696,14],[747,3,747,14],[503,15,504,15],[504,3,504,14],[554,3,554,14],[553,15,554,15],[615,15,616,15],[616,3,616,14],[503,3,503,14],[553,3,553,14],[615,3,615,14],[366,15,367,15],[413,3,413,14],[412,15,413,15],[459,3,459,14],[458,15,459,15],[366,3,366,14],[412,3,412,14],[458,3,458,14],[269,15,270,15],[319,15,320,15],[320,3,320,14],[269,3,269,14],[319,3,319,14],[57,15,58,15],[100,3,100,14],[99,15,100,15],[137,3,137,14],[136,15,137,15],[177,15,178,15],[178,3,178,14],[230,15,231,15],[231,3,231,14],[57,3,57,14],[99,3,99,14],[136,3,136,14],[230,3,230,14],[58,3,58,14]]}
["N.v.t.","NL-SfB codering","Discipline","Soort Informatie","g,e,p","Parameter","-","-","-","-","-","-","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[]
[{"$nulls":17},"Reeds aanwezig/\nBIM basis ILS","comment","IFC2x3","IFC4","AC 26","AC27","NL","BE","Classificatie","Bestaande property","Nieuwe property","Property mapping Archicad","Type mapping","level / niveau","Pset in IFC","Property in IFC","Property type","Value type",null,"opmerkingen"]
[null,null,"u","Leeswijzer"]
[null,null,"u","*Uitgangspunt is minimaal BIM basis ILS v1.0"]
[null,null,"u","*Opgesteld voor de inhoud van prestatiemodellen, met als enige uitzondering de eventuele verdere productuitwerking vanuit een adviseur tijdens de UO Fase."]
[null,null,"u","*Definities en inbegrepen op basis van NL-SfB (site BIM Loket)"]
[null,null,"u","*De NL-SfB code [38.1*- Inbouwpakketten] is een samenstelling van verschillende componenten, denk aan wanden, vloeren, plafonds, openingen, installatiecomponenten. Voor de gegevensbehoefte wordt hiervoor verwezen naar de van toepassing zijnde kaarten."]
[null,null,"u","*De NL-SfB code [48.1*- Afwerkingspakketten] is een samenstelling van verschillende componenten, denk aan wandafwerking, vloerafwerking, plafondsafwerking. Voor de gegevensbehoefte wordt hiervoor verwezen naar de van toepassing zijnde kaarten."]
[null,null,"u","*Verantwoordelijkheden t.a.v. het aanleveren, modelleren en valideren van de informatie in het model dienen te worden omschreven en een separaat afsprakendocument."]
[null,null,"u",null,"g","Generiek, voor alle elementen en over de projecten heen"]
[null,null,"u",null,"e","Element specifiek, over de projecten heen"]
[null,null,"u",null,"p","Project specifiek"]
[null,null,"u","*Fasering op basis van DNR STB 2014 aangevuld met as-build en as-maintained",null,null,"SO","VO","DO","TO","UO","AS-B"]
[null,null,"u","*Er mogen geen meerdere waarden in een parameter worden ingevuld."]
[null,null,"u","*Fase is uitgelicht wanneer er in de Fase een toevoeging, aanpassing of verdere detailuitwerking wordt verwacht van het betreffende element en bevat minimaal de informatie van de voorgaande Fases."]
[]
[]
[null,"00. ruimtes","b","00 - Ruimtes"]
[null,"00. ruimtes","b","De ruimte is het driedimensionale IFC-object dat in beginsel begrensd is door de haar omhullende materiële bouwwerkelementen (wanden, vloeren etc.) en in haar vorm op deze omhullende elementen aansluit. Een ruimte is hetzij een binnenruimte, hetzij een buitenruimte.\nContour:\nIn het algemeen volgt de contour van het driedimensionale object op vloerniveau de netto-contour van de ruimte langs de binnenzijde van de omhullende bouwwerkelementen. Interne bouwwerkelementen, zoals kolommen, zijn ongeacht hun grootte als inwendige contour van het ruimteobject uitgesloten.\n- Bij een ruimte in een trappenhuis, liftschacht of installatieschacht wordt in beginsel de netto-contour van de koker aangehouden.\n- Indien wet- en regelgeving dit vereist, mag een ruimte waar nodig opgesplitst worden afwijkend van de materiële omhullende bouwwerkelementen.\nHoogte:\nIn het algemeen is de hoogte van het driedimensionale object de netto-hoogte van de ruimte, gemeten vanaf de bovenzijde van de afgewerkte vloer tot aan de onderzijde van het element dat de ruimte aan de bovenzijde begrenst.\n- Voor binnenruimten: de bovenbegrenzing van de ruimte is doorgaans de onderzijde van het (verlaagd) plafond. Een ruimte kan een variërende hoogte hebben binnen dezelfde bouwlaag, maar kan ook lokaal of in haar geheel een hoogte hebben die de bouwlaaghoogte overstijgt, bijvoorbeeld door het ontbreken van (delen van) een vloer of door vloeropeningen. Bouwlaagoverstijgende ruimten worden per bouwlaag opgesplitst ter hoogte van het bijbehorende bouwlaagniveau. De ruimtedelen sluiten in verticale zin op elkaar aan.\n- Voor buitenruimten: bij het ontbreken van een materiële begrenzing aan de bovenzijde is de hoogte van de ruimte deze van de bouwlaag waartoe de ruimte behoort."]
[null,"00. ruimtes","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"00. ruimtes","b"]
[null,"00. ruimtes","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","ObjectType","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte (projectafhankelijk: BVO, GO, VVO), netto contour, netto hoogte"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"00. ruimtes","b"]
[null,"00. ruimtes","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","vastleggen in separaat afsprakendocument",null,"v"]
[null,"00. ruimtes","b",null,"g","Entiteit","-","-","-","-","-","-","IfcSpace, IfcZone","IfcClass","-",null,null,"v"]
[null,"00. ruimtes","b",null,"e","Ruimtenaam","-","-","-","-","-","-","Longname","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v",{"$nulls":11},"ifcContext","parent","Attributes","LongName",null,"ifcLabel"]
[null,"00. ruimtes","b",null,"e","Ruimtenummer","-","-","-","-","-","-","ShortName","-","-","Uniek nummer per ruimte (conform separaat afsprakendocument)",null,"v"]
[null,"00. ruimtes","b",null,"p","Bouwnummer","-","-","-","-","-","-","-","-","-"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"00. ruimtes","b"]
[null,"00. ruimtes","b","Eigenschappen","e","Binnen/ buitenruimte","-","-","-","-","-","-","IsExternal, benoemen in Custom Pset","true/ false","-","Benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Pset_SpaceCommon in Ifc 2x3",null,"x",{"$nulls":11},"ifcSpace","child -4th tier","Pset_SpaceCommon","IsExternal","SingleValue","ifcBoolean",null,"staat in BS, niet in ILS mapping"]
[{"$nulls":29},"ifcZone","child -4th tier","Pset_ZoneCommon","IsExternal","SingleValue","ifcBoolean"]
[null,"00. ruimtes","b",null,"e","Ruimtefunctie","-","-","-","-","-","-","ObjectType","-","-","Zoals gedefinieerd in het Bouwbesluit",{"$nulls":13},"ifcObject","parent (top) -1st tier","Attributes","ObjectType",null,"ifcLabel"]
[null,"00. ruimtes","b",null,"e","Wandafwerking","-","-","-","-","-","-","Pset_SpaceCommon:WallCovering","-","-","Wannneer niet los gemodelleerd, als eigenschap meenemen in de ruimte. Bij meerdere afwerkingen Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"v",{"$nulls":11},"ifcSpace","child -4th tier","Pset_SpaceCommon","WallCovering","SingleValue","ifcLabel"]
[null,"00. ruimtes","b",null,"e","Vloerafwerking","-","-","-","-","-","-","Pset_SpaceCommon:FloorCovering","-","-","Wannneer niet los gemodelleerd, als eigenschap meenemen in de ruimte. Bij meerdere afwerkingen Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"v",{"$nulls":11},"ifcSpace","child -4th tier","Pset_SpaceCommon","FloorCovering","SingleValue","ifcLabel"]
[null,"00. ruimtes","b",null,"e","Plafondafwerking","-","-","-","-","-","-","Pset_SpaceCommon:CeilingCovering","-","-","Wannneer niet los gemodelleerd, als eigenschap meenemen in de ruimte. Bij meerdere afwerkingen Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"v",{"$nulls":11},"ifcSpace","child -4th tier","Pset_SpaceCommon","CeilingCovering","SingleValue","ifcLabel"]
[null,"00. ruimtes","b",null,"p","Zonering Gebruiksfunctie","-","-","-","-","-","-","IfcSpace; is gerelateerd aan IfcZone","-","-"]
[null,"00. ruimtes","b",null,"p","Zonering Gebruiksgebied","-","-","-","-","-","-","IfcSpace; is gerelateerd aan IfcZone","-","-"]
[null,"00. ruimtes","b",null,"p","Zonering Verblijfsgebied","-","-","-","-","-","-","IfcSpace; is gerelateerd aan IfcZone","-","-"]
[null,"00. ruimtes","b",null,"p","Zonering Brandcompartimentering","-","-","-","-","-","-","IfcSpace; is gerelateerd aan IfcZone","-","-"]
[null,"00. ruimtes","b",null,"p","Zonering Vluchtroute","-","-","-","-","-","-","IfcSpace; is gerelateerd aan IfcZone","-","-"]
[null,"00. ruimtes","b",null,"p","Max. aantal pers. in Verblijfsgebied","-","-","-","-","-","-","Pset_SpaceOccupancyRequirements: OccupancyNumberPeak","aantal","stuks","Volgens vigerend bouwbesluit het aantal personen dat maximaal gelijktijdig in het verblijfsgebied aanwezig is. "]
[null,"00. ruimtes","b",null,"p","Aantal pers. in Verblijfsgebied","-","-","-","-","-","-","Pset_SpaceOccupancyRequirements: OccupancyNumber","aantal","stuks"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"00. ruimtes","b"]
[null,"00. ruimtes","b","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"00. ruimtes","b"]
[]
[null,"11.** bodemvoorzieningen","c","11.** - Bodemvoorzieningen; grond & water",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - verwijderen van oude opstallen, beplantingen en funderingsresten - maatvoering van het gebouw in het terrein, bouwramen - damwanden, taludvoorzieningen en grondverbeteringen ten behoeve van de bouwput - ontgraven van de bouwput - aanvullen van de bouwput - voorzieningen aan belendende percelen - verwijderen van tijdelijke voorzieningen/ - damwanden ten behoeve van de bemalingen - bemalingen inclusief leidingwerken, pompen en sleuven - lozingsvoorzieningen, inclusief vergunningen - energieverbruik van de bemalingen"]
[null,"11.** bodemvoorzieningen","c","Grond; Verzameling van grondvoorzieningen, die als voorbereidende werken noodzakelijk zijn voor het aanleggen van de gebouwfundatie, gerekend vanaf het toegankelijk maken van het terrein tot aan de funderingsconstructie.\n\nWater; Verzameling van tijdelijke voorzieningen, die noodzakelijk zijn voor de verlaging van grondwaterstanden en de afvoer van oppervlaktewater, voor het aanleggen van de gebouwfundatie."]
[null,"11.** bodemvoorzieningen","c",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"11.** bodemvoorzieningen","c"]
[null,"11.** bodemvoorzieningen","c","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, dikte, omtrek, volume"]
[null,"11.** bodemvoorzieningen","c",null,"e","Positiebepaling","-","-","-","-","-","-","-","-","-","Bijv. puntniveau t.o.v. peil, bovenkant t.o.v. NAP, onderkant t.o.v. NAP"]
[null,"11.** bodemvoorzieningen","c",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"]
[null,"11.** bodemvoorzieningen","c",null,"p","Hijsvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"11.** bodemvoorzieningen","c"]
[null,"11.** bodemvoorzieningen","c","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afspraken document",null,"v"]
[null,"11.** bodemvoorzieningen","c",null,"g","Entiteit","-","-","-","-","-","-","IfcSlab, IfcPlate, IfcBuildingElementProxy","IfcClass","-",null,null,"v",{"$nulls":11},"IfcSlab"]
[{"$nulls":29},"ifcPlate"]
[{"$nulls":29},"ifcBuildingElementProxy"]
[]
[null,"11.** bodemvoorzieningen","c",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v",{"$nulls":11},"ifcName"]
[{"$nulls":29},"ifcType"]
[null,"11.** bodemvoorzieningen","c",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"11.** bodemvoorzieningen","c",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"11.** bodemvoorzieningen","c"]
[null,"11.** bodemvoorzieningen","c","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"11.** bodemvoorzieningen","c",null,"e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","Indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"x","ifcPlate niet ok","x","x",{"$nulls":8},"ifcPlate","child","CPset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure",null,"staat op BS, niet in de ILS map"]
[{"$nulls":29},"ifcBuildingElementProxy","child","Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[{"$nulls":29},"IfcSlab","child","Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[null,"11.** bodemvoorzieningen","c",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","Indien entiteit IfcBuildingElementProxy: benoemen in Custom Pset omdat Pset_BuildingElementProxyCommon in Ifc 2x3 niet bestaat",null,"x","ifcBuildingElementProxy niet ok","x","x",{"$nulls":8},"ifcPlate","child","Pset_PlateCommon","LoadBearing","singlevalue","ifcBoolean"]
[{"$nulls":29},"ifcBuildingElementProxy","child","CPset_BuildingElementProxCommon","LoadBearing","singlevalue","ifcBoolean",null,"staat op BS"]
[{"$nulls":29},"IfcSlab","child","Pset_SlabCommon","LoadBearing","singlevalue","ifcBoolean"]
[null,"11.** bodemvoorzieningen","c",null,"p","Brandwerendheid hoofddraagconstructie","-","-","-","-","-","-","brandwerendheid tot bezwijken, benoemen in Custom Pset","moment tot bezwijken","minuten"]
[null,"11.** bodemvoorzieningen","c","#staal","p","Staalkwaliteit","-","-","-","-","-","-","staalkwaliteit, benoemen in Custom Pset","classificatie","-","Vb.: S235, S355"]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"11.** bodemvoorzieningen","c"]
[null,"11.** bodemvoorzieningen","c","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"11.** bodemvoorzieningen","c"]
[]
[null,"13.1* vloeren op grondslag; niet constructief","b","13.1* - Vloeren op grondslag; niet constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - tot de vloer behorende pompputten - egaliseren van de grondslag - vochtwerende lagen - werkvloeren onder de vloerconstructie - tot de vloer behorende verzwaringen - gebouwisolatievoorzieningen - vloerafwerkingen die één geheel vormen met de vloerconstructie",null,"Reeds aanwezig"]
[null,"13.1* vloeren op grondslag; niet constructief","b","Verzameling van niet tot de draagconstructie van het gebouw behorende vloeren, in rechtstreeks contact met de ondergrond aangebracht, gerekend vanaf de binnenzijde van de buitengevel of funderingsconstructie."]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"13.1* vloeren op grondslag; niet constructief","b"]
[null,"13.1* vloeren op grondslag; niet constructief","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, dikte, omtrek, volume",null,null,null,"Base quantities"]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,null,"Methode om sparingen te communiceren aanbieden (provision for void??)"]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"e","Nokken en sponningen","-","-","-","-","-","-","-","-","-",null,null,null,"Nog geen methode om dit te modelleren en te exporteren",{"$nulls":10},"??"]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,null,"Nog geen methode om dit te modelleren en te exporteren",{"$nulls":10},"IfcDiscreteAccessory"]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"13.1* vloeren op grondslag; niet constructief","b"]
[null,"13.1* vloeren op grondslag; niet constructief","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afspraken document",null,"v"]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"g","Entiteit","-","-","-","-","-","-","IfcSlab, IfcPlate","IfcClass","-",null,null,"v"]
[]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"13.1* vloeren op grondslag; niet constructief","b"]
[null,"13.1* vloeren op grondslag; niet constructief","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x","MAT"]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","False (niet constructief)",null,"v",{"$nulls":11},"ifcPlate","child","Pset_PlateCommon","LoadBearing","single value","ifcBoolean"]
[{"$nulls":29},"IfcSlab","child","Pset_SlabCommon","LoadBearing","single value","ifcBoolean"]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"p","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","Indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset"]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"p","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset"]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"p","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset.\n\nExclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)."]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"13.1* vloeren op grondslag; niet constructief","b"]
[null,"13.1* vloeren op grondslag; niet constructief","b","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"13.1* vloeren op grondslag; niet constructief","b"]
[]
[null,"13.2* vloeren op grondslag; constructief","c","13.2* - Vloeren op grondslag; constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - tot de vloer behorende liftputten - grondverbeteringen - egaliseren van de grondslag - vochtwerende lagen - werkvloeren onder de vloerconstructie - tot de vloer behorende verzwaringen - gebouwisolatievoorzieningen - vloerafwerkingen die één geheel vormen met de vloerconstructie - bodemonderzoek en sonderingen tijdens de uitvoering"]
[null,"13.2* vloeren op grondslag; constructief","c","Verzameling van tot de draagconstructie van het gebouw behorende vloeren in rechtstreeks contact met de ondergrond aangebracht,\ngerekend vanaf de buitenzijde van de buitengevel of funderingsconstructie."]
[null,"13.2* vloeren op grondslag; constructief","c",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"13.2* vloeren op grondslag; constructief","c"]
[null,"13.2* vloeren op grondslag; constructief","c","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, dikte, omtrek, volume"]
[null,"13.2* vloeren op grondslag; constructief","c",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"]
[null,"13.2* vloeren op grondslag; constructief","c",null,"e","Nokken en sponningen","-","-","-","-","-","-","-","-","-"]
[null,"13.2* vloeren op grondslag; constructief","c",null,"e","Dilataties","-","-","-","-","-","-","-","-","-"]
[null,"13.2* vloeren op grondslag; constructief","c",null,"p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"13.2* vloeren op grondslag; constructief","c"]
[null,"13.2* vloeren op grondslag; constructief","c","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument"]
[null,"13.2* vloeren op grondslag; constructief","c",null,"g","Entiteit","-","-","-","-","-","-","IfcSlab, IfcPlate","IfcClass","-",null,null,"v"]
[null,"13.2* vloeren op grondslag; constructief","c",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"13.2* vloeren op grondslag; constructief","c",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"13.2* vloeren op grondslag; constructief","c",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"13.2* vloeren op grondslag; constructief","c"]
[null,"13.2* vloeren op grondslag; constructief","c","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x","MAT"]
[null,"13.2* vloeren op grondslag; constructief","c",null,"e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","Indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"v","Massa van ?\nEen hele composite / prefab constructie of element component?",{"$nulls":7},"BM Density * Volume",null,"Nieuwe mapping\nPset_PrecastConcreteElementGeneral\n\nElementWeight","IfcSlab","child","Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure",null,"Elementweight property bestaat niet in BS, wel in ILS mapping"]
[{"$nulls":29},"ifcPlate","child","Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"," ","Elementweight property bestaat niet in BS"]
[null,"13.2* vloeren op grondslag; constructief","c",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","True (constructief)",null,"v",{"$nulls":11},"ifcPlate","child","Pset_PlateCommon","LoadBearing","Single value","ifcBoolean"]
[{"$nulls":29},"IfcSlab","child","Pset_SlabCommon","LoadBearing","Single value","ifcBoolean"]
[null,"13.2* vloeren op grondslag; constructief","c",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"v","Waar toevoegen?\nOpe elementniveau of BM?",{"$nulls":7},"Sterkteklasse",null,null,"ifcPlate","child","Pset_ConcreteElementGeneral","StructuralClass","Single value","ifcLabel",null,"staat op BS, niet in ILS map aanwezig. Maar BS omschrijft plate als steel, other metal, glass panels ?? Vloeit vanuit deze logica, dat deze Pset niet bestaat in ILS basis translator?"]
[{"$nulls":29},"IfcSlab","child","Pset_ConcreteElementGeneral","StructuralClass","Single value","ifcLabel"]
[null,"13.2* vloeren op grondslag; constructief","c",null,"e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset.\n\nExclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant).",null,"?","Beter te plaatsen onder building material ",{"$nulls":10},"IfcSlab","child","Pset_ConcreteElementGeneral","EnvironmentalClass","Single value","ifcLabel",null,"staat niet expliciet op BS"]
[{"$nulls":29},"ifcPlate","child","Pset_ConcreteElementGeneral","EnvironmentalClass","Single value","ifcLabel",null,"staat niet expliciet op BS"]
[null,"13.2* vloeren op grondslag; constructief","c",null,"p","Wapeningshoeveelheid","-","-","-","-","-","-","wapeningshoeveelheid, benoemen in Custom Pset","wapeningshoeveelheid","kg/m³"]
[null,"13.2* vloeren op grondslag; constructief","c",null,"p","Brandwerendheid hoofddraagconstructie","-","-","-","-","-","-","brandwerendheid tot bezwijken, benoemen in Custom Pset","moment tot bezwijken","minuten"]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"13.2* vloeren op grondslag; constructief","c"]
[null,"13.2* vloeren op grondslag; constructief","c","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"13.2* vloeren op grondslag; constructief","c"]
[]
[null,"16.** funderingsconstructies","c","16.** - Funderingsconstructies; voeten & balken en keerwanden",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - het egaliseren van de grondslag - grondverbeteringen - werkvloeren onder deze constructies - liftputten indien geen onderdeel van element (13) - funderingsmetselwerken - gevelmetselwerken vanaf de fundering tot 200 mm onder maaiveld - gebouwisolatievoorzieningen - bodemonderzoek en sonderingen tijdens de uitvoering/ - voorzieningen ten behoeve van de waterdichtheid"]
[null,"16.** funderingsconstructies","c","Verzameling van tot de draagconstructie van het gebouw behorende balken, voeten en poeren/ grondwerende keerconstructies, gerekend vanaf de dragende grondslag en/of de paalfundering tot aan de onderzijde van de laagst-liggende vloeren, met inbegrip van de omsluiting van onder de grondslag gelegen buitenruimten."]
[null,"16.** funderingsconstructies","c",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"16.** funderingsconstructies","c"]
[null,"16.** funderingsconstructies","c","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nBreedte, hoogte, lengte, volume"]
[null,"16.** funderingsconstructies","c",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"]
[null,"16.** funderingsconstructies","c",null,"e","Nokken en sponningen","-","-","-","-","-","-","-","-","-"]
[null,"16.** funderingsconstructies","c",null,"e","Dilataties","-","-","-","-","-","-","-","-","-"]
[null,"16.** funderingsconstructies","c",null,"p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"16.** funderingsconstructies","c"]
[null,"16.** funderingsconstructies","c","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"16.** funderingsconstructies","c",null,"g","Entiteit","-","-","-","-","-","-","IfcColumn, IfcBeam, IfcSlab, IfcFooting, IfcWall","IfcClass","-",null,null,"v"]
[null,"16.** funderingsconstructies","c",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"16.** funderingsconstructies","c",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"16.** funderingsconstructies","c",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"16.** funderingsconstructies","c",{"$nulls":33},"vb_start in AC translators"]
[null,"16.** funderingsconstructies","c","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x","MAT"]
[null,"16.** funderingsconstructies","c",null,"e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","Indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"v",{"$nulls":11},"ifcColumn","child","Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[{"$nulls":29},"ifcBeam","child","Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[{"$nulls":29},"ifcSlab","child","Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[{"$nulls":29},"ifcFooting"]
[{"$nulls":29},"ifcWall","child","Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[null,"16.** funderingsconstructies","c",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","Indien entiteit IfcFooting: benoemen in Custom Pset omdat Pset_FootingCommon niet bestaat",null,"x","ifcFooting niet ok",{"$nulls":10},"ifcColumn","child","Pset_<entitity>Common","LoadBearing","single value","ifcBoolean"]
[{"$nulls":29},"ifcBeam","child","Pset_<entitity>Common","LoadBearing","single value","ifcBoolean"]
[{"$nulls":29},"ifcSlab","child","Pset_<entitity>Common","LoadBearing","single value","ifcBoolean"]
[{"$nulls":29},"ifcFooting",null,"CPset_<entitity>Common","LoadBearing","Signle Value","ifcBoolean",null,"property bestaat niet op BS"]
[{"$nulls":29},"ifcWall","child","Pset_<entitity>Common","LoadBearing","single value","ifcBoolean"]
[null,"16.** funderingsconstructies","c",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"v",{"$nulls":11},"ifcColumn","child","Pset_<entitity>Common","LoadBearing","single value","ifcBoolean"]
[{"$nulls":29},"ifcBeam","child","Pset_ConcreteElementGeneral","StructuralClass",null,"ifcLabel"]
[{"$nulls":29},"ifcSlab","child","Pset_ConcreteElementGeneral","StructuralClass",null,"ifcLabel"]
[{"$nulls":29},"ifcFooting","child","Pset_ConcreteElementGeneral","StructuralClass",null,"ifcLabel"]
[{"$nulls":29},"ifcWall","child","Pset_ConcreteElementGeneral","StructuralClass",null,"ifcLabel"]
[null,"16.** funderingsconstructies","c",null,"e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset.\n\nExclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant).",null,"?","Beter te plaatsen onder building material"]
[null,"16.** funderingsconstructies","c",null,"p","Wapeningshoeveelheid","-","-","-","-","-","-","wapeningshoeveelheid, benoemen in Custom Pset","wapeningshoeveelheid","kg/m³"]
[null,"16.** funderingsconstructies","c",null,"p","Brandwerendheid hoofddraagconstructie","-","-","-","-","-","-","brandwerendheid tot bezwijken, benoemen in Custom Pset","moment tot bezwijken","minuten",{"$nulls":14},"ifcElement","parent","Pset_FireRatingProperties","FireResistanceRating",null,"ifcLabel"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"16.** funderingsconstructies","c"]
[null,"16.** funderingsconstructies","c","Componenten","e","Stekken","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten modelleren, ntb tijdens project; staalkwaliteit opgeven als Eigenschap"]
[null,"16.** funderingsconstructies","c",null,"p","Wapening","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten modelleren, ntb tijdens project; staalkwaliteit en dekking opgeven als Eigenschappen (noot: wanneer geen wapening wordt gemodelleerd, staalkwaliteit en dekking meegeven als Eigenschappen)"]
[null,"16.** funderingsconstructies","c",null,"p","Overige instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
[null,"16.** funderingsconstructies","c",null,"p","Randkist","-","-","-","-","-","-","-","-","-","Modelleren als 3D symbool (IfcBuildinElementProxy)"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"16.** funderingsconstructies","c"]
[]
[null,"17.** paalfunderingen","c","17.** - Paalfunderingen; niet geheid en geheid",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - pijlerfunderingen en putringen - bodeminjecties met een dragende functie - werkvloeren onder deze constructies - damwanden als definitief onderdeel van het gebouw - trekverankeringen - bodemonderzoek en sonderingen tijdens de uitvoering/ - voorzieningen ter voorkoming en/of beperking van risico en overlast voor de omgeving"]
[null,"17.** paalfunderingen","c","Verzameling van funderingsconstructies die de belasting van het gebouw overbrengen naar dieper gelegen draagkrachtige grondslagen en (niet geheid) zonder overlast/ (geheid) met overlast c.q. risico voor de omgeving worden aangebracht."]
[null,"17.** paalfunderingen","c",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"17.** paalfunderingen","c"]
[null,"17.** paalfunderingen","c","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm en locatie moet hetvolgende bepaald kunnen worden: \ndiameter, lengte, volume"]
[null,"17.** paalfunderingen","c",null,"e","Positiebepaling","-","-","-","-","-","-","-","-","-","Bijv. puntniveau t.o.v. peil, bovenkant t.o.v. NAP, onderkant t.o.v. NAP"]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"17.** paalfunderingen","c"]
[null,"17.** paalfunderingen","c","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"17.** paalfunderingen","c",null,"g","Entiteit","-","-","-","-","-","-","IfcFooting, IfcPile","IfcClass","-",null,null,"v"]
[null,"17.** paalfunderingen","c",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"17.** paalfunderingen","c",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"17.** paalfunderingen","c",null,"e","Paalnummer","-","-","-","-","-","-","-","-","-"]
[null,"17.** paalfunderingen","c",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"17.** paalfunderingen","c"]
[null,"17.** paalfunderingen","c","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"!","MAT"]
[null,"17.** paalfunderingen","c",null,"e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"v",{"$nulls":11},"ifcFooting","child","Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[{"$nulls":29},"ifcPile","child","Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[null,"17.** paalfunderingen","c",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","benoemen in custom Pset","true/ false","-","Indien entiteit IfcFooting, IfcPile: benoemen in Custom Pset omdat Pset_FootingCommon of Pset_PileCommon niet bestaat",null,"x","ifcFooting + ifcPile geen loading. ILS basis vermeld: IFC2X3TC1: IFCPILE HEEFT GEEN LOADBEARING EIGENSCHAP IN DE PSET_PILECOMMON. WANNEER JE WEL WILT AANGEVEN DAT DEZE FUNDERINGSPAAL (WEL OF JUIST NIET) CONSTRUCTIEF DRAGEND IS, DIEN JE IFC4 TE GEBRUIKEN OF DIT AAN TE GEVEN IN EEN EIGEN PROPERTYSET.",{"$nulls":10},"ifcFooting","child","Pset_FootingGeneral","LoadBearing","single value","ifcBoolean",null,"property bestaat ook niet in BS"]
[{"$nulls":29},"ifcPile","child","Pset_PileGeneral","LoadBearing","single value","ifcBoolean",null,"property bestaat ook niet in BS"]
[null,"17.** paalfunderingen","c",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"v",{"$nulls":11},"ifcFooting","child","Pset_ConcreteElementGeneral","StructuralClass",null,"ifcLabel"]
[{"$nulls":29},"ifcPile","child","Pset_ConcreteElementGeneral","StructuralClass",null,"ifcLabel"]
[null,"17.** paalfunderingen","c",null,"e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset.\n\nExclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant).",null,"?","In bulding Material "]
[]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"17.** paalfunderingen","c"]
[null,"17.** paalfunderingen","c","Componenten","p","Wapening","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten modelleren, ntb tijdens project; staalkwaliteit en dekking opgeven als Eigenschappen (noot: wanneer geen wapening wordt gemodelleerd, staalkwaliteit en dekking meegeven als Eigenschappen)"]
[null,"17.** paalfunderingen","c",null,"p","Stekken","-","-","-","-","-","-","-","-","-","ter plaatse moeilijke knooppunten modelleren, ntb tijdens project; staalkwaliteit opgeven als Eigenschap"]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"17.** paalfunderingen","c"]
[]
[null,"21.1* buitenwanden; niet constructief","b","21.1* - Buitenwanden; niet constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - kelderwanden, traditioneel samengestelde wanden, gordijngevels en systeemwanden - borstweringen, wandverzwaringen en terugliggende wanden van galerijen - schoorstenen die een onderdeel van de wand vormen - ventilatiekanalen die een onderdeel van de wand vormen - raaplagen in de spouwen en randaansluitingsvoorzieningen - gebouwisolatievoorzieningen - afwerkingen, die één geheel vormen met de buitenwand (incl. het voegwerk van schoon metselwerk) - verankeringen en bevestigingsmiddelen - dilatatievoegconstructies - gevelmetselwerken boven 200 mm onder maaiveld - boeiborden"]
[null,"21.1* buitenwanden; niet constructief","b","Verzameling van niet-constructieve buitenwanden, die de begrenzing vormen van het gebouw, gerekend vanaf de bovenzijde van de funderingsconstructies tot aan de bovenzijde van de dakconstructies.\nNoot: in het geval van een vliesgevel moeten de buitenwandopeningen voorzien zijn van de gegevensbehoefte onder 31.**."]
[null,"21.1* buitenwanden; niet constructief","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"21.1* buitenwanden; niet constructief","b"]
[null,"21.1* buitenwanden; niet constructief","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, dikte, hoogte, breedte (basisregel: geen samengestelde spouwwanden ivm hoeveelheden)"]
[null,"21.1* buitenwanden; niet constructief","b",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"]
[null,"21.1* buitenwanden; niet constructief","b",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-","Afwijkingen in Eigenschappen tussen vlakken, als losse elementen modelleren"]
[null,"21.1* buitenwanden; niet constructief","b",null,"e","Dilataties","-","-","-","-","-","-","-","-","-"]
[null,"21.1* buitenwanden; niet constructief","b",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"21.1* buitenwanden; niet constructief","b"]
[null,"21.1* buitenwanden; niet constructief","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"21.1* buitenwanden; niet constructief","b",null,"g","Entiteit","-","-","-","-","-","-","IfcWall, IfcCurtainWall","IfcClass","-",null,null,"v"]
[null,"21.1* buitenwanden; niet constructief","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"21.1* buitenwanden; niet constructief","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"21.1* buitenwanden; niet constructief","b",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"21.1* buitenwanden; niet constructief","b",null,"p","Merk","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelReference","-","-","Ten behoeve van onderhoud"]
[null,"21.1* buitenwanden; niet constructief","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"21.1* buitenwanden; niet constructief","b"]
[null,"21.1* buitenwanden; niet constructief","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"!","MAT"]
[null,"21.1* buitenwanden; niet constructief","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"!","MAT"]
[null,"21.1* buitenwanden; niet constructief","b",null,"e","Kleur","-","-","-","-","-","-","-","-","-","(RAL) kleurcode/ omschrijving (in het geval van metselwerk, Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file)",null,"!","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…",{"$nulls":12},"PsetWallFinishes","??","single value","ifcLabel"]
[null,"21.1* buitenwanden; niet constructief","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_WallCommon: Loadbearing","true/ false","-","False (niet constructief)\n\nIndien entiteit IfcCurtainWall, IfcWindow, IfcDoor: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"v",{"$nulls":11},"ifcWall","child","Pset_WallCommon","LoadBearing","Single Value","ifcLabel"]
[{"$nulls":29},"ifcCurtainWall",{"$nulls":6},"Vliesgevel heeft geen dragende functie => dus niet nodig??"]
[null,"21.1* buitenwanden; niet constructief","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-","True (isExternal)",null,"v",{"$nulls":11},"ifcWall","child","Pset_WallCommon","isExternal","Single Value","ifcBoolean"]
[{"$nulls":29},"ifcCurtainWall","child","Pset_CurtainWallCommon","isExternal","Single Value","ifc"]
[null,"21.1* buitenwanden; niet constructief","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"v",{"$nulls":11},"ifcElement","parent","Pset_FireRatingProperties","FireResistanceRating",null,"ifcLabel"]
[]
[null,"21.1* buitenwanden; niet constructief","b",null,"p","Weerstandsklasse","-","-","-","-","-","-","Pset_<entiteit>Common: SecurityRating","classificatie","-","Bijv.: WK1 conform NEN 5096\n\nIndien entiteit IfcWall, IfcCurtainWall, IfcPlate, IfcMember: benoemen in Custom Pset omdat 'SecurityRating' geen deel uitmaakt van Common Pset"]
[null,"21.1* buitenwanden; niet constructief","b","#metselwerk","p","Metselwerkverband","-","-","-","-","-","-","-","-","-"]
[null,"21.1* buitenwanden; niet constructief","b","#metselwerk","p","Voegtype","-","-","-","-","-","-","-","-","-"]
[null,"21.1* buitenwanden; niet constructief","b",null,"p","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset"]
[null,"21.1* buitenwanden; niet constructief","b","#beton","p","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset\nexclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)"]
[null,"21.1* buitenwanden; niet constructief","b","#beton","p","Oppervlakteklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN-EN 13670"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"21.1* buitenwanden; niet constructief","b"]
[null,"21.1* buitenwanden; niet constructief","b","Componenten","e","Isolatie","-","-","-","-","-","-","-","-","-","Tevens aangeven: isolatiewaarde en brandklasse"]
[null,"21.1* buitenwanden; niet constructief","b",null,"e","Folies, slabben","-","-","-","-","-","-","-","-","-","Volgens separaat uitganspunten/afsprakendocument"]
[null,"21.1* buitenwanden; niet constructief","b",null,"p","Geveldragers","-","-","-","-","-","-","-","-","-","Modelleren en voorzien van de bovenstaande Eigenschappen"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"21.1* buitenwanden; niet constructief","b"]
[]
[null,"21.2* buitenwanden; constructief","c","21.2* - Buitenwanden; constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - kelderwanden en traditioneel samengestelde wanden - borstweringen, wandverzwaringen en terugliggende wanden van galerijen - schoorstenen die een onderdeel van de wand vormen - ventilatiekanalen die een onderdeel van de wand vormen - raaplagen in de spouwen en randaansluitingsvoorzieningen - gebouwisolatievoorzieningen - afwerkingen die één geheel vormen met de buitenwand (incl. het voegwerk van schoon metselwerk) - verankeringen en bevestigingsmiddelen - dilatatievoegconstructies - gevelmetselwerken boven 200 mm onder maaiveld - boeiborden"]
[null,"21.2* buitenwanden; constructief","c","Verzameling van constructieve buitenwanden, die de begrenzing vormen van het gebouw, gerekend vanaf de bovenzijde van de funderingsconstructies tot aan de onderzijde van de dakconstructies."]
[null,"21.2* buitenwanden; constructief","c",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"21.2* buitenwanden; constructief","c"]
[null,"21.2* buitenwanden; constructief","c","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, breedte, hoogte, dikte, volume"]
[null,"21.2* buitenwanden; constructief","c",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"]
[null,"21.2* buitenwanden; constructief","c",null,"e","Nokken en sponningen","-","-","-","-","-","-","-","-","-"]
[null,"21.2* buitenwanden; constructief","c",null,"e","Dilataties","-","-","-","-","-","-","-","-","-"]
[null,"21.2* buitenwanden; constructief","c",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
[null,"21.2* buitenwanden; constructief","c",null,"p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"21.2* buitenwanden; constructief","c"]
[null,"21.2* buitenwanden; constructief","c","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"21.2* buitenwanden; constructief","c",null,"g","Entiteit","-","-","-","-","-","-","IfcWall, IfcCurtainWall","IfcClass","-",null,null,"v"]
[null,"21.2* buitenwanden; constructief","c",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"21.2* buitenwanden; constructief","c",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"21.2* buitenwanden; constructief","c",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"21.2* buitenwanden; constructief","c",{"$nulls":14},"v"]
[null,"21.2* buitenwanden; constructief","c","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"!","MAT"]
[null,"21.2* buitenwanden; constructief","c",null,"e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"v",{"$nulls":11},"ifcWall","child","Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[null,"21.2* buitenwanden; constructief","c",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_WallCommon: Loadbearing","true/ false","-","True (constructief)\n\nIndien entiteit IfcCurtainWall: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"v",{"$nulls":11},"ifcWall","child","Pset_WallCommon","LoadBearing","single value","ifcBoolean",null,"Vliesgevel heeft geen dragende functie => dus niet nodig??"]
[null,"21.2* buitenwanden; constructief","c",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-","True (isExternal)",null,"v",{"$nulls":11},"ifcWall","child","Pset_WallCommon","isExternal",null,"ifcBoolean"]
[{"$nulls":29},"ifcCurtainWall","child","Pset_CurtainWallCommon","isExternal",null,"ifcBoolean"]
[null,"21.2* buitenwanden; constructief","c",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"v",{"$nulls":11},"ifcElement","parent","Pset_FireRatingProperties","FireResistanceRating",null,"ifcLabel"]
[null,"21.2* buitenwanden; constructief","c",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"v",{"$nulls":11},"ifcWall","child","Pset_ConcreteElementGeneral","StructuralClass",null,"ifcLabel"]
[{"$nulls":29},"ifcCurtainWall","child","Pset_ConcreteElementGeneral","StructuralClass",null,"ifcLabel"]
[null,"21.2* buitenwanden; constructief","c",null,"e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset\nexclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)",null,"?","In bulding Material "]
[null,"21.2* buitenwanden; constructief","c",null,"p","Wapeningshoeveelheid","-","-","-","-","-","-","wapeningshoeveelheid, benoemen in Custom Pset","wapeningshoeveelheid","kg/m³"]
[null,"21.2* buitenwanden; constructief","c",null,"p","Brandwerendheid hoofddraagconstructie","-","-","-","-","-","-","brandwerendheid tot bezwijken, benoemen in Custom Pset","moment tot bezwijken","minuten"]
[null,"21.2* buitenwanden; constructief","c",null,"p","Weerstandsklasse","-","-","-","-","-","-","SecurityRating benoemen in custom Pset","classificatie","-","Bijv.: WK1 conform NEN 5096\n\nIndien entiteit IfcWall, IfcCurtainWall, IfcPlate, IfcMember: benoemen in Custom Pset omdat 'SecurityRating' geen deel uitmaakt van Common Pset"]
[null,"21.2* buitenwanden; constructief","c","#beton","p","Oppervlakteklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN-EN 13670"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"21.2* buitenwanden; constructief","c"]
[null,"21.2* buitenwanden; constructief","c","Componenten","p","Wapening","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten modelleren, ntb tijdens project; staalkwaliteit en dekking opgeven als Eigenschappen (noot: wanneer geen wapening wordt gemodelleerd, staalkwaliteit en dekking meegeven als Eigenschappen)"]
[null,"21.2* buitenwanden; constructief","c",null,"p","Op te nemen installaties","-","-","-","-","-","-","-","-","-","In overleg met Installateur"]
[null,"21.2* buitenwanden; constructief","c",null,"p","Geveldragers","-","-","-","-","-","-","-","-","-","Modelleren en voorzien van de bovenstaande Eigenschappen"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"21.2* buitenwanden; constructief","c"]
[]
[null,"22.1* binnenwanden; niet constructief","b","22.1* - Binnenwanden; niet constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - traditioneel samengestelde wanden en systeemwanden - brandwerende wanden - schoorstenen, die een onderdeel van de wand vormen - ventilatiekanalen die een onderdeel van de wand vormen - isolaties, die één geheel vormen met het wandsysteem - afwerkingen, die één geheel vormen met het wandsysteem (incl. het voegwerk van schoonmetselwerk) - randaansluitingsvoorzieningen - dilatatievoeg constructies - verankeringen en bevestigingsmiddelen"]
[null,"22.1* binnenwanden; niet constructief","b","Verzameling van niet-constructieve binnenwanden, gerekend vanaf de bovenzijde van de onderliggende vloer tot aan de onderzijde van de bovenliggende (dak)vloer."]
[null,"22.1* binnenwanden; niet constructief","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"22.1* binnenwanden; niet constructief","b"]
[null,"22.1* binnenwanden; niet constructief","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, dikte, hoogte, breedte"]
[null,"22.1* binnenwanden; niet constructief","b",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"]
[null,"22.1* binnenwanden; niet constructief","b",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-"]
[null,"22.1* binnenwanden; niet constructief","b",null,"e","Dilataties","-","-","-","-","-","-","-","-","-"]
[null,"22.1* binnenwanden; niet constructief","b",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"22.1* binnenwanden; niet constructief","b"]
[null,"22.1* binnenwanden; niet constructief","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"22.1* binnenwanden; niet constructief","b",null,"g","Entiteit","-","-","-","-","-","-","IfcWall, IfcCurtainWall","IfcClass","-",null,null,"v"]
[null,"22.1* binnenwanden; niet constructief","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"22.1* binnenwanden; niet constructief","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"22.1* binnenwanden; niet constructief","b",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"22.1* binnenwanden; niet constructief","b",null,"p","Merk","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelReference","-","-","Ten behoeve van onderhoud"]
[null,"22.1* binnenwanden; niet constructief","b",null,"p","Weerstandsklasse","-","-","-","-","-","-","SecurityRating benoemen in custom Pset","classificatie","-","Bijv.: WK1 conform NEN 5096\n\nIndien entiteit IfcWall, IfcCurtainWall, IfcPlate, IfcMember: benoemen in Custom Pset omdat 'SecurityRating' geen deel uitmaakt van Common Pset"]
[null,"22.1* binnenwanden; niet constructief","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"22.1* binnenwanden; niet constructief","b"]
[null,"22.1* binnenwanden; niet constructief","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"!","MAT"]
[null,"22.1* binnenwanden; niet constructief","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"!","MAT"]
[null,"22.1* binnenwanden; niet constructief","b",null,"e","Kleur","-","-","-","-","-","-","-","-","-","(RAL) kleurcode/ omschrijving (in het geval van metselwerk, Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file)",null,"!","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…"]
[null,"22.1* binnenwanden; niet constructief","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_WallCommon: Loadbearing","true/ false","-","False (niet constructief)\n\nIndien entiteit IfcCurtainWall: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"v",{"$nulls":11},"ifcWall","child","Pset_WallCommon","LoadBearing","single value","ifcBoolean"]
[null,"22.1* binnenwanden; niet constructief","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-","False",null,"v",{"$nulls":11},"ifcWall","child","Pset_WallCommon","isExternal",null,"ifcBoolean"]
[{"$nulls":29},"ifcCurtainWall","child","Pset_CurtainWallCommon","isExternal",null,"ifcBoolean"]
[null,"22.1* binnenwanden; niet constructief","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"v",{"$nulls":11},"ifcElement","parent","Pset_FireRatingProperties","FireResistanceRating",null,"ifcLabel"]
[null,"22.1* binnenwanden; niet constructief","b",null,"e","Luchtgeluidisolatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/inkoop/uitvoering.",null,"v",{"$nulls":8},"Geluidswering + Library Part Independent gebruikt",null,null,"ifcWall","child","Pset_WallCommon","AcousticRating",null,"ifcLabel"]
[{"$nulls":26},"Geluidswering + Library Part Independent gebruikt",null,null,"ifcWall","child","Pset_WallCommon","AcousticRating",null,"ifcLabel"]
[null,"22.1* binnenwanden; niet constructief","b",null,"p","Vlakheidsklasse","-","-","-","-","-","-","-","classificatie","-"]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"22.1* binnenwanden; niet constructief","b"]
[null,"22.1* binnenwanden; niet constructief","b","Componenten","p","Op te nemen installaties","-","-","-","-","-","-","-","-","-"]
[null,"22.1* binnenwanden; niet constructief","b",null,"p","Bouwfysische eis - brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument.",{"$nulls":13},"ifcElement","parent","Pset_FireRatingProperties","FireResistanceRating",null,"ifcLabel"]
[null,"22.1* binnenwanden; niet constructief","b",null,"p","Bouwfysische eis - luchtgeluidisoalatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"22.1* binnenwanden; niet constructief","b"]
[]
[null,"22.2* binnenwanden; constructief","c","22.2* - Binnenwanden; constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - traditioneel samengestelde wanden en systeemwanden - brandwerende wanden - schoorstenen, die een onderdeel van de wand vormen - ventilatiekanalen die een onderdeel van de wand vormen - isolaties, die één geheel vormen met het wandsysteem - afwerkingen, die één geheel vormen met het wandsysteem (incl. het voegwerk van schoonmetselwerk) - randaansluitingsvoorzieningen - dilatatievoeg constructies - verankeringen en bevestigingsmiddelen"]
[null,"22.2* binnenwanden; constructief","c","Verzameling van constructieve binnenwanden, gerekend vanaf de bovenzijde van de onderliggende vloer tot aan de onderzijde van de bovenliggende (dak)vloer."]
[null,"22.2* binnenwanden; constructief","c",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"22.2* binnenwanden; constructief","c"]
[null,"22.2* binnenwanden; constructief","c","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, breedte, dikte, volume"]
[null,"22.2* binnenwanden; constructief","c",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"]
[null,"22.2* binnenwanden; constructief","c",null,"e","Dilataties","-","-","-","-","-","-","-","-","-"]
[null,"22.2* binnenwanden; constructief","c",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
[null,"22.2* binnenwanden; constructief","c",null,"p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"22.2* binnenwanden; constructief","c"]
[null,"22.2* binnenwanden; constructief","c","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"22.2* binnenwanden; constructief","c",null,"g","Entiteit","-","-","-","-","-","-","IfcWall, IfcCurtainWall","IfcClass","-",null,null,"v"]
[null,"22.2* binnenwanden; constructief","c",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"22.2* binnenwanden; constructief","c",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"22.2* binnenwanden; constructief","c",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"22.2* binnenwanden; constructief","c"]
[null,"22.2* binnenwanden; constructief","c","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"!","MAT"]
[null,"22.2* binnenwanden; constructief","c",null,"e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"v",{"$nulls":11},"ifcWall","child","Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[null,"22.2* binnenwanden; constructief","c",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"!","MAT"]
[null,"22.2* binnenwanden; constructief","c",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_WallCommon: Loadbearing","true/ false","-","True (constructief)\n\nIndien entiteit IfcCurtainWall: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"v",{"$nulls":11},"ifcWall","child","Pset_WallCommon","LoadBearing",null,"ifcBoolean",null,"Vliesgevel heeft geen dragende functie => dus niet nodig??"]
[null,"22.2* binnenwanden; constructief","c",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-","False",null,"v"]
[null,"22.2* binnenwanden; constructief","c",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"v",{"$nulls":11},"ifcElement","parent","Pset_FireRatingProperties","FireResistanceRating",null,"ifcLabel"]
[null,"22.2* binnenwanden; constructief","c",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"v",{"$nulls":11},"ifcWall","child","Pset_ConcreteElementGeneral","StructuralClass",null,"ifcLabel"]
[{"$nulls":29},"ifcCurtainWall","child","Pset_ConcreteElementGeneral","StructuralClass",null,"if"]
[null,"22.2* binnenwanden; constructief","c",null,"e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset\nexclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)",null,"?","Building material specifiek?"]
[null,"22.2* binnenwanden; constructief","c",null,"p","Wapeningshoeveelheid","-","-","-","-","-","-","wapeningshoeveelheid, benoemen in Custom Pset","wapeningshoeveelheid","kg/m³"]
[null,"22.2* binnenwanden; constructief","c",null,"p","Brandwerendheid hoofddraagconstructie","-","-","-","-","-","-","brandwerendheid tot bezwijken, benoemen in Custom Pset","moment tot bezwijken","minuten"]
[null,"22.2* binnenwanden; constructief","c",null,"p","Weerstandsklasse","-","-","-","-","-","-","SecurityRating benoemen in custom Pset","classificatie","-","Bijv.: WK1 conform NEN 5096\n\nIndien entiteit IfcWall, IfcCurtainWall, IfcPlate, IfcMember: benoemen in Custom Pset omdat 'SecurityRating' geen deel uitmaakt van Common Pset"]
[null,"22.2* binnenwanden; constructief","c","#beton","p","Oppervlakteklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN-EN 13670"]
[null,"22.2* binnenwanden; constructief","c",null,"p","Vlakheidsklasse","-","-","-","-","-","-","-","classificatie","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"22.2* binnenwanden; constructief","c"]
[null,"22.2* binnenwanden; constructief","c","Componenten","p","Wapening","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten modelleren, ntb tijdens project; staalkwaliteit en dekking opgeven als Eigenschappen (noot: wanneer geen wapening wordt gemodelleerd, staalkwaliteit en dekking meegeven als Eigenschappen)"]
[null,"22.2* binnenwanden; constructief","c",null,"p","Op te nemen installaties","-","-","-","-","-","-","-","-","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"22.2* binnenwanden; constructief","c"]
[]
[null,"23.1* vloeren; niet constructief","b","23.1* - Vloeren; niet constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - beloopbare plafonds ten behoeve van installaties - wandaansluitingsvoorzieningen - tot de vloer behorende balken en verzwaringen - verankeringen en bevestigingsmiddelen - afwerkingen, die één geheel vormen met de vloerconstructie - gebouwisolatievoorzieningen - dilatatievoegconstructies"]
[null,"23.1* vloeren; niet constructief","b","Verzameling van niet-constructieve vrijdragende vloeren, inclusief galerijvloeren, balkons en bordessen, gerekend tot aan de binnenzijde van de buitenwanden."]
[null,"23.1* vloeren; niet constructief","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"23.1* vloeren; niet constructief","b"]
[null,"23.1* vloeren; niet constructief","b","Geometrie","g","Vorm buitenste profilering","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, omtrek, afschot"]
[null,"23.1* vloeren; niet constructief","b",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"]
[null,"23.1* vloeren; niet constructief","b",null,"e","Dilataties","-","-","-","-","-","-","-","-","-"]
[null,"23.1* vloeren; niet constructief","b",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"23.1* vloeren; niet constructief","b"]
[null,"23.1* vloeren; niet constructief","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"23.1* vloeren; niet constructief","b",null,"g","Entiteit","-","-","-","-","-","-","IfcSlab, IfcPlate","IfcClass","-",null,null,"v"]
[null,"23.1* vloeren; niet constructief","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"23.1* vloeren; niet constructief","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"23.1* vloeren; niet constructief","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"23.1* vloeren; niet constructief","b"]
[null,"23.1* vloeren; niet constructief","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"!","MAT"]
[null,"23.1* vloeren; niet constructief","b",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"?","bespreken: bij materiaal plaatsen?"]
[null,"23.1* vloeren; niet constructief","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"!","MAT"]
[null,"23.1* vloeren; niet constructief","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","False (niet constructief)",null,"v",{"$nulls":11},"ifcSlab","child","Pset_SlabCommon","LoadBearing",null,"ifcBoolean"]
[{"$nulls":29},"ifcPlate","child","Pset_PlateCommon","LoadBearing",null,"ifcBoolean"]
[null,"23.1* vloeren; niet constructief","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-",null,null,"v",{"$nulls":11},"ifcSlab","child","Pset_SlabCommon","IsExternal",null,"ifcBoolean"]
[{"$nulls":29},"ifcPlate","child","Pset_PlateCommon","IsExternal",null,"ifcBoolean"]
[null,"23.1* vloeren; niet constructief","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"v",{"$nulls":11},"ifcElement","parent","Pset_FireRatingProperties","FireResistanceRating",null,"ifcLabel"]
[null,"23.1* vloeren; niet constructief","b",null,"p","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset"]
[null,"23.1* vloeren; niet constructief","b",null,"p","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset\nexclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)"]
[null,"23.1* vloeren; niet constructief","b",null,"p","Wapeningshoeveelheid","-","-","-","-","-","-","wapeningshoeveelheid, benoemen in Custom Pset","wapeningshoeveelheid","kg/m³"]
[null,"23.1* vloeren; niet constructief","b","#beton","p","Oppervlakteklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN-EN 13670"]
[null,"23.1* vloeren; niet constructief","b",null,"p","Vlakheidsklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN 2747"]
[null,"23.1* vloeren; niet constructief","b",null,"p","Brandwerendheid hoofddraagconstructie","-","-","-","-","-","-","brandwerendheid tot bezwijken, benoemen in Custom Pset","moment tot bezwijken","minuten"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"23.1* vloeren; niet constructief","b",{"$nulls":14},"v"]
[null,"23.1* vloeren; niet constructief","b","Componenten","e","Isolatie","-","-","-","-","-","-","-","-","-","Tevens aangeven: isolatiewaarde en brandklasse"]
[null,"23.1* vloeren; niet constructief","b",null,"p","Toog/ zeeg","-","-","-","-","-","-","-","-","-","Ruimtereserveringsobject modelleren om rekening te kunnen houden met het effect van toog/ zeeg"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"23.1* vloeren; niet constructief","b"]
[]
[null,"23.2* vloeren; constructief","c","23.2* - Vloeren; constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - wandaansluitingsvoorzieningen - tot de vloer behorende balken en verzwaringen - verankeringen en bevestigingsmiddelen - afwerkingen, die één geheel vormen met de vloerconstructie - gebouwisolatievoorzieningen - dilatatievoegconstructies"]
[null,"23.2* vloeren; constructief","c","Verzameling van constructieve vrijdragende vloeren, inclusief galerijvloeren, balkons en bordessen, gerekend tot aan de binnenzijde van de buitenwanden, echter met inbegrip van de oplegvlakken. \nNoot: in afwijking van definitie NL-SfB worden hier de galerijvloeren, balkons en bordessen buiten bschouwing gelaten."]
[null,"23.2* vloeren; constructief","c",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"23.2* vloeren; constructief","c"]
[null,"23.2* vloeren; constructief","c","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Druklaag en afwerklaag separaat modelleren.\nUit vorm moet hetvolgende bepaald kunnen worden: \nomtrek, oppervlakte, dikte, volume, afschot"]
[null,"23.2* vloeren; constructief","c",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"]
[null,"23.2* vloeren; constructief","c",null,"e","Nokken en sponningen","-","-","-","-","-","-","-","-","-","In verband met oplegging"]
[null,"23.2* vloeren; constructief","c",null,"e","Dilataties","-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c"]
[null,"23.2* vloeren; constructief","c","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"23.2* vloeren; constructief","c",null,"g","Entiteit","-","-","-","-","-","-","IfcSlab","IfcClass","-",null,null,"v"]
[null,"23.2* vloeren; constructief","c",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"23.2* vloeren; constructief","c",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"23.2* vloeren; constructief","c",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c"]
[null,"23.2* vloeren; constructief","c","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar"]
[null,"23.2* vloeren; constructief","c","#beton","e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"v",{"$nulls":11},"ifcSlab","child","Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[null,"23.2* vloeren; constructief","c",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_SlabCommon: Loadbearing","true/ false","-","True (constructief)\n\nIndien entiteit IfcBuildingElementProxy: benoemen in Custom Pset omdat Common Pset in Ifc 2x3 niet bestaat",null,"v",{"$nulls":11},"ifcSlab","child","Pset_SlabCommon","LoadBearing",null,"ifcBoolean"]
[null,"23.2* vloeren; constructief","c",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_SlabCommon: IsExternal","true/ false","-","Indien entiteit IfcBuildingElementProxy: benoemen in Custom Pset omdat Pset_BuildingElementProxyCommon in Ifc 2x3 niet bestaat",null,"v",{"$nulls":11},"ifcSlab","child","Pset_SlabCommon","IsExternal",null,"ifcBoolean"]
[null,"23.2* vloeren; constructief","c",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_SlabCommon: FireRating","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering., volgens separaak afsprakendocument. 0, 20, 30, 60, etc... (WBDBO).\nIndien entiteit IfcBuildingElementProxy: benoemen in Custom Pset omdat Pset_IfcBuildingElementProxyCommon in Ifc 2x3 niet bestaat",null,"v",{"$nulls":11},"ifcElement","parent","Pset_FireRatingProperties","FireResistanceRating",null,"ifcLabel"]
[null,"23.2* vloeren; constructief","c",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"v",{"$nulls":11},"ifcSlab","child","Pset_ConcreteElementGeneral","StructuralClass",null,"ifcLabel"]
[null,"23.2* vloeren; constructief","c",null,"e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset\nexclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)",null,"?","Building material specifiek?"]
[null,"23.2* vloeren; constructief","c",null,"p","Wapeningshoeveelheid","-","-","-","-","-","-","wapeningshoeveelheid, benoemen in Custom Pset","wapeningshoeveelheid","kg/m³"]
[null,"23.2* vloeren; constructief","c",null,"p","Warmtedoorgangscoefficient","-","-","-","-","-","-","Pset_SlabCommon: ThermalTransmittance","U-waarde","W/ m².K","Warmteweerstand R = 1/ U\n\nIndien entiteit IfcBuildingElementProxy: benoemen in Custom Pset omdat Pset_BuildingElementProxyCommon in Ifc 2x3 niet bestaat"]
[null,"23.2* vloeren; constructief","c",null,"p","Brandwerendheid hoofddraagconstructie","-","-","-","-","-","-","brandwerendheid tot bezwijken, benoemen in Custom Pset","moment tot bezwijken","minuten"]
[null,"23.2* vloeren; constructief","c",null,"p","Overspanningsrichting","-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c","#beton","p","Oppervlakteklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN-EN 13670"]
[null,"23.2* vloeren; constructief","c",null,"p","Vlakheidsklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN 2747"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c"]
[null,"23.2* vloeren; constructief","c","Componenten","p","Wapening","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten modelleren, ntb tijdens project; staalkwaliteit en dekking opgeven als Eigenschappen (noot: wanneer geen wapening wordt gemodelleerd, staalkwaliteit en dekking meegeven als Eigenschappen)"]
[null,"23.2* vloeren; constructief","c",null,"p","Raveelijzers","-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c",null,"p","Randkist","-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c",null,"p","Koudebrugonderbrekingen","-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c",null,"p","Ankers/ isokorven","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten, ntb tijdens project; aangeven: staalkwaliteit en dekking"]
[null,"23.2* vloeren; constructief","c",null,"p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c",null,"p","Toog/ zeeg","-","-","-","-","-","-","-","-","-","Ruimtereserveringsobject modelleren om rekening te kunnen houden met het effect van toog/ zeeg"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c"]
[]
[null,"24.1* trappen en hellingen; trappen","b","24.1* - Trappen en hellingen; trappen",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - randaansluitingsvoorzieningen - verankeringen en bevestigingsmiddelen - afwerkingen die één geheel vormen met de trapconstructie"]
[null,"24.1* trappen en hellingen; trappen","b","Verzameling van trappen, zowel binnen als buiten het gebouw, inclusief de bijbehorende bordessen."]
[null,"24.1* trappen en hellingen; trappen","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"24.1* trappen en hellingen; trappen","b"]
[null,"24.1* trappen en hellingen; trappen","b","Geometrie","g","Vorm buitenste profilering","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \ntotale optrede, totale aantrede, totale breedte, volume, stootbord, trapbomen, schrobrand, welstuk, nokken"]
[null,"24.1* trappen en hellingen; trappen","b",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"]
[null,"24.1* trappen en hellingen; trappen","b",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"24.1* trappen en hellingen; trappen","b"]
[null,"24.1* trappen en hellingen; trappen","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"24.1* trappen en hellingen; trappen","b",null,"g","Entiteit","-","-","-","-","-","-","IfcStair, IfcStairFlight, IfcRailing, IfcSlab, IfcMember","IfcClass","-",null,null,"v"]
[null,"24.1* trappen en hellingen; trappen","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"24.1* trappen en hellingen; trappen","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"24.1* trappen en hellingen; trappen","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"24.1* trappen en hellingen; trappen","b"]
[null,"24.1* trappen en hellingen; trappen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"!","MAT"]
[null,"24.1* trappen en hellingen; trappen","b",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving). Bij meerdere afwerkingen Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"!","bespreken: bij materiaal plaatsen?"]
[null,"24.1* trappen en hellingen; trappen","b",null,"e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"v",{"$nulls":11},"ifcStair",null,"Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[{"$nulls":29},"ifcStairFlight",null,"Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[{"$nulls":29},"ifcRailing",null,"Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[{"$nulls":29},"ifcSlab",null,"Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[{"$nulls":29},"ifcMember",null,"Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[null,"24.1* trappen en hellingen; trappen","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","Indien entiteit IfcStair, IfcStairFlight, IfcRailing: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"x","IFC 4niet in buildingsmart opgenomen - custom pset",{"$nulls":6},"trap",null,null,null,"ifcStair",{"$nulls":6},"niet in BS "]
[{"$nulls":29},"ifcStairFlight",{"$nulls":6},"niet in BS "]
[{"$nulls":29},"ifcRailing",{"$nulls":6},"niet in BS "]
[{"$nulls":29},"ifcSlab",null,"Pset_<entiteit>Common","LoadBearing",null,"ifcBoolean"]
[{"$nulls":29},"ifcMember",null,"Pset_<entiteit>Common","LoadBearing",null,"ifcBoolean"]
[null,"24.1* trappen en hellingen; trappen","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-","Indien entiteit IfcStairFlight: benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset",null,"x","IFC 4 niet in buildingsmart opgenomen - custom pset",{"$nulls":6},"trap",null,null,null,"ifcStair",null,"Pset_<entiteit>Common","isExternal",null,"ifcBoolean"]
[{"$nulls":29},"ifcStairFlight",{"$nulls":6},"niet in BS"]
[{"$nulls":29},"ifcRailing",null,"Pset_<entiteit>Common","isExternal",null,"ifcBoolean"]
[{"$nulls":29},"ifcSlab",null,"Pset_<entiteit>Common","isExternal",null,"ifcBoolean"]
[{"$nulls":29},"ifcMember",null,"Pset_<entiteit>Common","isExternal",null,"ifcBoolean"]
[]
[null,"24.1* trappen en hellingen; trappen","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering., volgens separaat afsprakendocument. 0, 20, 30, 60, etc... (WBDBO)\nIndien entiteit IfcStairFlight, IfcRailing: benoemen in Custom Pset omdat 'FireRating' geen deel uitmaakt van Common Pset",null,"v",{"$nulls":11},"ifcElement","parent","Pset_FireRatingProperties","FireResistanceRating",null,"ifcLabel"]
[null,"24.1* trappen en hellingen; trappen","b","#beton","e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Zowel van treden als bordes. Bij meerdere afwerkingen Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"!","bespreken, hierop anticiperen? MAT"]
[null,"24.1* trappen en hellingen; trappen","b",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"v",{"$nulls":11},"ifcStair",null,"Pset_ConcreteElementGeneral","StructuralClass",null,"ifcLabel"]
[{"$nulls":29},"ifcStairFlight",null,"Pset_ConcreteElementGeneral","StructuralClass",null,"ifcLabel"]
[{"$nulls":29},"ifcRailing",null,"Pset_ConcreteElementGeneral","StructuralClass",null,"ifcLabel"]
[{"$nulls":29},"ifcSlab",null,"Pset_ConcreteElementGeneral","StructuralClass",null,"ifcLabel"]
[{"$nulls":29},"ifcMember",null,"Pset_ConcreteElementGeneral","StructuralClass",null,"ifcLabel"]
[]
[null,"24.1* trappen en hellingen; trappen","b","#beton","e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset\nexclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)",null,"?","Onder Building Material plaatsen?"]
[null,"24.1* trappen en hellingen; trappen","b","#staal","e","Staalkwaliteit","-","-","x","-","-","-","staalkwaliteit, benoemen in Custom Pset","classificatie","-","vb.: S235, S355",null,"?","bij BM te plaatsen? Trap geef je ook BM mee?",{"$nulls":6},"BM",null,"Staalkwaliteit",null,"ifcStair, ifcRailing. ifcSlab, ifcStairflight",null,"Pset_SteelRequirements","SteelQuality","enumerated value","ifcLabel"]
[null,"24.1* trappen en hellingen; trappen","b","#staal","e","Conservering","-","-","-","-","-","-","-","-","-"]
[null,"24.1* trappen en hellingen; trappen","b",null,"p","Optrede","-","-","-","-","-","-","Pset_StairCommon: RiserHeight","hoogte","mm"]
[null,"24.1* trappen en hellingen; trappen","b",null,"p","Aantrede","-","-","-","-","-","-","Pset_StairCommon: TreadLength","diepte","mm"]
[null,"24.1* trappen en hellingen; trappen","b","#beton","p","Oppervlakteklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN-EN 13670"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"24.1* trappen en hellingen; trappen","b"]
[null,"24.1* trappen en hellingen; trappen","b","Componenten","p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
[null,"24.1* trappen en hellingen; trappen","b",null,"p","Randaansluitingsvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"24.1* trappen en hellingen; trappen","b"]
[]
[null,"24.2* trappen en hellingen; hellingen","b","24.2* - Trappen en hellingen; hellingen",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - randaansluitingsvoorzieningen - verankeringen en bevestigingsmiddelen - afwerkingen die één geheel vormen met de hellingconstructie"]
[null,"24.2* trappen en hellingen; hellingen","b","Verzameling van beloopbare en berijdbare hellingen, inclusief de bijbehorende bordessen."]
[null,"24.2* trappen en hellingen; hellingen","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"24.2* trappen en hellingen; hellingen","b"]
[null,"24.2* trappen en hellingen; hellingen","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \ntotale breedte, volume"]
[null,"24.2* trappen en hellingen; hellingen","b",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"]
[null,"24.2* trappen en hellingen; hellingen","b",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"24.2* trappen en hellingen; hellingen","b"]
[null,"24.2* trappen en hellingen; hellingen","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"24.2* trappen en hellingen; hellingen","b",null,"g","Entiteit","-","-","-","-","-","-","IfcRamp, IfcSlab","IfcClass","-",null,null,"v"]
[null,"24.2* trappen en hellingen; hellingen","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"24.2* trappen en hellingen; hellingen","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"24.2* trappen en hellingen; hellingen","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"24.2* trappen en hellingen; hellingen","b"]
[null,"24.2* trappen en hellingen; hellingen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"!","MAT"]
[null,"24.2* trappen en hellingen; hellingen","b",null,"e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"v"]
[null,"24.2* trappen en hellingen; hellingen","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_SlabCommon: Loadbearing","true/ false","-","Indien entiteit IfcRamp: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"x","IFC 4 niet in buildingsmart opgenomen - custom pset",{"$nulls":6},"hellingsbaan",null,null,null,"ifcRamp",null,"?","isLoadbearing","single value","ifcBoolean",null,"niet opgenomen in BS"]
[{"$nulls":29},"ifcSlab","child","Pset<entiteit>Common","isLoadbearing",null,"ifcBoolean"]
[null,"24.2* trappen en hellingen; hellingen","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-",null,null,"v"]
[null,"24.2* trappen en hellingen; hellingen","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"v",{"$nulls":11},"ifcElement","parent","Pset_FireRatingProperties","FireResistanceRating",null,"ifcLabel"]
[null,"24.2* trappen en hellingen; hellingen","b","#beton","e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Zowel van treden als bordes. Bij meerdere afwerkingen Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"!","bespreken, hierop anticiperen? MAT"]
[null,"24.2* trappen en hellingen; hellingen","b",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"v",{"$nulls":11},"ifcRamp","child","Pset_ConcreteElementGeneral","StructuralClass","single value","ifcLabel"]
[{"$nulls":29},"ifcSlab","child","Pset_ConcreteElementGeneral","StructuralClass",null,"ifcLabel"]
[null,"24.2* trappen en hellingen; hellingen","b","#beton","e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset\nexclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)",null,"?","BuildingMaterial niveau?"]
[null,"24.2* trappen en hellingen; hellingen","b","#staal","e","Staalkwaliteit","-","-","-","-","-","-","staalkwaliteit, benoemen in Custom Pset","classificatie","-","vb.: S235, S355",null,"x","strenghtclass (IFC 4 bestaat binnen Pset_ConcreteElementGeneral)","x","v",{"$nulls":4},"BM",null,"Sterkteklasse",null,"ifcRamp, ifcSlab",null,"CPset_SteelRequirements","Strengthclass","enumerated value","ifcIdentifier"]
[null,"24.2* trappen en hellingen; hellingen","b","#staal","e","Conservering","-","-","-","-","-","-","-","-","-"]
[null,"24.2* trappen en hellingen; hellingen","b","#beton","p","Oppervlakteklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN-EN 13670"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"24.2* trappen en hellingen; hellingen","b"]
[null,"24.2* trappen en hellingen; hellingen","b","Componenten","p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
[null,"24.2* trappen en hellingen; hellingen","b",null,"p","Randaansluitingsvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"24.2* trappen en hellingen; hellingen","b"]
[]
[null,"27.1* daken; niet constructief","b","27.1* - Daken; niet constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - dakvloeren, dakoverstekken en luifels - kleine boeiboorden als dakrandafwerking - gootconstructies en dakranden - isolaties die één geheel vormen met de dakconstructie - isolaties die tevens het afschot vormen - afschotlagen en mastiekranden - dilatatievoegconstructies"]
[null,"27.1* daken; niet constructief","b","Verzameling van niet-constructieve daken, zowel hellend als vlak, die de begrenzing van het gebouw aan de bovenzijde vormen, gerekend vanaf de binnenzijde en vanaf de bovenzijde van de buitenwanden."]
[null,"27.1* daken; niet constructief","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"27.1* daken; niet constructief","b"]
[null,"27.1* daken; niet constructief","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, lengte, breedte, hellingshoek"]
[null,"27.1* daken; niet constructief","b",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"?","bespreken"]
[null,"27.1* daken; niet constructief","b",null,"e","Dilataties","-","-","-","-","-","-","-","-","-"]
[null,"27.1* daken; niet constructief","b",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"27.1* daken; niet constructief","b"]
[null,"27.1* daken; niet constructief","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"27.1* daken; niet constructief","b",null,"g","Entiteit","-","-","-","-","-","-","IfcRoof, IfcSlab","IfcClass","-",null,null,"v"]
[null,"27.1* daken; niet constructief","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"27.1* daken; niet constructief","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"27.1* daken; niet constructief","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"27.1* daken; niet constructief","b"]
[null,"27.1* daken; niet constructief","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"!","MAT"]
[null,"27.1* daken; niet constructief","b",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"!","bespreken - bij MAT/BM?"]
[null,"27.1* daken; niet constructief","b",null,"e","Afwerking","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar)",null,"!","bespreken - bij MAT/BM?"]
[null,"27.1* daken; niet constructief","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_SlabCommon: Loadbearing","true/ false","-","False (niet constructief)\n\nIndien entiteit IfcRoof, IfcFlowSegment, IfcBuildingElementProxy: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"v",{"$nulls":11},"ifcSlab","child","Pset_<entiteit>Common","Loadbearing",null,"ifcBoolean"]
[{"$nulls":29},"ifcRoof",null,null,"Loadbearing",null,"ifcBoolean",null,"niet in BS"]
[null,"27.1* daken; niet constructief","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_SlabCommon: IsExternal","true/ false","-","Indien entiteit IfcRoof, IfcSlab, IfcFlowSegment, IfcBuildingElementProxy: benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset",null,"v",{"$nulls":11},"ifcSlab","child","Pset_<entiteit>Common","isExternal",null,"ifcBoolean"]
[{"$nulls":29},"ifcRoof","child","Pset_<entiteit>Common","isExternal",null,"ifcBoolean"]
[null,"27.1* daken; niet constructief","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering., volgens separaat afsprakendocument. 0, 20, 30, 60, etc... (WBDBO)\nIndien entiteit IfcFlowSegment, IfcBuildingElementProxy: benoemen in Custom Pset omdat 'FireRating' geen deel uitmaakt van Common Pset",null,"v",{"$nulls":11},"ifcElement","parent","Pset_FireRatingProperties","FireResistanceRating",null,"ifcLabel"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"27.1* daken; niet constructief","b"]
[null,"27.1* daken; niet constructief","b","Componenten","e","Isolatie","-","-","-","-","-","-","-","-","-","Afschot modelleren; tevens aangeven: isolatiewaarde en brandklasse",null,"?","isolatie waarde => BM, brandklasses reeds toegevoegd aan ifcSlab en ifcRoof",{"$nulls":6},"BM","Thermal Conductivity",null,null,"ifcRoof, ifcSlab"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"27.1* daken; niet constructief","b"]
[]
[null,"27.2* daken; constructief","c","27.2* - Daken; constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - dakvloeren, dakoverstekken en luifels - kleine boeiboorden als onderdeel van de dakrandafwerking - gootconstructies en dakranden - isolaties die één geheel vormen met de dakconstructie - isolaties die tevens het afschot vormen - afschotlagen en mastiekranden - dilatatievoegconstructies"]
[null,"27.2* daken; constructief","c","Verzameling van constructieve daken, zowel hellend als vlak, die de begrenzing van het gebouw aan de bovenzijde vormen, gerekend vanaf de binnenzijde, echter met inbegrip van de oplegvlakken en vanaf de bovenzijde van de buitenwanden."]
[null,"27.2* daken; constructief","c",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"27.2* daken; constructief","c"]
[null,"27.2* daken; constructief","c","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, lengte, breedte, hellingshoek, volume"]
[null,"27.2* daken; constructief","c",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"]
[null,"27.2* daken; constructief","c",null,"e","Nokken en sponningen","-","-","-","-","-","-","-","-","-","In verband met oplegging"]
[null,"27.2* daken; constructief","c",null,"e","Dilataties","-","-","-","-","-","-","-","-","-"]
[null,"27.2* daken; constructief","c",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"27.2* daken; constructief","c"]
[null,"27.2* daken; constructief","c","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"27.2* daken; constructief","c",null,"g","Entiteit","-","-","-","-","-","-","IfcRoof, IfcSlab, IfcSlab","IfcClass","-",null,null,"v"]
[null,"27.2* daken; constructief","c",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"27.2* daken; constructief","c",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"27.2* daken; constructief","c",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"27.2* daken; constructief","c"]
[null,"27.2* daken; constructief","c","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"!","MAT","x","v"]
[null,"27.2* daken; constructief","c","#beton","e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"?","Op classificatie entiteit of op basis van BM? Classificatie laten berekenen aan hand met een expressie op basis van BM gewicht kg per m3? -WORKAROUND","x","v (pset aanwezig - prop niet)",{"$nulls":4},"Dak",null,"Massa",null,"ifcRoof, ifcSlab ",null,"Pset_PrecastConcreteElementGeneral","ElementWeight","Single Value","ifcMassMeasure"]
[null,"27.2* daken; constructief","c",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_SlabCommon: Loadbearing","true/ false","-","True (constructief)\n\nIndien entiteit IfcRoof, IfcFlowSegment, IfcBuildingElementProxy: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"v",{"$nulls":11},"ifcSlab","child","Pset_<entiteit>Common","Loadbearing",null,"ifcBoolean"]
[{"$nulls":29},"ifcRoof",null,null,"Loadbearing",null,"ifcBoolean",null,"niet in BS"]
[null,"27.2* daken; constructief","c",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_SlabCommon: IsExternal","true/ false","-","Indien entiteit IfcRoof, IfcSlab, IfcFlowSegment, IfcBuildingElementProxy: benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset",null,"v",{"$nulls":11},"ifcSlab","child","Pset_<entiteit>Common","isExternal",null,"ifcBoolean"]
[{"$nulls":29},"ifcRoof","child","Pset_<entiteit>Common","isExternal",null,"ifcBoolean"]
[null,"27.2* daken; constructief","c",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering., volgens separaat afsprakendocument. 0, 20, 30, 60, etc... (WBDBO)\nIndien entiteit IfcFlowSegment, IfcBuildingElementProxy: benoemen in Custom Pset omdat 'FireRating' geen deel uitmaakt van Common Pset",null,"v",{"$nulls":11},"ifcElement","parent","Pset_FireRatingProperties","FireResistanceRating",null,"ifcLabel"]
[null,"27.2* daken; constructief","c",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"v","BM = Sterkteklasse property aanwezig","V (structural class aanwezig - onder PsetConcreteElementGeneral)","V (structural class aanwezig - onder PsetConcreteElementGeneral)",{"$nulls":8},"ifcSlab","child","Pset_ConcreteElementGeneral","StructuralClass",null,"ifcLabel"]
[{"$nulls":29},"ifcRoof","child","Pset_ConcreteElementGeneral","StructuralClass",null,"ifcLabel"]
[null,"27.2* daken; constructief","c",null,"e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset\nexclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)",null,"?","staat niet in building smart onder de entiteiten en deze Pset - ook niet in onze AC entiteiten, BM heeft wel milieuklasse "]
[null,"27.2* daken; constructief","c",null,"p","Wapeningshoeveelheid","-","-","-","-","-","-","wapeningshoeveelheid, benoemen in Custom Pset","wapeningshoeveelheid","kg/m³"]
[null,"27.2* daken; constructief","c",null,"p","Warmtedoorgangscoefficient","-","-","-","-","-","-","Pset_SlabCommon: ThermalTransmittance","U-waarde","W/ m².K","Warmteweerstand R = 1/ U\n\nIndien entiteit IfcRoof, IfcFlowSegment, IfcBuildingElementProxy: benoemen in Custom Pset omdat 'ThermalTransmittance' geen deel uitmaakt van Common Pset"]
[null,"27.2* daken; constructief","c",null,"p","Brandwerendheid hoofddraagconstructie","-","-","-","-","-","-","brandwerendheid tot bezwijken, benoemen in Custom Pset","moment tot bezwijken","minuten"]
[null,"27.2* daken; constructief","c",null,"p","Overspanningsrichting","-","-","-","-","-","-","-","-","-"]
[null,"27.2* daken; constructief","c","#beton","p","Oppervlakteklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN-EN 13670"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"27.2* daken; constructief","c"]
[null,"27.2* daken; constructief","c","Componenten","p","Wapening","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten modelleren, ntb tijdens project; staalkwaliteit en dekking opgeven als Eigenschappen (noot: wanneer geen wapening wordt gemodelleerd, staalkwaliteit en dekking meegeven als Eigenschappen)"]
[null,"27.2* daken; constructief","c",null,"p","Raveelijzers","-","-","-","-","-","-","-","-","-"]
[null,"27.2* daken; constructief","c",null,"p","Randkist","-","-","-","-","-","-","-","-","-"]
[null,"27.2* daken; constructief","c",null,"p","Koudebrugonderbrekingen","-","-","-","-","-","-","-","-","-"]
[null,"27.2* daken; constructief","c",null,"p","Ankers/ isokorven","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten, ntb tijdens project; aangeven: staalkwaliteit en dekking"]
[null,"27.2* daken; constructief","c",null,"p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"27.2* daken; constructief","c"]
[]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","28.1* - Hoofddraagconstructies; kolommen en liggers",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - de volledige prefabricage en montage van de constructie - de verankeringen en bevestigingsmiddelen - conserveringsbehandelingen"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","Verzameling van hoofddraagconstructies van het gebouw indien deze voornamelijk uit kolommen, liggers en/of spanten bestaan en door constructieontwerp en/of uitvoeringsmethode niet te splitsen zijn in de groepen (21.0) t/m (27.0). Er zijn 3 hoofdgroepen op basis van materiaal te onderscheiden namelijk: IHWG en prefab beton; staal; hout."]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","Geometrie","g","Vorm buitenste profilering","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nbreedte, hoogte, lengte, diameter, volume, flensdikte, lijfdikte, profieltype",null,"?"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,null,"apart document/afspraak"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","#IHWG  #prefab beton","e","Nokken en sponningen","-","-","-","-","-","-","-","-","-","In verband met oplegging",null,"?"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"e","Dilataties","-","-","-","-","-","-","-","-","-"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"?"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"g","Entiteit","-","-","-","-","-","-","IfcBeam, IfcColumn,IfcMember","IfcClass","-",null,null,"v"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p","Kolomnummer","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelLabel","-","-"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p","Liggernummer","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelLabel","-","-"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"!","MAT","x","v"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"v",{"$nulls":11},"ifcBeam",null,"Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[{"$nulls":29},"ifcColumn",null,"Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[{"$nulls":29},"ifcMember",null,"Pset_PrecastConcreteElementGeneral","ElementWeight",null,"ifcMassMeasure"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"!","MAT"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","#staal","e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"!","MAT"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","#staal","e","Conservering","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","True (constructief)",null,"v",{"$nulls":11},"ifcBeam",null,"Pset_<entiteit>Common","LoadBearing",null,"ifcBoolean"]
[{"$nulls":29},"ifcColumn",null,"Pset_<entiteit>Common","LoadBearing",null,"ifcBoolean"]
[{"$nulls":29},"ifcMember",null,"Pset_<entiteit>Common","LoadBearing",null,"ifcBoolean"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-",null,null,"v",{"$nulls":11},"ifcBeam",null,"Pset_<entiteit>Common","isExternal",null,"ifcBoolean"]
[{"$nulls":29},"ifcColumn",null,"Pset_<entiteit>Common","isExternal",null,"ifcBoolean"]
[{"$nulls":29},"ifcMember",null,"Pset_<entiteit>Common","isExternal",null,"ifcBoolean"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"v",{"$nulls":11},"ifcElement","parent","Pset_FireRatingProperties","FireResistanceRating",null,"ifcLabel"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"v","BM = Sterkteklasse property aanwezig","V (structural class aanwezig - onder PsetConcreteElementGeneral)","V (structural class aanwezig - onder PsetConcreteElementGeneral)"]
[]
[]
[]
[]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","#beton","e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset\nexclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)",null,"?","Building material ?"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","#staal","e","Staalkwaliteit","-","-","-","-","-","-","staalkwaliteit, benoemen in Custom Pset","classificatie","-","vb.: S235, S355",null,"x","Maar kan natuurlijk ook op BM niveau? ",{"$nulls":10},"ifcBeam",null,null,"Structural",null,"ifcLabel",null,"enkel voor Beton voorzien in Pset (Pset ConcreteElement General"]
[{"$nulls":29},"ifcColumn",null,null,"Structural",null,"ifcLabel"]
[{"$nulls":29},"ifcMember",null,null,"Structural",null,"ifcLabel"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p","Brandwerendheid hoofddraagconstructie","-","-","-","-","-","-","brandwerendheid tot bezwijken, benoemen in Custom Pset","moment tot bezwijken","minuten"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","#beton","p","Oppervlakteklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN-EN 13670"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","Componenten","p","Wapening","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten modelleren, ntb tijdens project; staalkwaliteit en dekking opgeven als Eigenschappen (noot: wanneer geen wapening wordt gemodelleerd, staalkwaliteit en dekking meegeven als Eigenschappen)"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"e","Brandwerende omtimmering","-","-","-","-","-","-","-","-","true/ false","Aangeven wanneer van toepassing, uitwerking volgt onder 48.1* door de desbetreffende verantwoordelijke",null,"x"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p","Hulpconstructies","-","-","-","-","-","-","-","-","-","Hulpstaal verwerken in prestatiemodel ivm communicatie staal leverancier en afstemming meerdere disciplines"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p","Toog/ zeeg","-","-","-","-","-","-","-","-","-","Ruimtereserveringsobject modelleren om rekening te kunnen houden met het effect van toog/ zeeg"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c"]
[]
[null,"31.** buitenwandopeningen","b","31.1* - Buitenwandopeningen; niet gevuld",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.",null,"-"]
[null,"31.** buitenwandopeningen","b","Verzameling van niet-gevulde openingen in buitenwanden.",{"$nulls":13},"-"]
[null,"31.** buitenwandopeningen","b","31.2* - Buitenwandopeningen; gevuld met ramen",{"$nulls":13},"-"]
[null,"31.** buitenwandopeningen","b","Verzameling van met ramen en raamkozijnen gevulde openingen in buitenwanden.",{"$nulls":11},"[Ramen] Bijv.: - draai-, klep-, schuif-, tuimel-, taats- en overige typen ramen, - ventilatiekleppen en roosters in (raam)openingen",null,"-"]
[null,"31.** buitenwandopeningen","b","31.3* - Buitenwandopeningen; gevuld met deuren",{"$nulls":13},"-"]
[null,"31.** buitenwandopeningen","b","Verzameling van met deuren en deurkozijnen gevulde openingen in buitenwanden.",{"$nulls":11},"[Deuren] Bijv.: - draai-, schuif-, tuimel- en overige typen deuren, - luiken",null,"-"]
[null,"31.** buitenwandopeningen","b","31.4* - Buitenwandopeningen; gevuld met puien",{"$nulls":11},"[Puien] Bijv.: - alle raam- en deurtypes",null,"-"]
[null,"31.** buitenwandopeningen","b","Verzameling van met puien (inclusief ramen en deuren) gevulde openingen in buitenwanden.",{"$nulls":11},"[Allen] Bijv.: - randaansluitingsvoorzieningen, - lateien, dorpels en waterslagen, - vensterbanken en koven, - buitenzonweringen, rolluiken en verduisteringsvoorzieningen, - bevestigingsmiddelen en hang- en sluitwerken, - beveiligingsvoorzieningen, - bedieningen die één geheel vormen met een bepaald onderdeel, - beglazingen, - conserveringsbehandelingen, - afwerkingen",null,"-"]
[null,"31.** buitenwandopeningen","b","Noot: in verband met de complexiteit van samenstelling versus kozijn/vlakvulling is hier het basisuitgangspunt gekozen dat het minimaal herleidbaar moet zijn hoe de opbouw is. Het is een projectkeuze om het kozijn/vlakvulling los te modelleren of op te lossen middels parameters mee te geven aan de samenstelling.\nNoot: De aan 31.1* - Buitenwandopeningen; niet gevuld gelieerde componenten (dagkantafwerkingen, etc.) zijn verwerkt in de kaarten 41.**.",{"$nulls":13},"-"]
[null,"31.** buitenwandopeningen","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"31.** buitenwandopeningen","b"]
[null,"31.** buitenwandopeningen","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, breedte, omtrek, lengte stijlen, lengte regels",null,"x"]
[null,"31.** buitenwandopeningen","b",null,"e","Vlakverdeling/ rasters","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"31.** buitenwandopeningen","b",null,"p","Stelruimte t.o.v. omliggende geometrie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
[null,"31.** buitenwandopeningen","b",null,"p","Vorm buitenste profilering","-","-","-","-","-","-","-","-","-"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",{"$nulls":14},"v"]
[null,"31.** buitenwandopeningen","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"31.** buitenwandopeningen","b",null,"g","Entiteit","-","-","-","-","-","-","IfcWindow, IfcDoor","IfcClass","-","Gebruik voor onderdelen het meest geëigende type BIM-entiteit (panelen: IfcPlate,  stijlen en regels: IfcMember, beglazing/ramen: IfcWindow, deuren: IfcDoors)",null,"v"]
[null,"31.** buitenwandopeningen","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"31.** buitenwandopeningen","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"31.** buitenwandopeningen","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b","SAMENSTELLING"]
[null,"31.** buitenwandopeningen","b","Eigenschappen","e","Merk","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelReference","-","-","Unieke samenstellingscode is afhankelijk van merk kozijn en type vlakvulling",null,"x"]
[]
[null,"31.** buitenwandopeningen","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-",null,null,"v",{"$nulls":11},"ifcDoor",null,"Pset_<entiteit>Common","isExternal",null,"ifcBoolean"]
[{"$nulls":29},"ifcWindow",null,"Pset_<entiteit>Common","isExternal",null,"ifcBoolean"]
[null,"31.** buitenwandopeningen","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"v",{"$nulls":11},"ifcDoor","child (parent = ifcElement)","Pset_FireRatingProperties","FireResistanceRating",null,"ifcLabel"]
[{"$nulls":29},"ifcWindow","child (parent = ifcElement)","Pset_<entiteit>Common","FireResistanceRating",null,"ifcLabel"]
[null,"31.** buitenwandopeningen","b",null,"e","Luchtgeluidisolatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/inkoop/uitvoering.",null,"v",{"$nulls":11},"ifcDoor","parent","Pset_<entiteit>Common","AcousticRating",null,"ifcLabel"]
[{"$nulls":29},"ifcWindow","parent","Pset_<entiteit>Common","AcousticRating",null,"ifcLabel"]
[null,"31.** buitenwandopeningen","b",null,"p","Warmtedoorgangscoefficient","-","-","-","-","-","-","Pset_<entiteit>Common: ThermalTransmittance","U-waarde","W/ m².K","Warmteweerstand R = 1/ U\n\nIndien entiteit IfcMember: benoemen in Custom Pset omdat 'ThermalTransmittance' geen deel uitmaakt van Common Pset in Ifc 2x3"]
[null,"31.** buitenwandopeningen","b",null,"p","Weerstandsklasse","-","-","-","-","-","-","Pset_<entiteit>Common: SecurityRating","classificatie","-","Bijv.: WK1 conform NEN 5096\n\nIndien entiteit IfcWall, IfcCurtainWall, IfcPlate, IfcMember: benoemen in Custom Pset omdat 'SecurityRating' geen deel uitmaakt van Common Pset"]
[null,"31.** buitenwandopeningen","b",null,"p","Rookwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common: SmokeStop","true/ false","-","\nIndien entiteit IfcMember, IfcPlate: benoemen in Custom Pset omdat 'SmokeStop' geen deel uitmaakt van Common Pset"]
[null,"31.** buitenwandopeningen","b",null,"p","ITS (Integrale Toegankelijkheidsstandaard)","-","-","-","-","-","-","-","true/ false","-"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b","KOZIJN"]
[null,"31.** buitenwandopeningen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"!","v/x"]
[null,"31.** buitenwandopeningen","b",null,"e","Merk","-","-","-","-","-","-","-","-","-","Dient hetzelfde merk te zijn als de samenstelling voor de herleidbaarheid.",null,"x"]
[null,"31.** buitenwandopeningen","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"!","MAT"]
[null,"31.** buitenwandopeningen","b",null,"e","Kleur (binnenzijde, buitenzijde)","-","-","-","-","-","-","-","-","-","(RAL) kleurcode/ omschrijving. Als binnenkleur afwijkt van buitenkleur Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"x"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b","VLAKVULLING"]
[null,"31.** buitenwandopeningen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"31.** buitenwandopeningen","b",null,"e","Type vlakvulling","-","-","-","-","-","-","-","-","-","Projectkeuze: omschrijving (vb. draaikiepraam, paneel, vast glas) of code",null,"x"]
[null,"31.** buitenwandopeningen","b",null,"e","Kleur (binnenzijde, buitenzijde)","-","-","-","-","-","-","-","-","-","(RAL) kleurcode/ omschrijving. Als binnenkleur afwijkt van buitenkleur Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"x"]
[null,"31.** buitenwandopeningen","b",null,"e","Nooduitgang","-","-","-","-","-","-","Pset_DoorCommon: FireExit","true/ false","-",null,null,"x"]
[null,"31.** buitenwandopeningen","b",null,"p","Draairichting","-","-","-","-","-","-","verdeling: IfcWindowStyleOperationEnum\npositie paneel in verdeling: IfcWindowPanelPositionEnum\ndraairichting paneel: IfcWindowPanelOperationEnumeration","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","ZTA","-","-","-","-","-","-","Pset_DoorWindowGlazingType: BeamRadiationTransmittance","factor","-","G-waarde\n\n\n"]
[null,"31.** buitenwandopeningen","b",null,"p","LTA","-","-","-","-","-","-","Pset_DoorWindowGlazingType: Translucency","factor","-"]
[null,"31.** buitenwandopeningen","b",null,"p","Glas specificatie","-","-","-","-","-","-","-","-","-","Omschrijving glas (vb. veiligheidsglas, HR++)"]
[null,"31.** buitenwandopeningen","b",null,"p","Geintegreerde zonwering","-","-","-","-","-","-","-","true/ false","-"]
[null,"31.** buitenwandopeningen","b",null,"p","Doorvalbeveiliging","-","-","-","-","-","-","-","true/ false","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - uniek nummer","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - type scharnier","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - type slot (elektrisch)","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - type sluitplaat (elektrisch)","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - cilinder","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - beveiliging","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - kabeloverbrenging","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - standsignalering","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - schootsignalering","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - dranger (elektrisch)","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - E voeding","-","-","-","-","-","-","-","-","-"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b"]
[null,"31.** buitenwandopeningen","b","Componenten","e","Vensterbanken en koven","-","-","-","-","-","-","-","-","-",null,null,"?"]
[null,"31.** buitenwandopeningen","b",null,"e","Lateien, dorpels en waterslagen","-","-","-","-","-","-","-","-","-",null,null,"?"]
[null,"31.** buitenwandopeningen","b",null,"e","Ventilatierooster","-","-","-","-","-","-","-","-","-","Modelleren en tevens aangeven: ventilatiecapciteit",null,"?"]
[null,"31.** buitenwandopeningen","b",null,"p","Zonwering, rolluiken en verduisteringsvoorziening.","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","Bouwfysische eis - brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating","WBDBO","minuten","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument.",{"$nulls":13},"ifcElement","parent","Pset_FireRatingProperties","FireResistanceRating",null,"ifcLabel"]
[null,"31.** buitenwandopeningen","b",null,"p","Bouwfysische eis - luchtgeluidisoalatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b"]
[]
[null,"32.** binnenwandopeningen","b","32.1* - Binnenwandopeningen; niet gevuld",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.",null,"-"]
[null,"32.** binnenwandopeningen","b","Verzameling van niet-gevulde openingen in binnenwanden. ",{"$nulls":13},"-"]
[null,"32.** binnenwandopeningen","b","32.2* - Binnenwandopeningen; gevuld met ramen",{"$nulls":13},"-"]
[null,"32.** binnenwandopeningen","b","Verzameling van met ramen en raamkozijnen gevulde openingen in binnenwanden.",{"$nulls":11},"[Ramen] Bijv.: - draai-, schuif- en overige typen ramen, - brandwerende raamkozijnen, - vensterbanken en koven",null,"-"]
[null,"32.** binnenwandopeningen","b","32.3* - Binnenwandopeningen; gevuld met deuren",{"$nulls":13},"-"]
[null,"32.** binnenwandopeningen","b","Verzameling van met deuren en deurkozijnen gevulde openingen in binnenwanden.",{"$nulls":11},"[Deuren] Bijv.: - draai-, schuif- en overige typen deuren, - brandwerende deurkozijnen, - luiken",null,"-"]
[null,"32.** binnenwandopeningen","b","32.4* - Binnenwandopeningen; gevuld met puien",{"$nulls":13},"-"]
[null,"32.** binnenwandopeningen","b","Verzameling van met puien (inclusief ramen en deuren) gevulde openingen in binnenwanden.",{"$nulls":11},"[Puien] Bijv.: - alle raam- en deurtypen, - brandwerende puien, - vensterbanken en koven",null,"-"]
[null,"32.** binnenwandopeningen","b","Noot: in verband met de complexiteit van samenstelling versus kozijn/vlakvulling is hier het basisuitgangspunt gekozen dat het minimaal herleidbaar moet zijn hoe de opbouw is. Het is een projectkeuze om het kozijn/vlakvulling los te modelleren of op te lossen middels parameters mee te geven aan de samenstelling.\nNoot: De aan 32.1* - Buitenwandopeningen;niet gevuld gelieerde componenten (dagkantafwerkingen, etc.) zijn verwerkt in de kaarten 42.**.",{"$nulls":11},"[Allen] Bijv.: - randaansluitingsvoorzieningen, - lateien en dorpels, - verduisteringsvoorzieningen, - bevestigingsmiddelen en hang- en sluitwerken, - bedieningen die één geheel vormen met een bepaald onderdeel, - beglazingen, - conserveringsbehandelingen, - afwerkingen",null,"-"]
[null,"32.** binnenwandopeningen","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"32.** binnenwandopeningen","b"]
[null,"32.** binnenwandopeningen","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, breedte, omtrek, lengte stijlen, lengte regels",null,"x"]
[null,"32.** binnenwandopeningen","b",null,"e","Vlakverdeling/ rasters","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"32.** binnenwandopeningen","b",null,"p","Stelruimte t.o.v. omliggende geometrie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
[null,"32.** binnenwandopeningen","b",null,"p","Vorm buitenste profilering","-","-","-","-","-","-","-","-","-"]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b"]
[null,"32.** binnenwandopeningen","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"32.** binnenwandopeningen","b",null,"g","Entiteit","-","-","-","-","-","-","IfcWindow, IfcDoor","IfcClass","-","Gebruik voor onderdelen het meest geëigende type BIM-entiteit (panelen: IfcPlate,  stijlen en regels: IfcMember, beglazing/ramen: IfcWindow, deuren: IfcDoors)",null,"v"]
[null,"32.** binnenwandopeningen","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"32.** binnenwandopeningen","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"32.** binnenwandopeningen","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b","SAMENSTELLING"]
[null,"32.** binnenwandopeningen","b","Eigenschappen","e","Merk","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelReference","-","-","Unieke samenstellingscode is afhankelijk van merk kozijn en type vlakvulling",null,"x"]
[null,"32.** binnenwandopeningen","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-",null,null,"v"]
[null,"32.** binnenwandopeningen","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"v",{"$nulls":11},"ifcElement","parent","Pset_FireRatingProperties","FireResistanceRating",null,"ifcLabel"]
[null,"32.** binnenwandopeningen","b",null,"e","Luchtgeluidisolatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/inkoop/uitvoering.",null,"x",{"$nulls":11},"ifcDoor","parent","Pset_<entiteit>Common","AcousticRating",null,"ifcLabel"]
[{"$nulls":29},"ifcWindow","parent","Pset_<entiteit>Common","AcousticRating",null,"ifcLabel"]
[null,"32.** binnenwandopeningen","b",null,"p","Weerstandsklasse","-","-","-","-","-","-","Pset_<entiteit>Common: SecurityRating","classificatie","-","Bijv.: WK1 conform NEN 5096\n\nIndien entiteit IfcWall, IfcCurtainWall, IfcPlate, IfcMember: benoemen in Custom Pset omdat 'SecurityRating' geen deel uitmaakt van Common Pset"]
[null,"32.** binnenwandopeningen","b",null,"p","Rookwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common: SmokeStop","true/ false","-","\nIndien entiteit IfcMember, IfcPlate: benoemen in Custom Pset omdat 'SmokeStop' geen deel uitmaakt van Common Pset"]
[null,"32.** binnenwandopeningen","b",null,"p","ITS (Integrale Toegankelijkheidsstandaard)","-","-","-","-","-","-","-","true/ false","-"]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b","KOZIJN"]
[null,"32.** binnenwandopeningen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x","V/X"]
[null,"32.** binnenwandopeningen","b",null,"e","Kozijnmerk","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"32.** binnenwandopeningen","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"32.** binnenwandopeningen","b",null,"e","Kleur (binnenzijde, buitenzijde)","-","-","-","-","-","-","-","-","-","(RAL) kleurcode/ omschrijving. Als binnenkleur afwijkt van buitenkleur Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"x"]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b","VLAKVULLING"]
[null,"32.** binnenwandopeningen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x","V/X"]
[null,"32.** binnenwandopeningen","b",null,"e","Type vlakvulling","-","-","-","-","-","-","-","-","-","Projectkeuze: omschrijving (vb. draaikiepraam, paneel, vast glas) of code",null,"x"]
[null,"32.** binnenwandopeningen","b",null,"e","Kleur (binnenzijde, buitenzijde)","-","-","-","-","-","-","-","-","-","(RAL) kleurcode/ omschrijving. Als binnenkleur afwijkt van buitenkleur Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"x"]
[null,"32.** binnenwandopeningen","b",null,"e","Nooduitgang","-","-","-","-","-","-","Pset_DoorCommon: FireExit","true/ false","-",null,null,"x"]
[null,"32.** binnenwandopeningen","b",null,"p","Draairichting","-","-","-","-","-","-","verdeling: IfcWindowStyleOperationEnum\npositie paneel in verdeling: IfcWindowPanelPositionEnum\ndraairichting paneel: IfcWindowPanelOperationEnumeration","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","Glas specificatie","-","-","-","-","-","-","-","-","-","Omschrijving glas (vb. veiligheidsglas, HR++)"]
[null,"32.** binnenwandopeningen","b",null,"p","Doorvalbeveiliging","-","-","-","-","-","-","-","true/ false","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - uniek nummer","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - type scharnier","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - type slot (elektrisch)","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - type sluitplaat (elektrisch)","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - cilinder","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - beveiliging","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - kabeloverbrenging","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - standsignalering","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - schootsignalering","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - dranger (elektrisch)","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - E voeding","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","Uniek deurnummer","-","-","-","-","-","-","-","-","-","Uniek nummer t.b.v. sluitplannen etc."]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b"]
[null,"32.** binnenwandopeningen","b","Componenten","e","Vensterbanken en koven","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"32.** binnenwandopeningen","b",null,"e","Lateien en dorpels","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"32.** binnenwandopeningen","b",null,"p","Verduisteringsvoorzieningen","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","Bouwfysische eis - brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating","WBDBO","minuten","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
[null,"32.** binnenwandopeningen","b",null,"p","Bouwfysische eis - luchtgeluidisoalatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b"]
[]
[null,"33.** vloeropeningen","b","33.** - Vloeropeningen",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - toegangsluiken naar hogere of lagere niveaus - roostervloeren in leidingschachten - randaansluitingsvoorzieningen - ravelingen - bevestigingsmiddelen en hang- en sluitwerken - bedieningen die één geheel vormen met een bepaald onderdeel - beglazingen - conserveringsbehandelingen - afwerkingen"]
[null,"33.** vloeropeningen","b","Verzameling van met een vulling voorziene openingen in vloeren."]
[null,"33.** vloeropeningen","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"33.** vloeropeningen","b"]
[null,"33.** vloeropeningen","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, omtrek",null,"x"]
[null,"33.** vloeropeningen","b",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"33.** vloeropeningen","b"]
[null,"33.** vloeropeningen","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"-"]
[null,"33.** vloeropeningen","b",null,"g","Entiteit","-","-","-","-","-","-","IfcSlab, IfcPlate","IfcClass","-",null,null,"x"]
[null,"33.** vloeropeningen","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"33.** vloeropeningen","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"x"]
[null,"33.** vloeropeningen","b",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"33.** vloeropeningen","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"33.** vloeropeningen","b",{"$nulls":14},"x"]
[null,"33.** vloeropeningen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"33.** vloeropeningen","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"33.** vloeropeningen","b",null,"e","Kleur","-","-","-","-","-","-","-","-","-","(RAL) kleurcode/ omschrijving. Als binnenkleur afwijkt van buitenkleur Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"x"]
[null,"33.** vloeropeningen","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-",null,null,"x"]
[null,"33.** vloeropeningen","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-",null,null,"x"]
[null,"33.** vloeropeningen","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"x",{"$nulls":11},"ifcElement","parent","Pset_FireRatingProperties","FireResistanceRating",null,"ifcLabel"]
[null,"33.** vloeropeningen","b",null,"p","Warmtedoorgangscoefficient","-","-","-","-","-","-","Pset_<entiteit>Common: ThermalTransmittance","U-waarde","W/ m².K","Warmteweerstand R = 1/ U"]
[null,"33.** vloeropeningen","b",null,"p","Weerstandsklasse","-","-","-","-","-","-","SecurityRating benoemen in custom Pset","classificatie","-","Bijv.: WK1 conform NEN 5096\n\nIndien entiteit IfcPlate, IfcSlab: benoemen in Custom Pset omdat 'SecurityRating' geen deel uitmaakt van Common Pset"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"33.** vloeropeningen","b"]
[null,"33.** vloeropeningen","b","Componenten","e","Isolatie","-","-","-","-","-","-","-","-","-","Tevens aangeven: isolatiewaarde en brandklasse",null,"x"]
[null,"33.** vloeropeningen","b",null,"e","Randafwerking","-","-","-","-","-","-","-","-","-",null,null,"x"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"33.** vloeropeningen","b"]
[]
[null,"34.** balustrades en leuningen","b","34.** - Balustrades en leuningen",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - balustrades en leuningen langs dakranden - bevestigingsmiddelen - conserveringsbehandelingen - afwerkingen"]
[null,"34.** balustrades en leuningen","b","Verzameling van voltooiingen van balkons, galerijen, loggia's, vides, trappen, hellingen, vloeren dakopeningen en dakranden door middel van balustrades."]
[null,"34.** balustrades en leuningen","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"34.** balustrades en leuningen","b"]
[null,"34.** balustrades en leuningen","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte",null,"v"]
[null,"34.** balustrades en leuningen","b",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"34.** balustrades en leuningen","b",null,"p","Stelruimte t.o.v. omliggende geometrie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"34.** balustrades en leuningen","b"]
[null,"34.** balustrades en leuningen","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"34.** balustrades en leuningen","b",null,"g","Entiteit","-","-","-","-","-","-","IfcRailing","IfcClass","-",null,null,"v"]
[null,"34.** balustrades en leuningen","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"34.** balustrades en leuningen","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"34.** balustrades en leuningen","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"34.** balustrades en leuningen","b"]
[null,"34.** balustrades en leuningen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x","v/x"]
[null,"34.** balustrades en leuningen","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"34.** balustrades en leuningen","b",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving), bij meerdere waarden Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"x"]
[null,"34.** balustrades en leuningen","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_RailingCommon: IsExternal","true/ false","-",null,null,"v",{"$nulls":11},"ifcRailling","parent","Pset_RailingCommon","IsExternal",null,"ifcBoolean"]
[null,"34.** balustrades en leuningen","b",null,"p","Gebruiksklasse","-","-","-","-","-","-","-","classificatie","-","Klasse A t/m K (volgens NEN:EN1990-1-1)"]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"34.** balustrades en leuningen","b"]
[null,"34.** balustrades en leuningen","b","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"34.** balustrades en leuningen","b"]
[]
[null,"37.** dakopeningen","b","37.** - Dakopeningen",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - dakluiken, rookluiken en daklichten - randaansluitingsvoorzieningen - raveelconstructies - bevestigingsmiddelen en hang- en sluitwerken - beveiligingsvoorzieningen - bedieningen die één geheel vormen met een bepaald onderdeel - beglazingen - afwerkingen"]
[null,"37.** dakopeningen","b","Verzameling van met een vulling voorziene openingen in daken.\nNoot: in verband met de complexiteit van samenstelling versus kozijn/vlakvulling is hier het basisuitgangspunt gekozen dat het minimaal herleidbaar moet zijn hoe de opbouw is. Het is een projectkeuze om het kozijn/vlakvulling los te modelleren of op te lossen middels parameters mee te geven aan de samenstelling."]
[null,"37.** dakopeningen","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"37.** dakopeningen","b"]
[null,"37.** dakopeningen","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, breedte, omtrek, lengte stijlen, lengte regels",null,"x"]
[null,"37.** dakopeningen","b",null,"e","Vlakverdeling/ rasters","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"37.** dakopeningen","b",null,"p","Stelruimte t.o.v. omliggende geometrie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
[null,"37.** dakopeningen","b",null,"p","Vorm buitenste profilering","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b"]
[null,"37.** dakopeningen","b"]
[null,"37.** dakopeningen","b"]
[null,"37.** dakopeningen","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"x"]
[null,"37.** dakopeningen","b",null,"g","Entiteit","-","-","-","-","-","-","IfcWindow, IfcDoor","IfcClass","-","Gebruik voor onderdelen het meest geëigende type BIM-entiteit (panelen: IfcPlate,  stijlen en regels: IfcMember, beglazing/ramen: IfcWindow, deuren: IfcDoors)",null,"x"]
[null,"37.** dakopeningen","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"37.** dakopeningen","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"x"]
[null,"37.** dakopeningen","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b","SAMENSTELLING"]
[null,"37.** dakopeningen","b","Eigenschappen"]
[null,"37.** dakopeningen","b",null,"e","Merk","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelReference","-","-","Unieke samenstellingscode is afhankelijk van merk kozijn en type vlakvulling",null,"x"]
[null,"37.** dakopeningen","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-",null,null,"x"]
[null,"37.** dakopeningen","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"x",{"$nulls":11},"ifcElement","parent","Pset_FireRatingProperties","FireResistanceRating",null,"ifcLabel"]
[null,"37.** dakopeningen","b",null,"e","Luchtgeluidisolatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/inkoop/uitvoering.",null,"x"]
[null,"37.** dakopeningen","b",null,"p","Warmtedoorgangscoefficient","-","-","-","-","-","-","Pset_<entiteit>Common: ThermalTransmittance","U-waarde","W/ m².K","Warmteweerstand R = 1/ U"]
[null,"37.** dakopeningen","b",null,"p","Weerstandsklasse","-","-","-","-","-","-","Pset_<entiteit>Common: SecurityRating","classificatie","-","Bijv.: WK1 conform NEN 5096\n\nIndien entiteit IfcWall, IfcCurtainWall, IfcPlate, IfcMember: benoemen in Custom Pset omdat 'SecurityRating' geen deel uitmaakt van Common Pset"]
[null,"37.** dakopeningen","b",null,"p","Rookwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common: SmokeStop","true/ false","-"]
[null,"37.** dakopeningen","b",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b","KOZIJN"]
[null,"37.** dakopeningen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"37.** dakopeningen","b",null,"e","Kozijnmerk","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"37.** dakopeningen","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"37.** dakopeningen","b",null,"e","Kleur (binnenzijde, buitenzijde)","-","-","-","-","-","-","-","-","-","(RAL) kleurcode/ omschrijving. Als binnenkleur afwijkt van buitenkleur Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"x"]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b","VLAKVULLING"]
[null,"37.** dakopeningen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"37.** dakopeningen","b",null,"e","Type vlakvulling","-","-","-","-","-","-","-","-","-","Projectkeuze: omschrijving (vb. draaikiepraam, paneel, vast glas) of code",null,"x"]
[null,"37.** dakopeningen","b",null,"e","Kleur (binnenzijde, buitenzijde)","-","-","-","-","-","-","-","-","-","(RAL) kleurcode/ omschrijving. Als binnenkleur afwijkt van buitenkleur Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"x"]
[null,"37.** dakopeningen","b",null,"e","HSW - uniek nummer","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"37.** dakopeningen","b",null,"p","Draairichting","-","-","-","-","-","-","verdeling: IfcWindowStyleOperationEnum\npositie paneel in verdeling: IfcWindowPanelPositionEnum\ndraairichting paneel: IfcWindowPanelOperationEnumeration","-","-"]
[null,"37.** dakopeningen","b",null,"p","ZTA","-","-","-","-","-","-","Pset_DoorWindowGlazingType: BeamRadiationTransmittance","factor","-","G-waarde\n\n\n"]
[null,"37.** dakopeningen","b",null,"p","LTA","-","-","-","-","-","-","Pset_DoorWindowGlazingType: Translucency","factor","-"]
[null,"37.** dakopeningen","b",null,"p","Glas specificatie","-","-","-","-","-","-","-","-","-","Omschrijving glas (vb. veiligheidsglas, HR++)"]
[null,"37.** dakopeningen","b",null,"p","Geintegreerde zonwering","-","-","-","-","-","-","-","true/ false","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - type scharnier","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - type slot (elektrisch)","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - type sluitplaat (elektrisch)","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - cilinder","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - beveiliging","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - kabeloverbrenging","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - standsignalering","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - schootsignalering","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - dranger (elektrisch)","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - E voeding","-","-","-","-","-","-","-","-","-"]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b"]
[null,"37.** dakopeningen","b","Componenten","e","Randafwerking","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"37.** dakopeningen","b",null,"e","Ventilatierooster","-","-","-","-","-","-","-","-","-","Modelleren en tevens aangeven: ventilatiecapciteit",null,"x"]
[null,"37.** dakopeningen","b",null,"p","Zonwering, rolluiken en verduisteringsvoorziening.","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","Bouwfysische eis - brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating","WBDBO","minuten","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
[null,"37.** dakopeningen","b",null,"p","Bouwfysische eis - luchtgeluidisoalatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b"]
[]
[null,"41.1* buitenwandafwerkingen","b","41.1* - Buitenwandafwerkingen",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - isolerende, akoestische en brandwerende afwerkingen - gevelbekledingen en gevelbetimmeringen - bepleisteringen - betegelingen - schilderafwerkingen",null,"-"]
[null,"41.1* buitenwandafwerkingen","b","Verzameling van afwerkingen van de buitenzijde van buitenwanden, gerekend vanaf de wandconstructie."]
[null,"41.1* buitenwandafwerkingen","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"41.1* buitenwandafwerkingen","b"]
[null,"41.1* buitenwandafwerkingen","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, breedte, dikte\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"x"]
[null,"41.1* buitenwandafwerkingen","b",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"41.1* buitenwandafwerkingen","b",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,"x"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"41.1* buitenwandafwerkingen","b"]
[null,"41.1* buitenwandafwerkingen","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"x"]
[null,"41.1* buitenwandafwerkingen","b",null,"g","Entiteit","-","-","-","-","-","-","IfcPlate, IfcCovering, IfcWall, IfcBuildingElementProxy","IfcClass","-",null,null,"x"]
[null,"41.1* buitenwandafwerkingen","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"41.1* buitenwandafwerkingen","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"x"]
[null,"41.1* buitenwandafwerkingen","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"41.1* buitenwandafwerkingen","b"]
[null,"41.1* buitenwandafwerkingen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"41.1* buitenwandafwerkingen","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"41.1* buitenwandafwerkingen","b",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"x"]
[null,"41.1* buitenwandafwerkingen","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","Indien entiteit IfcCovering, IfcBuildingElementProxy: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"x"]
[null,"41.1* buitenwandafwerkingen","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-","Indien entiteit IfcCovering, IfcBuildingElementProxy: benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset",null,"x"]
[null,"41.1* buitenwandafwerkingen","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"x"]
[null,"41.1* buitenwandafwerkingen","b",null,"p","Brandwerende afwerking","-","-","-","-","-","-","-","-","-"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"41.1* buitenwandafwerkingen","b"]
[null,"41.1* buitenwandafwerkingen","b","Componenten","e","Dagkantafwerking, waterslagen","-","-","-","-","-","-","-","-","-","In het geval van 31.1* Buitenwandopeningen; niet gevuld",null,"x"]
[null,"41.1* buitenwandafwerkingen","b",null,"p","Verankering en bevestiging","-","-","-","-","-","-","-","-","-","Niet modelleren, wel terug laten komen in details"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"41.1* buitenwandafwerkingen","b"]
[]
[null,"42.1* binnenwandafwerkingen","i","42.1* - Binnenwandafwerkingen",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - isolerende, akoestische en brandwerende afwerkingen - wandbekledingen en wandbetimmeringen - bepleisteringen - betegelingen - schilderafwerkingen - hoekbeschermers en stootbanden die één geheel vormen met de wandafwerking",null,"-"]
[null,"42.1* binnenwandafwerkingen","i","Verzameling van afwerkingen van de binnenwanden en van de binnenzijde van de buitenwanden, gerekend vanaf de wandconstructie."]
[null,"42.1* binnenwandafwerkingen","i",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"42.1* binnenwandafwerkingen","i"]
[null,"42.1* binnenwandafwerkingen","i","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, breedte, dikte\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"x"]
[null,"42.1* binnenwandafwerkingen","i",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"42.1* binnenwandafwerkingen","i",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,"x"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"42.1* binnenwandafwerkingen","i"]
[null,"42.1* binnenwandafwerkingen","i","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"x"]
[null,"42.1* binnenwandafwerkingen","i",null,"g","Entiteit","-","-","-","-","-","-","IfcPlate, IfcCovering, IfcWall","IfcClass","-",null,null,"x"]
[null,"42.1* binnenwandafwerkingen","i",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"42.1* binnenwandafwerkingen","i",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"x"]
[null,"42.1* binnenwandafwerkingen","i",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"42.1* binnenwandafwerkingen","i"]
[null,"42.1* binnenwandafwerkingen","i","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"42.1* binnenwandafwerkingen","i",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"42.1* binnenwandafwerkingen","i",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"x"]
[null,"42.1* binnenwandafwerkingen","i",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","Indien entiteit IfcCovering: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"x"]
[null,"42.1* binnenwandafwerkingen","i",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-","Indien entiteit IfcCovering: benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset",null,"x"]
[null,"42.1* binnenwandafwerkingen","i",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"x"]
[null,"42.1* binnenwandafwerkingen","i",null,"p","Brandwerende afwerking","-","-","-","-","-","-","-","-","-"]
[null,"42.1* binnenwandafwerkingen","i",null,"p","Vlakheidsklasse","-","-","-","-","-","-","-","classificatie","-"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"42.1* binnenwandafwerkingen","i"]
[null,"42.1* binnenwandafwerkingen","i","Componenten","e","Dagkantafwerking","-","-","-","-","-","-",null,"-","-","In het geval van 32.1* Binnenwandopeningen; niet gevuld",null,"x"]
[null,"42.1* binnenwandafwerkingen","i",null,"p","Verankering en bevestiging","-","-","-","-","-","-","-","-","-","Niet modelleren, wel terug laten komen in details"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"42.1* binnenwandafwerkingen","i"]
[]
[null,"43.** vloerafwerkingen","i","43.** - Vloerafwerkingen; verhoogd en niet verhoogd",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - podiums en toneelvloeren - verhoogde computervloeren - randaansluitingsvoorzieningen - afwerkingen die één geheel vormen met de verhoogde vloerconstructie - dilatatievoegconstructies/ - isolerende, akoestische en brandwerende afwerkingen - dekvloeren samengesteld uit zand/cement of synthetische stoffen - terrazzovloeren - betegelde en natuursteenvloeren - houten (parket)vloerafwerkingen - vloerbedekkingen en afwerkingen op de dekvloeren - plinten - matomrandingen",null,"-"]
[null,"43.** vloerafwerkingen","i","Verzameling van afwerkingen van de bovenzijde van vloeren door middel van een verhoogde constructie/ rechtstreeks op de al dan niet verhoogde vloerconstructie aangebracht, gerekend vanaf de ondervloerconstructie."]
[null,"43.** vloerafwerkingen","i",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"43.** vloerafwerkingen","i"]
[null,"43.** vloerafwerkingen","i","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, omtrek\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"x"]
[null,"43.** vloerafwerkingen","i",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"x"]
[null,"43.** vloerafwerkingen","i",null,"e","Afschot","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"43.** vloerafwerkingen","i",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"43.** vloerafwerkingen","i",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,"x"]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"43.** vloerafwerkingen","i"]
[null,"43.** vloerafwerkingen","i","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"x"]
[null,"43.** vloerafwerkingen","i",null,"g","Entiteit","-","-","-","-","-","-","IfcSlab, IfcCovering","IfcClass","-",null,null,"x"]
[null,"43.** vloerafwerkingen","i",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"43.** vloerafwerkingen","i",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"x"]
[null,"43.** vloerafwerkingen","i",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"43.** vloerafwerkingen","i",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"43.** vloerafwerkingen","i",{"$nulls":14},"x"]
[null,"43.** vloerafwerkingen","i","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"43.** vloerafwerkingen","i",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"43.** vloerafwerkingen","i",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"x"]
[null,"43.** vloerafwerkingen","i",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_SlabCommon: Loadbearing","true/ false","-","Indien entiteit IfcCovering: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Pset_CoveringCommon",null,"x"]
[null,"43.** vloerafwerkingen","i",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_SlabCommon: IsExternal","-","true/ false","Indien entiteit IfcCovering: benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset",null,"x"]
[null,"43.** vloerafwerkingen","i",null,"p","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…"]
[null,"43.** vloerafwerkingen","i",null,"p","Brandwerende afwerking","-","-","-","-","-","-","-","-"]
[null,"43.** vloerafwerkingen","i",null,"p","Warmtedoorgangscoefficient","-","-","-","-","-","-","Pset_SlabCommon: ThermalTransmittance","U-waarde","W/ m².K","Warmteweerstand R = 1/ U\n\nIndien entiteit IfcCovering: benoemen in Custom Pset omdat 'ThermalTransmittance' geen deel uitmaakt van Common Pset in Ifc 2x3"]
[null,"43.** vloerafwerkingen","i",null,"e","Luchtgeluidisolatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/inkoop/uitvoering.",null,"x"]
[null,"43.** vloerafwerkingen","i",null,"p","Vlakheidsklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN 2747"]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"43.** vloerafwerkingen","i"]
[null,"43.** vloerafwerkingen","i","Componenten","p","Ondervloerconstructie","-","-","-","-","-","-","-","-","-","Ten behoeve van afstemming met installaties (bijvoorbeeld: pootjes computervloeren)\nNoot: ter plaatse moeilijke knooppunten modelleren, ntb tijdens project;"]
[null,"43.** vloerafwerkingen","i",null,"p","Randaansluitingsvoorzieningen","-","-","-","-","-","-","-","-","-"]
[null,"43.** vloerafwerkingen","i",null,"p","Bouwfysische eis - brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating","WBDBO","minuten","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
[null,"43.** vloerafwerkingen","i",null,"p","Bouwfysische eis - luchtgeluidisoalatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"43.** vloerafwerkingen","i"]
[]
[null,"44.** trap- en hellingafwerkingen","b","44.** - Trap- en hellingafwerkingen",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - isolerende, akoestische en brandwerende afwerkingen - afwerkingen op boven-, onder- en zijkanten van trappen/ hellingen en bordessen - terrazzoafwerkingen - betegelde - en natuursteenafwerkingen - houten trap-/ hellingafwerkingen - vloerbedekkingen op bordessen, trede-/ hellingen en stootbordbekledingen - trapneusprofielen - schilderwerken - randaansluitingsvoorzieningen - dilatatievoegconstructies/ - dekvloeren samengesteld uit zand/cement of synthetische stoffen",null,"-"]
[null,"44.** trap- en hellingafwerkingen","b","Verzameling van afwerkingen van trappen/ hellingen en tussenbordessen, gerekend vanaf de trap-/ hellingconstructie."]
[null,"44.** trap- en hellingafwerkingen","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"44.** trap- en hellingafwerkingen","b"]
[null,"44.** trap- en hellingafwerkingen","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, breedte, dikte\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"x"]
[null,"44.** trap- en hellingafwerkingen","b",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"x"]
[null,"44.** trap- en hellingafwerkingen","b",null,"e","Afschot","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"44.** trap- en hellingafwerkingen","b",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"44.** trap- en hellingafwerkingen","b",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"44.** trap- en hellingafwerkingen","b",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"44.** trap- en hellingafwerkingen","b"]
[null,"44.** trap- en hellingafwerkingen","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"x"]
[null,"44.** trap- en hellingafwerkingen","b",null,"g","Entiteit","-","-","-","-","-","-","IfcPlate, IfcCovering, IfcWall","IfcClass","-",null,null,"x"]
[null,"44.** trap- en hellingafwerkingen","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"44.** trap- en hellingafwerkingen","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"x"]
[null,"44.** trap- en hellingafwerkingen","b",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"44.** trap- en hellingafwerkingen","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"44.** trap- en hellingafwerkingen","b"]
[null,"44.** trap- en hellingafwerkingen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"44.** trap- en hellingafwerkingen","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"44.** trap- en hellingafwerkingen","b",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"x"]
[null,"44.** trap- en hellingafwerkingen","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","Indien entiteit IfcCovering: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Pset_CoveringCommon",null,"-","enkel ifccovering - Staat NIET op Building Smart. Daarnaast ook onlogisch dat een afwerking dragend zou kunnen zijn?"]
[null,"44.** trap- en hellingafwerkingen","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-","Indien entiteit IfcCovering: benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset",null,"-","enkel ifccovering - Staat op Building Smart. Binnen AC: Classificatie 2.0 > trapafwerking staat onder ifcMember geclassificeerd => deze heeft wel loadbearing en isExternal"]
[null,"44.** trap- en hellingafwerkingen","b",null,"p","Brandwerendheid","-","-","-","-","-","-","Pset_CoveringCommon:FireRating","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…"]
[null,"44.** trap- en hellingafwerkingen","b",null,"p","Brandwerende afwerking","-","-","-","-","-","-","-","-","-"]
[null,"44.** trap- en hellingafwerkingen","b",null,"p","Warmtedoorgangscoefficient","-","-","-","-","-","-","Pset_<entiteit>Common: ThermalTransmittance","U-waarde","W/ m².K","Warmteweerstand R = 1/ U\n\nIndien entiteit IfcCovering: benoemen in Custom Pset omdat 'ThermalTransmittance' geen deel uitmaakt van Common Pset in Ifc 2x3"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"44.** trap- en hellingafwerkingen","b"]
[null,"44.** trap- en hellingafwerkingen","b","Componenten","p","Randaansluitingsvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"44.** trap- en hellingafwerkingen","b"]
[]
[null,"45.** plafondafwerkingen","i","45.** - Plafondafwerkingen; verlaagd en niet verlaagd",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv. - isolerende, akoestische en brandwerende afwerkingen - randaansluitingsvoorzieningen - verticale plafondovergangen - plafondkoven en gordijnplanken - afwerkingen die één geheel vormen met de verlaagde plafondconstructie - schilderwerken - dilatatievoegconstructies/ - plafondbekledingen en plafondbetimmeringen - bepleisteringen - betegelingen - schilderafwerkingen - plafondkoven en gordijnplanken",null,"-"]
[null,"45.** plafondafwerkingen","i","Verzameling van afwerkingen van de onderzijde van vloeren of daken met een verlaagde constructie, gerekend vanaf de bovenliggende vloer- of dakconstructie/ rechtstreeks op de vloer- of dakconstructie aangebracht, gerekend vanaf de bovenliggende vloerconstructie."]
[null,"45.** plafondafwerkingen","i",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"45.** plafondafwerkingen","i"]
[null,"45.** plafondafwerkingen","i","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, breedte, dikte, omtrek\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"x"]
[null,"45.** plafondafwerkingen","i",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"x"]
[null,"45.** plafondafwerkingen","i",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"45.** plafondafwerkingen","i",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"45.** plafondafwerkingen","i",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"45.** plafondafwerkingen","i"]
[null,"45.** plafondafwerkingen","i","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"x"]
[null,"45.** plafondafwerkingen","i",null,"g","Entiteit","-","-","-","-","-","-","IfcCovering","IfcClass","-",null,null,"x"]
[null,"45.** plafondafwerkingen","i",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"45.** plafondafwerkingen","i",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"x"]
[null,"45.** plafondafwerkingen","i",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"45.** plafondafwerkingen","i",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"45.** plafondafwerkingen","i"]
[null,"45.** plafondafwerkingen","i","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"45.** plafondafwerkingen","i",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"45.** plafondafwerkingen","i",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"x"]
[null,"45.** plafondafwerkingen","i",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_PlateCommon: Loadbearing","true/ false","-","Indien entiteit IfcCovering: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Pset_CoveringCommon",null,"x"]
[null,"45.** plafondafwerkingen","i",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_PlateCommon: IsExternal","true/ false","-","Indien entiteit IfcCovering: benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset",null,"x"]
[null,"45.** plafondafwerkingen","i",null,"e","Luchtgeluidisolatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/inkoop/uitvoering.",null,"x"]
[null,"45.** plafondafwerkingen","i",null,"p","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…"]
[null,"45.** plafondafwerkingen","i",null,"p","Warmtedoorgangscoefficient","-","-","-","-","-","-","Pset_PlateCommon: ThermalTransmittance","U-waarde","W/ m².K","U-waarde in W/ m².K\nwarmteweerstand R = 1/ U\n\nU-waarde overgang binnen- en/of buitenlucht toekennen aan element dat aan buiten- en/of binnenruimte grenst\nU-waarde niet gemodelleerde spouw toekennen aan één element in de scheidingsconstructie\n\nalternatief: U-waarde alleen toekennen aan het element in de scheidingsconstructie dat het meest bijdraagt aan de isolatiewaarde van de gehele scheidingsconstructie"]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"45.** plafondafwerkingen","i",{"$nulls":14},"x"]
[null,"45.** plafondafwerkingen","i","Componenten","e","Koofconstructies en gordijnplanken","-","-","-","-","-","-","-","-","-"]
[null,"45.** plafondafwerkingen","i",null,"p","Ophangconstructie","-","-","-","-","-","-","-","-","-","Ten behoeve van afstemming met installaties\nNoot: ter plaatse moeilijke knooppunten modelleren, ntb tijdens project;"]
[null,"45.** plafondafwerkingen","i",null,"p","Bouwfysische eis - brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating","WBDBO","minuten","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
[null,"45.** plafondafwerkingen","i",null,"p","Bouwfysische eis - luchtgeluidisoalatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"45.** plafondafwerkingen","i"]
[]
[null,"47.** dakafwerkingen","i","47.** - Dakafwerkingen; afwerkingen en bekledingen",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - dakbedekkingen van bitumen, kunststof en steenachtige materialen/ behorend bij het afwerkingspakket - gebouwisolatievoorzieningen - brandwerende voorzieningen - randaansluitingsvoorzieningen - panlatten - daktrimmen - dilatatievoegconstructies - looppaden",null,"-"]
[null,"47.** dakafwerkingen","i","Verzameling van afwerkingen op de bovenzijde van horizontale en hellende daken en dakterrasafwerkingen, gerekend vanaf de (constructieve) dakvloeren/ dakterrassen, gerekend vanaf de dakafwerking.\n"]
[null,"47.** dakafwerkingen","i",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"47.** dakafwerkingen","i"]
[null,"47.** dakafwerkingen","i","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, omtrek\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"x"]
[null,"47.** dakafwerkingen","i",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"x"]
[null,"47.** dakafwerkingen","i",null,"e","Afschot","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"47.** dakafwerkingen","i",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"47.** dakafwerkingen","i",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,"x"]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"47.** dakafwerkingen","i",{"$nulls":14},"x"]
[null,"47.** dakafwerkingen","i","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"x"]
[null,"47.** dakafwerkingen","i",null,"g","Entiteit","-","-","-","-","-","-","IfcSlab, IfcCovering","IfcClass","-",null,null,"x"]
[null,"47.** dakafwerkingen","i",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"47.** dakafwerkingen","i",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"x"]
[null,"47.** dakafwerkingen","i",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"47.** dakafwerkingen","i"]
[null,"47.** dakafwerkingen","i","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"47.** dakafwerkingen","i",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"47.** dakafwerkingen","i",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"x"]
[null,"47.** dakafwerkingen","i",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_SlabCommon: Loadbearing","true/ false","-",null,null,"x"]
[null,"47.** dakafwerkingen","i",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_SlabCommon: IsExternal","true/ false","-",null,null,"x"]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"47.** dakafwerkingen","i",{"$nulls":14},"x"]
[null,"47.** dakafwerkingen","i","Componenten","p","Ondervloerconstructie","-","-","-","-","-","-","-","-","-","Ten behoeve van afstemming met installaties (bijvoorbeeld: pootjes computervloeren)\nNoot: ter plaatse moeilijke knooppunten modelleren, ntb tijdens project;"]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"47.** dakafwerkingen","i"]
[]
[null,"51.** warmte-opwekking","w","51.** - Warmte-opwekking",{"$nulls":13},"-"]
[null,"51.** warmte-opwekking","w","Verzameling van voorzieningen voor opwekken en ter beschikking stellen van warmte ten behoeve van klimaat en sanitair."]
[null,"51.** warmte-opwekking","w",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"51.** warmte-opwekking","w"]
[null,"51.** warmte-opwekking","w","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte, diameter"]
["x","51.** warmte-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","51.** warmte-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"51.** warmte-opwekking","w"]
[null,"51.** warmte-opwekking","w","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument"]
[null,"51.** warmte-opwekking","w",null,"g","Entiteit","-","-","-","-","-","-","IfcEnergyConversionDevice, IfcFlowTerminal, IfcFlowSegment, IfcFlowFitting, IfcBuildingElementProxy, IfcFlowStorageDevice, IfcFlowController, IfcCovering, IfcFlowMovingDevice","IfcClass","-"]
[null,"51.** warmte-opwekking","w",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar"]
[null,"51.** warmte-opwekking","w",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket"]
[null,"51.** warmte-opwekking","w",null,"e","Systeemtype","-","-","-","-","-","-","System Type","-","-","Duidelijk onderscheid makend in de verschillende aanvoer en/of retour systemen "]
["x","51.** warmte-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","51.** warmte-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"51.** warmte-opwekking","w"]
[null,"51.** warmte-opwekking","w","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","51.** warmte-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","51.** warmte-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","51.** warmte-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","51.** warmte-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"51.** warmte-opwekking","w"]
[null,"51.** warmte-opwekking","w","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","51.** warmte-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"51.** warmte-opwekking","w"]
[]
[null,"52.** afvoeren","w","52.** - Afvoeren",{"$nulls":13},"-"]
[null,"52.** afvoeren","w","Verzameling van voorzieningen voor afvoer opvang, zowel in als aan het gebouw, met de vaste ontvangstpunten."]
[null,"52.** afvoeren","w",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"52.** afvoeren","w"]
[null,"52.** afvoeren","w","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte, diameter"]
[null,"52.** afvoeren","w",null,"e","Afschot","-","-","-","-","-","-","-","-","-"]
["x","52.** afvoeren","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","52.** afvoeren","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"52.** afvoeren","w"]
[null,"52.** afvoeren","w","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument"]
[null,"52.** afvoeren","w",null,"g","Entiteit","-","-","-","-","-","-","IfcEnergyConversionDevice, IfcFlowTerminal, IfcFlowSegment, IfcFlowFitting, IfcBuildingElementProxy, IfcFlowController, IfcFlowMovingDevice","IfcClass","-"]
[null,"52.** afvoeren","w",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar"]
[null,"52.** afvoeren","w",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket"]
[null,"52.** afvoeren","w",null,"e","Systeemtype","-","-","-","-","-","-","System Type","-","-","Duidelijk onderscheid makend in de verschillende systemen "]
["x","52.** afvoeren","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","52.** afvoeren","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"52.** afvoeren","w"]
[null,"52.** afvoeren","w","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","52.** afvoeren","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","52.** afvoeren","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","52.** afvoeren","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","52.** afvoeren","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"52.** afvoeren","w"]
[null,"52.** afvoeren","w","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","52.** afvoeren","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"52.** afvoeren","w"]
[]
[null,"53.** water","w","53.** - Water"]
[null,"53.** water","w","Verzameling van voorzieningen voor transporteren van water, vanaf de hoofd- of dienstvoeding tot aan de verbruikspunten."]
[null,"53.** water","w",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"53.** water","w"]
[null,"53.** water","w","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte, diameter"]
["x","53.** water","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","53.** water","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"53.** water","w"]
[null,"53.** water","w","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument"]
[null,"53.** water","w",null,"g","Entiteit","-","-","-","-","-","-","IfcEnergyConversionDevice, IfcFlowSegment, IfcFlowFitting, IfcBuildingElementProxy, IfcFlowStorageDevice, IfcFlowController, IfcCovering, IfcFlowMovingDevice","IfcClass","-"]
[null,"53.** water","w",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar"]
[null,"53.** water","w",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket"]
[null,"53.** water","w",null,"e","Systeemtype","-","-","-","-","-","-","System Type","-","-","Duidelijk onderscheid makend in de verschillende systemen "]
["x","53.** water","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","53.** water","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"53.** water","w"]
[null,"53.** water","w","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","53.** water","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","53.** water","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","53.** water","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","53.** water","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"53.** water","w"]
[null,"53.** water","w","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","53.** water","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"53.** water","w"]
[]
[null,"54.** gassen","w","54.** - Gassen"]
[null,"54.** gassen","w","Verzameling van voorzieningen voor aansluitingen, opslag, distributie en gebruik van gassen, vanaf de hoofdverdeling of de opslag tot een met de verbruiksaansluiting."]
[null,"54.** gassen","w",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"54.** gassen","w"]
[null,"54.** gassen","w","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte, diameter"]
["x","54.** gassen","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","54.** gassen","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"54.** gassen","w"]
[null,"54.** gassen","w","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument"]
[null,"54.** gassen","w",null,"g","Entiteit","-","-","-","-","-","-","IfcFlowSegment, IfcFlowFitting, IfcBuildingElementProxy, IfcFlowStorageDevice, IfcFlowController, IfcFlowMovingDevice, IfcDistributionControlElement","IfcClass","-"]
[null,"54.** gassen","w",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar"]
[null,"54.** gassen","w",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket"]
[null,"54.** gassen","w",null,"e","Systeemtype","-","-","-","-","-","-","System Type","-","-","Duidelijk onderscheid makend in de verschillende systemen "]
["x","54.** gassen","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","54.** gassen","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"54.** gassen","w"]
[null,"54.** gassen","w","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","54.** gassen","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","54.** gassen","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","54.** gassen","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","54.** gassen","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"54.** gassen","w"]
[null,"54.** gassen","w","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","54.** gassen","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"54.** gassen","w"]
[]
[null,"55.** koude-opwekking","w","55.** - Koude-opwekking",{"$nulls":13},"-"]
[null,"55.** koude-opwekking","w","Verzameling van voorzieningen voor lokaal opwekken en afgeven van koude voor het onderhouden van een behaaglijkheids- en conserveringsklimaat"]
[null,"55.** koude-opwekking","w",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"55.** koude-opwekking","w"]
[null,"55.** koude-opwekking","w","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte, diameter"]
["x","55.** koude-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","55.** koude-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"55.** koude-opwekking","w"]
[null,"55.** koude-opwekking","w","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument"]
[null,"55.** koude-opwekking","w",null,"g","Entiteit","-","-","-","-","-","-","IfcEnergyConversionDevice, IfcFlowSegment, IfcFlowFitting, IfcBuildingElementProxy, IfcFlowStorageDevice, IfcFlowController, IfcCovering, IfcDistributionControlElement","IfcClass","-"]
[null,"55.** koude-opwekking","w",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar"]
[null,"55.** koude-opwekking","w",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket"]
[null,"55.** koude-opwekking","w",null,"e","Systeemtype","-","-","-","-","-","-","System Type","-","-","Duidelijk onderscheid makend in de verschillende systemen "]
["x","55.** koude-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","55.** koude-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"55.** koude-opwekking","w"]
[null,"55.** koude-opwekking","w","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","55.** koude-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","55.** koude-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","55.** koude-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","55.** koude-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"55.** koude-opwekking","w"]
[null,"55.** koude-opwekking","w","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","55.** koude-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"55.** koude-opwekking","w"]
[]
[null,"56.** warmtedistributie","w","56.** - Warmtedistributie"]
[null,"56.** warmtedistributie","w","Verzameling van voorzieningen voor transport, verdeling en afgifte van warmte met als medium water voor het klimaat, vanaf de hoofdverdeling van de warmte-opwekking tot en met de warmteafgifte- eenheden in ruimten."]
[null,"56.** warmtedistributie","w",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"56.** warmtedistributie","w"]
[null,"56.** warmtedistributie","w","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte, diameter"]
["x","56.** warmtedistributie","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","56.** warmtedistributie","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"56.** warmtedistributie","w"]
[null,"56.** warmtedistributie","w","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument"]
[null,"56.** warmtedistributie","w",null,"g","Entiteit","-","-","-","-","-","-","IfcEnergyConversionDevice, IfcFlowSegment, IfcFlowFitting, IfcBuildingElementProxy, IfcFlowController, IfcCovering, IfcFlowMovingDevice, IfcFlowTerminal, IfcTeatmentDevice, IfcFlowTreatmentDevice","IfcClass","-"]
[null,"56.** warmtedistributie","w",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar"]
[null,"56.** warmtedistributie","w",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket"]
[null,"56.** warmtedistributie","w",null,"e","Systeemtype","-","-","-","-","-","-","System Type","-","-","Duidelijk onderscheid makend in de verschillende systemen "]
["x","56.** warmtedistributie","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","56.** warmtedistributie","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"56.** warmtedistributie","w"]
[null,"56.** warmtedistributie","w","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","56.** warmtedistributie","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","56.** warmtedistributie","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","56.** warmtedistributie","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","56.** warmtedistributie","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"56.** warmtedistributie","w"]
[null,"56.** warmtedistributie","w","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","56.** warmtedistributie","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"56.** warmtedistributie","w"]
[]
[null,"57.** luchtbehandeling","w","57.** - Luchtbehandeling"]
[null,"57.** luchtbehandeling","w","Verzameling van voorzieningen voor mechanische ventilatie door toevoer en afvoer van lucht voor het klimaat."]
[null,"57.** luchtbehandeling","w",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"57.** luchtbehandeling","w"]
[null,"57.** luchtbehandeling","w","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte, diameter"]
["x","57.** luchtbehandeling","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","57.** luchtbehandeling","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"57.** luchtbehandeling","w"]
[null,"57.** luchtbehandeling","w","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument"]
[null,"57.** luchtbehandeling","w",null,"g","Entiteit","-","-","-","-","-","-","IfcEnergyConversionDevice, IfcFlowSegment, IfcFlowFitting, IfcBuildingElementProxy, IfcFlowController, IfcCovering, IfcFlowMovingDevice, IfcFlowTerminal, IfcTeatmentDevice, IfcFlowTreatmentDevice","IfcClass","-"]
[null,"57.** luchtbehandeling","w",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar"]
[null,"57.** luchtbehandeling","w",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket"]
[null,"57.** luchtbehandeling","w",null,"e","Systeemtype","-","-","-","-","-","-","System Type","-","-","Duidelijk onderscheid makend in de verschillende toevoer en/of retour en of afzuig systemen "]
["x","57.** luchtbehandeling","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","57.** luchtbehandeling","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"57.** luchtbehandeling","w"]
[null,"57.** luchtbehandeling","w","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","57.** luchtbehandeling","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","57.** luchtbehandeling","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","57.** luchtbehandeling","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","57.** luchtbehandeling","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"57.** luchtbehandeling","w"]
[null,"57.** luchtbehandeling","w","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","57.** luchtbehandeling","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"57.** luchtbehandeling","w"]
[]
[null,"58.** regeling klimaat en sanitair","e","58.** - Regeling klimaat en sanitair"]
[null,"58.** regeling klimaat en sanitair","e","Verzameling van voorzieningen voor melden, meten, en sturen van regelinstallaties voor klimaat sanitair, vanaf aan te sluiten hoofdvoeding tot en met de aan te sluiten regelingen."]
[null,"58.** regeling klimaat en sanitair","e",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"58.** regeling klimaat en sanitair","e"]
[null,"58.** regeling klimaat en sanitair","e","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nhoogte, breedte, dikte"]
[null,"58.** regeling klimaat en sanitair","e",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-"]
["x","58.** regeling klimaat en sanitair","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","58.** regeling klimaat en sanitair","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"58.** regeling klimaat en sanitair","e"]
[null,"58.** regeling klimaat en sanitair","e","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument"]
[null,"58.** regeling klimaat en sanitair","e",null,"g","Entiteit","-","-","-","-","-","-","IfcDistributionControlElement, IfcFlowController, IfcDistributionElement, IfcFlowTerminal, IfcFlowSegment, IfcFlowFitting","IfcClass","-"]
[null,"58.** regeling klimaat en sanitair","e",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar"]
[null,"58.** regeling klimaat en sanitair","e",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket"]
["x","58.** regeling klimaat en sanitair","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","58.** regeling klimaat en sanitair","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"58.** regeling klimaat en sanitair","e"]
[null,"58.** regeling klimaat en sanitair","e","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","58.** regeling klimaat en sanitair","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","58.** regeling klimaat en sanitair","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","58.** regeling klimaat en sanitair","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","58.** regeling klimaat en sanitair","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"58.** regeling klimaat en sanitair","e"]
[null,"58.** regeling klimaat en sanitair","e","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","58.** regeling klimaat en sanitair","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"58.** regeling klimaat en sanitair","e"]
[]
[null,"61.** centrale elektrotechnische voorzieningen","e","61.** - Centrale elektrotechnische voorzieningen"]
[null,"61.** centrale elektrotechnische voorzieningen","e","Verzameling van centrale elektrotechnische voorzieningen ten behoeve van energie, noodstroom, aarding, kanalisatie, hoogspanning, laagspanning, zeer lage spanning en bliksemafleiding."]
[null,"61.** centrale elektrotechnische voorzieningen","e",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"61.** centrale elektrotechnische voorzieningen","e"]
[null,"61.** centrale elektrotechnische voorzieningen","e","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: lengte, hoogte, breedte"]
["x","61.** centrale elektrotechnische voorzieningen","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","61.** centrale elektrotechnische voorzieningen","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"61.** centrale elektrotechnische voorzieningen","e"]
[null,"61.** centrale elektrotechnische voorzieningen","e","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument"]
[null,"61.** centrale elektrotechnische voorzieningen","e",null,"g","Entiteit","-","-","-","-","-","-","IfcEnergyConversionDevice, IfcBuildingElementProxy, IfcFlowController, IfcFlowSegment, IfcFlowFitting, IfcDistributionElement","IfcClass","-"]
[null,"61.** centrale elektrotechnische voorzieningen","e",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar"]
[null,"61.** centrale elektrotechnische voorzieningen","e",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket"]
[null,"61.** centrale elektrotechnische voorzieningen","e",null,"e","Groepsnaam/nummer","-","-","-","-","-","-",null,"-","-","Opvolgend benaming en/of codering waar het element aan is verbonden."]
[null,"61.** centrale elektrotechnische voorzieningen","e",null,"e","Groepenkast naam/nummer","-","-","-","-","-","-",null,"-","-","Korte benaming en/of codering waar het element aan is verbonden."]
["x","61.** centrale elektrotechnische voorzieningen","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","61.** centrale elektrotechnische voorzieningen","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"61.** centrale elektrotechnische voorzieningen","e"]
[null,"61.** centrale elektrotechnische voorzieningen","e","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","61.** centrale elektrotechnische voorzieningen","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","61.** centrale elektrotechnische voorzieningen","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","61.** centrale elektrotechnische voorzieningen","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","61.** centrale elektrotechnische voorzieningen","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"61.** centrale elektrotechnische voorzieningen","e"]
[null,"61.** centrale elektrotechnische voorzieningen","e","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","61.** centrale elektrotechnische voorzieningen","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"61.** centrale elektrotechnische voorzieningen","e"]
[]
[null,"62.** krachtstroom","e","62.** - Krachtstroom"]
[null,"62.** krachtstroom","e","Verzameling van voorzieningen lager dan 1Kv vanaf de hoofdverdelers tot aan de verbruikers. "]
[null,"62.** krachtstroom","e",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"62.** krachtstroom","e"]
[null,"62.** krachtstroom","e","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: lengte, hoogte, breedte"]
["x","62.** krachtstroom","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","62.** krachtstroom","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"62.** krachtstroom","e"]
[null,"62.** krachtstroom","e","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument"]
[null,"62.** krachtstroom","e",null,"g","Entiteit","-","-","-","-","-","-","IfcEnergyConversionDevice, IfcBuildingElementProxy, IfcFlowController, IfcFlowSegment, IfcFlowTerminal","IfcClass","-"]
[null,"62.** krachtstroom","e",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar"]
[null,"62.** krachtstroom","e",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket"]
[null,"62.** krachtstroom","e",null,"e","Groepsnaam/nummer","-","-","-","-","-","-",null,"-","-","Opvolgend benaming en/of codering waar het element aan is verbonden."]
[null,"62.** krachtstroom","e",null,"e","Groepenkast naam/nummer","-","-","-","-","-","-",null,"-","-","Korte benaming en/of codering waar het element aan is verbonden."]
["x","62.** krachtstroom","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","62.** krachtstroom","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"62.** krachtstroom","e"]
[null,"62.** krachtstroom","e","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","62.** krachtstroom","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","62.** krachtstroom","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","62.** krachtstroom","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","62.** krachtstroom","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"62.** krachtstroom","e"]
[null,"62.** krachtstroom","e","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","62.** krachtstroom","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"62.** krachtstroom","e"]
[]
[null,"63.** verlichting","e","63.** - Verlichting",{"$nulls":13},"-"]
[null,"63.** verlichting","e","Verzameling van voorzieningen lager dan 1Kv vanaf de hoofdverdelers tot aan de verbruikers. "]
[null,"63.** verlichting","e",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"63.** verlichting","e"]
[null,"63.** verlichting","e","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte"]
[null,"63.** verlichting","e",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-"]
["x","63.** verlichting","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","63.** verlichting","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"63.** verlichting","e"]
[null,"63.** verlichting","e","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument"]
[null,"63.** verlichting","e",null,"g","Entiteit","-","-","-","-","-","-","IfcBuildingElementProxy, IfcFlowController, IfcFlowSegment, IfcFlowTerminal","IfcClass","-"]
[null,"63.** verlichting","e",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar"]
[null,"63.** verlichting","e",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket"]
[null,"63.** verlichting","e",null,"e","Groepsnaam/nummer","-","-","-","-","-","-",null,"-","-","Opvolgend benaming en/of codering waar het element aan is verbonden."]
[null,"63.** verlichting","e",null,"e","Groepenkast naam/nummer","-","-","-","-","-","-",null,"-","-","Korte benaming en/of codering waar het element aan is verbonden."]
["x","63.** verlichting","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","63.** verlichting","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"63.** verlichting","e"]
[null,"63.** verlichting","e","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","63.** verlichting","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","63.** verlichting","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","63.** verlichting","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","63.** verlichting","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"63.** verlichting","e"]
[null,"63.** verlichting","e","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","63.** verlichting","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"63.** verlichting","e"]
[]
[null,"64.** communicatie","e","64.** - Communicatie"]
[null,"64.** communicatie","e","Verzameling van voorzieningen voor informatieoverdracht door middel van signalen, geluiden, beelden, data en de combinatie tussen allen. "]
[null,"64.** communicatie","e",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"64.** communicatie","e"]
[null,"64.** communicatie","e","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte, …"]
["x","64.** communicatie","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","64.** communicatie","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"64.** communicatie","e"]
[null,"64.** communicatie","e","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument"]
[null,"64.** communicatie","e",null,"g","Entiteit","-","-","-","-","-","-","IfcBuildingElementProxy, IfcFlowStorageDevice, IfcFlowSegment, IfcFlowTerminal, IfcFlowController","IfcClass","-"]
[null,"64.** communicatie","e",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar"]
[null,"64.** communicatie","e",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket"]
[null,"64.** communicatie","e",null,"e","Groepsnaam/nummer","-","-","-","-","-","-",null,"-","-","Opvolgend benaming en/of codering waar het element aan is verbonden."]
[null,"64.** communicatie","e",null,"e","Groepenkast naam/nummer","-","-","-","-","-","-",null,"-","-","Korte benaming en/of codering waar het element aan is verbonden."]
["x","64.** communicatie","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","64.** communicatie","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"64.** communicatie","e"]
[null,"64.** communicatie","e","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","64.** communicatie","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","64.** communicatie","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","64.** communicatie","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","64.** communicatie","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"64.** communicatie","e"]
[null,"64.** communicatie","e","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","64.** communicatie","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"64.** communicatie","e"]
[]
[null,"65.** beveiliging","e","65.** - Beveiliging"]
[null,"65.** beveiliging","e","Verzameling van voorzieningen voor het voorkomen, melden, beperken en bestrijden van brand, inbraak en uitbraak, overlast, sociale noden van personen en dieren, milieua-overlast, etc. "]
[null,"65.** beveiliging","e",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"65.** beveiliging","e"]
[null,"65.** beveiliging","e","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte, …"]
["x","65.** beveiliging","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","65.** beveiliging","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"65.** beveiliging","e"]
[null,"65.** beveiliging","e","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument"]
[null,"65.** beveiliging","e",null,"g","Entiteit","-","-","-","-","-","-","IfcBuildingElementProxy, IfcFlowStorageDevice, IfcFlowSegment, IfcFlowTerminal, IfcFlowController, IfcDistributionControlElement, IfcFlowFitting","IfcClass","-"]
[null,"65.** beveiliging","e",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar"]
[null,"65.** beveiliging","e",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket"]
[null,"65.** beveiliging","e",null,"e","Groepsnaam/nummer","-","-","-","-","-","-",null,"-","-","Opvolgend benaming en/of codering waar het element aan is verbonden."]
[null,"65.** beveiliging","e",null,"e","Groepenkast naam/nummer","-","-","-","-","-","-",null,"-","-","Korte benaming en/of codering waar het element aan is verbonden."]
["x","65.** beveiliging","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","65.** beveiliging","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"65.** beveiliging","e"]
[null,"65.** beveiliging","e","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","65.** beveiliging","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","65.** beveiliging","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","65.** beveiliging","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","65.** beveiliging","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"65.** beveiliging","e"]
[null,"65.** beveiliging","e","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","65.** beveiliging","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"65.** beveiliging","e"]
[]
[null,"66.** transport","b","66.** - Transport",{"$nulls":13},"-"]
[null,"66.** transport","b","Verzameling van voorzieningen voor het verticale en horizontale transport van personen en goederen door middel van liften en roltrappen\nNoot: Elementkaart is geconcentreerd op de bouwkundige gegevensbehoefte en esthetische verschijningsvorm binnen het prestatiemodel. Deze keuze is gemaakt vanwege de realisatie van liften/ roltrappen en daarin de rol van de liftleverancier en de installateur."]
[null,"66.** transport","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"66.** transport","b"]
[null,"66.** transport","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte",null,"v"]
[null,"66.** transport","b",null,"e","Ruimtebeslag tbv onderhoud","-","-","-","-","-","-","-","-","-",null,null,"x"]
[null,"66.** transport","b",null,"e","Vlakverdeling/ invullingen","-","-","-","-","-","-","-","-","-",null,null,"x"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"66.** transport","b"]
[null,"66.** transport","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"66.** transport","b",null,"g","Entiteit","-","-","-","-","-","-","IfcTransportElement, IfcBuildingElementProxy, IfcFlowSegment, IfcFlowFitting, IfcFlowMovingDevice, IfcFlowTerminal","IfcClass","-",null,null,"v"]
[null,"66.** transport","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"66.** transport","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"66.** transport","b",null,"p","Liftnummer","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelLabel","-","-","Uniek nummer per lift"]
[null,"66.** transport","b",null,"p","Systeemtype","-","-","-","-","-","-","System Type","-","-","In overleg met leverancier"]
[null,"66.** transport","b",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"66.** transport","b",null,"p","Merk","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelReference","-","-","Ten behoeve van onderhoud"]
[null,"66.** transport","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"66.** transport","b"]
[null,"66.** transport","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"x"]
[null,"66.** transport","b",null,"e","In/ uitwendig","-","-","-","-","-","-","IsExternal benoemen in custom Pset","true/ false","-","Benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Pset_SpaceCommon in Ifc 2x3",null,"-","ifcBuildingElementProxy ok, aan te maken voor overige eniteiten",null,"ifcTransportElement, ifcFlowSegment, ifcFlowFitting, ifcFlowMovingDevice, ifcFlowTerminal is been deprecated and will soon become abstract?",{"$nulls":4},"ifcTransportElement, ifcFlowSegment, ifcFlowFitting, ifcFlowMovingDevice, ifcFlowTerminal"]
[null,"66.** transport","b",null,"e","Brandwerendheid","-","-","-","-","-","-","FireRating benoemen in custom Pset","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering., volgens separaat afsprakendocument. 0, 20, 30, 60, etc... (WBDBO)(bij elementen ter plaatse doorgang brandwerend element)\n\nbenoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset voor meest geëigende entiteiten",null,"-","ifcBuildingElementProxy ok, aan te maken voor overige eniteiten",null,"ifcTransportElement, ifcFlowSegment, ifcFlowFitting, ifcFlowMovingDevice, ifcFlowTerminal is been deprecated and will soon become abstract?",{"$nulls":4},"ifcTransportElement, ifcFlowSegment, ifcFlowFitting, ifcFlowMovingDevice, ifcFlowTerminal"]
[null,"66.** transport","b",null,"p","Capaciteit (aantal personen)","-","-","-","-","-","-","-","-"]
[null,"66.** transport","b",null,"p","Vluchtdeur","-","-","-","-","-","-","Pset_TransportElementCommon: FireExit","true/ false","-","Indien entiteit IfcBuildingElementProxy, IfcFlowSegment, IfcFlowFitting, IfcFlowMovingDevice, IfcFlowTerminal: benoemen in Custom Pset omdat 'FireExit' geen deel uitmaakt van Common Pset"]
[null,"66.** transport","b",null,"p","Groepnaam/nummer","-","-","-","-","-","-","-","-","-","In overleg met Installateur"]
[null,"66.** transport","b",null,"p","Groepkast naam/ nummer","-","-","-","-","-","-","-","-","-","In overleg met Installateur"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"66.** transport","b"]
[null,"66.** transport","b","Componenten","e","Sparingsopgave","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"x"]
[null,"66.** transport","b",null,"e","Bediening","-","-","-","-","-","-","-","-","-","Twin, Tripple, etc",null,"x"]
[null,"66.** transport","b",null,"e","Verankering en bevestiging","-","-","-","-","-","-","-","-","-","Niet modelleren, wel terug laten komen in details",null,"x"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"66.** transport","b"]
[]
[null,"7*.** vaste inventaris","i","7*.** - Vaste inventaris",{"$nulls":13},"-"]
[null,"7*.** vaste inventaris","i","Onder vaste inventaris vallen; verkeersvoorzieningen, gebruikersvoorzieningen keukenvoorzieningen, sanitaire voorzieningen, schoonmaakvoorzieningen en opslagvoorzieningen\nNoot: Elementkaart is geconcentreerd op de bouwkundige gegevensbehoefte en esthetische verschijningsvorm binnen het prestatiemodel. "]
[null,"7*.** vaste inventaris","i",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"7*.** vaste inventaris","i"]
[null,"7*.** vaste inventaris","i","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte",null,"x"]
[null,"7*.** vaste inventaris","i",null,"e","Vlakverdeling/ invullingen","-","-","-","-","-","-","-","-","-",null,null,"x"]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"7*.** vaste inventaris","i"]
[null,"7*.** vaste inventaris","i","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"7*.** vaste inventaris","i",null,"g","Entiteit","-","-","-","-","-","-","IfcFurnishingElement, IfcBuildingElementProxy, IfcFlowTerminal, IfcStair, IfcStairFlight, IfcRailing, IfcSlab","IfcClass","-",null,null,"v"]
[null,"7*.** vaste inventaris","i",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"7*.** vaste inventaris","i",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"7*.** vaste inventaris","i",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"7*.** vaste inventaris","i",null,"p","Merk","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelReference","-","-","Ten behoeve van onderhoud"]
[null,"7*.** vaste inventaris","i",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"7*.** vaste inventaris","i"]
[null,"7*.** vaste inventaris","i","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"!","MAT"]
[null,"7*.** vaste inventaris","i",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"!","MAT"]
[null,"7*.** vaste inventaris","i",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_SlabCommon: Loadbearing","true/ false","-","Indien entiteit IfcFurnishingElement, IfcBuildingElementProxy, IfcFlowTerminal, IfcStair, IfcStairFlight, IfcRailing: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"v",{"$nulls":11}," IfcSlab","parent","Pset_<Entity>Common","LoadBearing",null,"ifcBoolean"]
[null,"7*.** vaste inventaris","i",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-","Indien entiteit IfcFurnishingElement, IfcBuildingElementProxy, IfcFlowTerminal, IfcStairFlight: benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset",null,"v",{"$nulls":11},"IfcStair, IfcStairFlight, IfcRailing, IfcSlab","parent","Pset_<Entity>Common","isExternal",null,"ifcBoolean"]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"7*.** vaste inventaris","i"]
[null,"7*.** vaste inventaris","i","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"7*.** vaste inventaris","i"]
[]
[null,"8*.** losse inventaris","i","8*.** - Losse inventaris",{"$nulls":13},"-"]
[null,"8*.** losse inventaris","i","Onder losse inventaris vallen; verkeersinventaris, gebruikersinventaris, keukeninventaris, sanitaire inventaris, schoonmaakinventaris.\nNoot: Elementkaart is geconcentreerd op de bouwkundige gegevensbehoefte en esthetische verschijningsvorm binnen het prestatiemodel. "]
[null,"8*.** losse inventaris","i",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"8*.** losse inventaris","i"]
[null,"8*.** losse inventaris","i","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte",null,"x"]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"8*.** losse inventaris","i"]
[null,"8*.** losse inventaris","i","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"8*.** losse inventaris","i",null,"g","Entiteit","-","-","-","-","-","-","IfcFurnishingElement, IfcBuildingElementProxy, IfcFlowTerminal","IfcClass","-",null,null,"v"]
[null,"8*.** losse inventaris","i",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"8*.** losse inventaris","i",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"8*.** losse inventaris","i",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"8*.** losse inventaris","i",null,"p","Merk","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelReference","-","-","Ten behoeve van onderhoud"]
[null,"8*.** losse inventaris","i",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"8*.** losse inventaris","i"]
[null,"8*.** losse inventaris","i","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"!","MAT"]
[null,"8*.** losse inventaris","i",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"!","MAT"]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"8*.** losse inventaris","i"]
[null,"8*.** losse inventaris","i","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"8*.** losse inventaris","i"]
[]
[null,"90.** terrein","t","90.** - Terrein",{"$nulls":13},"-"]
[null,"90.** terrein","t","Onder terrein vallen grondvoorziening, opstallen, omheiningen en  terreinafwerkingen."]
[null,"90.** terrein","t",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"90.** terrein","t"]
[null,"90.** terrein","t","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte",null,"x"]
[null,"90.** terrein","t",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,"x"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"90.** terrein","t"]
[null,"90.** terrein","t","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"v"]
[null,"90.** terrein","t",null,"g","Entiteit","-","-","-","-","-","-","IfcBuildingElementProxy","IfcClass","-",null,null,"v"]
[null,"90.** terrein","t",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"v"]
[null,"90.** terrein","t",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"v"]
[null,"90.** terrein","t",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"90.** terrein","t",null,"p","Merk","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelReference","-","-","Ten behoeve van onderhoud"]
[null,"90.** terrein","t",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"90.** terrein","t"]
[null,"90.** terrein","t","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"!","MAT"]
[null,"90.** terrein","t",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"!","MAT"]
[null,"90.** terrein","t",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","benoemen in custom Pset","true/ false","-","Indien entiteit IfcBuildingElementProxy: benoemen in Custom Pset omdat Pset_BuildingElementProxyCommon in Ifc 2x3 niet bestaat",null,"x","IFC2x3 PsetBUildingElementProxyCommon bestaat, enkel deze props niet - BS bestaat pset, maar prop niet","x","v"]
[null,"90.** terrein","t",null,"e","In/ uitwendig","-","-","-","-","-","-","IsExternal benoemen in custom Pset","true/ false","-","Indien entiteit IfcBuildingElementProxy: benoemen in Custom Pset omdat Pset_BuildingElementProxyCommon in Ifc 2x3 niet bestaat",null,"x","IFC2x3 PsetBUildingElementProxyCommon bestaat, enkel deze props niet - BS bestaat pset, maar prop niet","x","v"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"90.** terrein","t"]
[null,"90.** terrein","t","Componenten","e","Bevestigingsconstructies","-","-","-","-","-","-","-","-","-"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"90.** terrein","t"]

{"sheet":"ILS O&E in Archicad","index":1,"n_rows":1829,"n_cols":26,"rows_kept":1829,"cut":false,"hidden":false,"merged":[[4,3,4,11],[13,3,13,5],[18,3,18,14],[19,3,19,14],[58,3,58,14],[1,22,1,24],[178,15,179,15],[179,3,179,14],[231,3,231,14],[231,15,232,15],[232,3,232,14],[270,3,270,14],[270,15,271,15],[271,3,271,14],[58,15,59,15],[59,3,59,14],[100,3,100,14],[100,15,101,15],[101,3,101,14],[137,3,137,14],[137,15,138,15],[138,3,138,14],[413,3,413,14],[413,15,414,15],[414,3,414,14],[459,3,459,14],[459,15,460,15],[460,3,460,14],[320,3,320,14],[320,15,321,15],[321,3,321,14],[367,3,367,14],[367,15,368,15],[368,3,368,14],[616,3,616,14],[616,15,617,15],[617,3,617,14],[659,3,659,14],[659,15,660,15],[660,3,660,14],[504,3,504,14],[504,15,505,15],[505,3,505,14],[554,3,554,14],[554,15,555,15],[555,3,555,14],[809,3,809,14],[810,3,810,14],[811,3,811,14],[812,3,812,14],[813,3,813,14],[814,3,814,14],[697,3,697,14],[697,15,698,15],[698,3,698,14],[748,3,748,14],[748,15,749,15],[749,3,749,14],[894,3,894,14],[895,3,895,14],[896,3,896,14],[897,3,897,14],[898,3,898,14],[899,3,899,14],[815,3,815,14],[816,3,816,14],[816,15,817,15],[817,3,817,14],[891,3,891,14],[892,3,892,14],[1037,3,1037,14],[1037,15,1038,15],[1038,3,1038,14],[1106,3,1106,14],[1106,15,1107,15],[1107,3,1107,14],[966,3,966,14],[966,15,967,15],[967,3,967,14],[1004,3,1004,14],[1004,15,1005,15],[1005,3,1005,14],[1226,3,1226,14],[1226,15,1227,15],[1227,3,1227,14],[1267,3,1267,14],[1267,15,1268,15],[1268,3,1268,14],[1143,3,1143,14],[1143,15,1144,15],[1144,3,1144,14],[1181,3,1181,14],[1181,15,1182,15],[1182,3,1182,14],[1373,3,1373,14],[1399,3,1399,14],[1400,3,1400,14],[1425,3,1425,14],[1426,3,1426,14],[1451,3,1451,14],[1310,3,1310,14],[1310,15,1311,15],[1311,3,1311,14],[1346,3,1346,14],[1347,3,1347,14],[1372,3,1372,14],[1530,3,1530,14],[1555,3,1555,14],[1556,3,1556,14],[1582,3,1582,14],[1583,3,1583,14],[1609,3,1609,14],[1452,3,1452,14],[1477,3,1477,14],[1478,3,1478,14],[1503,3,1503,14],[1504,3,1504,14],[1529,3,1529,14],[1797,3,1797,14],[1692,3,1692,14],[1733,3,1733,14],[1734,3,1734,14],[1766,3,1766,14],[1767,3,1767,14],[1796,3,1796,14],[1610,3,1610,14],[1637,3,1637,14],[1638,3,1638,14],[1664,3,1664,14],[1665,3,1665,14],[1691,3,1691,14]]}
["N.v.t.","NL-SfB codering","Discipline","Soort Informatie","g,e,p","Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking",null,"Reeds aanwezig in BIM basis ILS","Bronwaarde in Archicad","Archicad Classification NED 2.0","Classificatie NL SfB","In te vullen in schedule","IFC Entiteit \n(kolom 1)","Property Set in IFC\n(kolom 2)","Property naam in IFC\n(kolom 2)","Waarde in IFC"]
[{"$nulls":22},"Property Mapping ILS O&E voor translator ILS-O&E BWK"]
[]
[null,null,"u","Leeswijzer"]
[null,null,"u","*Uitgangspunt is minimaal BIM basis ILS v1.0"]
[null,null,"u","*Opgesteld voor de inhoud van prestatiemodellen, met als enige uitzondering de eventuele verdere productuitwerking vanuit een adviseur tijdens de UO Fase."]
[null,null,"u","*Definities en inbegrepen op basis van NL-SfB (site BIM Loket)"]
[null,null,"u","*De NL-SfB code [38.1*- Inbouwpakketten] is een samenstelling van verschillende componenten, denk aan wanden, vloeren, plafonds, openingen, installatiecomponenten. Voor de gegevensbehoefte wordt hiervoor verwezen naar de van toepassing zijnde kaarten."]
[null,null,"u","*De NL-SfB code [48.1*- Afwerkingspakketten] is een samenstelling van verschillende componenten, denk aan wandafwerking, vloerafwerking, plafondsafwerking. Voor de gegevensbehoefte wordt hiervoor verwezen naar de van toepassing zijnde kaarten."]
[null,null,"u","*Verantwoordelijkheden t.a.v. het aanleveren, modelleren en valideren van de informatie in het model dienen te worden omschreven en een separaat afsprakendocument."]
[null,null,"u",null,"g","Generiek, voor alle elementen en over de projecten heen"]
[null,null,"u",null,"e","Element specifiek, over de projecten heen"]
[null,null,"u",null,"p","Project specifiek"]
[null,null,"u","*Fasering op basis van DNR STB 2014 aangevuld met as-build en as-maintained",null,null,"SO","VO","DO","TO","UO","AS-B"]
[null,null,"u","*Er mogen geen meerdere waarden in een parameter worden ingevuld."]
[null,null,"u","*Fase is uitgelicht wanneer er in de Fase een toevoeging, aanpassing of verdere detailuitwerking wordt verwacht van het betreffende element en bevat minimaal de informatie van de voorgaande Fases."]
[]
[]
[null,"00. ruimtes","b","00 - Ruimtes",{"$nulls":15},"Alle classificaties in tak 'Ruimte'","-",null,"IfcSpace"]
[null,"00. ruimtes","b","De ruimte is het driedimensionale IFC-object dat in beginsel begrensd is door de haar omhullende materiële bouwwerkelementen (wanden, vloeren etc.) en in haar vorm op deze omhullende elementen aansluit. Een ruimte is hetzij een binnenruimte, hetzij een buitenruimte.\nContour:\nIn het algemeen volgt de contour van het driedimensionale object op vloerniveau de netto-contour van de ruimte langs de binnenzijde van de omhullende bouwwerkelementen. Interne bouwwerkelementen, zoals kolommen, zijn ongeacht hun grootte als inwendige contour van het ruimteobject uitgesloten.\n- Bij een ruimte in een trappenhuis, liftschacht of installatieschacht wordt in beginsel de netto-contour van de koker aangehouden.\n- Indien wet- en regelgeving dit vereist, mag een ruimte waar nodig opgesplitst worden afwijkend van de materiële omhullende bouwwerkelementen.\nHoogte:\nIn het algemeen is de hoogte van het driedimensionale object de netto-hoogte van de ruimte, gemeten vanaf de bovenzijde van de afgewerkte vloer tot aan de onderzijde van het element dat de ruimte aan de bovenzijde begrenst.\n- Voor binnenruimten: de bovenbegrenzing van de ruimte is doorgaans de onderzijde van het (verlaagd) plafond. Een ruimte kan een variërende hoogte hebben binnen dezelfde bouwlaag, maar kan ook lokaal of in haar geheel een hoogte hebben die de bouwlaaghoogte overstijgt, bijvoorbeeld door het ontbreken van (delen van) een vloer of door vloeropeningen. Bouwlaagoverstijgende ruimten worden per bouwlaag opgesplitst ter hoogte van het bijbehorende bouwlaagniveau. De ruimtedelen sluiten in verticale zin op elkaar aan.\n- Voor buitenruimten: bij het ontbreken van een materiële begrenzing aan de bovenzijde is de hoogte van de ruimte deze van de bouwlaag waartoe de ruimte behoort."]
[null,"00. ruimtes","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"00. ruimtes","b"]
[null,"00. ruimtes","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","ObjectType","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte (projectafhankelijk: BVO, GO, VVO), netto contour, netto hoogte",null,"Ja","3D model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"00. ruimtes","b"]
[null,"00. ruimtes","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","vastleggen in separaat afsprakendocument",null,"Ja","Design > Story Settings",null,null,"n.v.t.","IfcBuildingStorey","n.v.t.","n.v.t.","IfcBuildingStorey"]
[null,"00. ruimtes","b",null,"g","Entiteit","-","-","-","-","-","-","IfcSpace, IfcZone","IfcClass","-",null,null,"Ja","Archicad Classification NED 2.0",null,null,"ILS 3.4-Entiteiten","n.v.t.","n.v.t.","n.v.t.","IfcSpace"]
[null,"00. ruimtes","b",null,"e","Ruimtenaam","-","-","-","-","-","-","Longname","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja","Zoneinstellingen > Zone Name",null,null,"O&E-00-Ruimtes, kolom Naam","IfcSpace","Attributes","Name","Longname"]
[null,"00. ruimtes","b",null,"e","Ruimtenummer","-","-","-","-","-","-","ShortName","-","-","Uniek nummer per ruimte (conform separaat afsprakendocument)",null,"Ja","Zoneinstellingen > Zone Number",null,null,"O&E-00-Ruimtes, kolom Zonenummer","IfcSpace","Attributes","GlobalId (ifcRoot)","Name"]
[null,"00. ruimtes","b",null,"p","Bouwnummer","-","-","-","-","-","-","-","-","-"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"00. ruimtes","b"]
[null,"00. ruimtes","b","Eigenschappen","e","Binnen/ buitenruimte","-","-","-","-","-","-","IsExternal, benoemen in Custom Pset","true/ false","-","Benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Pset_SpaceCommon in Ifc 2x3",null,"Nee","Zoneinstellingen > Classification and Properties  > IFC Properties > Is External (ILS O&E BWK)",null,null,"n.v.t. (zie instellingenvenster)","IfcSpace","ILS O&E BWK","IsExternal","True/False"]
[]
[null,"00. ruimtes","b",null,"e","Ruimtefunctie","-","-","-","-","-","-","ObjectType","-","-","Zoals gedefinieerd in het Bouwbesluit",null,"Nee","ACP: Gebruiksfunctie ",null,null,"O&E-00-Ruimtes, kolom Ruimtefunctie","IfcSpace\nIfcSpaceType","Pset_SpaceCommon\nAttributes","Category\nName (IfcRoot)","Category\nType"]
[{"$nulls":17},"Nee","Zone Category",null,null,"n.v.t. (zie instellingenvenster)","IfcSpace","Attributes","Description (IfcRoot)","Description"]
[null,"00. ruimtes","b",null,"e","Wandafwerking","-","-","-","-","-","-","Pset_SpaceCommon:WallCovering","-","-","Wannneer niet los gemodelleerd, als eigenschap meenemen in de ruimte. Bij meerdere afwerkingen Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"Nee","ACP: aanwezig en mapping actief",null,null,"O&E-00-Ruimtes, Afwerking wand","IfcSpace","Pset_SpaceCommon","WallCovering","WallCovering"]
[null,"00. ruimtes","b",null,"e","Vloerafwerking","-","-","-","-","-","-","Pset_SpaceCommon:FloorCovering","-","-","Wannneer niet los gemodelleerd, als eigenschap meenemen in de ruimte. Bij meerdere afwerkingen Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"Nee","ACP: aanwezig en mapping actief",null,null,"O&E-00-Ruimtes, Afwerking vloer","IfcSpace","Pset_SpaceCommon","FloorCovering","FloorCovering"]
[null,"00. ruimtes","b",null,"e","Plafondafwerking","-","-","-","-","-","-","Pset_SpaceCommon:CeilingCovering","-","-","Wannneer niet los gemodelleerd, als eigenschap meenemen in de ruimte. Bij meerdere afwerkingen Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"Nee","ACP: aanwezig en mapping actief",null,null,"O&E-00-Ruimtes, Afwerking plafond","IfcSpace","Pset_SpaceCommon","CeilingCovering","CeilingCovering"]
[null,"00. ruimtes","b",null,"p","Zonering Gebruiksfunctie","-","-","-","-","-","-","IfcSpace; is gerelateerd aan IfcZone","-","-"]
[null,"00. ruimtes","b",null,"p","Zonering Gebruiksgebied","-","-","-","-","-","-","IfcSpace; is gerelateerd aan IfcZone","-","-"]
[null,"00. ruimtes","b",null,"p","Zonering Verblijfsgebied","-","-","-","-","-","-","IfcSpace; is gerelateerd aan IfcZone","-","-"]
[null,"00. ruimtes","b",null,"p","Zonering Brandcompartimentering","-","-","-","-","-","-","IfcSpace; is gerelateerd aan IfcZone","-","-"]
[null,"00. ruimtes","b",null,"p","Zonering Vluchtroute","-","-","-","-","-","-","IfcSpace; is gerelateerd aan IfcZone","-","-"]
[null,"00. ruimtes","b",null,"p","Max. aantal pers. in Verblijfsgebied","-","-","-","-","-","-","Pset_SpaceOccupancyRequirements: OccupancyNumberPeak","aantal","stuks","Volgens vigerend bouwbesluit het aantal personen dat maximaal gelijktijdig in het verblijfsgebied aanwezig is. "]
[null,"00. ruimtes","b",null,"p","Aantal pers. in Verblijfsgebied","-","-","-","-","-","-","Pset_SpaceOccupancyRequirements: OccupancyNumber","aantal","stuks"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"00. ruimtes","b"]
[null,"00. ruimtes","b","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","00. ruimtes","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"00. ruimtes","b"]
[]
[null,"11.** bodemvoorzieningen","c","11.** - Bodemvoorzieningen; grond & water",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - verwijderen van oude opstallen, beplantingen en funderingsresten - maatvoering van het gebouw in het terrein, bouwramen - damwanden, taludvoorzieningen en grondverbeteringen ten behoeve van de bouwput - ontgraven van de bouwput - aanvullen van de bouwput - voorzieningen aan belendende percelen - verwijderen van tijdelijke voorzieningen/ - damwanden ten behoeve van de bemalingen - bemalingen inclusief leidingwerken, pompen en sleuven - lozingsvoorzieningen, inclusief vergunningen - energieverbruik van de bemalingen",null,null,null,"Terrein","11.** bodemvoorzieningen"]
[null,"11.** bodemvoorzieningen","c","Grond; Verzameling van grondvoorzieningen, die als voorbereidende werken noodzakelijk zijn voor het aanleggen van de gebouwfundatie, gerekend vanaf het toegankelijk maken van het terrein tot aan de funderingsconstructie.\n\nWater; Verzameling van tijdelijke voorzieningen, die noodzakelijk zijn voor de verlaging van grondwaterstanden en de afvoer van oppervlaktewater, voor het aanleggen van de gebouwfundatie."]
[null,"11.** bodemvoorzieningen","c",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"11.** bodemvoorzieningen","c"]
[null,"11.** bodemvoorzieningen","c","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, dikte, omtrek, volume",null,"Ja","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"11.** bodemvoorzieningen","c",null,"e","Positiebepaling","-","-","-","-","-","-","-","-","-","Bijv. puntniveau t.o.v. peil, bovenkant t.o.v. NAP, onderkant t.o.v. NAP",null,"Ja",{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"11.** bodemvoorzieningen","c",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee","Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'.",null,null,"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"]
[null,"11.** bodemvoorzieningen","c",null,"p","Hijsvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"11.** bodemvoorzieningen","c"]
[null,"11.** bodemvoorzieningen","c","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afspraken document",null,"Ja",{"$f":"$S$27","v":"Design > Story Settings"},null,null,{"$f":"$V$27","v":"n.v.t."},{"$f":"$W$27","v":"IfcBuildingStorey"},{"$f":"$X$27","v":"n.v.t."},{"$f":"$Y$27","v":"n.v.t."},{"$f":"$Z$27","v":"IfcBuildingStorey"}]
[null,"11.** bodemvoorzieningen","c",null,"g","Entiteit","-","-","-","-","-","-","IfcSlab, IfcPlate, IfcBuildingElementProxy","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcBuilding ElementProxy"]
[]
[]
[]
[null,"11.** bodemvoorzieningen","c",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja","NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID",null,null,"ILS 3.6-SfB omschrijving","(ifcElement)","Attributes","Name","00_<Entiteit>_<Element-x>"]
[]
[null,"11.** bodemvoorzieningen","c",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"11.** bodemvoorzieningen","c",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"11.** bodemvoorzieningen","c"]
[null,"11.** bodemvoorzieningen","c","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee","ACP: Building material properties",null,null,"n.v.t. (zie Building Material Settings)","IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan.","Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK.","Een of meerdere, afhankelijk van mapping","Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"]
[null,"11.** bodemvoorzieningen","c",null,"e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","Indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"Nee","A: Wordt voor Building Element Parts automatisch ingevuld (Mass):\nDensity in kg/m3 (Building Material Settings) x volume \n\nB: Gewicht volledig element moet handmatig ingevuld worden (zie Helpcenter)",null,null,"A: Automatisch (gekoppeld aan Building Materials)\n\nB: O&E-99-Gewicht samengestelde elementen (C)","A: IfcBuildingElementPart\n\nB: Ifc(Element)","A: Pset_PrecastConcreteElementGeneral\n\nB: ILS O&E BWK","A: ElementWeight\n\nB: Massa","A: ElementWeight in kg\n\nB: Massa in kg"]
[]
[]
[null,"11.** bodemvoorzieningen","c",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","Indien entiteit IfcBuildingElementProxy: benoemen in Custom Pset omdat Pset_BuildingElementProxyCommon in Ifc 2x3 niet bestaat",null,"Nee","Structural Function (instellingenvenster > Classifications and Properties)",null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},"ifcSlab, ifcPlate","ILS O&E BWK","LoadBearing","True/False"]
[]
[]
[null,"11.** bodemvoorzieningen","c",null,"p","Brandwerendheid hoofddraagconstructie","-","-","-","-","-","-","brandwerendheid tot bezwijken, benoemen in Custom Pset","moment tot bezwijken","minuten"]
[null,"11.** bodemvoorzieningen","c","#staal","p","Staalkwaliteit","-","-","-","-","-","-","staalkwaliteit, benoemen in Custom Pset","classificatie","-","Vb.: S235, S355"]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"11.** bodemvoorzieningen","c"]
[null,"11.** bodemvoorzieningen","c","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","11.** bodemvoorzieningen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"11.** bodemvoorzieningen","c"]
[]
[null,"13.1* vloeren op grondslag; niet constructief","b","13.1* - Vloeren op grondslag; niet constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - tot de vloer behorende pompputten - egaliseren van de grondslag - vochtwerende lagen - werkvloeren onder de vloerconstructie - tot de vloer behorende verzwaringen - gebouwisolatievoorzieningen - vloerafwerkingen die één geheel vormen met de vloerconstructie"]
[null,"13.1* vloeren op grondslag; niet constructief","b","Verzameling van niet tot de draagconstructie van het gebouw behorende vloeren, in rechtstreeks contact met de ondergrond aangebracht, gerekend vanaf de binnenzijde van de buitengevel of funderingsconstructie."]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"13.1* vloeren op grondslag; niet constructief","b"]
[null,"13.1* vloeren op grondslag; niet constructief","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, dikte, omtrek, volume",null,"Ja",{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee",{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."},null,null,{"$f":"$V$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$W$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$X$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Y$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Z$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"}]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"e","Nokken en sponningen","-","-","-","-","-","-","-","-","-",null,null,"Ja",{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,"Ja",{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"13.1* vloeren op grondslag; niet constructief","b"]
[null,"13.1* vloeren op grondslag; niet constructief","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afspraken document",null,"Ja","Design > Story Settings",null,null,"n.v.t.","IfcBuildingStorey","Attributes","IfcBuildingStorey","IfcBuildingStorey"]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"g","Entiteit","-","-","-","-","-","-","IfcSlab, IfcPlate","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcSlab"]
[]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset.",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"13.1* vloeren op grondslag; niet constructief","b"]
[null,"13.1* vloeren op grondslag; niet constructief","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","False (niet constructief)",null,"Ja",{"$f":"$S$86","v":"Structural Function (instellingenvenster > Classifications and Properties)"},null,null,"ILS 4.3-4 - Draagfunctie - Positie",{"$f":"$W$86","v":"ifcSlab, ifcPlate"},{"$f":"$X$86","v":"ILS O&E BWK"},{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"p","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","Indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"Nee",{"$f":"$S$83","v":"A: Wordt voor Building Element Parts automatisch ingevuld (Mass):\nDensity in kg/m3 (Building Material Settings) x volume \n\nB: Gewicht volledig element moet handmatig ingevuld worden (zie Helpcenter)"},null,null,{"$f":"$V$83","v":"A: Automatisch (gekoppeld aan Building Materials)\n\nB: O&E-99-Gewicht samengestelde elementen (C)"},{"$f":"$W$83","v":"A: IfcBuildingElementPart\n\nB: Ifc(Element)"},{"$f":"$X$83","v":"A: Pset_PrecastConcreteElementGeneral\n\nB: ILS O&E BWK"},{"$f":"$Y$83","v":"A: ElementWeight\n\nB: Massa"},{"$f":"$Z$83","v":"A: ElementWeight in kg\n\nB: Massa in kg"}]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"p","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset"]
[null,"13.1* vloeren op grondslag; niet constructief","b",null,"p","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset.\n\nExclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)."]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"13.1* vloeren op grondslag; niet constructief","b"]
[null,"13.1* vloeren op grondslag; niet constructief","b","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.1* vloeren op grondslag; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"13.1* vloeren op grondslag; niet constructief","b"]
[]
[null,"13.2* vloeren op grondslag; constructief","c","13.2* - Vloeren op grondslag; constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - tot de vloer behorende liftputten - grondverbeteringen - egaliseren van de grondslag - vochtwerende lagen - werkvloeren onder de vloerconstructie - tot de vloer behorende verzwaringen - gebouwisolatievoorzieningen - vloerafwerkingen die één geheel vormen met de vloerconstructie - bodemonderzoek en sonderingen tijdens de uitvoering"]
[null,"13.2* vloeren op grondslag; constructief","c","Verzameling van tot de draagconstructie van het gebouw behorende vloeren in rechtstreeks contact met de ondergrond aangebracht,\ngerekend vanaf de buitenzijde van de buitengevel of funderingsconstructie."]
[null,"13.2* vloeren op grondslag; constructief","c",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"13.2* vloeren op grondslag; constructief","c"]
[null,"13.2* vloeren op grondslag; constructief","c","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, dikte, omtrek, volume",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"13.2* vloeren op grondslag; constructief","c",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee",{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."},null,null,{"$f":"$V$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$W$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$X$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Y$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Z$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"}]
[null,"13.2* vloeren op grondslag; constructief","c",null,"e","Nokken en sponningen","-","-","-","-","-","-","-","-","-",null,null,{"$f":"$R$113","v":"Ja"},"3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"13.2* vloeren op grondslag; constructief","c",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,{"$f":"$R$113","v":"Ja"},"3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"13.2* vloeren op grondslag; constructief","c",null,"p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"13.2* vloeren op grondslag; constructief","c"]
[null,"13.2* vloeren op grondslag; constructief","c","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"13.2* vloeren op grondslag; constructief","c",null,"g","Entiteit","-","-","-","-","-","-","IfcSlab, IfcPlate","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcSlab, IfcPlate"]
[null,"13.2* vloeren op grondslag; constructief","c",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"13.2* vloeren op grondslag; constructief","c",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"13.2* vloeren op grondslag; constructief","c",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"13.2* vloeren op grondslag; constructief","c"]
[null,"13.2* vloeren op grondslag; constructief","c","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"13.2* vloeren op grondslag; constructief","c",null,"e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","Indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"Nee",{"$f":"$S$83","v":"A: Wordt voor Building Element Parts automatisch ingevuld (Mass):\nDensity in kg/m3 (Building Material Settings) x volume \n\nB: Gewicht volledig element moet handmatig ingevuld worden (zie Helpcenter)"},null,null,{"$f":"$V$83","v":"A: Automatisch (gekoppeld aan Building Materials)\n\nB: O&E-99-Gewicht samengestelde elementen (C)"},{"$f":"$W$83","v":"A: IfcBuildingElementPart\n\nB: Ifc(Element)"},{"$f":"$X$83","v":"A: Pset_PrecastConcreteElementGeneral\n\nB: ILS O&E BWK"},{"$f":"$Y$83","v":"A: ElementWeight\n\nB: Massa"},{"$f":"$Z$83","v":"A: ElementWeight in kg\n\nB: Massa in kg"}]
[]
[null,"13.2* vloeren op grondslag; constructief","c",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","True (constructief)",null,"Ja",{"$f":"$S$86","v":"Structural Function (instellingenvenster > Classifications and Properties)"},null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},{"$f":"$W$86","v":"ifcSlab, ifcPlate"},{"$f":"$X$86","v":"ILS O&E BWK"},{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[]
[null,"13.2* vloeren op grondslag; constructief","c",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"Nee","ACP: Sterkteklasse (beschikbaar voor Building Materials in de Building Material Settings)",null,null,"n.v.t.","(ifcElement)","ILS O&E BWK","Sterkteklasse","Sterkteklasse"]
[]
[null,"13.2* vloeren op grondslag; constructief","c",null,"e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset.\n\nExclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant).",null,"Nee","ACP: Milieuklasse (beschikbaar voor Building Materials in de Building Material Settings)",null,null,"n.v.t.","(ifcElement)","ILS O&E BWK","Milieuklasse","Milieuklasse"]
[]
[null,"13.2* vloeren op grondslag; constructief","c",null,"p","Wapeningshoeveelheid","-","-","-","-","-","-","wapeningshoeveelheid, benoemen in Custom Pset","wapeningshoeveelheid","kg/m³"]
[null,"13.2* vloeren op grondslag; constructief","c",null,"p","Brandwerendheid hoofddraagconstructie","-","-","-","-","-","-","brandwerendheid tot bezwijken, benoemen in Custom Pset","moment tot bezwijken","minuten"]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"13.2* vloeren op grondslag; constructief","c"]
[null,"13.2* vloeren op grondslag; constructief","c","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","13.2* vloeren op grondslag; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"13.2* vloeren op grondslag; constructief","c"]
[]
[null,"16.** funderingsconstructies","c","16.** - Funderingsconstructies; voeten & balken en keerwanden",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - het egaliseren van de grondslag - grondverbeteringen - werkvloeren onder deze constructies - liftputten indien geen onderdeel van element (13) - funderingsmetselwerken - gevelmetselwerken vanaf de fundering tot 200 mm onder maaiveld - gebouwisolatievoorzieningen - bodemonderzoek en sonderingen tijdens de uitvoering/ - voorzieningen ten behoeve van de waterdichtheid"]
[null,"16.** funderingsconstructies","c","Verzameling van tot de draagconstructie van het gebouw behorende balken, voeten en poeren/ grondwerende keerconstructies, gerekend vanaf de dragende grondslag en/of de paalfundering tot aan de onderzijde van de laagst-liggende vloeren, met inbegrip van de omsluiting van onder de grondslag gelegen buitenruimten."]
[null,"16.** funderingsconstructies","c",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"16.** funderingsconstructies","c"]
[null,"16.** funderingsconstructies","c","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nBreedte, hoogte, lengte, volume",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"16.** funderingsconstructies","c",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee",{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."},null,null,{"$f":"$V$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$W$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$X$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Y$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Z$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"}]
[null,"16.** funderingsconstructies","c",null,"e","Nokken en sponningen","-","-","-","-","-","-","-","-","-",null,null,{"$f":"$R$113","v":"Ja"},"3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"16.** funderingsconstructies","c",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,"Ja","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"16.** funderingsconstructies","c",null,"p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"16.** funderingsconstructies","c"]
[null,"16.** funderingsconstructies","c","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"16.** funderingsconstructies","c",null,"g","Entiteit","-","-","-","-","-","-","IfcColumn, IfcBeam, IfcSlab, IfcFooting, IfcWall","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcColumn, IfcBeam, IfcSlab, IfcFooting, IfcWall"]
[null,"16.** funderingsconstructies","c",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"16.** funderingsconstructies","c",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"16.** funderingsconstructies","c",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"16.** funderingsconstructies","c"]
[null,"16.** funderingsconstructies","c","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"16.** funderingsconstructies","c",null,"e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","Indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"Nee",{"$f":"$S$83","v":"A: Wordt voor Building Element Parts automatisch ingevuld (Mass):\nDensity in kg/m3 (Building Material Settings) x volume \n\nB: Gewicht volledig element moet handmatig ingevuld worden (zie Helpcenter)"},null,null,{"$f":"$V$83","v":"A: Automatisch (gekoppeld aan Building Materials)\n\nB: O&E-99-Gewicht samengestelde elementen (C)"},{"$f":"$W$83","v":"A: IfcBuildingElementPart\n\nB: Ifc(Element)"},{"$f":"$X$83","v":"A: Pset_PrecastConcreteElementGeneral\n\nB: ILS O&E BWK"},{"$f":"$Y$83","v":"A: ElementWeight\n\nB: Massa"},{"$f":"$Z$83","v":"A: ElementWeight in kg\n\nB: Massa in kg"}]
[]
[]
[]
[]
[null,"16.** funderingsconstructies","c",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","Indien entiteit IfcFooting: benoemen in Custom Pset omdat Pset_FootingCommon niet bestaat",null,"Nee",{"$f":"$S$86","v":"Structural Function (instellingenvenster > Classifications and Properties)"},null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},"ifcFooting","ILS O&E BWK","LoadBearing","True/False"]
[{"$nulls":17},"Ja","ACP: LoadBearing",null,null,null,"ifc<Entiteit>","Pset_<entiteit>Common","LoadBearing","True/False"]
[]
[]
[]
[null,"16.** funderingsconstructies","c",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"Nee",{"$f":"$S$163","v":"ACP: Sterkteklasse (beschikbaar voor Building Materials in de Building Material Settings)"},null,null,{"$f":"$V$163","v":"n.v.t."},{"$f":"$W$163","v":"(ifcElement)"},{"$f":"$X$163","v":"ILS O&E BWK"},{"$f":"$Y$163","v":"Sterkteklasse"},{"$f":"$Z$163","v":"Sterkteklasse"}]
[]
[]
[]
[]
[null,"16.** funderingsconstructies","c",null,"e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset.\n\nExclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant).",null,"Nee",{"$f":"$S$165","v":"ACP: Milieuklasse (beschikbaar voor Building Materials in de Building Material Settings)"},null,null,{"$f":"$V$165","v":"n.v.t."},"(ifcElement)","ILS O&E BWK","Milieuklasse",{"$f":"$Z$165","v":"Milieuklasse"}]
[null,"16.** funderingsconstructies","c",null,"p","Wapeningshoeveelheid","-","-","-","-","-","-","wapeningshoeveelheid, benoemen in Custom Pset","wapeningshoeveelheid","kg/m³"]
[null,"16.** funderingsconstructies","c",null,"p","Brandwerendheid hoofddraagconstructie","-","-","-","-","-","-","brandwerendheid tot bezwijken, benoemen in Custom Pset","moment tot bezwijken","minuten"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"16.** funderingsconstructies","c"]
[null,"16.** funderingsconstructies","c","Componenten","e","Stekken","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten modelleren, ntb tijdens project; staalkwaliteit opgeven als Eigenschap"]
[null,"16.** funderingsconstructies","c",null,"p","Wapening","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten modelleren, ntb tijdens project; staalkwaliteit en dekking opgeven als Eigenschappen (noot: wanneer geen wapening wordt gemodelleerd, staalkwaliteit en dekking meegeven als Eigenschappen)"]
[null,"16.** funderingsconstructies","c",null,"p","Overige instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
[null,"16.** funderingsconstructies","c",null,"p","Randkist","-","-","-","-","-","-","-","-","-","Modelleren als 3D symbool (IfcBuildinElementProxy)"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","16.** funderingsconstructies","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"16.** funderingsconstructies","c"]
[]
[null,"17.** paalfunderingen","c","17.** - Paalfunderingen; niet geheid en geheid",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - pijlerfunderingen en putringen - bodeminjecties met een dragende functie - werkvloeren onder deze constructies - damwanden als definitief onderdeel van het gebouw - trekverankeringen - bodemonderzoek en sonderingen tijdens de uitvoering/ - voorzieningen ter voorkoming en/of beperking van risico en overlast voor de omgeving"]
[null,"17.** paalfunderingen","c","Verzameling van funderingsconstructies die de belasting van het gebouw overbrengen naar dieper gelegen draagkrachtige grondslagen en (niet geheid) zonder overlast/ (geheid) met overlast c.q. risico voor de omgeving worden aangebracht."]
[null,"17.** paalfunderingen","c",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"17.** paalfunderingen","c"]
[null,"17.** paalfunderingen","c","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm en locatie moet hetvolgende bepaald kunnen worden: \ndiameter, lengte, volume",null,"Ja","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"17.** paalfunderingen","c",null,"e","Positiebepaling","-","-","-","-","-","-","-","-","-","Bijv. puntniveau t.o.v. peil, bovenkant t.o.v. NAP, onderkant t.o.v. NAP",null,"Ja","Archicad property 'Positiebepaling'\nLocation Settings",null,null,null,"ifcFooting ifcPile","ILS O&E BWK","Positiebepaling"]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"17.** paalfunderingen","c"]
[null,"17.** paalfunderingen","c","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"17.** paalfunderingen","c",null,"g","Entiteit","-","-","-","-","-","-","IfcFooting, IfcPile","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcFooting, IfcPile"]
[null,"17.** paalfunderingen","c",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"17.** paalfunderingen","c",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"17.** paalfunderingen","c",null,"e","Paalnummer","-","-","-","-","-","-","-","-","-",null,null,"Nee","Archicad property 'Paalnummer'",null,null,null,"ifcFooting / ifcPile","ILS O&E BWK","Paalnummer","Paalnummer"]
[null,"17.** paalfunderingen","c",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"17.** paalfunderingen","c"]
[null,"17.** paalfunderingen","c","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"17.** paalfunderingen","c",null,"e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,null,{"$f":"$S$83","v":"A: Wordt voor Building Element Parts automatisch ingevuld (Mass):\nDensity in kg/m3 (Building Material Settings) x volume \n\nB: Gewicht volledig element moet handmatig ingevuld worden (zie Helpcenter)"},null,null,{"$f":"$V$83","v":"A: Automatisch (gekoppeld aan Building Materials)\n\nB: O&E-99-Gewicht samengestelde elementen (C)"},{"$f":"$W$83","v":"A: IfcBuildingElementPart\n\nB: Ifc(Element)"},{"$f":"$X$83","v":"A: Pset_PrecastConcreteElementGeneral\n\nB: ILS O&E BWK"},{"$f":"$Y$83","v":"A: ElementWeight\n\nB: Massa"},{"$f":"$Z$83","v":"A: ElementWeight in kg\n\nB: Massa in kg"}]
[]
[null,"17.** paalfunderingen","c",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","benoemen in custom Pset","true/ false","-","Indien entiteit IfcFooting, IfcPile: benoemen in Custom Pset omdat Pset_FootingCommon of Pset_PileCommon niet bestaat",null,"Nee","Archicad property 'Draagfunctie fundering' <Expression>",null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},"ifcPile, ifcFooting","ILS O&E BWK","LoadBearing","True/False"]
[]
[null,"17.** paalfunderingen","c",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"Nee",{"$f":"$S$163","v":"ACP: Sterkteklasse (beschikbaar voor Building Materials in de Building Material Settings)"},null,null,{"$f":"$V$163","v":"n.v.t."},{"$f":"$W$163","v":"(ifcElement)"},{"$f":"$X$163","v":"ILS O&E BWK"},{"$f":"$Y$163","v":"Sterkteklasse"},{"$f":"$Z$163","v":"Sterkteklasse"}]
[]
[null,"17.** paalfunderingen","c",null,"e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset.\n\nExclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant).",null,"Nee",{"$f":"$S$165","v":"ACP: Milieuklasse (beschikbaar voor Building Materials in de Building Material Settings)"},null,null,{"$f":"$V$165","v":"n.v.t."},"(ifcElement)","ILS O&E BWK","Milieuklasse",{"$f":"$Z$165","v":"Milieuklasse"}]
[]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"17.** paalfunderingen","c"]
[null,"17.** paalfunderingen","c","Componenten","p","Wapening","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten modelleren, ntb tijdens project; staalkwaliteit en dekking opgeven als Eigenschappen (noot: wanneer geen wapening wordt gemodelleerd, staalkwaliteit en dekking meegeven als Eigenschappen)"]
[null,"17.** paalfunderingen","c",null,"p","Stekken","-","-","-","-","-","-","-","-","-","ter plaatse moeilijke knooppunten modelleren, ntb tijdens project; staalkwaliteit opgeven als Eigenschap"]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","17.** paalfunderingen","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"17.** paalfunderingen","c"]
[]
[null,"21.1* buitenwanden; niet constructief","b","21.1* - Buitenwanden; niet constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - kelderwanden, traditioneel samengestelde wanden, gordijngevels en systeemwanden - borstweringen, wandverzwaringen en terugliggende wanden van galerijen - schoorstenen die een onderdeel van de wand vormen - ventilatiekanalen die een onderdeel van de wand vormen - raaplagen in de spouwen en randaansluitingsvoorzieningen - gebouwisolatievoorzieningen - afwerkingen, die één geheel vormen met de buitenwand (incl. het voegwerk van schoon metselwerk) - verankeringen en bevestigingsmiddelen - dilatatievoegconstructies - gevelmetselwerken boven 200 mm onder maaiveld - boeiborden"]
[null,"21.1* buitenwanden; niet constructief","b","Verzameling van niet-constructieve buitenwanden, die de begrenzing vormen van het gebouw, gerekend vanaf de bovenzijde van de funderingsconstructies tot aan de bovenzijde van de dakconstructies.\nNoot: in het geval van een vliesgevel moeten de buitenwandopeningen voorzien zijn van de gegevensbehoefte onder 31.**."]
[null,"21.1* buitenwanden; niet constructief","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"21.1* buitenwanden; niet constructief","b"]
[null,"21.1* buitenwanden; niet constructief","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, dikte, hoogte, breedte (basisregel: geen samengestelde spouwwanden ivm hoeveelheden)",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"21.1* buitenwanden; niet constructief","b",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee",{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."},null,null,{"$f":"$V$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$W$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$X$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Y$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Z$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"}]
[null,"21.1* buitenwanden; niet constructief","b",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-","Afwijkingen in Eigenschappen tussen vlakken, als losse elementen modelleren",null,{"$f":"$R$113","v":"Ja"},"3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"21.1* buitenwanden; niet constructief","b",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,{"$f":"$R$113","v":"Ja"},"3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"21.1* buitenwanden; niet constructief","b",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"21.1* buitenwanden; niet constructief","b"]
[null,"21.1* buitenwanden; niet constructief","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"21.1* buitenwanden; niet constructief","b",null,"g","Entiteit","-","-","-","-","-","-","IfcWall, IfcCurtainWall","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcWall, IfcCurtainWall"]
[null,"21.1* buitenwanden; niet constructief","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"21.1* buitenwanden; niet constructief","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"21.1* buitenwanden; niet constructief","b",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"21.1* buitenwanden; niet constructief","b",null,"p","Merk","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelReference","-","-","Ten behoeve van onderhoud"]
[null,"21.1* buitenwanden; niet constructief","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"21.1* buitenwanden; niet constructief","b"]
[null,"21.1* buitenwanden; niet constructief","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"21.1* buitenwanden; niet constructief","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"Nee","ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'",null,null,"O&E 21/22Wanden(C)/(E)","(ifcElement)","ILS O&E BWK","Afwerking / Behandeling","Afwerking/Behandeling (element), Afwerking/Behandeling (materiaal)"]
[null,"21.1* buitenwanden; niet constructief","b",null,"e","Kleur","-","-","-","-","-","-","-","-","-","(RAL) kleurcode/ omschrijving (in het geval van metselwerk, Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file)",null,"Nee","ACP: 'Kleur (element)'\nACP: 'Kleur (materiaal)'",null,null,"O&E 21/22Wanden(C)/(E)","(ifcElement)","ILS O&E BWK","Kleur","kleur (element) / kleur (materiaal)"]
[null,"21.1* buitenwanden; niet constructief","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_WallCommon: Loadbearing","true/ false","-","False (niet constructief)\n\nIndien entiteit IfcCurtainWall, IfcWindow, IfcDoor: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"Ja",{"$f":"$S$86","v":"Structural Function (instellingenvenster > Classifications and Properties)"},null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},"ifcWall","Pset_WallCommon",{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[]
[null,"21.1* buitenwanden; niet constructief","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-","True (isExternal)",null,"Ja","Instellingenvenster > onder ID and Categories > Position",null,null,"ILS 4.3-4-Draagfunctie - Positie","ifc<Entiteit>","Pset_<entiteit>Common","isExternal","True/False"]
[]
[null,"21.1* buitenwanden; niet constructief","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"Ja","ACP: WBDBO",null,null,"ILS 4.5 Brandwerendheid","ifcWall","ifc<Entiteit>Common","FireRating","WBDBO"]
[]
[null,"21.1* buitenwanden; niet constructief","b",null,"p","Weerstandsklasse","-","-","-","-","-","-","Pset_<entiteit>Common: SecurityRating","classificatie","-","Bijv.: WK1 conform NEN 5096\n\nIndien entiteit IfcWall, IfcCurtainWall, IfcPlate, IfcMember: benoemen in Custom Pset omdat 'SecurityRating' geen deel uitmaakt van Common Pset"]
[null,"21.1* buitenwanden; niet constructief","b","#metselwerk","p","Metselwerkverband","-","-","-","-","-","-","-","-","-"]
[null,"21.1* buitenwanden; niet constructief","b","#metselwerk","p","Voegtype","-","-","-","-","-","-","-","-","-"]
[null,"21.1* buitenwanden; niet constructief","b",null,"p","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset"]
[null,"21.1* buitenwanden; niet constructief","b","#beton","p","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset\nexclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)"]
[null,"21.1* buitenwanden; niet constructief","b","#beton","p","Oppervlakteklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN-EN 13670"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"21.1* buitenwanden; niet constructief","b"]
[null,"21.1* buitenwanden; niet constructief","b","Componenten","e","Isolatie","-","-","-","-","-","-","-","-","-","Tevens aangeven: isolatiewaarde en brandklasse"]
[null,"21.1* buitenwanden; niet constructief","b",null,"e","Folies, slabben","-","-","-","-","-","-","-","-","-","Volgens separaat uitganspunten/afsprakendocument"]
[null,"21.1* buitenwanden; niet constructief","b",null,"p","Geveldragers","-","-","-","-","-","-","-","-","-","Modelleren en voorzien van de bovenstaande Eigenschappen"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.1* buitenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"21.1* buitenwanden; niet constructief","b"]
[]
[null,"21.2* buitenwanden; constructief","c","21.2* - Buitenwanden; constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - kelderwanden en traditioneel samengestelde wanden - borstweringen, wandverzwaringen en terugliggende wanden van galerijen - schoorstenen die een onderdeel van de wand vormen - ventilatiekanalen die een onderdeel van de wand vormen - raaplagen in de spouwen en randaansluitingsvoorzieningen - gebouwisolatievoorzieningen - afwerkingen die één geheel vormen met de buitenwand (incl. het voegwerk van schoon metselwerk) - verankeringen en bevestigingsmiddelen - dilatatievoegconstructies - gevelmetselwerken boven 200 mm onder maaiveld - boeiborden"]
[null,"21.2* buitenwanden; constructief","c","Verzameling van constructieve buitenwanden, die de begrenzing vormen van het gebouw, gerekend vanaf de bovenzijde van de funderingsconstructies tot aan de onderzijde van de dakconstructies."]
[null,"21.2* buitenwanden; constructief","c",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"21.2* buitenwanden; constructief","c"]
[null,"21.2* buitenwanden; constructief","c","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, breedte, hoogte, dikte, volume",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"21.2* buitenwanden; constructief","c",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee",{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."},null,null,{"$f":"$V$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$W$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$X$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Y$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Z$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"}]
[null,"21.2* buitenwanden; constructief","c",null,"e","Nokken en sponningen","-","-","-","-","-","-","-","-","-",null,null,{"$f":"$R$113","v":"Ja"},"3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"21.2* buitenwanden; constructief","c",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,{"$f":"$R$113","v":"Ja"},"3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"21.2* buitenwanden; constructief","c",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
[null,"21.2* buitenwanden; constructief","c",null,"p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"21.2* buitenwanden; constructief","c"]
[null,"21.2* buitenwanden; constructief","c","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"21.2* buitenwanden; constructief","c",null,"g","Entiteit","-","-","-","-","-","-","IfcWall, IfcCurtainWall","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcWall, IfcCurtainWall"]
[null,"21.2* buitenwanden; constructief","c",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"21.2* buitenwanden; constructief","c",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"21.2* buitenwanden; constructief","c",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"21.2* buitenwanden; constructief","c"]
[null,"21.2* buitenwanden; constructief","c","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"21.2* buitenwanden; constructief","c",null,"e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"Nee",{"$f":"$S$83","v":"A: Wordt voor Building Element Parts automatisch ingevuld (Mass):\nDensity in kg/m3 (Building Material Settings) x volume \n\nB: Gewicht volledig element moet handmatig ingevuld worden (zie Helpcenter)"},null,null,{"$f":"$V$83","v":"A: Automatisch (gekoppeld aan Building Materials)\n\nB: O&E-99-Gewicht samengestelde elementen (C)"},{"$f":"$W$83","v":"A: IfcBuildingElementPart\n\nB: Ifc(Element)"},{"$f":"$X$83","v":"A: Pset_PrecastConcreteElementGeneral\n\nB: ILS O&E BWK"},{"$f":"$Y$83","v":"A: ElementWeight\n\nB: Massa"},{"$f":"$Z$83","v":"A: ElementWeight in kg\n\nB: Massa in kg"}]
[null,"21.2* buitenwanden; constructief","c",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_WallCommon: Loadbearing","true/ false","-","True (constructief)\n\nIndien entiteit IfcCurtainWall: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"Ja",{"$f":"$S$86","v":"Structural Function (instellingenvenster > Classifications and Properties)"},null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},"ifcWall","Pset_WallCommon",{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[null,"21.2* buitenwanden; constructief","c",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-","True (isExternal)",null,"Ja",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$W$298","v":"ifc<Entiteit>"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[]
[null,"21.2* buitenwanden; constructief","c",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"Ja",{"$f":"$S$300","v":"ACP: WBDBO"},null,null,{"$f":"$V$300","v":"ILS 4.5 Brandwerendheid"},{"$f":"$W$300","v":"ifcWall"},{"$f":"$X$300","v":"ifc<Entiteit>Common"},{"$f":"$Y$300","v":"FireRating"},{"$f":"$Z$300","v":"WBDBO"}]
[null,"21.2* buitenwanden; constructief","c",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"Nee",{"$f":"$S$163","v":"ACP: Sterkteklasse (beschikbaar voor Building Materials in de Building Material Settings)"},null,null,{"$f":"$V$163","v":"n.v.t."},{"$f":"$W$163","v":"(ifcElement)"},{"$f":"$X$163","v":"ILS O&E BWK"},{"$f":"$Y$163","v":"Sterkteklasse"},{"$f":"$Z$163","v":"Sterkteklasse"}]
[]
[null,"21.2* buitenwanden; constructief","c",null,"e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset\nexclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)",null,"Nee",{"$f":"$S$165","v":"ACP: Milieuklasse (beschikbaar voor Building Materials in de Building Material Settings)"},null,null,{"$f":"$V$165","v":"n.v.t."},"(ifcElement)","ILS O&E BWK","Milieuklasse",{"$f":"$Z$165","v":"Milieuklasse"}]
[null,"21.2* buitenwanden; constructief","c",null,"p","Wapeningshoeveelheid","-","-","-","-","-","-","wapeningshoeveelheid, benoemen in Custom Pset","wapeningshoeveelheid","kg/m³"]
[null,"21.2* buitenwanden; constructief","c",null,"p","Brandwerendheid hoofddraagconstructie","-","-","-","-","-","-","brandwerendheid tot bezwijken, benoemen in Custom Pset","moment tot bezwijken","minuten"]
[null,"21.2* buitenwanden; constructief","c",null,"p","Weerstandsklasse","-","-","-","-","-","-","SecurityRating benoemen in custom Pset","classificatie","-","Bijv.: WK1 conform NEN 5096\n\nIndien entiteit IfcWall, IfcCurtainWall, IfcPlate, IfcMember: benoemen in Custom Pset omdat 'SecurityRating' geen deel uitmaakt van Common Pset"]
[null,"21.2* buitenwanden; constructief","c","#beton","p","Oppervlakteklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN-EN 13670"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"21.2* buitenwanden; constructief","c"]
[null,"21.2* buitenwanden; constructief","c","Componenten","p","Wapening","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten modelleren, ntb tijdens project; staalkwaliteit en dekking opgeven als Eigenschappen (noot: wanneer geen wapening wordt gemodelleerd, staalkwaliteit en dekking meegeven als Eigenschappen)"]
[null,"21.2* buitenwanden; constructief","c",null,"p","Op te nemen installaties","-","-","-","-","-","-","-","-","-","In overleg met Installateur"]
[null,"21.2* buitenwanden; constructief","c",null,"p","Geveldragers","-","-","-","-","-","-","-","-","-","Modelleren en voorzien van de bovenstaande Eigenschappen"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","21.2* buitenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"21.2* buitenwanden; constructief","c"]
[]
[null,"22.1* binnenwanden; niet constructief","b","22.1* - Binnenwanden; niet constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - traditioneel samengestelde wanden en systeemwanden - brandwerende wanden - schoorstenen, die een onderdeel van de wand vormen - ventilatiekanalen die een onderdeel van de wand vormen - isolaties, die één geheel vormen met het wandsysteem - afwerkingen, die één geheel vormen met het wandsysteem (incl. het voegwerk van schoonmetselwerk) - randaansluitingsvoorzieningen - dilatatievoeg constructies - verankeringen en bevestigingsmiddelen"]
[null,"22.1* binnenwanden; niet constructief","b","Verzameling van niet-constructieve binnenwanden, gerekend vanaf de bovenzijde van de onderliggende vloer tot aan de onderzijde van de bovenliggende (dak)vloer."]
[null,"22.1* binnenwanden; niet constructief","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"22.1* binnenwanden; niet constructief","b"]
[null,"22.1* binnenwanden; niet constructief","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, dikte, hoogte, breedte",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"22.1* binnenwanden; niet constructief","b",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee",{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."},null,null,{"$f":"$V$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$W$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$X$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Y$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Z$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"}]
[null,"22.1* binnenwanden; niet constructief","b",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,{"$f":"$R$113","v":"Ja"},"3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"22.1* binnenwanden; niet constructief","b",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,"Ja","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"22.1* binnenwanden; niet constructief","b",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"22.1* binnenwanden; niet constructief","b"]
[null,"22.1* binnenwanden; niet constructief","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"22.1* binnenwanden; niet constructief","b",null,"g","Entiteit","-","-","-","-","-","-","IfcWall, IfcCurtainWall","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcWall, IfcCurtainWall"]
[null,"22.1* binnenwanden; niet constructief","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"22.1* binnenwanden; niet constructief","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"22.1* binnenwanden; niet constructief","b",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"22.1* binnenwanden; niet constructief","b",null,"p","Merk","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelReference","-","-","Ten behoeve van onderhoud"]
[null,"22.1* binnenwanden; niet constructief","b",null,"p","Weerstandsklasse","-","-","-","-","-","-","SecurityRating benoemen in custom Pset","classificatie","-","Bijv.: WK1 conform NEN 5096\n\nIndien entiteit IfcWall, IfcCurtainWall, IfcPlate, IfcMember: benoemen in Custom Pset omdat 'SecurityRating' geen deel uitmaakt van Common Pset"]
[null,"22.1* binnenwanden; niet constructief","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"22.1* binnenwanden; niet constructief","b"]
[null,"22.1* binnenwanden; niet constructief","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"22.1* binnenwanden; niet constructief","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,{"$f":"$V$294","v":"O&E 21/22Wanden(C)/(E)"},{"$f":"$W$294","v":"(ifcElement)"},{"$f":"$X$294","v":"ILS O&E BWK"},{"$f":"$Y$294","v":"Afwerking / Behandeling"},{"$f":"$Z$294","v":"Afwerking/Behandeling (element), Afwerking/Behandeling (materiaal)"}]
[null,"22.1* binnenwanden; niet constructief","b",null,"e","Kleur","-","-","-","-","-","-","-","-","-","(RAL) kleurcode/ omschrijving (in het geval van metselwerk, Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file)",null,"Nee","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…",null,null,{"$f":"$V$294","v":"O&E 21/22Wanden(C)/(E)"},{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
[null,"22.1* binnenwanden; niet constructief","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_WallCommon: Loadbearing","true/ false","-","False (niet constructief)\n\nIndien entiteit IfcCurtainWall: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"Ja",{"$f":"$S$86","v":"Structural Function (instellingenvenster > Classifications and Properties)"},null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},"ifcWall","Pset_WallCommon",{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[null,"22.1* binnenwanden; niet constructief","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-","False",null,"Ja",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$W$298","v":"ifc<Entiteit>"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[]
[null,"22.1* binnenwanden; niet constructief","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"Ja",{"$f":"$S$300","v":"ACP: WBDBO"},null,null,{"$f":"$V$300","v":"ILS 4.5 Brandwerendheid"},{"$f":"$W$300","v":"ifcWall"},{"$f":"$X$300","v":"ifc<Entiteit>Common"},{"$f":"$Y$300","v":"FireRating"},{"$f":"$Z$300","v":"WBDBO"}]
[null,"22.1* binnenwanden; niet constructief","b",null,"e","Luchtgeluidisolatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/inkoop/uitvoering.",null,"Ja","ACP: Geluidwering",null,null,null,"ifcWall","Pset_WallCommon","AcousticRating","Geluidwering"]
[]
[null,"22.1* binnenwanden; niet constructief","b",null,"p","Vlakheidsklasse","-","-","-","-","-","-","-","classificatie","-"]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"22.1* binnenwanden; niet constructief","b"]
[null,"22.1* binnenwanden; niet constructief","b","Componenten","p","Op te nemen installaties","-","-","-","-","-","-","-","-","-"]
[null,"22.1* binnenwanden; niet constructief","b",null,"p","Bouwfysische eis - brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
[null,"22.1* binnenwanden; niet constructief","b",null,"p","Bouwfysische eis - luchtgeluidisoalatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.1* binnenwanden; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"22.1* binnenwanden; niet constructief","b"]
[]
[null,"22.2* binnenwanden; constructief","c","22.2* - Binnenwanden; constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - traditioneel samengestelde wanden en systeemwanden - brandwerende wanden - schoorstenen, die een onderdeel van de wand vormen - ventilatiekanalen die een onderdeel van de wand vormen - isolaties, die één geheel vormen met het wandsysteem - afwerkingen, die één geheel vormen met het wandsysteem (incl. het voegwerk van schoonmetselwerk) - randaansluitingsvoorzieningen - dilatatievoeg constructies - verankeringen en bevestigingsmiddelen"]
[null,"22.2* binnenwanden; constructief","c","Verzameling van constructieve binnenwanden, gerekend vanaf de bovenzijde van de onderliggende vloer tot aan de onderzijde van de bovenliggende (dak)vloer."]
[null,"22.2* binnenwanden; constructief","c",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"22.2* binnenwanden; constructief","c"]
[null,"22.2* binnenwanden; constructief","c","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, breedte, dikte, volume",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"22.2* binnenwanden; constructief","c",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee",{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."},null,null,{"$f":"$V$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$W$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$X$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Y$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Z$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"}]
[null,"22.2* binnenwanden; constructief","c",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,{"$f":"$R$113","v":"Ja"},"3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"22.2* binnenwanden; constructief","c",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
[null,"22.2* binnenwanden; constructief","c",null,"p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"22.2* binnenwanden; constructief","c"]
[null,"22.2* binnenwanden; constructief","c","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"22.2* binnenwanden; constructief","c",null,"g","Entiteit","-","-","-","-","-","-","IfcWall, IfcCurtainWall","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcWall, IfcCurtainWall"]
[null,"22.2* binnenwanden; constructief","c",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"22.2* binnenwanden; constructief","c",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"22.2* binnenwanden; constructief","c",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"22.2* binnenwanden; constructief","c"]
[null,"22.2* binnenwanden; constructief","c","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"22.2* binnenwanden; constructief","c",null,"e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"Nee",{"$f":"$S$83","v":"A: Wordt voor Building Element Parts automatisch ingevuld (Mass):\nDensity in kg/m3 (Building Material Settings) x volume \n\nB: Gewicht volledig element moet handmatig ingevuld worden (zie Helpcenter)"},null,null,{"$f":"$V$83","v":"A: Automatisch (gekoppeld aan Building Materials)\n\nB: O&E-99-Gewicht samengestelde elementen (C)"},{"$f":"$W$83","v":"A: IfcBuildingElementPart\n\nB: Ifc(Element)"},{"$f":"$X$83","v":"A: Pset_PrecastConcreteElementGeneral\n\nB: ILS O&E BWK"},{"$f":"$Y$83","v":"A: ElementWeight\n\nB: Massa"},{"$f":"$Z$83","v":"A: ElementWeight in kg\n\nB: Massa in kg"}]
[null,"22.2* binnenwanden; constructief","c",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,{"$f":"$V$294","v":"O&E 21/22Wanden(C)/(E)"},{"$f":"$W$294","v":"(ifcElement)"},{"$f":"$X$294","v":"ILS O&E BWK"},{"$f":"$Y$294","v":"Afwerking / Behandeling"},{"$f":"$Z$294","v":"Afwerking/Behandeling (element), Afwerking/Behandeling (materiaal)"}]
[null,"22.2* binnenwanden; constructief","c",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_WallCommon: Loadbearing","true/ false","-","True (constructief)\n\nIndien entiteit IfcCurtainWall: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"Ja",{"$f":"$S$86","v":"Structural Function (instellingenvenster > Classifications and Properties)"},null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},"ifcWall","Pset_WallCommon",{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[null,"22.2* binnenwanden; constructief","c",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-","False",null,"Ja",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$W$298","v":"ifc<Entiteit>"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[null,"22.2* binnenwanden; constructief","c",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"Ja",{"$f":"$S$300","v":"ACP: WBDBO"},null,null,{"$f":"$V$300","v":"ILS 4.5 Brandwerendheid"},{"$f":"$W$300","v":"ifcWall"},{"$f":"$X$300","v":"ifc<Entiteit>Common"},{"$f":"$Y$300","v":"FireRating"},{"$f":"$Z$300","v":"WBDBO"}]
[null,"22.2* binnenwanden; constructief","c",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"Nee",{"$f":"$S$163","v":"ACP: Sterkteklasse (beschikbaar voor Building Materials in de Building Material Settings)"},null,null,{"$f":"$V$163","v":"n.v.t."},{"$f":"$W$163","v":"(ifcElement)"},{"$f":"$X$163","v":"ILS O&E BWK"},{"$f":"$Y$163","v":"Sterkteklasse"},{"$f":"$Z$163","v":"Sterkteklasse"}]
[]
[null,"22.2* binnenwanden; constructief","c",null,"e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset\nexclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)",null,"Nee",{"$f":"$S$165","v":"ACP: Milieuklasse (beschikbaar voor Building Materials in de Building Material Settings)"},null,null,{"$f":"$V$165","v":"n.v.t."},"(ifcElement)","ILS O&E BWK","Milieuklasse",{"$f":"$Z$165","v":"Milieuklasse"}]
[null,"22.2* binnenwanden; constructief","c",null,"p","Wapeningshoeveelheid","-","-","-","-","-","-","wapeningshoeveelheid, benoemen in Custom Pset","wapeningshoeveelheid","kg/m³"]
[null,"22.2* binnenwanden; constructief","c",null,"p","Brandwerendheid hoofddraagconstructie","-","-","-","-","-","-","brandwerendheid tot bezwijken, benoemen in Custom Pset","moment tot bezwijken","minuten"]
[null,"22.2* binnenwanden; constructief","c",null,"p","Weerstandsklasse","-","-","-","-","-","-","SecurityRating benoemen in custom Pset","classificatie","-","Bijv.: WK1 conform NEN 5096\n\nIndien entiteit IfcWall, IfcCurtainWall, IfcPlate, IfcMember: benoemen in Custom Pset omdat 'SecurityRating' geen deel uitmaakt van Common Pset"]
[null,"22.2* binnenwanden; constructief","c","#beton","p","Oppervlakteklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN-EN 13670"]
[null,"22.2* binnenwanden; constructief","c",null,"p","Vlakheidsklasse","-","-","-","-","-","-","-","classificatie","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"22.2* binnenwanden; constructief","c"]
[null,"22.2* binnenwanden; constructief","c","Componenten","p","Wapening","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten modelleren, ntb tijdens project; staalkwaliteit en dekking opgeven als Eigenschappen (noot: wanneer geen wapening wordt gemodelleerd, staalkwaliteit en dekking meegeven als Eigenschappen)"]
[null,"22.2* binnenwanden; constructief","c",null,"p","Op te nemen installaties","-","-","-","-","-","-","-","-","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","22.2* binnenwanden; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"22.2* binnenwanden; constructief","c"]
[]
[null,"23.1* vloeren; niet constructief","b","23.1* - Vloeren; niet constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - beloopbare plafonds ten behoeve van installaties - wandaansluitingsvoorzieningen - tot de vloer behorende balken en verzwaringen - verankeringen en bevestigingsmiddelen - afwerkingen, die één geheel vormen met de vloerconstructie - gebouwisolatievoorzieningen - dilatatievoegconstructies"]
[null,"23.1* vloeren; niet constructief","b","Verzameling van niet-constructieve vrijdragende vloeren, inclusief galerijvloeren, balkons en bordessen, gerekend tot aan de binnenzijde van de buitenwanden."]
[null,"23.1* vloeren; niet constructief","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"23.1* vloeren; niet constructief","b"]
[null,"23.1* vloeren; niet constructief","b","Geometrie","g","Vorm buitenste profilering","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, omtrek, afschot",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"23.1* vloeren; niet constructief","b",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee",{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."},null,null,{"$f":"$V$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$W$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$X$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Y$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Z$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"}]
[null,"23.1* vloeren; niet constructief","b",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,{"$f":"$R$113","v":"Ja"},"3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"23.1* vloeren; niet constructief","b",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"23.1* vloeren; niet constructief","b"]
[null,"23.1* vloeren; niet constructief","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"23.1* vloeren; niet constructief","b",null,"g","Entiteit","-","-","-","-","-","-","IfcSlab, IfcPlate","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcSlab"]
[null,"23.1* vloeren; niet constructief","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"23.1* vloeren; niet constructief","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"23.1* vloeren; niet constructief","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"23.1* vloeren; niet constructief","b"]
[null,"23.1* vloeren; niet constructief","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"23.1* vloeren; niet constructief","b",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"Nee","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…",null,null,"O&E 23-Vloeren(C)/(E)",{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
[null,"23.1* vloeren; niet constructief","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,"O&E 23-Vloeren(C)/(E)",{"$f":"$W$294","v":"(ifcElement)"},{"$f":"$X$294","v":"ILS O&E BWK"},{"$f":"$Y$294","v":"Afwerking / Behandeling"},{"$f":"$Z$294","v":"Afwerking/Behandeling (element), Afwerking/Behandeling (materiaal)"}]
[null,"23.1* vloeren; niet constructief","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","False (niet constructief)",null,"Ja",{"$f":"$S$86","v":"Structural Function (instellingenvenster > Classifications and Properties)"},null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},{"$f":"$M$472","v":"IfcSlab, IfcPlate"},"Pset_<entiteit>Common",{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[]
[null,"23.1* vloeren; niet constructief","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-",null,null,"Ja",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$M$472","v":"IfcSlab, IfcPlate"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[]
[null,"23.1* vloeren; niet constructief","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"Ja",{"$f":"$S$300","v":"ACP: WBDBO"},null,null,{"$f":"$V$300","v":"ILS 4.5 Brandwerendheid"},{"$f":"$M$472","v":"IfcSlab, IfcPlate"},{"$f":"$X$300","v":"ifc<Entiteit>Common"},{"$f":"$Y$300","v":"FireRating"},{"$f":"$Z$300","v":"WBDBO"}]
[null,"23.1* vloeren; niet constructief","b",null,"p","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset"]
[null,"23.1* vloeren; niet constructief","b",null,"p","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset\nexclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)"]
[null,"23.1* vloeren; niet constructief","b",null,"p","Wapeningshoeveelheid","-","-","-","-","-","-","wapeningshoeveelheid, benoemen in Custom Pset","wapeningshoeveelheid","kg/m³"]
[null,"23.1* vloeren; niet constructief","b","#beton","p","Oppervlakteklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN-EN 13670"]
[null,"23.1* vloeren; niet constructief","b",null,"p","Vlakheidsklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN 2747"]
[null,"23.1* vloeren; niet constructief","b",null,"p","Brandwerendheid hoofddraagconstructie","-","-","-","-","-","-","brandwerendheid tot bezwijken, benoemen in Custom Pset","moment tot bezwijken","minuten"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"23.1* vloeren; niet constructief","b"]
[null,"23.1* vloeren; niet constructief","b","Componenten","e","Isolatie","-","-","-","-","-","-","-","-","-","Tevens aangeven: isolatiewaarde en brandklasse"]
[null,"23.1* vloeren; niet constructief","b",null,"p","Toog/ zeeg","-","-","-","-","-","-","-","-","-","Ruimtereserveringsobject modelleren om rekening te kunnen houden met het effect van toog/ zeeg"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.1* vloeren; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"23.1* vloeren; niet constructief","b"]
[]
[null,"23.2* vloeren; constructief","c","23.2* - Vloeren; constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - wandaansluitingsvoorzieningen - tot de vloer behorende balken en verzwaringen - verankeringen en bevestigingsmiddelen - afwerkingen, die één geheel vormen met de vloerconstructie - gebouwisolatievoorzieningen - dilatatievoegconstructies"]
[null,"23.2* vloeren; constructief","c","Verzameling van constructieve vrijdragende vloeren, inclusief galerijvloeren, balkons en bordessen, gerekend tot aan de binnenzijde van de buitenwanden, echter met inbegrip van de oplegvlakken. \nNoot: in afwijking van definitie NL-SfB worden hier de galerijvloeren, balkons en bordessen buiten bschouwing gelaten."]
[null,"23.2* vloeren; constructief","c",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"23.2* vloeren; constructief","c"]
[null,"23.2* vloeren; constructief","c","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Druklaag en afwerklaag separaat modelleren.\nUit vorm moet hetvolgende bepaald kunnen worden: \nomtrek, oppervlakte, dikte, volume, afschot",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"23.2* vloeren; constructief","c",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee",{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."},null,null,{"$f":"$V$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$W$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$X$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Y$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Z$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"}]
[null,"23.2* vloeren; constructief","c",null,"e","Nokken en sponningen","-","-","-","-","-","-","-","-","-","In verband met oplegging",null,{"$f":"$R$113","v":"Ja"},"3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"23.2* vloeren; constructief","c",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,"Ja","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"23.2* vloeren; constructief","c",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c"]
[null,"23.2* vloeren; constructief","c","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"23.2* vloeren; constructief","c",null,"g","Entiteit","-","-","-","-","-","-","IfcSlab","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcSlab"]
[null,"23.2* vloeren; constructief","c",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"23.2* vloeren; constructief","c",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"23.2* vloeren; constructief","c",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c"]
[null,"23.2* vloeren; constructief","c","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"23.2* vloeren; constructief","c","#beton","e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"Nee",{"$f":"$S$83","v":"A: Wordt voor Building Element Parts automatisch ingevuld (Mass):\nDensity in kg/m3 (Building Material Settings) x volume \n\nB: Gewicht volledig element moet handmatig ingevuld worden (zie Helpcenter)"},null,null,{"$f":"$V$83","v":"A: Automatisch (gekoppeld aan Building Materials)\n\nB: O&E-99-Gewicht samengestelde elementen (C)"},{"$f":"$W$83","v":"A: IfcBuildingElementPart\n\nB: Ifc(Element)"},{"$f":"$X$83","v":"A: Pset_PrecastConcreteElementGeneral\n\nB: ILS O&E BWK"},{"$f":"$Y$83","v":"A: ElementWeight\n\nB: Massa"},{"$f":"$Z$83","v":"A: ElementWeight in kg\n\nB: Massa in kg"}]
[null,"23.2* vloeren; constructief","c",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_SlabCommon: Loadbearing","true/ false","-","True (constructief)\n\nIndien entiteit IfcBuildingElementProxy: benoemen in Custom Pset omdat Common Pset in Ifc 2x3 niet bestaat",null,"Ja",{"$f":"$S$86","v":"Structural Function (instellingenvenster > Classifications and Properties)"},null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},"ifcSlab","Pset_SlabCommon",{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[null,"23.2* vloeren; constructief","c",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_SlabCommon: IsExternal","true/ false","-","Indien entiteit IfcBuildingElementProxy: benoemen in Custom Pset omdat Pset_BuildingElementProxyCommon in Ifc 2x3 niet bestaat",null,"Ja",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$W$298","v":"ifc<Entiteit>"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[null,"23.2* vloeren; constructief","c",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_SlabCommon: FireRating","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering., volgens separaak afsprakendocument. 0, 20, 30, 60, etc... (WBDBO).\nIndien entiteit IfcBuildingElementProxy: benoemen in Custom Pset omdat Pset_IfcBuildingElementProxyCommon in Ifc 2x3 niet bestaat",null,"Ja",{"$f":"$S$300","v":"ACP: WBDBO"},null,null,{"$f":"$V$300","v":"ILS 4.5 Brandwerendheid"},"ifc<entiteit>",{"$f":"$X$300","v":"ifc<Entiteit>Common"},{"$f":"$Y$300","v":"FireRating"},{"$f":"$Z$300","v":"WBDBO"}]
[null,"23.2* vloeren; constructief","c",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"Nee",{"$f":"$S$163","v":"ACP: Sterkteklasse (beschikbaar voor Building Materials in de Building Material Settings)"},null,null,{"$f":"$V$163","v":"n.v.t."},{"$f":"$W$163","v":"(ifcElement)"},{"$f":"$X$163","v":"ILS O&E BWK"},{"$f":"$Y$163","v":"Sterkteklasse"},{"$f":"$Z$163","v":"Sterkteklasse"}]
[null,"23.2* vloeren; constructief","c",null,"e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset\nexclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)",null,"Nee",{"$f":"$S$165","v":"ACP: Milieuklasse (beschikbaar voor Building Materials in de Building Material Settings)"},null,null,{"$f":"$V$165","v":"n.v.t."},"(ifcElement)","ILS O&E BWK","Milieuklasse",{"$f":"$Z$165","v":"Milieuklasse"}]
[null,"23.2* vloeren; constructief","c",null,"p","Wapeningshoeveelheid","-","-","-","-","-","-","wapeningshoeveelheid, benoemen in Custom Pset","wapeningshoeveelheid","kg/m³"]
[null,"23.2* vloeren; constructief","c",null,"p","Warmtedoorgangscoefficient","-","-","-","-","-","-","Pset_SlabCommon: ThermalTransmittance","U-waarde","W/ m².K","Warmteweerstand R = 1/ U\n\nIndien entiteit IfcBuildingElementProxy: benoemen in Custom Pset omdat Pset_BuildingElementProxyCommon in Ifc 2x3 niet bestaat"]
[null,"23.2* vloeren; constructief","c",null,"p","Brandwerendheid hoofddraagconstructie","-","-","-","-","-","-","brandwerendheid tot bezwijken, benoemen in Custom Pset","moment tot bezwijken","minuten"]
[null,"23.2* vloeren; constructief","c",null,"p","Overspanningsrichting","-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c","#beton","p","Oppervlakteklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN-EN 13670"]
[null,"23.2* vloeren; constructief","c",null,"p","Vlakheidsklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN 2747"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c"]
[null,"23.2* vloeren; constructief","c","Componenten","p","Wapening","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten modelleren, ntb tijdens project; staalkwaliteit en dekking opgeven als Eigenschappen (noot: wanneer geen wapening wordt gemodelleerd, staalkwaliteit en dekking meegeven als Eigenschappen)"]
[null,"23.2* vloeren; constructief","c",null,"p","Raveelijzers","-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c",null,"p","Randkist","-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c",null,"p","Koudebrugonderbrekingen","-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c",null,"p","Ankers/ isokorven","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten, ntb tijdens project; aangeven: staalkwaliteit en dekking"]
[null,"23.2* vloeren; constructief","c",null,"p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c",null,"p","Toog/ zeeg","-","-","-","-","-","-","-","-","-","Ruimtereserveringsobject modelleren om rekening te kunnen houden met het effect van toog/ zeeg"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","23.2* vloeren; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"23.2* vloeren; constructief","c"]
[]
[null,"24.1* trappen en hellingen; trappen","b","24.1* - Trappen en hellingen; trappen",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - randaansluitingsvoorzieningen - verankeringen en bevestigingsmiddelen - afwerkingen die één geheel vormen met de trapconstructie"]
[null,"24.1* trappen en hellingen; trappen","b","Verzameling van trappen, zowel binnen als buiten het gebouw, inclusief de bijbehorende bordessen."]
[null,"24.1* trappen en hellingen; trappen","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"24.1* trappen en hellingen; trappen","b"]
[null,"24.1* trappen en hellingen; trappen","b","Geometrie","g","Vorm buitenste profilering","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \ntotale optrede, totale aantrede, totale breedte, volume, stootbord, trapbomen, schrobrand, welstuk, nokken",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"24.1* trappen en hellingen; trappen","b",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee",{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."},null,null,{"$f":"$V$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$W$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$X$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Y$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Z$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"}]
[null,"24.1* trappen en hellingen; trappen","b",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"24.1* trappen en hellingen; trappen","b"]
[null,"24.1* trappen en hellingen; trappen","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"24.1* trappen en hellingen; trappen","b",null,"g","Entiteit","-","-","-","-","-","-","IfcStair, IfcStairFlight, IfcRailing, IfcSlab, IfcMember","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcStair,  IfcMember"]
[null,"24.1* trappen en hellingen; trappen","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"24.1* trappen en hellingen; trappen","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"24.1* trappen en hellingen; trappen","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"24.1* trappen en hellingen; trappen","b"]
[null,"24.1* trappen en hellingen; trappen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"24.1* trappen en hellingen; trappen","b",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving). Bij meerdere afwerkingen Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"Nee","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…",null,null,"O&E 24-Trappen en hellingen(E)",{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
[null,"24.1* trappen en hellingen; trappen","b",null,"e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"Nee",{"$f":"$S$83","v":"A: Wordt voor Building Element Parts automatisch ingevuld (Mass):\nDensity in kg/m3 (Building Material Settings) x volume \n\nB: Gewicht volledig element moet handmatig ingevuld worden (zie Helpcenter)"},null,null,{"$f":"$V$83","v":"A: Automatisch (gekoppeld aan Building Materials)\n\nB: O&E-99-Gewicht samengestelde elementen (C)"},{"$f":"$W$83","v":"A: IfcBuildingElementPart\n\nB: Ifc(Element)"},{"$f":"$X$83","v":"A: Pset_PrecastConcreteElementGeneral\n\nB: ILS O&E BWK"},{"$f":"$Y$83","v":"A: ElementWeight\n\nB: Massa"},{"$f":"$Z$83","v":"A: ElementWeight in kg\n\nB: Massa in kg"}]
[]
[]
[]
[]
[null,"24.1* trappen en hellingen; trappen","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","Indien entiteit IfcStair, IfcStairFlight, IfcRailing: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"Ja",{"$f":"$S$86","v":"Structural Function (instellingenvenster > Classifications and Properties)"},null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},{"$f":"$W$86","v":"ifcSlab, ifcPlate"},{"$f":"$X$86","v":"ILS O&E BWK"},{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[]
[]
[]
[]
[null,"24.1* trappen en hellingen; trappen","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-","Indien entiteit IfcStairFlight: benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset",null,"Nee",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$W$298","v":"ifc<Entiteit>"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[]
[]
[]
[]
[]
[null,"24.1* trappen en hellingen; trappen","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering., volgens separaat afsprakendocument. 0, 20, 30, 60, etc... (WBDBO)\nIndien entiteit IfcStairFlight, IfcRailing: benoemen in Custom Pset omdat 'FireRating' geen deel uitmaakt van Common Pset",null,"Ja","ACP: WBDBO",null,null,{"$f":"$V$300","v":"ILS 4.5 Brandwerendheid"},"ifc<entiteit>",{"$f":"$X$300","v":"ifc<Entiteit>Common"},{"$f":"$Y$300","v":"FireRating"},{"$f":"$Z$300","v":"WBDBO"}]
[null,"24.1* trappen en hellingen; trappen","b","#beton","e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Zowel van treden als bordes. Bij meerdere afwerkingen Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,"O&E 24-Trappen en hellingen(E)",{"$f":"$W$294","v":"(ifcElement)"},{"$f":"$X$294","v":"ILS O&E BWK"},{"$f":"$Y$294","v":"Afwerking / Behandeling"},{"$f":"$Z$294","v":"Afwerking/Behandeling (element), Afwerking/Behandeling (materiaal)"}]
[null,"24.1* trappen en hellingen; trappen","b",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"Nee",{"$f":"$S$163","v":"ACP: Sterkteklasse (beschikbaar voor Building Materials in de Building Material Settings)"},null,null,{"$f":"$V$163","v":"n.v.t."},{"$f":"$W$163","v":"(ifcElement)"},{"$f":"$X$163","v":"ILS O&E BWK"},{"$f":"$Y$163","v":"Sterkteklasse"},{"$f":"$Z$163","v":"Sterkteklasse"}]
[]
[]
[]
[]
[]
[null,"24.1* trappen en hellingen; trappen","b","#beton","e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset\nexclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)",null,"Nee",{"$f":"$S$165","v":"ACP: Milieuklasse (beschikbaar voor Building Materials in de Building Material Settings)"},null,null,{"$f":"$V$165","v":"n.v.t."},"(ifcElement)","ILS O&E BWK","Milieuklasse",{"$f":"$Z$165","v":"Milieuklasse"}]
[null,"24.1* trappen en hellingen; trappen","b","#staal","e","Staalkwaliteit","-","-","x","-","-","-","staalkwaliteit, benoemen in Custom Pset","classificatie","-","vb.: S235, S355",null,"Nee","ACP: Sterkteklasse",null,null,"O&E 24-Trappen en hellingen(E)","(ifcElement)","ILS O&E BWK","Sterkteklasse","Sterkteklasse"]
[null,"24.1* trappen en hellingen; trappen","b","#staal","e","Conservering","-","-","-","-","-","-","-","-","-",null,null,"Nee","ACP: Conservering",null,null,"O&E 24-Trappen en hellingen(E)","(ifcElement)","ILS O&E BWK","Conservering","Conservering (element)"]
[null,"24.1* trappen en hellingen; trappen","b",null,"p","Optrede","-","-","-","-","-","-","Pset_StairCommon: RiserHeight","hoogte","mm"]
[null,"24.1* trappen en hellingen; trappen","b",null,"p","Aantrede","-","-","-","-","-","-","Pset_StairCommon: TreadLength","diepte","mm"]
[null,"24.1* trappen en hellingen; trappen","b","#beton","p","Oppervlakteklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN-EN 13670"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"24.1* trappen en hellingen; trappen","b"]
[null,"24.1* trappen en hellingen; trappen","b","Componenten","p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
[null,"24.1* trappen en hellingen; trappen","b",null,"p","Randaansluitingsvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.1* trappen en hellingen; trappen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"24.1* trappen en hellingen; trappen","b"]
[]
[null,"24.2* trappen en hellingen; hellingen","b","24.2* - Trappen en hellingen; hellingen",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - randaansluitingsvoorzieningen - verankeringen en bevestigingsmiddelen - afwerkingen die één geheel vormen met de hellingconstructie"]
[null,"24.2* trappen en hellingen; hellingen","b","Verzameling van beloopbare en berijdbare hellingen, inclusief de bijbehorende bordessen."]
[null,"24.2* trappen en hellingen; hellingen","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"24.2* trappen en hellingen; hellingen","b"]
[null,"24.2* trappen en hellingen; hellingen","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \ntotale breedte, volume",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"24.2* trappen en hellingen; hellingen","b",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee",{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."},null,null,{"$f":"$V$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$W$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$X$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Y$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Z$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"}]
[null,"24.2* trappen en hellingen; hellingen","b",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"24.2* trappen en hellingen; hellingen","b"]
[null,"24.2* trappen en hellingen; hellingen","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"24.2* trappen en hellingen; hellingen","b",null,"g","Entiteit","-","-","-","-","-","-","IfcRamp, IfcSlab","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcRamp, IfcStair"]
[null,"24.2* trappen en hellingen; hellingen","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"24.2* trappen en hellingen; hellingen","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"24.2* trappen en hellingen; hellingen","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"24.2* trappen en hellingen; hellingen","b"]
[null,"24.2* trappen en hellingen; hellingen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"24.2* trappen en hellingen; hellingen","b",null,"e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"Nee",{"$f":"$S$83","v":"A: Wordt voor Building Element Parts automatisch ingevuld (Mass):\nDensity in kg/m3 (Building Material Settings) x volume \n\nB: Gewicht volledig element moet handmatig ingevuld worden (zie Helpcenter)"},null,null,{"$f":"$V$83","v":"A: Automatisch (gekoppeld aan Building Materials)\n\nB: O&E-99-Gewicht samengestelde elementen (C)"},{"$f":"$W$83","v":"A: IfcBuildingElementPart\n\nB: Ifc(Element)"},{"$f":"$X$83","v":"A: Pset_PrecastConcreteElementGeneral\n\nB: ILS O&E BWK"},{"$f":"$Y$83","v":"A: ElementWeight\n\nB: Massa"},{"$f":"$Z$83","v":"A: ElementWeight in kg\n\nB: Massa in kg"}]
[null,"24.2* trappen en hellingen; hellingen","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_SlabCommon: Loadbearing","true/ false","-","Indien entiteit IfcRamp: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"Ja",{"$f":"$S$86","v":"Structural Function (instellingenvenster > Classifications and Properties)"},null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},"ifcSlab","Pset_SlabCommon",{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[]
[null,"24.2* trappen en hellingen; hellingen","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-",null,null,"Ja",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$W$298","v":"ifc<Entiteit>"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[null,"24.2* trappen en hellingen; hellingen","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"Ja",{"$f":"$S$300","v":"ACP: WBDBO"},null,null,{"$f":"$V$300","v":"ILS 4.5 Brandwerendheid"},"ifc<entiteit>",{"$f":"$X$300","v":"ifc<Entiteit>Common"},{"$f":"$Y$300","v":"FireRating"},{"$f":"$Z$300","v":"WBDBO"}]
[null,"24.2* trappen en hellingen; hellingen","b","#beton","e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Zowel van treden als bordes. Bij meerdere afwerkingen Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,"O&E 24-Trappen en hellingen(E)",{"$f":"$W$294","v":"(ifcElement)"},{"$f":"$X$294","v":"ILS O&E BWK"},{"$f":"$Y$294","v":"Afwerking / Behandeling"},{"$f":"$Z$294","v":"Afwerking/Behandeling (element), Afwerking/Behandeling (materiaal)"}]
[null,"24.2* trappen en hellingen; hellingen","b",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"Nee",{"$f":"$S$163","v":"ACP: Sterkteklasse (beschikbaar voor Building Materials in de Building Material Settings)"},null,null,{"$f":"$V$163","v":"n.v.t."},{"$f":"$W$163","v":"(ifcElement)"},{"$f":"$X$163","v":"ILS O&E BWK"},{"$f":"$Y$163","v":"Sterkteklasse"},{"$f":"$Z$163","v":"Sterkteklasse"}]
[]
[null,"24.2* trappen en hellingen; hellingen","b","#beton","e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset\nexclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)",null,"Nee",{"$f":"$S$165","v":"ACP: Milieuklasse (beschikbaar voor Building Materials in de Building Material Settings)"},null,null,{"$f":"$V$165","v":"n.v.t."},"(ifcElement)","ILS O&E BWK","Milieuklasse",{"$f":"$Z$165","v":"Milieuklasse"}]
[null,"24.2* trappen en hellingen; hellingen","b","#staal","e","Staalkwaliteit","-","-","-","-","-","-","staalkwaliteit, benoemen in Custom Pset","classificatie","-","vb.: S235, S355",null,"Nee","strenghtclass (IFC 4 bestaat binnen Pset_ConcreteElementGeneral)",null,null,"O&E 24-Trappen en hellingen(E)",{"$f":"$W$600","v":"(ifcElement)"},{"$f":"$X$600","v":"ILS O&E BWK"},{"$f":"$Y$600","v":"Sterkteklasse"},{"$f":"$Z$600","v":"Sterkteklasse"}]
[null,"24.2* trappen en hellingen; hellingen","b","#staal","e","Conservering","-","-","-","-","-","-","-","-","-",null,null,"Nee",{"$f":"$S$601","v":"ACP: Conservering"},null,null,"O&E 24-Trappen en hellingen(E)",{"$f":"$W$601","v":"(ifcElement)"},{"$f":"$X$601","v":"ILS O&E BWK"},{"$f":"$Y$601","v":"Conservering"},{"$f":"$Z$601","v":"Conservering (element)"}]
[null,"24.2* trappen en hellingen; hellingen","b","#beton","p","Oppervlakteklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN-EN 13670"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"24.2* trappen en hellingen; hellingen","b"]
[null,"24.2* trappen en hellingen; hellingen","b","Componenten","p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
[null,"24.2* trappen en hellingen; hellingen","b",null,"p","Randaansluitingsvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","24.2* trappen en hellingen; hellingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"24.2* trappen en hellingen; hellingen","b"]
[]
[null,"27.1* daken; niet constructief","b","27.1* - Daken; niet constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - dakvloeren, dakoverstekken en luifels - kleine boeiboorden als dakrandafwerking - gootconstructies en dakranden - isolaties die één geheel vormen met de dakconstructie - isolaties die tevens het afschot vormen - afschotlagen en mastiekranden - dilatatievoegconstructies"]
[null,"27.1* daken; niet constructief","b","Verzameling van niet-constructieve daken, zowel hellend als vlak, die de begrenzing van het gebouw aan de bovenzijde vormen, gerekend vanaf de binnenzijde en vanaf de bovenzijde van de buitenwanden."]
[null,"27.1* daken; niet constructief","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"27.1* daken; niet constructief","b"]
[null,"27.1* daken; niet constructief","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, lengte, breedte, hellingshoek",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"27.1* daken; niet constructief","b",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee",{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."},null,null,{"$f":"$V$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$W$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$X$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Y$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Z$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"}]
[null,"27.1* daken; niet constructief","b",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,{"$f":"$R$113","v":"Ja"},"3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"27.1* daken; niet constructief","b",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"27.1* daken; niet constructief","b"]
[null,"27.1* daken; niet constructief","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"27.1* daken; niet constructief","b",null,"g","Entiteit","-","-","-","-","-","-","IfcRoof, IfcSlab","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcRoof, IfcSlab"]
[null,"27.1* daken; niet constructief","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"27.1* daken; niet constructief","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"27.1* daken; niet constructief","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"27.1* daken; niet constructief","b"]
[null,"27.1* daken; niet constructief","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"27.1* daken; niet constructief","b",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"Nee","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…",null,null,"O&E 27-Daken (C)/(E)",{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
[null,"27.1* daken; niet constructief","b",null,"e","Afwerking","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar)",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,"O&E 27-Daken (C)/(E)",{"$f":"$W$294","v":"(ifcElement)"},{"$f":"$X$294","v":"ILS O&E BWK"},{"$f":"$Y$294","v":"Afwerking / Behandeling"}]
[null,"27.1* daken; niet constructief","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_SlabCommon: Loadbearing","true/ false","-","False (niet constructief)\n\nIndien entiteit IfcRoof, IfcFlowSegment, IfcBuildingElementProxy: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"Ja","Structural Function (instellingenvenster > Classifications and Properties)",null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},{"$f":"$M$672","v":"IfcRoof, IfcSlab"},"Pset_SlabCommon",{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[{"$nulls":17},"Ja","Structural Function (instellingenvenster > Classifications and Properties)",null,null,"O&E 24-Trappen en hellingen( c )/( e )"," IfcBuilding Element Proxy","ILS O&E BWK","LoadBearing","True/False"]
[null,"27.1* daken; niet constructief","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_SlabCommon: IsExternal","true/ false","-","Indien entiteit IfcRoof, IfcSlab, IfcFlowSegment, IfcBuildingElementProxy: benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset",null,"Ja",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$M$672","v":"IfcRoof, IfcSlab"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[]
[null,"27.1* daken; niet constructief","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering., volgens separaat afsprakendocument. 0, 20, 30, 60, etc... (WBDBO)\nIndien entiteit IfcFlowSegment, IfcBuildingElementProxy: benoemen in Custom Pset omdat 'FireRating' geen deel uitmaakt van Common Pset",null,"Ja",{"$f":"$S$300","v":"ACP: WBDBO"},null,null,{"$f":"$V$300","v":"ILS 4.5 Brandwerendheid"},{"$f":"$M$672","v":"IfcRoof, IfcSlab"},{"$f":"$X$300","v":"ifc<Entiteit>Common"},{"$f":"$Y$300","v":"FireRating"},{"$f":"$Z$300","v":"WBDBO"}]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"27.1* daken; niet constructief","b"]
[null,"27.1* daken; niet constructief","b","Componenten","e","Isolatie","-","-","-","-","-","-","-","-","-","Afschot modelleren; tevens aangeven: isolatiewaarde en brandklasse",null,"Nee","ACP: Brandklasse in te stellen onder Building Material Settings  > Classifications and Properties",null,null,"n.v.t.","IfcBuilding ElementPart","Pset_FireRatingProperties","FlammabilityRating","Brandklasse"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.1* daken; niet constructief","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"27.1* daken; niet constructief","b"]
[]
[null,"27.2* daken; constructief","c","27.2* - Daken; constructief",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - dakvloeren, dakoverstekken en luifels - kleine boeiboorden als onderdeel van de dakrandafwerking - gootconstructies en dakranden - isolaties die één geheel vormen met de dakconstructie - isolaties die tevens het afschot vormen - afschotlagen en mastiekranden - dilatatievoegconstructies"]
[null,"27.2* daken; constructief","c","Verzameling van constructieve daken, zowel hellend als vlak, die de begrenzing van het gebouw aan de bovenzijde vormen, gerekend vanaf de binnenzijde, echter met inbegrip van de oplegvlakken en vanaf de bovenzijde van de buitenwanden."]
[null,"27.2* daken; constructief","c",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"27.2* daken; constructief","c"]
[null,"27.2* daken; constructief","c","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, lengte, breedte, hellingshoek, volume",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"27.2* daken; constructief","c",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee",{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."},null,null,{"$f":"$V$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$W$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$X$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Y$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Z$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"}]
[null,"27.2* daken; constructief","c",null,"e","Nokken en sponningen","-","-","-","-","-","-","-","-","-","In verband met oplegging",null,{"$f":"$R$113","v":"Ja"},"3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"27.2* daken; constructief","c",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,"Ja","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"27.2* daken; constructief","c",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"27.2* daken; constructief","c"]
[null,"27.2* daken; constructief","c","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"27.2* daken; constructief","c",null,"g","Entiteit","-","-","-","-","-","-","IfcRoof, IfcSlab, IfcSlab","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcRoof, IfcSlab"]
[null,"27.2* daken; constructief","c",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"27.2* daken; constructief","c",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"27.2* daken; constructief","c",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"27.2* daken; constructief","c"]
[null,"27.2* daken; constructief","c","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"27.2* daken; constructief","c","#beton","e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"Nee",{"$f":"$S$83","v":"A: Wordt voor Building Element Parts automatisch ingevuld (Mass):\nDensity in kg/m3 (Building Material Settings) x volume \n\nB: Gewicht volledig element moet handmatig ingevuld worden (zie Helpcenter)"},null,null,{"$f":"$V$83","v":"A: Automatisch (gekoppeld aan Building Materials)\n\nB: O&E-99-Gewicht samengestelde elementen (C)"},{"$f":"$W$83","v":"A: IfcBuildingElementPart\n\nB: Ifc(Element)"},{"$f":"$X$83","v":"A: Pset_PrecastConcreteElementGeneral\n\nB: ILS O&E BWK"},{"$f":"$Y$83","v":"A: ElementWeight\n\nB: Massa"},{"$f":"$Z$83","v":"A: ElementWeight in kg\n\nB: Massa in kg"}]
[null,"27.2* daken; constructief","c",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_SlabCommon: Loadbearing","true/ false","-","True (constructief)\n\nIndien entiteit IfcRoof, IfcFlowSegment, IfcBuildingElementProxy: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"Ja","Structural Function (instellingenvenster > Classifications and Properties)",null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},"ifcSlab","Pset_SlabCommon",{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[{"$nulls":17},"Ja","Structural Function (instellingenvenster > Classifications and Properties)",null,null,"O&E 24-Trappen en hellingen( c )/( e )"," IfcBuilding Element Proxy, IfcRoof, IfcFlowSegment,","ILS O&E BWK","LoadBearing","True/False"]
[null,"27.2* daken; constructief","c",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_SlabCommon: IsExternal","true/ false","-","Indien entiteit IfcRoof, IfcSlab, IfcFlowSegment, IfcBuildingElementProxy: benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset",null,"Ja",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$M$711","v":"IfcRoof, IfcSlab, IfcSlab"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[]
[null,"27.2* daken; constructief","c",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering., volgens separaat afsprakendocument. 0, 20, 30, 60, etc... (WBDBO)\nIndien entiteit IfcFlowSegment, IfcBuildingElementProxy: benoemen in Custom Pset omdat 'FireRating' geen deel uitmaakt van Common Pset",null,"Ja",{"$f":"$S$300","v":"ACP: WBDBO"},null,null,{"$f":"$V$300","v":"ILS 4.5 Brandwerendheid"},{"$f":"$M$711","v":"IfcRoof, IfcSlab, IfcSlab"},{"$f":"$X$300","v":"ifc<Entiteit>Common"},{"$f":"$Y$300","v":"FireRating"},{"$f":"$Z$300","v":"WBDBO"}]
[null,"27.2* daken; constructief","c",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"Nee",{"$f":"$S$163","v":"ACP: Sterkteklasse (beschikbaar voor Building Materials in de Building Material Settings)"},null,null,{"$f":"$V$163","v":"n.v.t."},{"$f":"$W$163","v":"(ifcElement)"},{"$f":"$X$163","v":"ILS O&E BWK"},{"$f":"$Y$163","v":"Sterkteklasse"},{"$f":"$Z$163","v":"Sterkteklasse"}]
[]
[null,"27.2* daken; constructief","c",null,"e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset\nexclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)",null,"Nee",{"$f":"$S$165","v":"ACP: Milieuklasse (beschikbaar voor Building Materials in de Building Material Settings)"},null,null,{"$f":"$V$165","v":"n.v.t."},"(ifcElement)","ILS O&E BWK","Milieuklasse",{"$f":"$Z$165","v":"Milieuklasse"}]
[null,"27.2* daken; constructief","c",null,"p","Wapeningshoeveelheid","-","-","-","-","-","-","wapeningshoeveelheid, benoemen in Custom Pset","wapeningshoeveelheid","kg/m³"]
[null,"27.2* daken; constructief","c",null,"p","Warmtedoorgangscoefficient","-","-","-","-","-","-","Pset_SlabCommon: ThermalTransmittance","U-waarde","W/ m².K","Warmteweerstand R = 1/ U\n\nIndien entiteit IfcRoof, IfcFlowSegment, IfcBuildingElementProxy: benoemen in Custom Pset omdat 'ThermalTransmittance' geen deel uitmaakt van Common Pset"]
[null,"27.2* daken; constructief","c",null,"p","Brandwerendheid hoofddraagconstructie","-","-","-","-","-","-","brandwerendheid tot bezwijken, benoemen in Custom Pset","moment tot bezwijken","minuten"]
[null,"27.2* daken; constructief","c",null,"p","Overspanningsrichting","-","-","-","-","-","-","-","-","-"]
[null,"27.2* daken; constructief","c","#beton","p","Oppervlakteklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN-EN 13670"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"27.2* daken; constructief","c"]
[null,"27.2* daken; constructief","c","Componenten","p","Wapening","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten modelleren, ntb tijdens project; staalkwaliteit en dekking opgeven als Eigenschappen (noot: wanneer geen wapening wordt gemodelleerd, staalkwaliteit en dekking meegeven als Eigenschappen)"]
[null,"27.2* daken; constructief","c",null,"p","Raveelijzers","-","-","-","-","-","-","-","-","-"]
[null,"27.2* daken; constructief","c",null,"p","Randkist","-","-","-","-","-","-","-","-","-"]
[null,"27.2* daken; constructief","c",null,"p","Koudebrugonderbrekingen","-","-","-","-","-","-","-","-","-"]
[null,"27.2* daken; constructief","c",null,"p","Ankers/ isokorven","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten, ntb tijdens project; aangeven: staalkwaliteit en dekking"]
[null,"27.2* daken; constructief","c",null,"p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","27.2* daken; constructief","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"27.2* daken; constructief","c"]
[]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","28.1* - Hoofddraagconstructies; kolommen en liggers",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - de volledige prefabricage en montage van de constructie - de verankeringen en bevestigingsmiddelen - conserveringsbehandelingen"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","Verzameling van hoofddraagconstructies van het gebouw indien deze voornamelijk uit kolommen, liggers en/of spanten bestaan en door constructieontwerp en/of uitvoeringsmethode niet te splitsen zijn in de groepen (21.0) t/m (27.0). Er zijn 3 hoofdgroepen op basis van materiaal te onderscheiden namelijk: IHWG en prefab beton; staal; hout."]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","Geometrie","g","Vorm buitenste profilering","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nbreedte, hoogte, lengte, diameter, volume, flensdikte, lijfdikte, profieltype",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee",{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."},null,null,{"$f":"$V$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$W$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$X$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Y$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Z$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"}]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","#IHWG  #prefab beton","e","Nokken en sponningen","-","-","-","-","-","-","-","-","-","In verband met oplegging",null,{"$f":"$R$113","v":"Ja"},"3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,"Ja","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"g","Entiteit","-","-","-","-","-","-","IfcBeam, IfcColumn,IfcMember","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcBeam, IfcColumn,IfcMember"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p","Kolomnummer","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelLabel","-","-"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p","Liggernummer","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelLabel","-","-"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"e","Massa","-","-","-","-","-","-","voor prefab beton: Pset_PrecastConcreteElementGeneral: ElementWeight\n\nvoor alle andere gebouwonderdelen:\nmassa, benoemen in Custom Pset","massa","kg","indien Pset_PrecastConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'massa' benoemen in Custom Pset",null,"Nee",{"$f":"$S$83","v":"A: Wordt voor Building Element Parts automatisch ingevuld (Mass):\nDensity in kg/m3 (Building Material Settings) x volume \n\nB: Gewicht volledig element moet handmatig ingevuld worden (zie Helpcenter)"},null,null,{"$f":"$V$83","v":"A: Automatisch (gekoppeld aan Building Materials)\n\nB: O&E-99-Gewicht samengestelde elementen (C)"},{"$f":"$W$83","v":"A: IfcBuildingElementPart\n\nB: Ifc(Element)"},{"$f":"$X$83","v":"A: Pset_PrecastConcreteElementGeneral\n\nB: ILS O&E BWK"},{"$f":"$Y$83","v":"A: ElementWeight\n\nB: Massa"},{"$f":"$Z$83","v":"A: ElementWeight in kg\n\nB: Massa in kg"}]
[]
[]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,"O&E 28-Hoofddraagconstructies (E)/(C)",{"$f":"$W$294","v":"(ifcElement)"},{"$f":"$X$294","v":"ILS O&E BWK"},{"$f":"$Y$294","v":"Afwerking / Behandeling"},{"$f":"$Z$294","v":"Afwerking/Behandeling (element), Afwerking/Behandeling (materiaal)"}]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","#staal","e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"Nee","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…",null,null,"O&E 28-Hoofddraagconstructies (C)/(E)",{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","#staal","e","Conservering","-","-","-","-","-","-","-","-","-",null,null,"Nee",{"$f":"$S$601","v":"ACP: Conservering"},null,null,"O&E 24-Trappen en hellingen(E)",{"$f":"$W$601","v":"(ifcElement)"},{"$f":"$X$601","v":"ILS O&E BWK"},{"$f":"$Y$601","v":"Conservering"},{"$f":"$Z$601","v":"Conservering (element)"}]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","True (constructief)",null,"Ja","Structural Function (instellingenvenster > Classifications and Properties)",null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},{"$f":"$M$761","v":"IfcBeam, IfcColumn,IfcMember"},"Pset_<entiteit>Common",{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[]
[]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-",null,null,"Ja",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$M$761","v":"IfcBeam, IfcColumn,IfcMember"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[]
[]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"Ja",{"$f":"$S$300","v":"ACP: WBDBO"},null,null,{"$f":"$V$300","v":"ILS 4.5 Brandwerendheid"},{"$f":"$M$761","v":"IfcBeam, IfcColumn,IfcMember"},{"$f":"$X$300","v":"ifc<Entiteit>Common"},{"$f":"$Y$300","v":"FireRating"},{"$f":"$Z$300","v":"WBDBO"}]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"e","Sterkteklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: StructuralClass\n\nvoor alle andere gebouwonderdelen:\nsterkteklasse, benoemen in Custom Pset","classificatie","-","Bijv. C20/25 ; C25/30 volgens NEN-EN206-1:2014\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Sterkteklasse' benoemen in Custom Pset",null,"Nee",{"$f":"$S$163","v":"ACP: Sterkteklasse (beschikbaar voor Building Materials in de Building Material Settings)"},null,null,{"$f":"$V$163","v":"n.v.t."},{"$f":"$M$761","v":"IfcBeam, IfcColumn,IfcMember"},{"$f":"$X$163","v":"ILS O&E BWK"},{"$f":"$Y$163","v":"Sterkteklasse"},{"$f":"$Z$163","v":"Sterkteklasse"}]
[]
[]
[]
[]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","#beton","e","Milieuklasse","-","-","-","-","-","-","voor beton: Pset_ConcreteElementGeneral: EnviromentalClass\n\nvoor alle andere gebouwonderdelen:\nmilieuklasse, benoemen in Custom Pset","classificatie","-","Bijv. XC/ XD volgens NEN-EN206-1/8005\n\nIndien Pset_ConcreteElementGeneral niet ondersteund wordt in de modelleersoftware: 'Milieuklasse' benoemen in Custom Pset\nexclusief info over wapeningsdekking, die is orientatiespecifiek (bovenkant anders dan zijkant)",null,"Nee",{"$f":"$S$165","v":"ACP: Milieuklasse (beschikbaar voor Building Materials in de Building Material Settings)"},null,null,{"$f":"$V$165","v":"n.v.t."},"(ifcElement)","ILS O&E BWK","Milieuklasse",{"$f":"$Z$165","v":"Milieuklasse"}]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","#staal","e","Staalkwaliteit","-","-","-","-","-","-","staalkwaliteit, benoemen in Custom Pset","classificatie","-","vb.: S235, S355",null,"Nee",{"$f":"S600","v":"ACP: Sterkteklasse"},null,null,"O&E 28-Hoofddraagconstructies (C)",{"$f":"$W$600","v":"(ifcElement)"},{"$f":"$X$600","v":"ILS O&E BWK"},{"$f":"$Y$600","v":"Sterkteklasse"},{"$f":"$Z$600","v":"Sterkteklasse"}]
[]
[]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p","Brandwerendheid hoofddraagconstructie","-","-","-","-","-","-","brandwerendheid tot bezwijken, benoemen in Custom Pset","moment tot bezwijken","minuten"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","#beton","p","Oppervlakteklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN-EN 13670"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c","Componenten","p","Wapening","-","-","-","-","-","-","-","-","-","Ter plaatse moeilijke knooppunten modelleren, ntb tijdens project; staalkwaliteit en dekking opgeven als Eigenschappen (noot: wanneer geen wapening wordt gemodelleerd, staalkwaliteit en dekking meegeven als Eigenschappen)"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"e","Brandwerende omtimmering","-","-","-","-","-","-","-","-","true/ false","Aangeven wanneer van toepassing, uitwerking volgt onder 48.1* door de desbetreffende verantwoordelijke",null,"x"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p","Hulpconstructies","-","-","-","-","-","-","-","-","-","Hulpstaal verwerken in prestatiemodel ivm communicatie staal leverancier en afstemming meerdere disciplines"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p","Instortvoorzieningen","-","-","-","-","-","-","-","-","-"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p","Toog/ zeeg","-","-","-","-","-","-","-","-","-","Ruimtereserveringsobject modelleren om rekening te kunnen houden met het effect van toog/ zeeg"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","28.1* hoofddraagconstructies; kolommen en liggers","c",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"28.1* hoofddraagconstructies; kolommen en liggers","c"]
[]
[null,"31.** buitenwandopeningen","b","31.1* - Buitenwandopeningen; niet gevuld",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.",null,null,{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."}]
[null,"31.** buitenwandopeningen","b","Verzameling van niet-gevulde openingen in buitenwanden."]
[null,"31.** buitenwandopeningen","b","31.2* - Buitenwandopeningen; gevuld met ramen"]
[null,"31.** buitenwandopeningen","b","Verzameling van met ramen en raamkozijnen gevulde openingen in buitenwanden.",{"$nulls":11},"[Ramen] Bijv.: - draai-, klep-, schuif-, tuimel-, taats- en overige typen ramen, - ventilatiekleppen en roosters in (raam)openingen"]
[null,"31.** buitenwandopeningen","b","31.3* - Buitenwandopeningen; gevuld met deuren"]
[null,"31.** buitenwandopeningen","b","Verzameling van met deuren en deurkozijnen gevulde openingen in buitenwanden.",{"$nulls":11},"[Deuren] Bijv.: - draai-, schuif-, tuimel- en overige typen deuren, - luiken"]
[null,"31.** buitenwandopeningen","b","31.4* - Buitenwandopeningen; gevuld met puien",{"$nulls":11},"[Puien] Bijv.: - alle raam- en deurtypes"]
[null,"31.** buitenwandopeningen","b","Verzameling van met puien (inclusief ramen en deuren) gevulde openingen in buitenwanden.",{"$nulls":11},"[Allen] Bijv.: - randaansluitingsvoorzieningen, - lateien, dorpels en waterslagen, - vensterbanken en koven, - buitenzonweringen, rolluiken en verduisteringsvoorzieningen, - bevestigingsmiddelen en hang- en sluitwerken, - beveiligingsvoorzieningen, - bedieningen die één geheel vormen met een bepaald onderdeel, - beglazingen, - conserveringsbehandelingen, - afwerkingen"]
[null,"31.** buitenwandopeningen","b","Noot: in verband met de complexiteit van samenstelling versus kozijn/vlakvulling is hier het basisuitgangspunt gekozen dat het minimaal herleidbaar moet zijn hoe de opbouw is. Het is een projectkeuze om het kozijn/vlakvulling los te modelleren of op te lossen middels parameters mee te geven aan de samenstelling.\nNoot: De aan 31.1* - Buitenwandopeningen; niet gevuld gelieerde componenten (dagkantafwerkingen, etc.) zijn verwerkt in de kaarten 41.**.",{"$nulls":14},"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."]
[null,"31.** buitenwandopeningen","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"31.** buitenwandopeningen","b"]
[null,"31.** buitenwandopeningen","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, breedte, omtrek, lengte stijlen, lengte regels",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"31.** buitenwandopeningen","b",null,"e","Vlakverdeling/ rasters","-","-","-","-","-","-","-","-","-",null,null,null,"3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"31.** buitenwandopeningen","b",null,"p","Stelruimte t.o.v. omliggende geometrie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
[null,"31.** buitenwandopeningen","b",null,"p","Vorm buitenste profilering","-","-","-","-","-","-","-","-","-"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b"]
[null,"31.** buitenwandopeningen","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"31.** buitenwandopeningen","b",null,"g","Entiteit","-","-","-","-","-","-","IfcWindow, IfcDoor","IfcClass","-","Gebruik voor onderdelen het meest geëigende type BIM-entiteit (panelen: IfcPlate,  stijlen en regels: IfcMember, beglazing/ramen: IfcWindow, deuren: IfcDoors)",null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcWindow, IfcDoor"]
[null,"31.** buitenwandopeningen","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"31.** buitenwandopeningen","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"31.** buitenwandopeningen","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b","SAMENSTELLING"]
[null,"31.** buitenwandopeningen","b","Eigenschappen","e","Merk","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelReference","-","-","Unieke samenstellingscode is afhankelijk van merk kozijn en type vlakvulling",null,null,"Element ID",null,null,"ILS 3.5 Naamgeving "]
[]
[null,"31.** buitenwandopeningen","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-",null,null,"Ja",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$M$829","v":"IfcWindow, IfcDoor"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[{"$nulls":21},"ILS 3.5 Naamgeving "]
[null,"31.** buitenwandopeningen","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"Ja",{"$f":"$S$300","v":"ACP: WBDBO"},null,null,{"$f":"$V$300","v":"ILS 4.5 Brandwerendheid"},{"$f":"$M$829","v":"IfcWindow, IfcDoor"},{"$f":"$X$300","v":"ifc<Entiteit>Common"},{"$f":"$Y$300","v":"FireRating"},{"$f":"$Z$300","v":"WBDBO"}]
[]
[null,"31.** buitenwandopeningen","b",null,"e","Luchtgeluidisolatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/inkoop/uitvoering."]
[]
[null,"31.** buitenwandopeningen","b",null,"p","Warmtedoorgangscoefficient","-","-","-","-","-","-","Pset_<entiteit>Common: ThermalTransmittance","U-waarde","W/ m².K","Warmteweerstand R = 1/ U\n\nIndien entiteit IfcMember: benoemen in Custom Pset omdat 'ThermalTransmittance' geen deel uitmaakt van Common Pset in Ifc 2x3"]
[null,"31.** buitenwandopeningen","b",null,"p","Weerstandsklasse","-","-","-","-","-","-","Pset_<entiteit>Common: SecurityRating","classificatie","-","Bijv.: WK1 conform NEN 5096\n\nIndien entiteit IfcWall, IfcCurtainWall, IfcPlate, IfcMember: benoemen in Custom Pset omdat 'SecurityRating' geen deel uitmaakt van Common Pset"]
[null,"31.** buitenwandopeningen","b",null,"p","Rookwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common: SmokeStop","true/ false","-","\nIndien entiteit IfcMember, IfcPlate: benoemen in Custom Pset omdat 'SmokeStop' geen deel uitmaakt van Common Pset"]
[null,"31.** buitenwandopeningen","b",null,"p","ITS (Integrale Toegankelijkheidsstandaard)","-","-","-","-","-","-","-","true/ false","-"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b","KOZIJN"]
[null,"31.** buitenwandopeningen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"31.** buitenwandopeningen","b",null,"e","Merk","-","-","-","-","-","-","-","-","-","Dient hetzelfde merk te zijn als de samenstelling voor de herleidbaarheid."]
[null,"31.** buitenwandopeningen","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,null,{"$f":"$W$294","v":"(ifcElement)"},{"$f":"$X$294","v":"ILS O&E BWK"},{"$f":"$Y$294","v":"Afwerking / Behandeling"},{"$f":"$Z$294","v":"Afwerking/Behandeling (element), Afwerking/Behandeling (materiaal)"}]
[null,"31.** buitenwandopeningen","b",null,"e","Kleur (binnenzijde, buitenzijde)","-","-","-","-","-","-","-","-","-","(RAL) kleurcode/ omschrijving. Als binnenkleur afwijkt van buitenkleur Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"Nee","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…",null,null,"O&E 31/32 Deuren, O&E 31/32 Ramen",{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b","VLAKVULLING"]
[null,"31.** buitenwandopeningen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"31.** buitenwandopeningen","b",null,"e","Type vlakvulling","-","-","-","-","-","-","-","-","-","Projectkeuze: omschrijving (vb. draaikiepraam, paneel, vast glas) of code"]
[null,"31.** buitenwandopeningen","b",null,"e","Kleur (binnenzijde, buitenzijde)","-","-","-","-","-","-","-","-","-","(RAL) kleurcode/ omschrijving. Als binnenkleur afwijkt van buitenkleur Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"Nee","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…",null,null,"O&E 31/32 Deuren, O&E 31/32 Ramen",{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
[null,"31.** buitenwandopeningen","b",null,"e","Nooduitgang","-","-","-","-","-","-","Pset_DoorCommon: FireExit","true/ false","-"]
[null,"31.** buitenwandopeningen","b",null,"p","Draairichting","-","-","-","-","-","-","verdeling: IfcWindowStyleOperationEnum\npositie paneel in verdeling: IfcWindowPanelPositionEnum\ndraairichting paneel: IfcWindowPanelOperationEnumeration","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","ZTA","-","-","-","-","-","-","Pset_DoorWindowGlazingType: BeamRadiationTransmittance","factor","-","G-waarde\n\n\n"]
[null,"31.** buitenwandopeningen","b",null,"p","LTA","-","-","-","-","-","-","Pset_DoorWindowGlazingType: Translucency","factor","-"]
[null,"31.** buitenwandopeningen","b",null,"p","Glas specificatie","-","-","-","-","-","-","-","-","-","Omschrijving glas (vb. veiligheidsglas, HR++)"]
[null,"31.** buitenwandopeningen","b",null,"p","Geintegreerde zonwering","-","-","-","-","-","-","-","true/ false","-"]
[null,"31.** buitenwandopeningen","b",null,"p","Doorvalbeveiliging","-","-","-","-","-","-","-","true/ false","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - uniek nummer","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - type scharnier","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - type slot (elektrisch)","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - type sluitplaat (elektrisch)","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - cilinder","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - beveiliging","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - kabeloverbrenging","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - standsignalering","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - schootsignalering","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - dranger (elektrisch)","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","HSW - E voeding","-","-","-","-","-","-","-","-","-"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b"]
[null,"31.** buitenwandopeningen","b","Componenten","e","Vensterbanken en koven","-","-","-","-","-","-","-","-","-",null,null,"Nee",null,null,null,"O&E 31/32 Deuren, O&E 31/32 Ramen",{"$f":"$M$911","v":"IfcWindow, IfcDoor"},"ILS O&E BWK ramen en deuren","Kleur draaiend deel binnenzijde/Kleur draaiend deel buitenzijdew","Surface parameter uit object"]
[null,"31.** buitenwandopeningen","b",null,"e","Lateien, dorpels en waterslagen","-","-","-","-","-","-","-","-","-",null,null,"Nee",null,null,null,"O&E 31/32 Deuren, O&E 31/32 Ramen",{"$f":"$M$911","v":"IfcWindow, IfcDoor"},"ILS O&E BWK ramen en deuren","Onderdorpel (Type), Onderdorpel (materiaal)","Type:Type Onderdorpel; Materiaal: Object parameter"]
[null,"31.** buitenwandopeningen","b",null,"e","Ventilatierooster","-","-","-","-","-","-","-","-","-","Modelleren en tevens aangeven: ventilatiecapciteit",null,"Nee",null,null,null,"O&E 31/32 Deuren, O&E 31/32 Ramen",{"$f":"$M$911","v":"IfcWindow, IfcDoor"},"ILS O&E BWK ramen en deuren","Ventilatie (type), ventilatie rooster","Type:Type ventilatie; Ventilatie rooster: Object parameter"]
[null,"31.** buitenwandopeningen","b",null,"p","Zonwering, rolluiken en verduisteringsvoorziening.","-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b",null,"p","Bouwfysische eis - brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating","WBDBO","minuten","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
[null,"31.** buitenwandopeningen","b",null,"p","Bouwfysische eis - luchtgeluidisoalatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","31.** buitenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"31.** buitenwandopeningen","b"]
[]
[null,"32.** binnenwandopeningen","b","32.1* - Binnenwandopeningen; niet gevuld",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies."]
[null,"32.** binnenwandopeningen","b","Verzameling van niet-gevulde openingen in binnenwanden. "]
[null,"32.** binnenwandopeningen","b","32.2* - Binnenwandopeningen; gevuld met ramen"]
[null,"32.** binnenwandopeningen","b","Verzameling van met ramen en raamkozijnen gevulde openingen in binnenwanden.",{"$nulls":11},"[Ramen] Bijv.: - draai-, schuif- en overige typen ramen, - brandwerende raamkozijnen, - vensterbanken en koven"]
[null,"32.** binnenwandopeningen","b","32.3* - Binnenwandopeningen; gevuld met deuren"]
[null,"32.** binnenwandopeningen","b","Verzameling van met deuren en deurkozijnen gevulde openingen in binnenwanden.",{"$nulls":11},"[Deuren] Bijv.: - draai-, schuif- en overige typen deuren, - brandwerende deurkozijnen, - luiken"]
[null,"32.** binnenwandopeningen","b","32.4* - Binnenwandopeningen; gevuld met puien"]
[null,"32.** binnenwandopeningen","b","Verzameling van met puien (inclusief ramen en deuren) gevulde openingen in binnenwanden.",{"$nulls":11},"[Puien] Bijv.: - alle raam- en deurtypen, - brandwerende puien, - vensterbanken en koven"]
[null,"32.** binnenwandopeningen","b","Noot: in verband met de complexiteit van samenstelling versus kozijn/vlakvulling is hier het basisuitgangspunt gekozen dat het minimaal herleidbaar moet zijn hoe de opbouw is. Het is een projectkeuze om het kozijn/vlakvulling los te modelleren of op te lossen middels parameters mee te geven aan de samenstelling.\nNoot: De aan 32.1* - Buitenwandopeningen;niet gevuld gelieerde componenten (dagkantafwerkingen, etc.) zijn verwerkt in de kaarten 42.**.",{"$nulls":11},"[Allen] Bijv.: - randaansluitingsvoorzieningen, - lateien en dorpels, - verduisteringsvoorzieningen, - bevestigingsmiddelen en hang- en sluitwerken, - bedieningen die één geheel vormen met een bepaald onderdeel, - beglazingen, - conserveringsbehandelingen, - afwerkingen",null,null,"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."]
[null,"32.** binnenwandopeningen","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"32.** binnenwandopeningen","b"]
[null,"32.** binnenwandopeningen","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, breedte, omtrek, lengte stijlen, lengte regels",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"32.** binnenwandopeningen","b",null,"e","Vlakverdeling/ rasters","-","-","-","-","-","-","-","-","-",null,null,"Ja","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"32.** binnenwandopeningen","b",null,"p","Stelruimte t.o.v. omliggende geometrie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
[null,"32.** binnenwandopeningen","b",null,"p","Vorm buitenste profilering","-","-","-","-","-","-","-","-","-"]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b"]
[null,"32.** binnenwandopeningen","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"32.** binnenwandopeningen","b",null,"g","Entiteit","-","-","-","-","-","-","IfcWindow, IfcDoor","IfcClass","-","Gebruik voor onderdelen het meest geëigende type BIM-entiteit (panelen: IfcPlate,  stijlen en regels: IfcMember, beglazing/ramen: IfcWindow, deuren: IfcDoors)",null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcWindow, IfcDoor"]
[null,"32.** binnenwandopeningen","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"32.** binnenwandopeningen","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"32.** binnenwandopeningen","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b","SAMENSTELLING"]
[null,"32.** binnenwandopeningen","b","Eigenschappen","e","Merk","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelReference","-","-","Unieke samenstellingscode is afhankelijk van merk kozijn en type vlakvulling",null,"Ja","Element ID",null,null,"ILS 3.5 Naamgeving "]
[null,"32.** binnenwandopeningen","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-",null,null,"Ja",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$M$911","v":"IfcWindow, IfcDoor"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[null,"32.** binnenwandopeningen","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"Ja",{"$f":"$S$300","v":"ACP: WBDBO"},null,null,{"$f":"$V$300","v":"ILS 4.5 Brandwerendheid"},{"$f":"$M$911","v":"IfcWindow, IfcDoor"},{"$f":"$X$300","v":"ifc<Entiteit>Common"},{"$f":"$Y$300","v":"FireRating"},{"$f":"$Z$300","v":"WBDBO"}]
[null,"32.** binnenwandopeningen","b",null,"e","Luchtgeluidisolatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/inkoop/uitvoering."]
[]
[null,"32.** binnenwandopeningen","b",null,"p","Weerstandsklasse","-","-","-","-","-","-","Pset_<entiteit>Common: SecurityRating","classificatie","-","Bijv.: WK1 conform NEN 5096\n\nIndien entiteit IfcWall, IfcCurtainWall, IfcPlate, IfcMember: benoemen in Custom Pset omdat 'SecurityRating' geen deel uitmaakt van Common Pset"]
[null,"32.** binnenwandopeningen","b",null,"p","Rookwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common: SmokeStop","true/ false","-","\nIndien entiteit IfcMember, IfcPlate: benoemen in Custom Pset omdat 'SmokeStop' geen deel uitmaakt van Common Pset"]
[null,"32.** binnenwandopeningen","b",null,"p","ITS (Integrale Toegankelijkheidsstandaard)","-","-","-","-","-","-","-","true/ false","-"]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b","KOZIJN"]
[null,"32.** binnenwandopeningen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"32.** binnenwandopeningen","b",null,"e","Kozijnmerk","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,null,{"$f":"$W$294","v":"(ifcElement)"},{"$f":"$X$294","v":"ILS O&E BWK"},{"$f":"$Y$294","v":"Afwerking / Behandeling"},{"$f":"$Z$294","v":"Afwerking/Behandeling (element), Afwerking/Behandeling (materiaal)"}]
[null,"32.** binnenwandopeningen","b",null,"e","Kleur (binnenzijde, buitenzijde)","-","-","-","-","-","-","-","-","-","(RAL) kleurcode/ omschrijving. Als binnenkleur afwijkt van buitenkleur Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"Nee","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…",null,null,"O&E 31/32 Deuren, O&E 31/32 Ramen",{"$f":"$M$911","v":"IfcWindow, IfcDoor"},"ILS O&E BWK ramen en deuren","Kleur draaiend deel binnenzijde/Kleur draaiend deel buitenzijdew","Surface parameter uit object"]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b","VLAKVULLING"]
[null,"32.** binnenwandopeningen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"32.** binnenwandopeningen","b",null,"e","Type vlakvulling","-","-","-","-","-","-","-","-","-","Projectkeuze: omschrijving (vb. draaikiepraam, paneel, vast glas) of code",null,"Nee","ACP: Productinformatie",null,null,"O&E 31/32 Deuren, O&E 31/32 Ramen",{"$f":"$M$911","v":"IfcWindow, IfcDoor"},"ILS O&E BWK ramen en deuren","Aanvullende productinformatie","Productinformatie"]
[null,"32.** binnenwandopeningen","b",null,"e","Kleur (binnenzijde, buitenzijde)","-","-","-","-","-","-","-","-","-","(RAL) kleurcode/ omschrijving. Als binnenkleur afwijkt van buitenkleur Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"Nee","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…",null,null,"O&E 31/32 Deuren, O&E 31/32 Ramen",{"$f":"$M$911","v":"IfcWindow, IfcDoor"},"ILS O&E BWK ramen en deuren","Kleur draaiend deel binnenzijde/Kleur draaiend deel buitenzijdew","Surface parameter uit object"]
[null,"32.** binnenwandopeningen","b",null,"e","Nooduitgang","-","-","-","-","-","-","Pset_DoorCommon: FireExit","true/ false","-",null,null,"Nee",null,null,null,"O&E 31/32 Deuren, O&E 31/32 Ramen",{"$f":"$M$911","v":"IfcWindow, IfcDoor"},"Pset_<Entiteit>Common","FireExit","True/False"]
[null,"32.** binnenwandopeningen","b",null,"p","Draairichting","-","-","-","-","-","-","verdeling: IfcWindowStyleOperationEnum\npositie paneel in verdeling: IfcWindowPanelPositionEnum\ndraairichting paneel: IfcWindowPanelOperationEnumeration","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","Glas specificatie","-","-","-","-","-","-","-","-","-","Omschrijving glas (vb. veiligheidsglas, HR++)"]
[null,"32.** binnenwandopeningen","b",null,"p","Doorvalbeveiliging","-","-","-","-","-","-","-","true/ false","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - uniek nummer","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - type scharnier","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - type slot (elektrisch)","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - type sluitplaat (elektrisch)","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - cilinder","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - beveiliging","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - kabeloverbrenging","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - standsignalering","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - schootsignalering","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - dranger (elektrisch)","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","HSW - E voeding","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","Uniek deurnummer","-","-","-","-","-","-","-","-","-","Uniek nummer t.b.v. sluitplannen etc."]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b"]
[null,"32.** binnenwandopeningen","b","Componenten","e","Vensterbanken en koven","-","-","-","-","-","-","-","-","-",null,null,"Nee",null,null,null,"O&E 31/32 Deuren, O&E 31/32 Ramen",{"$f":"$M$911","v":"IfcWindow, IfcDoor"},"ILS O&E BWK ramen en deuren","Kleur draaiend deel binnenzijde/Kleur draaiend deel buitenzijdew","Surface parameter uit object"]
[null,"32.** binnenwandopeningen","b",null,"e","Lateien en dorpels","-","-","-","-","-","-","-","-","-",null,null,"Nee",null,null,null,"O&E 31/32 Deuren, O&E 31/32 Ramen",{"$f":"$M$911","v":"IfcWindow, IfcDoor"},"ILS O&E BWK ramen en deuren","Onderdorpel (Type), Onderdorpel (materiaal)","Type:Type Onderdorpel; Materiaal: Object parameter"]
[null,"32.** binnenwandopeningen","b",null,"p","Verduisteringsvoorzieningen","-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b",null,"p","Bouwfysische eis - brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating","WBDBO","minuten","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
[null,"32.** binnenwandopeningen","b",null,"p","Bouwfysische eis - luchtgeluidisoalatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","32.** binnenwandopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"32.** binnenwandopeningen","b"]
[]
[null,"33.** vloeropeningen","b","33.** - Vloeropeningen",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - toegangsluiken naar hogere of lagere niveaus - roostervloeren in leidingschachten - randaansluitingsvoorzieningen - ravelingen - bevestigingsmiddelen en hang- en sluitwerken - bedieningen die één geheel vormen met een bepaald onderdeel - beglazingen - conserveringsbehandelingen - afwerkingen"]
[null,"33.** vloeropeningen","b","Verzameling van met een vulling voorziene openingen in vloeren.",{"$nulls":14},"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'.",null,null,"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"]
[null,"33.** vloeropeningen","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"33.** vloeropeningen","b"]
[null,"33.** vloeropeningen","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, omtrek",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"33.** vloeropeningen","b",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"33.** vloeropeningen","b"]
[null,"33.** vloeropeningen","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"33.** vloeropeningen","b",null,"g","Entiteit","-","-","-","-","-","-","IfcSlab, IfcPlate","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcSlab"]
[null,"33.** vloeropeningen","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"33.** vloeropeningen","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"33.** vloeropeningen","b",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"33.** vloeropeningen","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"33.** vloeropeningen","b"]
[null,"33.** vloeropeningen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"33.** vloeropeningen","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,null,{"$f":"$W$294","v":"(ifcElement)"},{"$f":"$X$294","v":"ILS O&E BWK"},{"$f":"$Y$294","v":"Afwerking / Behandeling"},{"$f":"$Z$294","v":"Afwerking/Behandeling (element), Afwerking/Behandeling (materiaal)"}]
[null,"33.** vloeropeningen","b",null,"e","Kleur","-","-","-","-","-","-","-","-","-","(RAL) kleurcode/ omschrijving. Als binnenkleur afwijkt van buitenkleur Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"Nee","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…",null,null,null,{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
[null,"33.** vloeropeningen","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-",null,null,"Nee","Structural Function (instellingenvenster > Classifications and Properties)",null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},{"$f":"$M$977","v":"IfcSlab, IfcPlate"},"Pset_<entiteit>Common",{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[null,"33.** vloeropeningen","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-",null,null,"Ja",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$M$977","v":"IfcSlab, IfcPlate"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[null,"33.** vloeropeningen","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"Nee",{"$f":"$S$300","v":"ACP: WBDBO"},null,null,{"$f":"$V$300","v":"ILS 4.5 Brandwerendheid"},{"$f":"$M$977","v":"IfcSlab, IfcPlate"},{"$f":"$X$300","v":"ifc<Entiteit>Common"},{"$f":"$Y$300","v":"FireRating"},{"$f":"$Z$300","v":"WBDBO"}]
[null,"33.** vloeropeningen","b",null,"p","Warmtedoorgangscoefficient","-","-","-","-","-","-","Pset_<entiteit>Common: ThermalTransmittance","U-waarde","W/ m².K","Warmteweerstand R = 1/ U"]
[null,"33.** vloeropeningen","b",null,"p","Weerstandsklasse","-","-","-","-","-","-","SecurityRating benoemen in custom Pset","classificatie","-","Bijv.: WK1 conform NEN 5096\n\nIndien entiteit IfcPlate, IfcSlab: benoemen in Custom Pset omdat 'SecurityRating' geen deel uitmaakt van Common Pset"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"33.** vloeropeningen","b"]
[null,"33.** vloeropeningen","b","Componenten","e","Isolatie","-","-","-","-","-","-","-","-","-","Tevens aangeven: isolatiewaarde en brandklasse",null,"Nee","ACP: Building Material > Classifications and Properties"]
[null,"33.** vloeropeningen","b",null,"e","Randafwerking","-","-","-","-","-","-","-","-","-",null,null,"Nee"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","33.** vloeropeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"33.** vloeropeningen","b"]
[]
[null,"34.** balustrades en leuningen","b","34.** - Balustrades en leuningen",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - balustrades en leuningen langs dakranden - bevestigingsmiddelen - conserveringsbehandelingen - afwerkingen"]
[null,"34.** balustrades en leuningen","b","Verzameling van voltooiingen van balkons, galerijen, loggia's, vides, trappen, hellingen, vloeren dakopeningen en dakranden door middel van balustrades."]
[null,"34.** balustrades en leuningen","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"34.** balustrades en leuningen","b"]
[null,"34.** balustrades en leuningen","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"34.** balustrades en leuningen","b",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,"Nee","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"34.** balustrades en leuningen","b",null,"p","Stelruimte t.o.v. omliggende geometrie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"34.** balustrades en leuningen","b"]
[null,"34.** balustrades en leuningen","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"34.** balustrades en leuningen","b",null,"g","Entiteit","-","-","-","-","-","-","IfcRailing","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcRailing, IfcMember"]
[null,"34.** balustrades en leuningen","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"34.** balustrades en leuningen","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"34.** balustrades en leuningen","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"34.** balustrades en leuningen","b"]
[null,"34.** balustrades en leuningen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"34.** balustrades en leuningen","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,"O&E 34-Balustrades en leuningen (E)",{"$f":"$W$294","v":"(ifcElement)"},{"$f":"$X$294","v":"ILS O&E BWK"},{"$f":"$Y$294","v":"Afwerking / Behandeling"},{"$f":"$Z$294","v":"Afwerking/Behandeling (element), Afwerking/Behandeling (materiaal)"}]
[null,"34.** balustrades en leuningen","b",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving), bij meerdere waarden Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"Nee","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…",null,null,"O&E 34-Balustrades en leuningen (E)",{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
[null,"34.** balustrades en leuningen","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_RailingCommon: IsExternal","true/ false","-",null,null,"Ja",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$W$298","v":"ifc<Entiteit>"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[null,"34.** balustrades en leuningen","b",null,"p","Gebruiksklasse","-","-","-","-","-","-","-","classificatie","-","Klasse A t/m K (volgens NEN:EN1990-1-1)"]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"34.** balustrades en leuningen","b"]
[null,"34.** balustrades en leuningen","b","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","34.** balustrades en leuningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"34.** balustrades en leuningen","b"]
[]
[null,"37.** dakopeningen","b","37.** - Dakopeningen",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - dakluiken, rookluiken en daklichten - randaansluitingsvoorzieningen - raveelconstructies - bevestigingsmiddelen en hang- en sluitwerken - beveiligingsvoorzieningen - bedieningen die één geheel vormen met een bepaald onderdeel - beglazingen - afwerkingen"]
[null,"37.** dakopeningen","b","Verzameling van met een vulling voorziene openingen in daken.\nNoot: in verband met de complexiteit van samenstelling versus kozijn/vlakvulling is hier het basisuitgangspunt gekozen dat het minimaal herleidbaar moet zijn hoe de opbouw is. Het is een projectkeuze om het kozijn/vlakvulling los te modelleren of op te lossen middels parameters mee te geven aan de samenstelling."]
[null,"37.** dakopeningen","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"37.** dakopeningen","b"]
[null,"37.** dakopeningen","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, breedte, omtrek, lengte stijlen, lengte regels",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"37.** dakopeningen","b",null,"e","Vlakverdeling/ rasters","-","-","-","-","-","-","-","-","-",null,null,"Nee","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"37.** dakopeningen","b",null,"p","Stelruimte t.o.v. omliggende geometrie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
[null,"37.** dakopeningen","b",null,"p","Vorm buitenste profilering","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b"]
[null,"37.** dakopeningen","b"]
[null,"37.** dakopeningen","b"]
[null,"37.** dakopeningen","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"37.** dakopeningen","b",null,"g","Entiteit","-","-","-","-","-","-","IfcWindow, IfcDoor","IfcClass","-","Gebruik voor onderdelen het meest geëigende type BIM-entiteit (panelen: IfcPlate,  stijlen en regels: IfcMember, beglazing/ramen: IfcWindow, deuren: IfcDoors)",null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcWindow, IfcDoor"]
[null,"37.** dakopeningen","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"37.** dakopeningen","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"37.** dakopeningen","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b","SAMENSTELLING"]
[null,"37.** dakopeningen","b","Eigenschappen"]
[null,"37.** dakopeningen","b",null,"e","Merk","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelReference","-","-","Unieke samenstellingscode is afhankelijk van merk kozijn en type vlakvulling",null,{"$f":"$R$113","v":"Ja"},"Element ID"]
[null,"37.** dakopeningen","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-",null,null,"Nee",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$M$1050","v":"IfcWindow, IfcDoor"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[null,"37.** dakopeningen","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"Nee",{"$f":"$S$300","v":"ACP: WBDBO"},null,null,{"$f":"$V$300","v":"ILS 4.5 Brandwerendheid"},null,{"$f":"$X$300","v":"ifc<Entiteit>Common"},{"$f":"$Y$300","v":"FireRating"},{"$f":"$Z$300","v":"WBDBO"}]
[null,"37.** dakopeningen","b",null,"e","Luchtgeluidisolatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/inkoop/uitvoering."]
[null,"37.** dakopeningen","b",null,"p","Warmtedoorgangscoefficient","-","-","-","-","-","-","Pset_<entiteit>Common: ThermalTransmittance","U-waarde","W/ m².K","Warmteweerstand R = 1/ U"]
[null,"37.** dakopeningen","b",null,"p","Weerstandsklasse","-","-","-","-","-","-","Pset_<entiteit>Common: SecurityRating","classificatie","-","Bijv.: WK1 conform NEN 5096\n\nIndien entiteit IfcWall, IfcCurtainWall, IfcPlate, IfcMember: benoemen in Custom Pset omdat 'SecurityRating' geen deel uitmaakt van Common Pset"]
[null,"37.** dakopeningen","b",null,"p","Rookwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common: SmokeStop","true/ false","-"]
[null,"37.** dakopeningen","b",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b","KOZIJN"]
[null,"37.** dakopeningen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"37.** dakopeningen","b",null,"e","Kozijnmerk","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,"O&E 37-Dakopeningen",{"$f":"$W$294","v":"(ifcElement)"},{"$f":"$X$294","v":"ILS O&E BWK"},{"$f":"$Y$294","v":"Afwerking / Behandeling"},{"$f":"$Z$294","v":"Afwerking/Behandeling (element), Afwerking/Behandeling (materiaal)"}]
[null,"37.** dakopeningen","b",null,"e","Kleur (binnenzijde, buitenzijde)","-","-","-","-","-","-","-","-","-","(RAL) kleurcode/ omschrijving. Als binnenkleur afwijkt van buitenkleur Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"Nee","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…",null,null,null,{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b","VLAKVULLING"]
[null,"37.** dakopeningen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"37.** dakopeningen","b",null,"e","Type vlakvulling","-","-","-","-","-","-","-","-","-","Projectkeuze: omschrijving (vb. draaikiepraam, paneel, vast glas) of code",null,"Nee"]
[null,"37.** dakopeningen","b",null,"e","Kleur (binnenzijde, buitenzijde)","-","-","-","-","-","-","-","-","-","(RAL) kleurcode/ omschrijving. Als binnenkleur afwijkt van buitenkleur Native Parameter niet gebruiken maar, Custom parameters benoemen in Pset file.",null,"Nee","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…",null,null,null,{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
[null,"37.** dakopeningen","b",null,"e","HSW - uniek nummer","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","Draairichting","-","-","-","-","-","-","verdeling: IfcWindowStyleOperationEnum\npositie paneel in verdeling: IfcWindowPanelPositionEnum\ndraairichting paneel: IfcWindowPanelOperationEnumeration","-","-"]
[null,"37.** dakopeningen","b",null,"p","ZTA","-","-","-","-","-","-","Pset_DoorWindowGlazingType: BeamRadiationTransmittance","factor","-","G-waarde\n\n\n"]
[null,"37.** dakopeningen","b",null,"p","LTA","-","-","-","-","-","-","Pset_DoorWindowGlazingType: Translucency","factor","-"]
[null,"37.** dakopeningen","b",null,"p","Glas specificatie","-","-","-","-","-","-","-","-","-","Omschrijving glas (vb. veiligheidsglas, HR++)"]
[null,"37.** dakopeningen","b",null,"p","Geintegreerde zonwering","-","-","-","-","-","-","-","true/ false","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - type scharnier","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - type slot (elektrisch)","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - type sluitplaat (elektrisch)","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - cilinder","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - beveiliging","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - kabeloverbrenging","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - standsignalering","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - schootsignalering","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - dranger (elektrisch)","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","HSW - E voeding","-","-","-","-","-","-","-","-","-"]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b"]
[null,"37.** dakopeningen","b","Componenten","e","Randafwerking","-","-","-","-","-","-","-","-","-",null,null,"Nee",{"$nulls":4},{"$f":"$M$1050","v":"IfcWindow, IfcDoor"},"ILS O&E ramen en deuren","Afwerking dagkant binnen/buiten ","Parameters object "]
[null,"37.** dakopeningen","b",null,"e","Ventilatierooster","-","-","-","-","-","-","-","-","-","Modelleren en tevens aangeven: ventilatiecapciteit",null,"Nee","ACP: Type Ventilatie",null,null,null,{"$f":"$M$1050","v":"IfcWindow, IfcDoor"},"ILS O&E ramen en deuren","Ventilatie (type), Ventilatierooster","Type Ventilatie, Parameters object "]
[null,"37.** dakopeningen","b",null,"p","Zonwering, rolluiken en verduisteringsvoorziening.","-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b",null,"p","Bouwfysische eis - brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating","WBDBO","minuten","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
[null,"37.** dakopeningen","b",null,"p","Bouwfysische eis - luchtgeluidisoalatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","37.** dakopeningen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"37.** dakopeningen","b"]
[]
[null,"41.1* buitenwandafwerkingen","b","41.1* - Buitenwandafwerkingen",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - isolerende, akoestische en brandwerende afwerkingen - gevelbekledingen en gevelbetimmeringen - bepleisteringen - betegelingen - schilderafwerkingen"]
[null,"41.1* buitenwandafwerkingen","b","Verzameling van afwerkingen van de buitenzijde van buitenwanden, gerekend vanaf de wandconstructie."]
[null,"41.1* buitenwandafwerkingen","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"41.1* buitenwandafwerkingen","b"]
[null,"41.1* buitenwandafwerkingen","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, breedte, dikte\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"Nee",{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"41.1* buitenwandafwerkingen","b",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,"Nee","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"41.1* buitenwandafwerkingen","b",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,"Nee","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"41.1* buitenwandafwerkingen","b"]
[null,"41.1* buitenwandafwerkingen","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"x",{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"41.1* buitenwandafwerkingen","b",null,"g","Entiteit","-","-","-","-","-","-","IfcPlate, IfcCovering, IfcWall, IfcBuildingElementProxy","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcCovering"]
[null,"41.1* buitenwandafwerkingen","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"41.1* buitenwandafwerkingen","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"41.1* buitenwandafwerkingen","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"41.1* buitenwandafwerkingen","b"]
[null,"41.1* buitenwandafwerkingen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"41.1* buitenwandafwerkingen","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,"O&E 41*-47*-Afwerkingen(E)",{"$f":"$W$294","v":"(ifcElement)"},{"$f":"$X$294","v":"ILS O&E BWK"},{"$f":"$Y$294","v":"Afwerking / Behandeling"},{"$f":"$Z$294","v":"Afwerking/Behandeling (element), Afwerking/Behandeling (materiaal)"}]
[null,"41.1* buitenwandafwerkingen","b",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"Nee","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…",null,null,"O&E 41*-47*-Afwerkingen(E)",{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
[null,"41.1* buitenwandafwerkingen","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","Indien entiteit IfcCovering, IfcBuildingElementProxy: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"Nee","Structural Function (instellingenvenster > Classifications and Properties)",null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"}," IfcBuildingElementProxy ifcCovering","ILS O&E BWK",{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[null,"41.1* buitenwandafwerkingen","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-","Indien entiteit IfcCovering, IfcBuildingElementProxy: benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset",null,"Nee",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$M$1118","v":"IfcPlate, IfcCovering, IfcWall, IfcBuildingElementProxy"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[null,"41.1* buitenwandafwerkingen","b",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"Nee",{"$f":"$S$300","v":"ACP: WBDBO"},null,null,{"$f":"$V$300","v":"ILS 4.5 Brandwerendheid"},{"$f":"$M$1118","v":"IfcPlate, IfcCovering, IfcWall, IfcBuildingElementProxy"},{"$f":"$X$300","v":"ifc<Entiteit>Common"},{"$f":"$Y$300","v":"FireRating"},{"$f":"$Z$300","v":"WBDBO"}]
[null,"41.1* buitenwandafwerkingen","b",null,"p","Brandwerende afwerking","-","-","-","-","-","-","-","-","-"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"41.1* buitenwandafwerkingen","b"]
[null,"41.1* buitenwandafwerkingen","b","Componenten","e","Dagkantafwerking, waterslagen","-","-","-","-","-","-","-","-","-","In het geval van 31.1* Buitenwandopeningen; niet gevuld"]
[null,"41.1* buitenwandafwerkingen","b",null,"p","Verankering en bevestiging","-","-","-","-","-","-","-","-","-","Niet modelleren, wel terug laten komen in details"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","41.1* buitenwandafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"41.1* buitenwandafwerkingen","b"]
[]
[null,"42.1* binnenwandafwerkingen","i","42.1* - Binnenwandafwerkingen",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - isolerende, akoestische en brandwerende afwerkingen - wandbekledingen en wandbetimmeringen - bepleisteringen - betegelingen - schilderafwerkingen - hoekbeschermers en stootbanden die één geheel vormen met de wandafwerking"]
[null,"42.1* binnenwandafwerkingen","i","Verzameling van afwerkingen van de binnenwanden en van de binnenzijde van de buitenwanden, gerekend vanaf de wandconstructie."]
[null,"42.1* binnenwandafwerkingen","i",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"42.1* binnenwandafwerkingen","i"]
[null,"42.1* binnenwandafwerkingen","i","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, breedte, dikte\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"Ja",{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"42.1* binnenwandafwerkingen","i",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,"Ja","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"42.1* binnenwandafwerkingen","i",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,"Ja","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"42.1* binnenwandafwerkingen","i"]
[null,"42.1* binnenwandafwerkingen","i","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"Nee",{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"42.1* binnenwandafwerkingen","i",null,"g","Entiteit","-","-","-","-","-","-","IfcPlate, IfcCovering, IfcWall","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcCovering"]
[null,"42.1* binnenwandafwerkingen","i",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"42.1* binnenwandafwerkingen","i",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"42.1* binnenwandafwerkingen","i",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"42.1* binnenwandafwerkingen","i"]
[null,"42.1* binnenwandafwerkingen","i","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"42.1* binnenwandafwerkingen","i",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,"O&E 41*-47*-Afwerkingen(E)",{"$f":"$W$294","v":"(ifcElement)"},{"$f":"$X$294","v":"ILS O&E BWK"},{"$f":"$Y$294","v":"Afwerking / Behandeling"},{"$f":"$Z$294","v":"Afwerking/Behandeling (element), Afwerking/Behandeling (materiaal)"}]
[null,"42.1* binnenwandafwerkingen","i",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"Nee","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…",null,null,"O&E 41*-47*-Afwerkingen(E)",{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
[null,"42.1* binnenwandafwerkingen","i",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","Indien entiteit IfcCovering: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",null,"Nee","Structural Function (instellingenvenster > Classifications and Properties)",null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},null,"ILS O&E BWK",{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[null,"42.1* binnenwandafwerkingen","i",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-","Indien entiteit IfcCovering: benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset",null,"Nee",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$W$298","v":"ifc<Entiteit>"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[null,"42.1* binnenwandafwerkingen","i",null,"e","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…",null,"Nee",{"$f":"$S$300","v":"ACP: WBDBO"},null,null,{"$f":"$V$300","v":"ILS 4.5 Brandwerendheid"},"ifc<entiteit>",{"$f":"$X$300","v":"ifc<Entiteit>Common"},{"$f":"$Y$300","v":"FireRating"},{"$f":"$Z$300","v":"WBDBO"}]
[null,"42.1* binnenwandafwerkingen","i",null,"p","Brandwerende afwerking","-","-","-","-","-","-","-","-","-"]
[null,"42.1* binnenwandafwerkingen","i",null,"p","Vlakheidsklasse","-","-","-","-","-","-","-","classificatie","-"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"42.1* binnenwandafwerkingen","i"]
[null,"42.1* binnenwandafwerkingen","i","Componenten","e","Dagkantafwerking","-","-","-","-","-","-",null,"-","-","In het geval van 32.1* Binnenwandopeningen; niet gevuld"]
[null,"42.1* binnenwandafwerkingen","i",null,"p","Verankering en bevestiging","-","-","-","-","-","-","-","-","-","Niet modelleren, wel terug laten komen in details"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","42.1* binnenwandafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"42.1* binnenwandafwerkingen","i"]
[]
[null,"43.** vloerafwerkingen","i","43.** - Vloerafwerkingen; verhoogd en niet verhoogd",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - podiums en toneelvloeren - verhoogde computervloeren - randaansluitingsvoorzieningen - afwerkingen die één geheel vormen met de verhoogde vloerconstructie - dilatatievoegconstructies/ - isolerende, akoestische en brandwerende afwerkingen - dekvloeren samengesteld uit zand/cement of synthetische stoffen - terrazzovloeren - betegelde en natuursteenvloeren - houten (parket)vloerafwerkingen - vloerbedekkingen en afwerkingen op de dekvloeren - plinten - matomrandingen"]
[null,"43.** vloerafwerkingen","i","Verzameling van afwerkingen van de bovenzijde van vloeren door middel van een verhoogde constructie/ rechtstreeks op de al dan niet verhoogde vloerconstructie aangebracht, gerekend vanaf de ondervloerconstructie."]
[null,"43.** vloerafwerkingen","i",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"43.** vloerafwerkingen","i"]
[null,"43.** vloerafwerkingen","i","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, omtrek\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"Nee",{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"43.** vloerafwerkingen","i",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee",{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."},null,null,{"$f":"$V$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$W$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$X$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Y$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Z$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"}]
[null,"43.** vloerafwerkingen","i",null,"e","Afschot","-","-","-","-","-","-","-","-","-",null,null,"Nee","ACP: Afschot",null,null,null,{"$f":"M1195","v":"IfcSlab, IfcCovering"},"ILS O&E BWK","Afschot","Afschot"]
[null,"43.** vloerafwerkingen","i",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,"Nee","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"43.** vloerafwerkingen","i",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,"Nee","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"43.** vloerafwerkingen","i"]
[null,"43.** vloerafwerkingen","i","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument"]
[null,"43.** vloerafwerkingen","i",null,"g","Entiteit","-","-","-","-","-","-","IfcSlab, IfcCovering","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcCovering"]
[null,"43.** vloerafwerkingen","i",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,"(ifcElement)","()",{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"43.** vloerafwerkingen","i",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"43.** vloerafwerkingen","i",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"43.** vloerafwerkingen","i",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"43.** vloerafwerkingen","i"]
[null,"43.** vloerafwerkingen","i","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"43.** vloerafwerkingen","i",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,"O&E 41*-47*-Afwerkingen(E)",{"$f":"$W$294","v":"(ifcElement)"},{"$f":"$X$294","v":"ILS O&E BWK"},{"$f":"$Y$294","v":"Afwerking / Behandeling"},{"$f":"$Z$294","v":"Afwerking/Behandeling (element), Afwerking/Behandeling (materiaal)"}]
[null,"43.** vloerafwerkingen","i",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"Nee","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…",null,null,"O&E 41*-47*-Afwerkingen(E)",{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
[null,"43.** vloerafwerkingen","i",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_SlabCommon: Loadbearing","true/ false","-","Indien entiteit IfcCovering: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Pset_CoveringCommon",null,"Nee","Structural Function (instellingenvenster > Classifications and Properties)",null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"}," IfcBuilding Element Proxy","ILS O&E BWK",{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[null,"43.** vloerafwerkingen","i",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_SlabCommon: IsExternal","-","true/ false","Indien entiteit IfcCovering: benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset",null,"Nee",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$W$298","v":"ifc<Entiteit>"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[null,"43.** vloerafwerkingen","i",null,"p","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…"]
[null,"43.** vloerafwerkingen","i",null,"p","Brandwerende afwerking","-","-","-","-","-","-","-","-"]
[null,"43.** vloerafwerkingen","i",null,"p","Warmtedoorgangscoefficient","-","-","-","-","-","-","Pset_SlabCommon: ThermalTransmittance","U-waarde","W/ m².K","Warmteweerstand R = 1/ U\n\nIndien entiteit IfcCovering: benoemen in Custom Pset omdat 'ThermalTransmittance' geen deel uitmaakt van Common Pset in Ifc 2x3"]
[null,"43.** vloerafwerkingen","i",null,"e","Luchtgeluidisolatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/inkoop/uitvoering.",null,"Nee","ACP: Geluidwering",null,null,null,{"$f":"M1195","v":"IfcSlab, IfcCovering"},"Pset_<Eintiteit>Common","AcousticRating","Geluidwering"]
[null,"43.** vloerafwerkingen","i",null,"p","Vlakheidsklasse","-","-","-","-","-","-","-","classificatie","-","Conform NEN 2747"]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"43.** vloerafwerkingen","i"]
[null,"43.** vloerafwerkingen","i","Componenten","p","Ondervloerconstructie","-","-","-","-","-","-","-","-","-","Ten behoeve van afstemming met installaties (bijvoorbeeld: pootjes computervloeren)\nNoot: ter plaatse moeilijke knooppunten modelleren, ntb tijdens project;"]
[null,"43.** vloerafwerkingen","i",null,"p","Randaansluitingsvoorzieningen","-","-","-","-","-","-","-","-","-"]
[null,"43.** vloerafwerkingen","i",null,"p","Bouwfysische eis - brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating","WBDBO","minuten","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
[null,"43.** vloerafwerkingen","i",null,"p","Bouwfysische eis - luchtgeluidisoalatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","43.** vloerafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"43.** vloerafwerkingen","i"]
[]
[null,"44.** trap- en hellingafwerkingen","b","44.** - Trap- en hellingafwerkingen",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - isolerende, akoestische en brandwerende afwerkingen - afwerkingen op boven-, onder- en zijkanten van trappen/ hellingen en bordessen - terrazzoafwerkingen - betegelde - en natuursteenafwerkingen - houten trap-/ hellingafwerkingen - vloerbedekkingen op bordessen, trede-/ hellingen en stootbordbekledingen - trapneusprofielen - schilderwerken - randaansluitingsvoorzieningen - dilatatievoegconstructies/ - dekvloeren samengesteld uit zand/cement of synthetische stoffen"]
[null,"44.** trap- en hellingafwerkingen","b","Verzameling van afwerkingen van trappen/ hellingen en tussenbordessen, gerekend vanaf de trap-/ hellingconstructie."]
[null,"44.** trap- en hellingafwerkingen","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"44.** trap- en hellingafwerkingen","b"]
[null,"44.** trap- en hellingafwerkingen","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, breedte, dikte\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"Nee",{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"44.** trap- en hellingafwerkingen","b",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee",{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."},null,null,{"$f":"$V$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$W$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$X$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Y$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Z$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"}]
[null,"44.** trap- en hellingafwerkingen","b",null,"e","Afschot","-","-","-","-","-","-","-","-","-",null,null,"Nee",{"$f":"$S$1188","v":"ACP: Afschot"},{"$nulls":4},{"$f":"$X$1188","v":"ILS O&E BWK"},{"$f":"$Y$1188","v":"Afschot"},{"$f":"$Z$1188","v":"Afschot"}]
[null,"44.** trap- en hellingafwerkingen","b",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,"Nee","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"44.** trap- en hellingafwerkingen","b",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,"Nee","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"44.** trap- en hellingafwerkingen","b",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"44.** trap- en hellingafwerkingen","b"]
[null,"44.** trap- en hellingafwerkingen","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"Nee",{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"44.** trap- en hellingafwerkingen","b",null,"g","Entiteit","-","-","-","-","-","-","IfcPlate, IfcCovering, IfcWall","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcCovering"]
[null,"44.** trap- en hellingafwerkingen","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"44.** trap- en hellingafwerkingen","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"44.** trap- en hellingafwerkingen","b",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"44.** trap- en hellingafwerkingen","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"44.** trap- en hellingafwerkingen","b"]
[null,"44.** trap- en hellingafwerkingen","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"44.** trap- en hellingafwerkingen","b",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,"O&E 41*-47*-Afwerkingen(E)",{"$f":"$W$294","v":"(ifcElement)"},{"$f":"$X$294","v":"ILS O&E BWK"},{"$f":"$Y$294","v":"Afwerking / Behandeling"},{"$f":"$Z$294","v":"Afwerking/Behandeling (element), Afwerking/Behandeling (materiaal)"}]
[null,"44.** trap- en hellingafwerkingen","b",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,"O&E 41*-47*-Afwerkingen(E)",{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
[null,"44.** trap- en hellingafwerkingen","b",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_<entiteit>Common: Loadbearing","true/ false","-","Indien entiteit IfcCovering: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Pset_CoveringCommon",null,"Nee","Structural Function (instellingenvenster > Classifications and Properties)",null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},null,"ILS O&E BWK",{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[null,"44.** trap- en hellingafwerkingen","b",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-","Indien entiteit IfcCovering: benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset",null,"Nee",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$W$298","v":"ifc<Entiteit>"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[null,"44.** trap- en hellingafwerkingen","b",null,"p","Brandwerendheid","-","-","-","-","-","-","Pset_CoveringCommon:FireRating","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…"]
[null,"44.** trap- en hellingafwerkingen","b",null,"p","Brandwerende afwerking","-","-","-","-","-","-","-","-","-"]
[null,"44.** trap- en hellingafwerkingen","b",null,"p","Warmtedoorgangscoefficient","-","-","-","-","-","-","Pset_<entiteit>Common: ThermalTransmittance","U-waarde","W/ m².K","Warmteweerstand R = 1/ U\n\nIndien entiteit IfcCovering: benoemen in Custom Pset omdat 'ThermalTransmittance' geen deel uitmaakt van Common Pset in Ifc 2x3"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"44.** trap- en hellingafwerkingen","b"]
[null,"44.** trap- en hellingafwerkingen","b","Componenten","p","Randaansluitingsvoorzieningen","-","-","-","-","-","-","-","-","-"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","44.** trap- en hellingafwerkingen","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"44.** trap- en hellingafwerkingen","b"]
[]
[null,"45.** plafondafwerkingen","i","45.** - Plafondafwerkingen; verlaagd en niet verlaagd",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv. - isolerende, akoestische en brandwerende afwerkingen - randaansluitingsvoorzieningen - verticale plafondovergangen - plafondkoven en gordijnplanken - afwerkingen die één geheel vormen met de verlaagde plafondconstructie - schilderwerken - dilatatievoegconstructies/ - plafondbekledingen en plafondbetimmeringen - bepleisteringen - betegelingen - schilderafwerkingen - plafondkoven en gordijnplanken"]
[null,"45.** plafondafwerkingen","i","Verzameling van afwerkingen van de onderzijde van vloeren of daken met een verlaagde constructie, gerekend vanaf de bovenliggende vloer- of dakconstructie/ rechtstreeks op de vloer- of dakconstructie aangebracht, gerekend vanaf de bovenliggende vloerconstructie."]
[null,"45.** plafondafwerkingen","i",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"45.** plafondafwerkingen","i"]
[null,"45.** plafondafwerkingen","i","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, breedte, dikte, omtrek\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"Nee",{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"45.** plafondafwerkingen","i",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee",{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."},null,null,{"$f":"$V$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$W$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$X$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Y$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Z$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"}]
[null,"45.** plafondafwerkingen","i",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,"Nee","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"45.** plafondafwerkingen","i",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,"Nee","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"45.** plafondafwerkingen","i",null,"p","Stelruimte t.o.v. hoofddraagconstructie","-","-","-","-","-","-","-","-","-","Stelruimtes afstemmen per onderdeel, vastleggen in uitgangspunten/afsprakendocument"]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"45.** plafondafwerkingen","i"]
[null,"45.** plafondafwerkingen","i","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"Nee",{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"45.** plafondafwerkingen","i",null,"g","Entiteit","-","-","-","-","-","-","IfcCovering","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcCovering"]
[null,"45.** plafondafwerkingen","i",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"45.** plafondafwerkingen","i",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"45.** plafondafwerkingen","i",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"45.** plafondafwerkingen","i",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"45.** plafondafwerkingen","i"]
[null,"45.** plafondafwerkingen","i","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"45.** plafondafwerkingen","i",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,"O&E 41*-47*-Afwerkingen(E)",{"$f":"$W$294","v":"(ifcElement)"},{"$f":"$X$294","v":"ILS O&E BWK"},{"$f":"$Y$294","v":"Afwerking / Behandeling"},{"$f":"$Z$294","v":"Afwerking/Behandeling (element), Afwerking/Behandeling (materiaal)"}]
[null,"45.** plafondafwerkingen","i",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,"O&E 41*-47*-Afwerkingen(E)",{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
[null,"45.** plafondafwerkingen","i",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_PlateCommon: Loadbearing","true/ false","-","Indien entiteit IfcCovering: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Pset_CoveringCommon",null,"Nee","Structural Function (instellingenvenster > Classifications and Properties)",null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},"ifcPlate","Pset_PlateCommon",{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[null,"45.** plafondafwerkingen","i",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_PlateCommon: IsExternal","true/ false","-","Indien entiteit IfcCovering: benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset",null,"Nee",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$W$298","v":"ifc<Entiteit>"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
[null,"45.** plafondafwerkingen","i",null,"e","Luchtgeluidisolatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/inkoop/uitvoering.",null,"Nee","ACP: Geluidwering",null,null,"O&E 41*-47*-Afwerkingen (E)",{"$f":"$M$1281","v":"IfcCovering"},"Pset_<Eintiteit>Common","AcousticRating","Geluidwering"]
[null,"45.** plafondafwerkingen","i",null,"p","Brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating\n","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering. 0, 20, 30, 60, etc…"]
[null,"45.** plafondafwerkingen","i",null,"p","Warmtedoorgangscoefficient","-","-","-","-","-","-","Pset_PlateCommon: ThermalTransmittance","U-waarde","W/ m².K","U-waarde in W/ m².K\nwarmteweerstand R = 1/ U\n\nU-waarde overgang binnen- en/of buitenlucht toekennen aan element dat aan buiten- en/of binnenruimte grenst\nU-waarde niet gemodelleerde spouw toekennen aan één element in de scheidingsconstructie\n\nalternatief: U-waarde alleen toekennen aan het element in de scheidingsconstructie dat het meest bijdraagt aan de isolatiewaarde van de gehele scheidingsconstructie"]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"45.** plafondafwerkingen","i",{"$nulls":14},"x"]
[null,"45.** plafondafwerkingen","i","Componenten","e","Koofconstructies en gordijnplanken","-","-","-","-","-","-","-","-","-"]
[null,"45.** plafondafwerkingen","i",null,"p","Ophangconstructie","-","-","-","-","-","-","-","-","-","Ten behoeve van afstemming met installaties\nNoot: ter plaatse moeilijke knooppunten modelleren, ntb tijdens project;"]
[null,"45.** plafondafwerkingen","i",null,"p","Bouwfysische eis - brandwerendheid","-","-","-","-","-","-","Pset_<entiteit>Common:FireRating","WBDBO","minuten","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
[null,"45.** plafondafwerkingen","i",null,"p","Bouwfysische eis - luchtgeluidisoalatie","-","-","-","-","-","-","Pset_<entiteit>Common: AcousticRating","DnT,A,K","dB","3D-component (dummy wanden/vloeren/vlakken) welke grafisch de scheidingen aangeven m.b.t. de bouwfysische eis, aan dit element is de parameter gekoppeld met de eiswaarde. Uitvoering afstemmen in separaat uitgangspunten/afsprakendocument."]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","45.** plafondafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"45.** plafondafwerkingen","i"]
[]
[null,"47.** dakafwerkingen","i","47.** - Dakafwerkingen; afwerkingen en bekledingen",{"$nulls":11},"Inbegrepen in de definitie van deze code (begripsvorming, niet tbv modelleer technische eisen): \nBenodigde materialen, arbeid, materieel en hulpconstructies.\nBijv.: - dakbedekkingen van bitumen, kunststof en steenachtige materialen/ behorend bij het afwerkingspakket - gebouwisolatievoorzieningen - brandwerende voorzieningen - randaansluitingsvoorzieningen - panlatten - daktrimmen - dilatatievoegconstructies - looppaden"]
[null,"47.** dakafwerkingen","i","Verzameling van afwerkingen op de bovenzijde van horizontale en hellende daken en dakterrasafwerkingen, gerekend vanaf de (constructieve) dakvloeren/ dakterrassen, gerekend vanaf de dakafwerking.\n"]
[null,"47.** dakafwerkingen","i",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"47.** dakafwerkingen","i"]
[null,"47.** dakafwerkingen","i","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \noppervlakte, hoogte, omtrek\nNoot: maak een projectkeuze welke afwerkingen gemodelleerd worden en wat als eigenschap van een element/ ruimte wordt meegegeven.",null,"Nee",{"$f":"$S$63","v":"3D Model"},null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"47.** dakafwerkingen","i",null,"e","Sparingen","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee",{"$f":"$S$65","v":"Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'."},null,null,{"$f":"$V$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$W$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$X$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Y$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"},{"$f":"$Z$65","v":"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"}]
[null,"47.** dakafwerkingen","i",null,"e","Afschot","-","-","-","-","-","-","-","-","-",null,null,"Nee",{"$f":"$S$1188","v":"ACP: Afschot"},{"$nulls":4},{"$f":"$X$1188","v":"ILS O&E BWK"},{"$f":"$Y$1188","v":"Afschot"},{"$f":"$Z$1188","v":"Afschot"}]
[null,"47.** dakafwerkingen","i",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,"Nee","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"47.** dakafwerkingen","i",null,"e","Dilataties","-","-","-","-","-","-","-","-","-",null,null,"Nee","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"47.** dakafwerkingen","i",{"$nulls":14},"x"]
[null,"47.** dakafwerkingen","i","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"x",{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"47.** dakafwerkingen","i",null,"g","Entiteit","-","-","-","-","-","-","IfcSlab, IfcCovering","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcCovering"]
[null,"47.** dakafwerkingen","i",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"47.** dakafwerkingen","i",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"47.** dakafwerkingen","i",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"47.** dakafwerkingen","i"]
[null,"47.** dakafwerkingen","i","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"47.** dakafwerkingen","i",null,"e","Afwerking/ behandeling","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$294","v":"ACP: 'Afwerking / Behandeling (element)'\nACP: 'Afwerking / Behandeling (materiaal)'"},null,null,"O&E 41*-47*-Afwerkingen(E)",{"$f":"$W$294","v":"(ifcElement)"},{"$f":"$X$294","v":"ILS O&E BWK"},{"$f":"$Y$294","v":"Afwerking / Behandeling"},{"$f":"$Z$294","v":"Afwerking/Behandeling (element), Afwerking/Behandeling (materiaal)"}]
[null,"47.** dakafwerkingen","i",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"Nee","bespreken beste plan van aanpak. Ook ongeschreven regels benaming Psets…",null,null,"O&E 41*-47*-Afwerkingen(E)",{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
[null,"47.** dakafwerkingen","i",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_SlabCommon: Loadbearing","true/ false","-",null,null,"Nee","Structural Function (instellingenvenster > Classifications and Properties)",null,null,{"$f":"$V$123","v":"ILS 4.3-4 - Draagfunctie - Positie"},"ifcSlab","Pset_SlabCommon",{"$f":"$Y$86","v":"LoadBearing"},{"$f":"$Z$86","v":"True/False"}]
[null,"47.** dakafwerkingen","i",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_SlabCommon: IsExternal","true/ false","-",null,null,"Nee",{"$f":"$S$298","v":"Instellingenvenster > onder ID and Categories > Position"},null,null,{"$f":"$V$298","v":"ILS 4.3-4-Draagfunctie - Positie"},{"$f":"$W$298","v":"ifc<Entiteit>"},{"$f":"$X$298","v":"Pset_<entiteit>Common"},{"$f":"$Y$298","v":"isExternal"},{"$f":"$Z$298","v":"True/False"}]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"47.** dakafwerkingen","i"]
[null,"47.** dakafwerkingen","i","Componenten","p","Ondervloerconstructie","-","-","-","-","-","-","-","-","-","Ten behoeve van afstemming met installaties (bijvoorbeeld: pootjes computervloeren)\nNoot: ter plaatse moeilijke knooppunten modelleren, ntb tijdens project;"]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","47.** dakafwerkingen","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"47.** dakafwerkingen","i"]
[]
[null,"51.** warmte-opwekking","w","51.** - Warmte-opwekking",{"$nulls":15},"Installaties en onderliggende entiteiten","51.** - Warmte-opwekking"]
[null,"51.** warmte-opwekking","w","Verzameling van voorzieningen voor opwekken en ter beschikking stellen van warmte ten behoeve van klimaat en sanitair."]
[null,"51.** warmte-opwekking","w",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"51.** warmte-opwekking","w"]
[null,"51.** warmte-opwekking","w","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte, diameter",null,"Ja",{"$f":"$S$63","v":"3D Model"},null,null,{"$f":"$V$63","v":"n.v.t."},{"$f":"$W$63","v":"n.v.t."},{"$f":"$X$63","v":"n.v.t."},{"$f":"$Y$63","v":"n.v.t."},{"$f":"$Z$63","v":"n.v.t."}]
["x","51.** warmte-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","51.** warmte-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"51.** warmte-opwekking","w"]
[null,"51.** warmte-opwekking","w","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"Ja",{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"51.** warmte-opwekking","w",null,"g","Entiteit","-","-","-","-","-","-","IfcEnergyConversionDevice, IfcFlowTerminal, IfcFlowSegment, IfcFlowFitting, IfcBuildingElementProxy, IfcFlowStorageDevice, IfcFlowController, IfcCovering, IfcFlowMovingDevice","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcEnergyConversionDevice"]
[null,"51.** warmte-opwekking","w",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"51.** warmte-opwekking","w",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"51.** warmte-opwekking","w",null,"e","Systeemtype","-","-","-","-","-","-","System Type","-","-","Duidelijk onderscheid makend in de verschillende aanvoer en/of retour systemen ",null,"Nee","ACP: Systeemtype\nen / of\nObjectparameter: MEP Systeem",null,null,"ILS O&E - 5*-Installaties werktuigbouwkundig","IfcDistributionElement","ILS O&E BWK","Systeemtype","Ingevulde waarde\nen / of\nInstelling objectparameter"]
["x","51.** warmte-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","51.** warmte-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"51.** warmte-opwekking","w"]
[null,"51.** warmte-opwekking","w","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","51.** warmte-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","51.** warmte-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","51.** warmte-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","51.** warmte-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"51.** warmte-opwekking","w"]
[null,"51.** warmte-opwekking","w","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","51.** warmte-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"51.** warmte-opwekking","w"]
[]
[null,"52.** afvoeren","w","52.** - Afvoeren",{"$nulls":15},"Installaties en onderliggende entiteiten","52.** - Afvoeren"]
[null,"52.** afvoeren","w","Verzameling van voorzieningen voor afvoer opvang, zowel in als aan het gebouw, met de vaste ontvangstpunten."]
[null,"52.** afvoeren","w",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"52.** afvoeren","w"]
[null,"52.** afvoeren","w","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte, diameter",null,"Ja",{"$f":"$S$63","v":"3D Model"},null,null,{"$f":"$V$63","v":"n.v.t."},{"$f":"$W$63","v":"n.v.t."},{"$f":"$X$63","v":"n.v.t."},{"$f":"$Y$63","v":"n.v.t."},{"$f":"$Z$63","v":"n.v.t."}]
[null,"52.** afvoeren","w",null,"e","Afschot","-","-","-","-","-","-","-","-","-",null,null,"Nee","ACP: Afschot"]
["x","52.** afvoeren","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","52.** afvoeren","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"52.** afvoeren","w"]
[null,"52.** afvoeren","w","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,null,{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"52.** afvoeren","w",null,"g","Entiteit","-","-","-","-","-","-","IfcEnergyConversionDevice, IfcFlowTerminal, IfcFlowSegment, IfcFlowFitting, IfcBuildingElementProxy, IfcFlowController, IfcFlowMovingDevice","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcFlowSegment"]
[null,"52.** afvoeren","w",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"52.** afvoeren","w",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"52.** afvoeren","w",null,"e","Systeemtype","-","-","-","-","-","-","System Type","-","-","Duidelijk onderscheid makend in de verschillende systemen ",null,"Nee","ACP: Systeemtype\nen / of\nObjectparameter: MEP Systeem",null,null,"ILS O&E - 5*-Installaties werktuigbouwkundig","IfcDistributionElement","ILS O&E BWK","Systeemtype","Ingevulde waarde\nen / of\nInstelling objectparameter"]
["x","52.** afvoeren","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","52.** afvoeren","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"52.** afvoeren","w"]
[null,"52.** afvoeren","w","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","52.** afvoeren","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","52.** afvoeren","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","52.** afvoeren","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","52.** afvoeren","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"52.** afvoeren","w"]
[null,"52.** afvoeren","w","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","52.** afvoeren","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"52.** afvoeren","w"]
[]
[null,"53.** water","w","53.** - Water",{"$nulls":15},"Installaties en onderliggende entiteiten","53.** - Water"]
[null,"53.** water","w","Verzameling van voorzieningen voor transporteren van water, vanaf de hoofd- of dienstvoeding tot aan de verbruikspunten."]
[null,"53.** water","w",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"53.** water","w"]
[null,"53.** water","w","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte, diameter",null,"Ja",{"$f":"$S$63","v":"3D Model"},null,null,{"$f":"$V$63","v":"n.v.t."},{"$f":"$W$63","v":"n.v.t."},{"$f":"$X$63","v":"n.v.t."},{"$f":"$Y$63","v":"n.v.t."},{"$f":"$Z$63","v":"n.v.t."}]
["x","53.** water","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","53.** water","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"53.** water","w"]
[null,"53.** water","w","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"Ja",{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"53.** water","w",null,"g","Entiteit","-","-","-","-","-","-","IfcEnergyConversionDevice, IfcFlowSegment, IfcFlowFitting, IfcBuildingElementProxy, IfcFlowStorageDevice, IfcFlowController, IfcCovering, IfcFlowMovingDevice","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcFlowSegment, IfcFlowFitting, IfcFlowStorageDevice, IfcFlowController"]
[null,"53.** water","w",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"53.** water","w",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"53.** water","w",null,"e","Systeemtype","-","-","-","-","-","-","System Type","-","-","Duidelijk onderscheid makend in de verschillende systemen ",null,"Nee","ACP: Systeemtype\nen / of\nObjectparameter: MEP Systeem",null,null,"ILS O&E - 5*-Installaties werktuigbouwkundig","IfcDistributionElement","ILS O&E BWK","Systeemtype","Ingevulde waarde\nen / of\nInstelling objectparameter"]
["x","53.** water","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","53.** water","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"53.** water","w"]
[null,"53.** water","w","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","53.** water","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","53.** water","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","53.** water","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","53.** water","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"53.** water","w"]
[null,"53.** water","w","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","53.** water","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"53.** water","w"]
[]
[null,"54.** gassen","w","54.** - Gassen",{"$nulls":15},"Installaties en onderliggende entiteiten","54.** - Gassen"]
[null,"54.** gassen","w","Verzameling van voorzieningen voor aansluitingen, opslag, distributie en gebruik van gassen, vanaf de hoofdverdeling of de opslag tot een met de verbruiksaansluiting."]
[null,"54.** gassen","w",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"54.** gassen","w"]
[null,"54.** gassen","w","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte, diameter",null,"Ja",{"$f":"$S$63","v":"3D Model"},null,null,{"$f":"$V$63","v":"n.v.t."},{"$f":"$W$63","v":"n.v.t."},{"$f":"$X$63","v":"n.v.t."},{"$f":"$Y$63","v":"n.v.t."},{"$f":"$Z$63","v":"n.v.t."}]
["x","54.** gassen","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","54.** gassen","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"54.** gassen","w"]
[null,"54.** gassen","w","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"Ja"]
[null,"54.** gassen","w",null,"g","Entiteit","-","-","-","-","-","-","IfcFlowSegment, IfcFlowFitting, IfcBuildingElementProxy, IfcFlowStorageDevice, IfcFlowController, IfcFlowMovingDevice, IfcDistributionControlElement","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcFlowSegment, IfcFlowFitting, IfcFlowStorageDevice, IfcFlowController"]
[null,"54.** gassen","w",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"54.** gassen","w",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"54.** gassen","w",null,"e","Systeemtype","-","-","-","-","-","-","System Type","-","-","Duidelijk onderscheid makend in de verschillende systemen ",null,"Nee","ACP: Systeemtype\nen / of\nObjectparameter: MEP Systeem",null,null,"ILS O&E - 5*-Installaties werktuigbouwkundig","IfcDistributionElement","ILS O&E BWK","Systeemtype","Ingevulde waarde\nen / of\nInstelling objectparameter"]
["x","54.** gassen","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","54.** gassen","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"54.** gassen","w"]
[null,"54.** gassen","w","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","54.** gassen","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","54.** gassen","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","54.** gassen","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","54.** gassen","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"54.** gassen","w"]
[null,"54.** gassen","w","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","54.** gassen","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"54.** gassen","w"]
[]
[null,"55.** koude-opwekking","w","55.** - Koude-opwekking",{"$nulls":15},"Installaties en onderliggende entiteiten","55.** - Koude-opwekking"]
[null,"55.** koude-opwekking","w","Verzameling van voorzieningen voor lokaal opwekken en afgeven van koude voor het onderhouden van een behaaglijkheids- en conserveringsklimaat"]
[null,"55.** koude-opwekking","w",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"55.** koude-opwekking","w"]
[null,"55.** koude-opwekking","w","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte, diameter",null,"Ja",{"$f":"$S$63","v":"3D Model"},null,null,{"$f":"$V$63","v":"n.v.t."},{"$f":"$W$63","v":"n.v.t."},{"$f":"$X$63","v":"n.v.t."},{"$f":"$Y$63","v":"n.v.t."},{"$f":"$Z$63","v":"n.v.t."}]
["x","55.** koude-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","55.** koude-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"55.** koude-opwekking","w"]
[null,"55.** koude-opwekking","w","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"Ja",{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"55.** koude-opwekking","w",null,"g","Entiteit","-","-","-","-","-","-","IfcEnergyConversionDevice, IfcFlowSegment, IfcFlowFitting, IfcBuildingElementProxy, IfcFlowStorageDevice, IfcFlowController, IfcCovering, IfcDistributionControlElement","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcChiller, IfcFlowSegment, IfcFlowFitting, IfcFlowStorageDevice, IfcFlowController"]
[null,"55.** koude-opwekking","w",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"55.** koude-opwekking","w",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"55.** koude-opwekking","w",null,"e","Systeemtype","-","-","-","-","-","-","System Type","-","-","Duidelijk onderscheid makend in de verschillende systemen ",null,"Nee","ACP: Systeemtype\nen / of\nObjectparameter: MEP Systeem",null,null,"ILS O&E - 5*-Installaties werktuigbouwkundig","IfcDistributionElement","ILS O&E BWK","Systeemtype","Ingevulde waarde\nen / of\nInstelling objectparameter"]
["x","55.** koude-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","55.** koude-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"55.** koude-opwekking","w"]
[null,"55.** koude-opwekking","w","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","55.** koude-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","55.** koude-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","55.** koude-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","55.** koude-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"55.** koude-opwekking","w"]
[null,"55.** koude-opwekking","w","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","55.** koude-opwekking","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"55.** koude-opwekking","w"]
[]
[null,"56.** warmtedistributie","w","56.** - Warmtedistributie",{"$nulls":15},"Installaties en onderliggende entiteiten","56.** - Warmtedistributie"]
[null,"56.** warmtedistributie","w","Verzameling van voorzieningen voor transport, verdeling en afgifte van warmte met als medium water voor het klimaat, vanaf de hoofdverdeling van de warmte-opwekking tot en met de warmteafgifte- eenheden in ruimten."]
[null,"56.** warmtedistributie","w",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"56.** warmtedistributie","w"]
[null,"56.** warmtedistributie","w","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte, diameter",null,"Ja",{"$f":"$S$63","v":"3D Model"},null,null,{"$f":"$V$63","v":"n.v.t."},{"$f":"$W$63","v":"n.v.t."},{"$f":"$X$63","v":"n.v.t."},{"$f":"$Y$63","v":"n.v.t."},{"$f":"$Z$63","v":"n.v.t."}]
["x","56.** warmtedistributie","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","56.** warmtedistributie","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"56.** warmtedistributie","w"]
[null,"56.** warmtedistributie","w","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"Ja",{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"56.** warmtedistributie","w",null,"g","Entiteit","-","-","-","-","-","-","IfcEnergyConversionDevice, IfcFlowSegment, IfcFlowFitting, IfcBuildingElementProxy, IfcFlowController, IfcCovering, IfcFlowMovingDevice, IfcFlowTerminal, IfcTeatmentDevice, IfcFlowTreatmentDevice","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcBoiler, IfcEnergyConversionDevice,IfcFlowSegment, IfcFlowFitting, IfcFlowStorageDevice, IfcFlowController"]
[null,"56.** warmtedistributie","w",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"56.** warmtedistributie","w",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"56.** warmtedistributie","w",null,"e","Systeemtype","-","-","-","-","-","-","System Type","-","-","Duidelijk onderscheid makend in de verschillende systemen ",null,"Nee","ACP: Systeemtype\nen / of\nObjectparameter: MEP Systeem",null,null,"ILS O&E - 5*-Installaties werktuigbouwkundig","IfcDistributionElement","ILS O&E BWK","Systeemtype","Ingevulde waarde\nen / of\nInstelling objectparameter"]
["x","56.** warmtedistributie","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","56.** warmtedistributie","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"56.** warmtedistributie","w"]
[null,"56.** warmtedistributie","w","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","56.** warmtedistributie","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","56.** warmtedistributie","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","56.** warmtedistributie","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","56.** warmtedistributie","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"56.** warmtedistributie","w"]
[null,"56.** warmtedistributie","w","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","56.** warmtedistributie","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"56.** warmtedistributie","w"]
[]
[null,"57.** luchtbehandeling","w","57.** - Luchtbehandeling",{"$nulls":15},"Installaties en onderliggende entiteiten","57.** - Luchtbehandeling"]
[null,"57.** luchtbehandeling","w","Verzameling van voorzieningen voor mechanische ventilatie door toevoer en afvoer van lucht voor het klimaat."]
[null,"57.** luchtbehandeling","w",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"57.** luchtbehandeling","w"]
[null,"57.** luchtbehandeling","w","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte, diameter",null,"Ja",{"$f":"$S$63","v":"3D Model"},null,null,{"$f":"$V$63","v":"n.v.t."},{"$f":"$W$63","v":"n.v.t."},{"$f":"$X$63","v":"n.v.t."},{"$f":"$Y$63","v":"n.v.t."},{"$f":"$Z$63","v":"n.v.t."}]
["x","57.** luchtbehandeling","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","57.** luchtbehandeling","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"57.** luchtbehandeling","w"]
[null,"57.** luchtbehandeling","w","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"Ja",{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"57.** luchtbehandeling","w",null,"g","Entiteit","-","-","-","-","-","-","IfcEnergyConversionDevice, IfcFlowSegment, IfcFlowFitting, IfcBuildingElementProxy, IfcFlowController, IfcCovering, IfcFlowMovingDevice, IfcFlowTerminal, IfcTeatmentDevice, IfcFlowTreatmentDevice","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcEnergyConversionDevice, IfcFlowSegment, IfcFlowFitting,  IfcFlowController,  , IfcFlowTerminal, IfcTeatmentDevice, IfcFlowTreatmentDevice"]
[null,"57.** luchtbehandeling","w",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"57.** luchtbehandeling","w",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"57.** luchtbehandeling","w",null,"e","Systeemtype","-","-","-","-","-","-","System Type","-","-","Duidelijk onderscheid makend in de verschillende toevoer en/of retour en of afzuig systemen ",null,"Nee","ACP: Systeemtype\nen / of\nObjectparameter: MEP Systeem",null,null,"ILS O&E - 5*-Installaties werktuigbouwkundig","IfcDistributionElement","ILS O&E BWK","Systeemtype","Ingevulde waarde\nen / of\nInstelling objectparameter"]
["x","57.** luchtbehandeling","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","57.** luchtbehandeling","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"57.** luchtbehandeling","w"]
[null,"57.** luchtbehandeling","w","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","57.** luchtbehandeling","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","57.** luchtbehandeling","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","57.** luchtbehandeling","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","57.** luchtbehandeling","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"57.** luchtbehandeling","w"]
[null,"57.** luchtbehandeling","w","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","57.** luchtbehandeling","w",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"57.** luchtbehandeling","w"]
[]
[null,"58.** regeling klimaat en sanitair","e","58.** - Regeling klimaat en sanitair",{"$nulls":15},"Installaties en onderliggende entiteiten","58.** - Regeling klimaat en sanitair"]
[null,"58.** regeling klimaat en sanitair","e","Verzameling van voorzieningen voor melden, meten, en sturen van regelinstallaties voor klimaat sanitair, vanaf aan te sluiten hoofdvoeding tot en met de aan te sluiten regelingen."]
[null,"58.** regeling klimaat en sanitair","e",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"58.** regeling klimaat en sanitair","e"]
[null,"58.** regeling klimaat en sanitair","e","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nhoogte, breedte, dikte",null,"Ja","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"58.** regeling klimaat en sanitair","e",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,"Ja","3D Model"]
["x","58.** regeling klimaat en sanitair","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","58.** regeling klimaat en sanitair","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"58.** regeling klimaat en sanitair","e"]
[null,"58.** regeling klimaat en sanitair","e","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"Ja",{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"58.** regeling klimaat en sanitair","e",null,"g","Entiteit","-","-","-","-","-","-","IfcDistributionControlElement, IfcFlowController, IfcDistributionElement, IfcFlowTerminal, IfcFlowSegment, IfcFlowFitting","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcEnergyConversionDevice, IfcFlowSegment, IfcFlowFitting,  IfcFlowController,  , IfcFlowTerminal, IfcTeatmentDevice, IfcFlowTreatmentDevice"]
[null,"58.** regeling klimaat en sanitair","e",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"58.** regeling klimaat en sanitair","e",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
["x","58.** regeling klimaat en sanitair","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","58.** regeling klimaat en sanitair","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"58.** regeling klimaat en sanitair","e"]
[null,"58.** regeling klimaat en sanitair","e","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","58.** regeling klimaat en sanitair","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","58.** regeling klimaat en sanitair","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","58.** regeling klimaat en sanitair","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","58.** regeling klimaat en sanitair","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"58.** regeling klimaat en sanitair","e"]
[null,"58.** regeling klimaat en sanitair","e","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","58.** regeling klimaat en sanitair","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"58.** regeling klimaat en sanitair","e"]
[]
[null,"61.** centrale elektrotechnische voorzieningen","e","61.** - Centrale elektrotechnische voorzieningen",{"$nulls":15},"Installaties en onderliggende entiteiten","61.** - Centrale elektrotechnische voorzieningen"]
[null,"61.** centrale elektrotechnische voorzieningen","e","Verzameling van centrale elektrotechnische voorzieningen ten behoeve van energie, noodstroom, aarding, kanalisatie, hoogspanning, laagspanning, zeer lage spanning en bliksemafleiding."]
[null,"61.** centrale elektrotechnische voorzieningen","e",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"61.** centrale elektrotechnische voorzieningen","e"]
[null,"61.** centrale elektrotechnische voorzieningen","e","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: lengte, hoogte, breedte",null,"Ja",{"$f":"$S$63","v":"3D Model"},null,null,{"$f":"$V$63","v":"n.v.t."},{"$f":"$W$63","v":"n.v.t."},{"$f":"$X$63","v":"n.v.t."},{"$f":"$Y$63","v":"n.v.t."},{"$f":"$Z$63","v":"n.v.t."}]
["x","61.** centrale elektrotechnische voorzieningen","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","61.** centrale elektrotechnische voorzieningen","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"61.** centrale elektrotechnische voorzieningen","e"]
[null,"61.** centrale elektrotechnische voorzieningen","e","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"Ja",{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"61.** centrale elektrotechnische voorzieningen","e",null,"g","Entiteit","-","-","-","-","-","-","IfcEnergyConversionDevice, IfcBuildingElementProxy, IfcFlowController, IfcFlowSegment, IfcFlowFitting, IfcDistributionElement","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."}]
[null,"61.** centrale elektrotechnische voorzieningen","e",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"61.** centrale elektrotechnische voorzieningen","e",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"61.** centrale elektrotechnische voorzieningen","e",null,"e","Groepsnaam/nummer","-","-","-","-","-","-",null,"-","-","Opvolgend benaming en/of codering waar het element aan is verbonden.",null,"Nee","ACP: Groepsnaam/nummer",null,null,"O&E 6*-Installaties elektrotechnisch","IfcDistributionElement","ILS O&E BWK","Groepsnaam / nummer","<Ingevulde tekst>"]
[null,"61.** centrale elektrotechnische voorzieningen","e",null,"e","Groepenkast naam/nummer","-","-","-","-","-","-",null,"-","-","Korte benaming en/of codering waar het element aan is verbonden.",null,"Nee","ACP: Groepenkast naam/nummer",null,null,"O&E 6*-Installaties elektrotechnisch","IfcDistributionElement","ILS O&E BWK","Groepenkast naam / nummer","<Ingevulde tekst>"]
["x","61.** centrale elektrotechnische voorzieningen","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","61.** centrale elektrotechnische voorzieningen","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"61.** centrale elektrotechnische voorzieningen","e"]
[null,"61.** centrale elektrotechnische voorzieningen","e","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","61.** centrale elektrotechnische voorzieningen","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","61.** centrale elektrotechnische voorzieningen","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","61.** centrale elektrotechnische voorzieningen","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","61.** centrale elektrotechnische voorzieningen","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"61.** centrale elektrotechnische voorzieningen","e"]
[null,"61.** centrale elektrotechnische voorzieningen","e","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","61.** centrale elektrotechnische voorzieningen","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"61.** centrale elektrotechnische voorzieningen","e"]
[]
[null,"62.** krachtstroom","e","62.** - Krachtstroom",{"$nulls":15},"Installaties en onderliggende entiteiten","62.** - Krachtstroom"]
[null,"62.** krachtstroom","e","Verzameling van voorzieningen lager dan 1Kv vanaf de hoofdverdelers tot aan de verbruikers. "]
[null,"62.** krachtstroom","e",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"62.** krachtstroom","e"]
[null,"62.** krachtstroom","e","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: lengte, hoogte, breedte",null,"Ja",{"$f":"$S$63","v":"3D Model"},null,null,{"$f":"$V$63","v":"n.v.t."},{"$f":"$W$63","v":"n.v.t."},{"$f":"$X$63","v":"n.v.t."},{"$f":"$Y$63","v":"n.v.t."},{"$f":"$Z$63","v":"n.v.t."}]
["x","62.** krachtstroom","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","62.** krachtstroom","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"62.** krachtstroom","e"]
[null,"62.** krachtstroom","e","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"Ja",{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"62.** krachtstroom","e",null,"g","Entiteit","-","-","-","-","-","-","IfcEnergyConversionDevice, IfcBuildingElementProxy, IfcFlowController, IfcFlowSegment, IfcFlowTerminal","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."}]
[null,"62.** krachtstroom","e",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"62.** krachtstroom","e",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"62.** krachtstroom","e",null,"e","Groepsnaam/nummer","-","-","-","-","-","-",null,"-","-","Opvolgend benaming en/of codering waar het element aan is verbonden.",null,"Nee","ACP: Groepsnaam/nummer",null,null,"O&E 6*-Installaties elektrotechnisch","IfcDistributionElement","ILS O&E BWK","Groepsnaam / nummer","<Ingevulde tekst>"]
[null,"62.** krachtstroom","e",null,"e","Groepenkast naam/nummer","-","-","-","-","-","-",null,"-","-","Korte benaming en/of codering waar het element aan is verbonden.",null,"Nee","ACP: Groepenkast naam/nummer",null,null,"O&E 6*-Installaties elektrotechnisch","IfcDistributionElement","ILS O&E BWK","Groepenkast naam / nummer","<Ingevulde tekst>"]
["x","62.** krachtstroom","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","62.** krachtstroom","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"62.** krachtstroom","e"]
[null,"62.** krachtstroom","e","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","62.** krachtstroom","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","62.** krachtstroom","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","62.** krachtstroom","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","62.** krachtstroom","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"62.** krachtstroom","e"]
[null,"62.** krachtstroom","e","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","62.** krachtstroom","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"62.** krachtstroom","e"]
[]
[null,"63.** verlichting","e","63.** - Verlichting",{"$nulls":15},"Installaties en onderliggende entiteiten","63.** - Verlichting"]
[null,"63.** verlichting","e","Verzameling van voorzieningen lager dan 1Kv vanaf de hoofdverdelers tot aan de verbruikers. "]
[null,"63.** verlichting","e",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"63.** verlichting","e"]
[null,"63.** verlichting","e","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte",null,"Ja",{"$f":"$S$63","v":"3D Model"},null,null,{"$f":"$V$63","v":"n.v.t."},{"$f":"$W$63","v":"n.v.t."},{"$f":"$X$63","v":"n.v.t."},{"$f":"$Y$63","v":"n.v.t."},{"$f":"$Z$63","v":"n.v.t."}]
[null,"63.** verlichting","e",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,"Ja","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
["x","63.** verlichting","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","63.** verlichting","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"63.** verlichting","e"]
[null,"63.** verlichting","e","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"Ja",{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"63.** verlichting","e",null,"g","Entiteit","-","-","-","-","-","-","IfcBuildingElementProxy, IfcFlowController, IfcFlowSegment, IfcFlowTerminal","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."}]
[null,"63.** verlichting","e",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"63.** verlichting","e",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"63.** verlichting","e",null,"e","Groepsnaam/nummer","-","-","-","-","-","-",null,"-","-","Opvolgend benaming en/of codering waar het element aan is verbonden.",null,"Nee","ACP: Groepsnaam/nummer",null,null,"O&E 6*-Installaties elektrotechnisch","IfcDistributionElement","ILS O&E BWK","Groepsnaam / nummer","<Ingevulde tekst>"]
[null,"63.** verlichting","e",null,"e","Groepenkast naam/nummer","-","-","-","-","-","-",null,"-","-","Korte benaming en/of codering waar het element aan is verbonden.",null,"Nee","ACP: Groepenkast naam/nummer",null,null,"O&E 6*-Installaties elektrotechnisch","IfcDistributionElement","ILS O&E BWK","Groepenkast naam / nummer","<Ingevulde tekst>"]
["x","63.** verlichting","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","63.** verlichting","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"63.** verlichting","e"]
[null,"63.** verlichting","e","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","63.** verlichting","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","63.** verlichting","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","63.** verlichting","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","63.** verlichting","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"63.** verlichting","e"]
[null,"63.** verlichting","e","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","63.** verlichting","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"63.** verlichting","e"]
[]
[null,"64.** communicatie","e","64.** - Communicatie",{"$nulls":15},"Installaties en onderliggende entiteiten","64.** - Communicatie"]
[null,"64.** communicatie","e","Verzameling van voorzieningen voor informatieoverdracht door middel van signalen, geluiden, beelden, data en de combinatie tussen allen. "]
[null,"64.** communicatie","e",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"64.** communicatie","e"]
[null,"64.** communicatie","e","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte, …",null,"Ja",{"$f":"$S$63","v":"3D Model"},null,null,{"$f":"$V$63","v":"n.v.t."},{"$f":"$W$63","v":"n.v.t."},{"$f":"$X$63","v":"n.v.t."},{"$f":"$Y$63","v":"n.v.t."},{"$f":"$Z$63","v":"n.v.t."}]
["x","64.** communicatie","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","64.** communicatie","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"64.** communicatie","e"]
[null,"64.** communicatie","e","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"Ja",{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"64.** communicatie","e",null,"g","Entiteit","-","-","-","-","-","-","IfcBuildingElementProxy, IfcFlowStorageDevice, IfcFlowSegment, IfcFlowTerminal, IfcFlowController","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."}]
[null,"64.** communicatie","e",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"64.** communicatie","e",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"64.** communicatie","e",null,"e","Groepsnaam/nummer","-","-","-","-","-","-",null,"-","-","Opvolgend benaming en/of codering waar het element aan is verbonden.",null,"Nee","ACP: Groepsnaam/nummer",null,null,"O&E 6*-Installaties elektrotechnisch","IfcDistributionElement","ILS O&E BWK","Groepsnaam / nummer","<Ingevulde tekst>"]
[null,"64.** communicatie","e",null,"e","Groepenkast naam/nummer","-","-","-","-","-","-",null,"-","-","Korte benaming en/of codering waar het element aan is verbonden.",null,"Nee","ACP: Groepenkast naam/nummer",null,null,"O&E 6*-Installaties elektrotechnisch","IfcDistributionElement","ILS O&E BWK","Groepenkast naam / nummer","<Ingevulde tekst>"]
["x","64.** communicatie","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","64.** communicatie","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"64.** communicatie","e"]
[null,"64.** communicatie","e","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","64.** communicatie","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","64.** communicatie","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","64.** communicatie","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","64.** communicatie","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"64.** communicatie","e"]
[null,"64.** communicatie","e","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","64.** communicatie","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"64.** communicatie","e"]
[]
[null,"65.** beveiliging","e","65.** - Beveiliging",{"$nulls":15},"Installaties en onderliggende entiteiten","65.** - Beveiliging"]
[null,"65.** beveiliging","e","Verzameling van voorzieningen voor het voorkomen, melden, beperken en bestrijden van brand, inbraak en uitbraak, overlast, sociale noden van personen en dieren, milieua-overlast, etc. "]
[null,"65.** beveiliging","e",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"65.** beveiliging","e"]
[null,"65.** beveiliging","e","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte, …",null,"Ja",{"$f":"$S$63","v":"3D Model"},null,null,{"$f":"$V$63","v":"n.v.t."},{"$f":"$W$63","v":"n.v.t."},{"$f":"$X$63","v":"n.v.t."},{"$f":"$Y$63","v":"n.v.t."},{"$f":"$Z$63","v":"n.v.t."}]
["x","65.** beveiliging","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","65.** beveiliging","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"65.** beveiliging","e"]
[null,"65.** beveiliging","e","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,"Ja",{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"65.** beveiliging","e",null,"g","Entiteit","-","-","-","-","-","-","IfcBuildingElementProxy, IfcFlowStorageDevice, IfcFlowSegment, IfcFlowTerminal, IfcFlowController, IfcDistributionControlElement, IfcFlowFitting","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."}]
[null,"65.** beveiliging","e",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"65.** beveiliging","e",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"65.** beveiliging","e",null,"e","Groepsnaam/nummer","-","-","-","-","-","-",null,"-","-","Opvolgend benaming en/of codering waar het element aan is verbonden.",null,"Nee","ACP: Groepsnaam/nummer",null,null,"O&E 6*-Installaties elektrotechnisch","IfcDistributionElement","ILS O&E BWK","Groepsnaam / nummer","<Ingevulde tekst>"]
[null,"65.** beveiliging","e",null,"e","Groepenkast naam/nummer","-","-","-","-","-","-",null,"-","-","Korte benaming en/of codering waar het element aan is verbonden.",null,"Nee","ACP: Groepenkast naam/nummer",null,null,"O&E 6*-Installaties elektrotechnisch","IfcDistributionElement","ILS O&E BWK","Groepenkast naam / nummer","<Ingevulde tekst>"]
["x","65.** beveiliging","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","65.** beveiliging","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"65.** beveiliging","e"]
[null,"65.** beveiliging","e","Eigenschappen","p",null,"-","-","-","-","-","-","-","-","-"]
["x","65.** beveiliging","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","65.** beveiliging","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","65.** beveiliging","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","65.** beveiliging","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"65.** beveiliging","e"]
[null,"65.** beveiliging","e","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","65.** beveiliging","e",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"65.** beveiliging","e"]
[]
[null,"66.** transport","b","66.** - Transport",{"$nulls":15},"Transportvoorzieningen en onderliggende entiteiten","66.** - Transport"]
[null,"66.** transport","b","Verzameling van voorzieningen voor het verticale en horizontale transport van personen en goederen door middel van liften en roltrappen\nNoot: Elementkaart is geconcentreerd op de bouwkundige gegevensbehoefte en esthetische verschijningsvorm binnen het prestatiemodel. Deze keuze is gemaakt vanwege de realisatie van liften/ roltrappen en daarin de rol van de liftleverancier en de installateur."]
[null,"66.** transport","b",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"66.** transport","b"]
[null,"66.** transport","b","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,{"$f":"$V$63","v":"n.v.t."},{"$f":"$W$63","v":"n.v.t."},{"$f":"$X$63","v":"n.v.t."},{"$f":"$Y$63","v":"n.v.t."},{"$f":"$Z$63","v":"n.v.t."}]
[null,"66.** transport","b",null,"e","Ruimtebeslag tbv onderhoud","-","-","-","-","-","-","-","-","-",null,null,"Nee","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"66.** transport","b",null,"e","Vlakverdeling/ invullingen","-","-","-","-","-","-","-","-","-",null,null,"Nee","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"66.** transport","b"]
[null,"66.** transport","b","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"66.** transport","b",null,"g","Entiteit","-","-","-","-","-","-","IfcTransportElement, IfcBuildingElementProxy, IfcFlowSegment, IfcFlowFitting, IfcFlowMovingDevice, IfcFlowTerminal","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcTransportElement,"]
[null,"66.** transport","b",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"66.** transport","b",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"66.** transport","b",null,"p","Liftnummer","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelLabel","-","-","Uniek nummer per lift"]
[null,"66.** transport","b",null,"p","Systeemtype","-","-","-","-","-","-","System Type","-","-","In overleg met leverancier"]
[null,"66.** transport","b",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"66.** transport","b",null,"p","Merk","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelReference","-","-","Ten behoeve van onderhoud"]
[null,"66.** transport","b",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"66.** transport","b"]
[null,"66.** transport","b","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"66.** transport","b",null,"e","In/ uitwendig","-","-","-","-","-","-","IsExternal benoemen in custom Pset","true/ false","-","Benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Pset_SpaceCommon in Ifc 2x3",null,"Ja","Position (instellingenvenster > Classifications and Properties)",null,null,"ILS 4.3-4 - Draagfunctie - Positie","ifcTransportElement, ifcFlowSegment, ifcFlowFitting, ifcFlowMovingDevice, ifcFlowTerminal","ILS O&E BWK","IsExternal","True/False"]
[null,"66.** transport","b",null,"e","Brandwerendheid","-","-","-","-","-","-","FireRating benoemen in custom Pset","WBDBO","minuten","Gekozen waarde voor gehele component op basis van bouwfysisch advies. Dit is de waarde welke gebruikt gaat worden t.b.v. aansturing inkoop/uitvoering., volgens separaat afsprakendocument. 0, 20, 30, 60, etc... (WBDBO)(bij elementen ter plaatse doorgang brandwerend element)\n\nbenoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset voor meest geëigende entiteiten",null,"Nee","ifcBuildingElementProxy ok, aan te maken voor overige eniteiten",null,null,"O&E 66*-Transport","ifcTransportElement, ifcFlowSegment, ifcFlowFitting, ifcFlowMovingDevice, ifcFlowTerminal","Pset_<Entiteit>Common","FireRating","WBDBO"]
[null,"66.** transport","b",null,"p","Capaciteit (aantal personen)","-","-","-","-","-","-","-","-"]
[null,"66.** transport","b",null,"p","Vluchtdeur","-","-","-","-","-","-","Pset_TransportElementCommon: FireExit","true/ false","-","Indien entiteit IfcBuildingElementProxy, IfcFlowSegment, IfcFlowFitting, IfcFlowMovingDevice, IfcFlowTerminal: benoemen in Custom Pset omdat 'FireExit' geen deel uitmaakt van Common Pset"]
[null,"66.** transport","b",null,"p","Groepnaam/nummer","-","-","-","-","-","-","-","-","-","In overleg met Installateur"]
[null,"66.** transport","b",null,"p","Groepkast naam/ nummer","-","-","-","-","-","-","-","-","-","In overleg met Installateur"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"66.** transport","b"]
[null,"66.** transport","b","Componenten","e","Sparingsopgave","-","-","-","-","-","-","-","-","-","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument",null,"Nee","Zie Helpcenter artikel 'Sparingen conform Uniforme Sparings Opgave in een model'.",null,null,"Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument","Zelf op te stellen sparingsprocedure, vastleggen in spearaat afsprakendocument"]
[null,"66.** transport","b",null,"e","Bediening","-","-","-","-","-","-","-","-","-","Twin, Tripple, etc",null,"Nee","ACP: Bediening",null,null,"O&E - 66*-Transport","IfcTransportElement","ILS O&E BWK","Bediening","<Ingevulde tekst>"]
[null,"66.** transport","b",null,"e","Verankering en bevestiging","-","-","-","-","-","-","-","-","-","Niet modelleren, wel terug laten komen in details"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","66.** transport","b",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"66.** transport","b"]
[]
[null,"7*.** vaste inventaris","i","7*.** - Vaste inventaris",{"$nulls":15},"Inrichting en onderliggende entiteiten","7*.** - Vaste inventaris"]
[null,"7*.** vaste inventaris","i","Onder vaste inventaris vallen; verkeersvoorzieningen, gebruikersvoorzieningen keukenvoorzieningen, sanitaire voorzieningen, schoonmaakvoorzieningen en opslagvoorzieningen\nNoot: Elementkaart is geconcentreerd op de bouwkundige gegevensbehoefte en esthetische verschijningsvorm binnen het prestatiemodel. "]
[null,"7*.** vaste inventaris","i",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"7*.** vaste inventaris","i"]
[null,"7*.** vaste inventaris","i","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte",null,"x",{"$f":"$S$63","v":"3D Model"},null,null,{"$f":"$V$63","v":"n.v.t."},{"$f":"$W$63","v":"n.v.t."},{"$f":"$X$63","v":"n.v.t."},{"$f":"$Y$63","v":"n.v.t."},{"$f":"$Z$63","v":"n.v.t."}]
[null,"7*.** vaste inventaris","i",null,"e","Vlakverdeling/ invullingen","-","-","-","-","-","-","-","-","-",null,null,"x","3D Model",null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"7*.** vaste inventaris","i"]
[null,"7*.** vaste inventaris","i","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"7*.** vaste inventaris","i",null,"g","Entiteit","-","-","-","-","-","-","IfcFurnishingElement, IfcBuildingElementProxy, IfcFlowTerminal, IfcStair, IfcStairFlight, IfcRailing, IfcSlab","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcFurnishingElement"]
[null,"7*.** vaste inventaris","i",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"7*.** vaste inventaris","i",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"7*.** vaste inventaris","i",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"7*.** vaste inventaris","i",null,"p","Merk","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelReference","-","-","Ten behoeve van onderhoud"]
[null,"7*.** vaste inventaris","i",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"7*.** vaste inventaris","i"]
[null,"7*.** vaste inventaris","i","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"7*.** vaste inventaris","i",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"Nee","ACP: Kleur",null,null,null,{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
[null,"7*.** vaste inventaris","i",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","Pset_SlabCommon: Loadbearing","true/ false","-","Indien entiteit IfcFurnishingElement, IfcBuildingElementProxy, IfcFlowTerminal, IfcStair, IfcStairFlight, IfcRailing: benoemen in Custom Pset omdat 'Loadbearing' geen deel uitmaakt van Common Pset",{"$nulls":5},"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"7*.** vaste inventaris","i",null,"e","In/ uitwendig","-","-","-","-","-","-","Pset_<entiteit>Common: IsExternal","true/ false","-","Indien entiteit IfcFurnishingElement, IfcBuildingElementProxy, IfcFlowTerminal, IfcStairFlight: benoemen in Custom Pset omdat 'IsExternal' geen deel uitmaakt van Common Pset",{"$nulls":5},"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"7*.** vaste inventaris","i"]
[null,"7*.** vaste inventaris","i","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","7*.** vaste inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"7*.** vaste inventaris","i"]
[]
[null,"8*.** losse inventaris","i","8*.** - Losse inventaris",{"$nulls":15},"Inrichting en onderliggende entiteiten","8*.** - Losse inventaris"]
[null,"8*.** losse inventaris","i","Onder losse inventaris vallen; verkeersinventaris, gebruikersinventaris, keukeninventaris, sanitaire inventaris, schoonmaakinventaris.\nNoot: Elementkaart is geconcentreerd op de bouwkundige gegevensbehoefte en esthetische verschijningsvorm binnen het prestatiemodel. "]
[null,"8*.** losse inventaris","i",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"8*.** losse inventaris","i"]
[null,"8*.** losse inventaris","i","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,{"$f":"$V$63","v":"n.v.t."},{"$f":"$W$63","v":"n.v.t."},{"$f":"$X$63","v":"n.v.t."},{"$f":"$Y$63","v":"n.v.t."},{"$f":"$Z$63","v":"n.v.t."}]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"8*.** losse inventaris","i"]
[null,"8*.** losse inventaris","i","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"8*.** losse inventaris","i",null,"g","Entiteit","-","-","-","-","-","-","IfcFurnishingElement, IfcBuildingElementProxy, IfcFlowTerminal","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcFurnishingElement"]
[null,"8*.** losse inventaris","i",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"8*.** losse inventaris","i",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"8*.** losse inventaris","i",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"8*.** losse inventaris","i",null,"p","Merk","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelReference","-","-","Ten behoeve van onderhoud"]
[null,"8*.** losse inventaris","i",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"8*.** losse inventaris","i"]
[null,"8*.** losse inventaris","i","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"8*.** losse inventaris","i",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"Nee","ACP: Kleur",null,null,null,{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"8*.** losse inventaris","i"]
[null,"8*.** losse inventaris","i","Componenten","p",null,"-","-","-","-","-","-","-","-","-"]
["x","8*.** losse inventaris","i",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"8*.** losse inventaris","i"]
[]
[null,"90.** terrein","t","90.** - Terrein",{"$nulls":15},"Terrein","90.** - Terrein"]
[null,"90.** terrein","t","Onder terrein vallen grondvoorziening, opstallen, omheiningen en  terreinafwerkingen."]
[null,"90.** terrein","t",null,null,"Parameter","SO","VO","DO","TO","UO","AS-B","IFC datadrager","Invulwaarde","Eenheid","Opmerking"]
[null,"90.** terrein","t"]
[null,"90.** terrein","t","Geometrie","g","Vorm buitenste contouren","-","-","-","-","-","-","-","-","-","Uit vorm moet het volgende bepaald kunnen worden: \nlengte, hoogte, breedte",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$63","v":"3D Model"},null,null,{"$f":"$V$63","v":"n.v.t."},{"$f":"$W$63","v":"n.v.t."},{"$f":"$X$63","v":"n.v.t."},{"$f":"$Y$63","v":"n.v.t."},{"$f":"$Z$63","v":"n.v.t."}]
[null,"90.** terrein","t",null,"e","Vlakverdeling/ invullingen/ rasters","-","-","-","-","-","-","-","-","-",null,null,"Nee","3D Model"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"90.** terrein","t"]
[null,"90.** terrein","t","Structuur","g","Bouwlaag","-","-","-","-","-","-","IfcRelContainedInSpatialStructure: IfcBuildingStorey","-","-","Conform separaat afsprakendocument",null,{"$f":"$R$113","v":"Ja"},{"$f":"$S$113","v":"Design > Story Settings"},null,null,{"$f":"$V$113","v":"n.v.t."},{"$f":"$W$113","v":"IfcBuildingStorey"},{"$f":"$X$113","v":"Attributes"},{"$f":"$Y$113","v":"IfcBuildingStorey"},{"$f":"$Z$113","v":"IfcBuildingStorey"}]
[null,"90.** terrein","t",null,"g","Entiteit","-","-","-","-","-","-","IfcBuildingElementProxy","IfcClass","-",null,null,"Ja",{"$f":"$S$28","v":"Archicad Classification NED 2.0"},null,null,{"$f":"$V$28","v":"ILS 3.4-Entiteiten"},{"$f":"$W$28","v":"n.v.t."},{"$f":"$X$28","v":"n.v.t."},{"$f":"$Y$28","v":"n.v.t."},"IfcBuildingElementProxy, IfcSite"]
[null,"90.** terrein","t",null,"g","Naamgeving element","-","-","-","-","-","-","IfcName, IfcType","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Ja",{"$f":"$S$75","v":"NL SfB classificatie  (2 cijfers)\n_\nArchicad Classification NED 2.0\n_\nElement ID"},null,null,{"$f":"$V$75","v":"ILS 3.6-SfB omschrijving"},{"$f":"$W$75","v":"(ifcElement)"},{"$f":"$X$75","v":"Attributes"},{"$f":"$Y$75","v":"Name"},{"$f":"$Z$75","v":"00_<Entiteit>_<Element-x>"}]
[null,"90.** terrein","t",null,"g","Codering - NL-SfB","-","-","-","-","-","-","IfcRelAssociatesClassification: IfcClassification","-","-","4-cijferig, conform vigerende versie BIM Loket",null,"Ja","NL SfB classificatie  (4 cijfers)",null,null,"ILS 3.6-SfB omschrijving","n.v.t.","n.v.t.","n.v.t.","00.00, <Elementtype SfB>"]
[null,"90.** terrein","t",null,"p","Leverancier/ fabrikant","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: Manufacturer","-","-","Ten behoeve van onderhoud"]
[null,"90.** terrein","t",null,"p","Merk","-","-","-","-","-","-","Pset_ManufacturerTypeInformation: ModelReference","-","-","Ten behoeve van onderhoud"]
[null,"90.** terrein","t",null,"p","Fase","-","-","-","-","-","-","Phase","-","-","Fase van het onderdeel (bijvoorbeeld bestaand, nieuwbouw,fase 1 etc.). Custom parameter benoemen in Custom Pset."]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"90.** terrein","t"]
[null,"90.** terrein","t","Eigenschappen","g","Materiaal","-","-","-","-","-","-","IfcRelAssociatesMaterial: … : IfcMaterial","-","-","Betekenisvol, Begrijpelijk, Logisch, Inzichtelijk, Consistent, Herkenbaar",null,"Nee",{"$f":"$S$82","v":"ACP: Building material properties"},null,null,{"$f":"$V$82","v":"n.v.t. (zie Building Material Settings)"},{"$f":"$W$82","v":"IfcBuildingElementPart en andere entiteiten die uit samengestelde elementen bestaan."},{"$f":"$X$82","v":"Een of meerdere, afhankelijk van mapping als 'Building Material Properties and Classifications aangevinkt staat in het IFC Translator Preset Data Conversion.\n\nMateriaalbenamingen volgens NAA.K.T. kunnen in de Building Material Settings ingesteld worden en zijn dan te vinden onder 'ILS O&E BWK."},{"$f":"$Y$82","v":"Een of meerdere, afhankelijk van mapping"},{"$f":"$Z$82","v":"Material Properties (IFC 2x3)\nMaterial (IFC 4):\nEen of meerdere, afhankelijk van mapping"}]
[null,"90.** terrein","t",null,"e","Kleur","-","-","-","-","-","-","-","-","-","In het geval van zichtwerk (RAL) kleurcode/ omschrijving)",null,"Nee","ACP: Kleur",null,null,null,{"$f":"$W$392","v":"(ifcElement)"},{"$f":"$X$392","v":"ILS O&E BWK"},"Kleur",{"$f":"$Z$295","v":"kleur (element) / kleur (materiaal)"}]
[null,"90.** terrein","t",null,"e","Dragend/ niet dragend","-","-","-","-","-","-","benoemen in custom Pset","true/ false","-","Indien entiteit IfcBuildingElementProxy: benoemen in Custom Pset omdat Pset_BuildingElementProxyCommon in Ifc 2x3 niet bestaat",null,"Nee",null,null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
[null,"90.** terrein","t",null,"e","In/ uitwendig","-","-","-","-","-","-","IsExternal benoemen in custom Pset","true/ false","-","Indien entiteit IfcBuildingElementProxy: benoemen in Custom Pset omdat Pset_BuildingElementProxyCommon in Ifc 2x3 niet bestaat",null,"Nee",null,null,null,"n.v.t.","n.v.t.","n.v.t.","n.v.t.","n.v.t."]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"90.** terrein","t"]
[null,"90.** terrein","t","Componenten","e","Bevestigingsconstructies","-","-","-","-","-","-","-","-","-"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
["x","90.** terrein","t",null,"p",null,"-","-","-","-","-","-","-","-","-"]
[null,"90.** terrein","t"]

{"sheet":"legende","index":2,"n_rows":4,"n_cols":2,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
[null,"BS = Building smart"]
[null,"ACP = Archicad property"]
[null,"BMP = Building Material Property"]
[null,"MAT = Materiaal"]