{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["DRAAITABEL ART.NR. EN ELEMENTEN"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"DRAAITABEL ART.NR. EN ELEMENTEN","index":0,"n_rows":4167,"n_cols":11,"rows_kept":4167,"cut":false,"hidden":false,"merged":[]}
[null,null,null,"Wat?","Opzet","Extra info"]
[null,null,"TYPE 1","Building Material","Metselwerken met verdeling volgens een bepaald materiaal, dikte en Layer","20.XX.XX."]
[null,null,"TYPE 2","Building Material","Eindigend op .XX. of .aX. (a= getal)","Eindigend op .XX. of .aX. (a= getal)"]
[null,null,"TYPE 3","Building Material","Volgens exacte VMSW artikelcode"]
[null,null,"TYPE 4","ARCHICAD property","Keuze maken bij een bepaald element"]
[null,null,"TYPE 5","Classification","Ken de te gebruiken VMSW artikelcode toe bij het element"]
[]
["Delen","Hfdst.","Art_nr.","Omschrijving","Aard","EH","TYPE ","Element","Element specificatie","Wat rekent de Meetstaat Manager?","Aandachtspunten"]
[0,"00.","00.","ALGEMENE BEPALINGEN"]
[0,"00.","00.10.","projectgegevens"]
[0,"00.","00.20.","ontwerpteam"]
[0,"00.","00.21.","ontwerpteam - architecturaal ontwerp"]
[0,"00.","00.22.","ontwerpteam - studie stabiliteit"]
[0,"00.","00.23.","ontwerpteam - studie technieken"]
[0,"00.","00.24.","ontwerpteam - veiligheidscoördinatie"]
[0,"00.","00.25.","ontwerpteam - EPB verslaggeving"]
[0,"00.","00.30.","documenten"]
[0,"00.","00.31.","documenten - architectuur"]
[0,"00.","00.32.","documenten - stabiliteit"]
[0,"00.","00.33.","documenten - technieken"]
[0,"00.","00.34.","documenten - veiligheidscoördinatie"]
[0,"00.","00.35.","documenten - EPB verslaggeving"]
[0,"00.","00.36.","documenten - diepsonderingsverslag"]
[0,"00.","00.37.","documenten - verslag milieutechnisch bodemonderzoek"]
[0,"00."]
[0,"01.","01.","AANNEMINGSMODALITEITEN"]
[0,"01.","01.00.","aannemingsmodaliteiten - algemeen"]
[0,"01.","01.01.","aannemingsmodaliteiten - bestek ","PM"]
[0,"01.","01.02.","aannemingsmodaliteiten - voorafgaand plaatsbezoek ","PM"]
[0,"01.","01.03.","aannemingsmodaliteiten - burgerlijke aansprakelijkheid ","PM"]
[0,"01.","01.04.","aannemingsmodaliteiten - volledigheid van inschrijving ","PM"]
[0,"01.","01.05.","aannemingsmodaliteiten - onderaanneming ","PM"]
[0,"01.","01.06.","aannemingsmodaliteiten - verrekeningen ","PM"]
[0,"01.","01.07.","aannemingsmodaliteiten - keuringsattesten ","PM"]
[0,"01.","01.08.","aannemingsmodaliteiten - materialenlijst ","PM"]
[0,"01.","01.10.","plaatsbeschrijvingen - algemeen"]
[0,"01.","01.11.","plaatsbeschrijvingen - aangrenzende constructies"]
[0,"01.","01.11.10.","plaatsbeschrijvingen – aangrenzende constructies/bij aanvang van de werken","PM"]
[0,"01.","01.11.20.","plaatsbeschrijvingen – aangrenzende constructies/staat van vergelijking","PM"]
[0,"01.","01.12.","plaatsbeschrijvingen - te renoveren constructies"]
[0,"01.","01.12.10.","plaatsbeschrijvingen – te renoveren constructies/bij aanvang van de werken","PM"]
[0,"01.","01.12.20.","plaatsbeschrijvingen – te renoveren constructies/staat van vergelijking","PM"]
[0,"01.","01.13.","plaatsbeschrijvingen - inboedel bij blijvende bewoning"]
[0,"01.","01.13.10.","plaatsbeschrijvingen – inboedel bij blijvende bewoning/bij aanvang van de werken","PM"]
[0,"01.","01.13.20.","plaatsbeschrijvingen – inboedel bij blijvende bewoning/staat van vergelijking","PM"]
[0,"01.","01.14.","plaatsbeschrijvingen - wegenis en voetpaden"]
[0,"01.","01.14.10.","plaatsbeschrijvingen – wegenis en voetpaden bij aanvang van de werken","PM"]
[0,"01.","01.14.20.","plaatsbeschrijvingen – wegenis en voetpaden/staat van vergelijking","PM"]
[0,"01.","01.15.","plaatsbeschrijvingen - beplanting"]
[0,"01.","01.15.10.","plaatsbeschrijvingen – beplanting/bij aanvang van de werken","PM"]
[0,"01.","01.15.20.","plaatsbeschrijvingen – beplanting/staat van vergelijking","PM"]
[0,"01.","01.20.","werfcoördinatie - algemeen"]
[0,"01.","01.21.","werfcoördinatie - planning van de werken ","PM"]
[0,"01.","01.22.","werfcoördinatie - werfleiding en controle ","PM"]
[0,"01.","01.23.","werfcoördinatie - werfvergaderingen ","PM"]
[0,"01.","01.24.","werfcoördinatie - uitzetten bouwwerken ","PM"]
[0,"01.","01.25.","werfcoördinatie - as-builtdossier ","PM"]
[0,"01.","01.26.","werfcoördinatie - renovaties met blijvende bewoning ","PM"]
[0,"01.","01.30.","werfcondities - algemeen"]
[0,"01.","01.31.","werfcondities - orde en netheid ","PM"]
[0,"01.","01.32.","werfcondities - geluids- en stofhinder ","PM"]
[0,"01.","01.33.","werfcondities - nazorg ","PM"]
[0,"01.","01.40.","veiligheidsvoorschriften - algemeen ","PM"]
[0,"01."]
[0,"02.","02.","BOUWPLAATSVOORZIENINGEN"]
[0,"02.","02.00.","bouwplaatsvoorzieningen - algemeen"]
[0,"02.","02.10.","beschermingswerken - algemeen"]
[0,"02.","02.11.","beschermingwerken - openbare weg ","PM"]
[0,"02.","02.12.","beschermingswerken - beplantingen"]
[0,"02.","02.12.10.","beschermingswerken – beplantingen/bomen","FH","st","TYPE 5","Object",null,"Stuks"]
[0,"02.",null,null,"PM"]
[0,"02.","02.12.20.","beschermingswerken – beplantingen/struiken en hagen"]
[{"$nulls":4},"PM"]
[0,"02.","02.20.","opruiming beplantingen - algemeen"]
[0,"02.","02.21.","opruiming beplantingen - bomen ","PM "]
[0,"02.",null,null,"SOG"]
[0,"02.","02.22.","opruiming beplantingen - struiken en hagen ","PM"]
[0,"02.","02.30.","toegangswegen - algemeen"]
[0,"02.","02.31.","toegangswegen - voorlopige verharding voor voetgangers ","PM"]
[0,"02.","02.32.","toegangswegen - voorlopige verharding voor zware lasten ","PM"]
[0,"02.","02.33.","toegangswegen - parkeerruimte voor laden en lossen ","PM"]
[0,"02.","02.40.","voorlopige omheining - algemeen"]
[0,"02.","02.50.","aankondiging werf - algemeen"]
[0,"02.","02.51.","aankondiging werf - werfbord ","PM"]
[0,"02.","02.52.","aankondiging werf - werfdoek ","PM"]
[0,"02.","02.60.","werflokalen - algemeen"]
[0,"02.","02.61.","werflokalen - berging van materieel en bouwmaterialen ","PM"]
[0,"02.","02.62.","werflokalen - kantoorruimte ","PM"]
[0,"02.","02.63.","werflokalen - personeelslokaal ","PM"]
[0,"02.","02.64.","werflokalen - sanitaire voorzieningen ","PM"]
[0,"02.","02.70.","voorlopige aansluitingen - algemeen"]
[0,"02.","02.71.","voorlopige aansluitingen - stroomvoorziening ","PM"]
[0,"02.","02.72.","voorlopige aansluitingen - watervoorziening ","PM"]
[0,"02.","02.73.","voorlopige aansluitingen - waterafvoer ","PM"]
[0,"02.","02.80.","arbeidsmiddelen - algemeen"]
[0,"02.","02.81.","arbeidsmiddelen - werken op hoogte"]
[0,"02.","02.81.10","arbeidsmiddelen - werken op hoogte/ladders","PM"]
[0,"02.","02.81.20","arbeidsmiddelen - werken op hoogte/steigers","PM"]
[0,"02.","02.82.","arbeidsmiddelen - hijsen en heffen van lasten ","PM"]
[0,"02."]
[0,"03.","03.","AFBRAAKWERKEN"]
[0,"03.","03.00.","afbraakwerken - algemeen"]
[0,"03.","03.01.","afbraakwerken - asbestverwijdering"]
[0,"03.","03.02.","afbraakwerken - schoring"]
[0,"03.","03.03.","afbraakwerken - in bewoonde gebouwen"]
[0,"03.","03.10.","afbraak volledige constructie - algemeen"]
[0,"03.","03.11.","afbraak volledige constructie - vrijstaand"]
[0,"03.","03.11.10.","afbraak volledige constructie - vrijstaand/asbestverwijdering"]
[0,"03.","03.11.11.","afbraak volledige constructie – vrijstaand/asbestverwijdering - dakbedekking","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Shell",null,"Top Surface"]
[0,"03.","03.11.12.","afbraak volledige constructie – vrijstaand/asbestverwijdering - onderdak","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Shell",null,"Top Surface"]
[0,"03.","03.11.13.","afbraak volledige constructie – vrijstaand/asbestverwijdering - asbestcementbuizen","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom","Let op! Enkel Horizontale lengte wordt gemeten"]
[0,"03.",{"$nulls":4},"TYPE 5","Object",null,"Lengte"]
[0,"03.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[0,"03.",{"$nulls":4},"TYPE 5","Object",null,"Stuks","waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.","03.11.14.","afbraak volledige constructie – vrijstaand/asbestverwijdering - vloerafwerking","FH","m2","TYPE 3","Slab",null,"Top Surface"]
[0,"03.","03.11.15.","afbraak volledige constructie – vrijstaand/asbestverwijdering - plaatmateriaal","FH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[0,"03.","03.11.16.","afbraak volledige constructie – vrijstaand/asbestverwijdering - buisisolatie","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[0,"03.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[0,"03.","03.11.17.","afbraak volledige constructie – vrijstaand/asbestverwijdering - asbestkoord","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[0,"03.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[0,"03.","03.11.18.","afbraak volledige constructie – vrijstaand/asbestverwijdering - raam- en deurkitten","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[0,"03.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[0,"03.","03.11.20.","afbraak volledige constructie - vrijstaand/slopen gebouw","FH","m3","TYPE 5","Morph",null,"Net Volume"]
[0,"03.",null,null,"SOG"]
[0,"03.","03.11.30.","afbraak volledige constructie - vrijstaand/ondergrondse massieven","VH","m3","TYPE 3","Beam",null,"Net Volume"]
[0,"03.",{"$nulls":5},"Wall",null,"Net Volume"]
[0,"03.",{"$nulls":4},"TYPE 5","Morph",null,"Net Volume"]
[0,"03.","03.11.40.","afbraak volledige constructie - vrijstaand/te behouden gevels","PM"]
[0,"03.","03.12.","afbraak volledige constructie - grenzend aan andere gebouwen"]
[0,"03.","03.12.10.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering"]
[0,"03.","03.12.11.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - dakbedekking","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Shell",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.","03.12.12.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - onderdak","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Shell",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.","03.12.13.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - asbestcementbuizen","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[0,"03.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[0,"03.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[0,"03.",{"$nulls":4},"TYPE 5","Object",null,"Stuks"]
[0,"03.","03.12.14.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - vloerafwerking","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.","03.12.15.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - plaatmateriaal","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[0,"03.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[0,"03.","03.12.16.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - buisisolatie","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[0,"03.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[0,"03.","03.12.17.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - asbestkoord","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[0,"03.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[0,"03.","03.12.18.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - raam- en deurkitten","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[0,"03.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[0,"03.","03.12.20.","afbraak volledige constructie – grenzend aan andere gebouwen/slopen gebouw","FH","m3","TYPE 5","Morph",null,"Net Volume"]
[0,"03.",null,null,"SOG"]
[0,"03.","03.12.30.","afbraak volledige constructie – grenzend aan andere gebouwen/ondergrondse massieven","VH","m3","TYPE 3","Beam",null,"Net Volume"]
[0,"03.",{"$nulls":5},"Wall",null,"Net Volume"]
[0,"03.",{"$nulls":4},"TYPE 5","Morph",null,"Net Volume"]
[0,"03.","03.12.40.","afbraak volledige constructie – grenzend aan andere gebouwen/te behouden gevels","PM"]
[0,"03.","03.20.","afbraak ruwbouwelementen - algemeen"]
[0,"03.","03.21.","afbraak ruwbouwelementen - muren"]
[0,"03.","03.21.10.","afbraak ruwbouwelementen – muren/metselwerk","FH of VH","m3","TYPE 3","Wall",null,"Net Volume"]
[0,"03.","03.21.20.","afbraak ruwbouwelementen – muren/beton","FH of VH","m3","TYPE 3","Wall",null,"Net Volume"]
[0,"03.","03.21.30.","afbraak ruwbouwelementen – muren/houtskelet","FH of VH","m3","TYPE 3","Wall",null,"Net Volume"]
[0,"03.","03.22.","afbraak ruwbouwelementen - vloeren"]
[0,"03.","03.22.10.","afbraak ruwbouwelementen – vloeren/potten en balken","FH of VH","m2","TYPE 3","Roof",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Shell",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.",{"$nulls":5},"Slab",null,"Top Surface"]
[0,"03.","03.22.20.","afbraak ruwbouwelementen – vloeren/beton"]
[0,"03.","03.22.21.","afbraak ruwbouwelementen – vloeren/beton - verdiepingsvloer","FH of VH","m2","TYPE 3","Roof",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Shell",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.","03.22.22.","afbraak ruwbouwelementen – vloeren/beton - vloer op volle grond","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.","03.22.30.","afbraak ruwbouwelementen – vloeren/houten roostering","FH of VH","m2","TYPE 3","Roof",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Shell",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.","03.30.","afbraak dakelementen - algemeen"]
[0,"03.","03.31.","afbraak dakelementen - hellend dak"]
[0,"03.","03.31.10.","afbraak dakelementen – hellend dak/asbestverwijdering"]
[0,"03.","03.31.11.","afbraak dakelementen – hellend dak/asbestverwijdering - dakbedekking","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Shell",null,"Top Surface"]
[0,"03.","03.31.12.","afbraak dakelementen – hellend dak/asbestverwijdering - onderdak","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Shell",null,"Top Surface"]
[0,"03.","03.31.13.","afbraak dakelementen – hellend dak/asbestverwijdering - asbestcement","FH","st","TYPE 3","Roof",null,"Stuks"]
[0,"03.",{"$nulls":5},"Shell",null,"Stuks"]
[0,"03.","03.31.20.","afbraak dakelementen – hellend dak/volledige dakopbouw","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Shell",null,"Top Surface"]
[0,"03.",null,null,"SOG"]
[0,"03.","03.31.30.","afbraak dakelementen – hellend dak/dakbedekking","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Shell",null,"Top Surface"]
[0,"03.","03.31.40.","afbraak dakelementen – hellend dak/dakisolatie","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Shell",null,"Top Surface"]
[0,"03.",null,null,"PM"]
[0,"03.","03.31.50.","afbraak dakelementen – hellend dak/daklichtelementen","FH","st","TYPE 5","Object",null,"Stuks"]
[0,"03.",{"$nulls":5},"Skylight",null,"Stuks"]
[0,"03.",null,null,"PM"]
[0,"03.","03.31.60.","afbraak dakelementen – hellend dak/dakdoorvoeren en schouwen","FH","st","TYPE 5","Object",null,"Stuks"]
[0,"03.",{"$nulls":5},"Skylight",null,"Stuks"]
[0,"03.",null,null,"PM"]
[0,"03.","03.32.","afbraak dakelementen - plat dak"]
[0,"03.","03.32.10.","afbraak dakelementen – plat dak/asbestverwijdering"]
[0,"03.","03.32.11.","afbraak dakelementen – plat dak/asbestverwijdering - asbestcement","FH","st","TYPE 3","Roof",null,"Stuks"]
[0,"03.",{"$nulls":5},"Slab",null,"Stuks"]
[0,"03.","03.32.20.","afbraak dakelementen – plat dak/volledige dakopbouw","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Slab",null,"Top Surface"]
[0,"03.",null,null,"SOG"]
[0,"03.","03.32.30.","afbraak dakelementen – plat dak/dakdichting","FH","m2","TYPE 3","Roof",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.",{"$nulls":5},"Slab",null,"Top Surface"]
[0,"03.","03.32.40.","afbraak dakelementen – plat dak/dakisolatie","FH","m2","TYPE 3","Roof",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.",{"$nulls":5},"Slab",null,"Top Surface"]
[0,"03.",null,null,"PM"]
[0,"03.","03.32.50.","afbraak dakelementen – plat dak/daklichtelementen","FH","st","TYPE 5","Object",null,"Stuks","waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.",{"$nulls":5},"Skylight",null,"Stuks"]
[0,"03.",null,null,"PM"]
[0,"03.","03.32.60.","afbraak dakelementen – plat dak/dakdoorvoeren","FH","st","TYPE 5","Morph",null,"Stuks"]
[0,"03.",{"$nulls":5},"Object",null,"Stuks"]
[0,"03.","03.40.","afbraak gevelelementen - algemeen"]
[0,"03.","03.41.","afbraak gevelelementen - gevelmetselwerk ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[0,"03.","03.42.","afbraak gevelelementen - leien"]
[0,"03.","03.42.10.","afbraak gevelelementen – leien/asbesthoudend","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[0,"03.","03.42.20.","afbraak gevelelementen – leien/niet-asbesthoudend","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[0,"03.","03.43.","afbraak gevelelementen - beplating ","FH","m2","TYPE 3","Wall",null,"Projected Area on the side opposite to the reference line"]
[0,"03.","03.44.","afbraak gevelelementen - buitenschrijnwerk"]
[0,"03.","03.44.10.","afbraak gevelelementen – buitenschrijnwerk/asbestverwijdering"]
[0,"03.","03.44.11.","afbraak gevelelementen – buitenschrijnwerk/asbestverwijdering - kitten","FH","m","TYPE 5","Object",null,"Lengte"]
[0,"03.","03.44.20.","afbraak gevelelementen – buitenschrijnwerk/ramen, deuren en poorten","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area"]
[0,"03.",{"$nulls":5},"Window",null,"W/D Opening Surface on the Reveal Side","Let op! Enkel Horizontale lengte wordt gemeten"]
[0,"03.",null,null,"PM"]
[0,"03.","03.45.","afbraak gevelelementen - buitentrappen ","FH","m2","TYPE 5","Stair ","Tread total area","Net Area"]
[0,"03.",null,null,"PM"]
[0,"03.",null,null,"SOG"]
[0,"03.","03.46.","afbraak gevelelementen - balustraden ","FH","st","TYPE 5","Railing",null,"Stuks"]
[0,"03.",null,null,"PM"]
[0,"03.",null,null,"SOG"]
[0,"03.","03.50.","afbraak binnenafwerking - algemeen"]
[0,"03.","03.51.","afbraak binnenafwerking - volledige ontmanteling ","SOG"]
[0,"03.","03.52.","afbraak binnenafwerking - afkappen pleisterwerk ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Wall",null,"Netto oppervlak binnenkant wand"]
[0,"03.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[0,"03.","03.53.","afbraak binnenafwerking - plaatafwerking"]
[0,"03.","03.53.10.","afbraak binnenafwerking – plaatafwerking/asbestverwijdering","FH","m2","TYPE 3","Slab",null,"Top Surface"]
[0,"03.",{"$nulls":5},"Wall",null,"Netto oppervlak binnenkant wand","waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[0,"03.","03.53.20.","afbraak binnenafwerking – plaatafwerking/lichte scheidingswanden","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[0,"03.",null,null,"SOG",{"$nulls":5},"waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.","03.53.30.","afbraak binnenafwerking – plaatafwerking/plafondafwerking","FH","m2","TYPE 3","Slab",null,"Top Surface"]
[0,"03.",null,null,"SOG"]
[0,"03.","03.53.40.","afbraak binnenafwerking – plaatafwerking/uitbekleding wanden","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand"]
[0,"03.",null,null,"SOG"]
[0,"03.","03.54.","afbraak binnenafwerking - dekvloer",{"$nulls":5},"Property: Oppervlakte middenas wand","waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.","03.54.10.","afbraak binnenafwerking – dekvloer/asbestverwijdering","FH","m2","TYPE 3","Slab",null,"Top Surface"]
[0,"03.","03.54.20.","afbraak binnenafwerking – dekvloer/tot op draagstructuur","FH","m2","TYPE 3","Slab",null,"Top Surface"]
[0,"03.","03.55.","afbraak binnenafwerking - vloerafwerking"]
[0,"03.","03.55.10.","afbraak binnenafwerking – vloerafwerking/asbestverwijdering","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.","03.55.20.","afbraak binnenafwerking – vloerafwerking/linoleum","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.",null,null,"PM"]
[0,"03.","03.55.30.","afbraak binnenafwerking – vloerafwerking/tegels",{"$nulls":6},"waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.","03.55.31.","afbraak binnenafwerking – vloerafwerking/tegels - op dekvloer","FH","m2","TYPE 3","Slab",null,"Top Surface"]
[0,"03.",null,null,"PM",{"$nulls":5},"waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.","03.55.32.","afbraak binnenafwerking – vloerafwerking/tegels - op zandbed","FH","m2","TYPE 3","Slab",null,"Top Surface"]
[0,"03.",null,null,"PM"]
[0,"03.","03.55.40.","afbraak binnenafwerking – vloerafwerking/houten vloer","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.",null,null,"PM"]
[0,"03.","03.56.","afbraak binnenafwerking - binnendeuren ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area","waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.",null,null,"PM"]
[0,"03.","03.57.","afbraak binnenafwerking - trappen en leuningen ","FH","st","TYPE 5","Object",null,"Stuks","waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"03.",{"$nulls":5},"Railing",null,"Stuks"]
[0,"03.",{"$nulls":5},"Stair",null,"Stuks"]
[0,"03.",null,null,"PM"]
[0,"03.","03.58.","afbraak binnenafwerking - vast meubilair"]
[0,"03.","03.58.10.","afbraak binnenafwerking – vast meubilair/keukenmeubilair","FH","st","TYPE 5","Object",null,"Stuks"]
[0,"03.",null,null,"PM"]
[0,"03.","03.58.20.","afbraak binnenafwerking – vast meubilair/badkamermeubilair","FH","st","TYPE 5","Object",null,"Stuks"]
[0,"03.",null,null,"PM"]
[0,"03.","03.60.","afbraak technieken fluïda - algemeen"]
[0,"03.","03.61.","afbraak technieken fluïda - leidingen"]
[0,"03.","03.61.10.","afbraak technieken fluïda – leidingen/asbestverwijdering"]
[0,"03.","03.61.11.","afbraak technieken fluïda – leidingen/asbestverwijdering - asbestcement","FH of VH","m","TYPE 5","Object",null,"Lengte"]
[0,"03.",null,null,null,"st","TYPE 5","Object",null,"Stuks"]
[0,"03.","03.61.12.","afbraak technieken fluïda – leidingen/asbestverwijdering - leidingisolatie","FH of VH","m","TYPE 5","Object",null,"Lengte"]
[0,"03.",null,null,null,"st","TYPE 5","Object",null,"Stuks","Let op! Enkel Horizontale lengte wordt gemeten"]
[0,"03.","03.61.20.","afbraak technieken fluïda – leidingen/toevoer en afvoerleidingen","PM"]
[0,"03.",null,null,"SOG",{"$nulls":5},"Let op! Enkel Horizontale lengte wordt gemeten"]
[0,"03.","03.62.","afbraak technieken fluïda - sanitaire toestellen ","FH","st","TYPE 5","Object",null,"Stuks"]
[0,"03.",null,null,"PM"]
[0,"03.",null,null,"SOG"]
[0,"03.","03.63.","afbraak technieken fluïda - radiatoren & toebehoren","FH","st","TYPE 5","Object",null,"Stuks"]
[0,"03.",null,null,"PM"]
[0,"03.",null,null,"SOG"]
[0,"03.","03.64.","afbraak technieken fluïda - gasleidingen & toebehoren","FH","st","TYPE 5","Object",null,"Stuks"]
[0,"03.",null,null,"PM"]
[0,"03.",null,null,"SOG"]
[0,"03.","03.65.","afbraak technieken fluïda - CV-ketel & toebehoren","FH","st","TYPE 5","Object",null,"Stuks"]
[0,"03.",null,null,"PM"]
[0,"03.",null,null,"SOG"]
[0,"03.","03.70.","afbraak technieken elektro - algemeen"]
[0,"03.","03.71.","afbraak technieken elektro - leidingnet ","FH","m2","TYPE 3","Slab",null,"Top Surface"]
[0,"03.",null,null,"PM"]
[0,"03.",null,null,"SOG"]
[0,"03."]
[0,"03."]
[0,"03.",{"$nulls":8},"waarden detailmeetstaat correct indien vloer rechthoekig"]
[0,"04.","04.","GEBOUWPRESTATIES"]
[0,"04.","04.00.","gebouwprestaties - algemeen"]
[0,"04.","04.10.","energieprestatie en binnenklimaat (EPB) - algemeen ","PM"]
[0,"04.","04.20.","luchtdichtheid - algemeen ","PM"]
[0,"04.","04.30.","akoestiek - algemeen ","PM"]
[0,"04.","04.40.","brandveiligheid - algemeen ","PM"]
[0,"04."]
[0,"05.","05.","PROEVEN"]
[0,"05.","05.00.","proeven - algemeen"]
[0,"05.","05.10.","proeven - luchtdichtheidsmeting"]
[0,"05.","05.11.","proeven - luchtdichtheidsmeting / wooneenheid ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks"]
[0,"05.","05.12.","proeven - luchtdichtheidsmeting / gebouw ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks"]
[0,"05.","05.20.","proeven - akoestiek"]
[0,"05.","05.21.","proeven - akoestiek / luchtgeluidiolatie ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks"]
[0,"05.","05.22.","proeven - akoestiek / contactgeluidiolatie ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks"]
[0,"05.","05.23.","proeven - akoestiek / geluidisolatie van de gevel ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks"]
[0,"05.","05.24.","proeven - akoestiek / geluid van technische installaties ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks"]
[0,"05."]
[1,"10.","10.","GRONDWERKEN"]
[1,"10.","10.00.","grondwerken - algemeen"]
[1,"10.","10.10.","voorafgaande afgraving van het terrein - algemeen"]
[1,"10.","10.11.","voorafgaande afgraving terrein - ontzoden ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"10.",{"$nulls":4},"TYPE 5","Mesh",null,"Projected Area"]
[1,"10.",null,null,"PM"]
[1,"10.",null,null,"SOG"]
[1,"10.","10.12.","voorafgaande afgraving terrein - afgraven teelaarde ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"10.",{"$nulls":4},"TYPE 5","Mesh",null,"Projected Area"]
[1,"10.",null,null,"PM"]
[1,"10.",null,null,"SOG"]
[1,"10.","10.13.","voorafgaande afgraving terrein - machinale nivellering ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"10.",{"$nulls":4},"TYPE 5","Mesh",null,"Projected Area"]
[1,"10.",null,null,"PM"]
[1,"10.",null,null,"SOG"]
[1,"10.","10.20.","uitgraving bouwputten - algemeen"]
[1,"10.","10.21.","uitgraving bouwputten - gewone bouwputten ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume"]
[1,"10.","10.22.","uitgraving bouwputten - prefabkelders ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume"]
[1,"10.",null,null,"PM"]
[1,"10.","10.23.","uitgraving bouwputten - rioleringselementen ","PM"]
[1,"10.","10.30.","uitgraving sleuven - algemeen"]
[1,"10.","10.31.","uitgraving sleuven - funderingssleuven ","FH/VH","m3","TYPE 5","Morph",null,"Net Volume"]
[1,"10.",null,null,null,"m3","TYPE 3","Beam",null,"Net Volume"]
[1,"10.","10.32.","uitgraving sleuven - funderingsbalken ","FH/VH","m3","TYPE 5","Morph",null,"Net Volume"]
[1,"10.","10.33.","uitgraving sleuven - ondergrondse leidingen ","FH/VH","m3","TYPE 5","Morph",null,"Net Volume"]
[1,"10.",null,null,"PM"]
[1,"10.","10.40.","grondverzet - algemeen"]
[1,"10.","10.41.","grondverzet - projectopvolging ","SOG"]
[1,"10.","10.42.","grondverzet - hergebruik uitgegraven grond op werf ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"10.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume"]
[1,"10.",{"$nulls":5},"Morph",null,"Net Volume"]
[1,"10.","10.43.","grondverzet - afvoer uitgegraven bodem"]
[1,"10.","10.43.10.","grondverzet - afvoer uitgegraven bodem/naar bestemming voor gebruik"]
[1,"10.","10.43.11.","grondverzet - afvoer uitgegraven bodem/naar bestemming voor gebruik - kwaliteit vrij gebruik ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"10.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume"]
[1,"10.",{"$nulls":5},"Morph",null,"Net Volume"]
[1,"10.","10.43.12.","grondverzet - afvoer uitgegraven bodem/naar bestemming voor gebruik - kwaliteit bouwkundig bodemgebruik ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"10.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume"]
[1,"10.",{"$nulls":5},"Morph",null,"Net Volume"]
[1,"10.","10.43.20.","grondverzet - afvoer uitgegraven bodem/naar tussentijdse opslagplaats (TOP) ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"10.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume"]
[1,"10.",{"$nulls":5},"Morph",null,"Net Volume"]
[1,"10.","10.43.30.","grondverzet - afvoer uitgegraven bodem/naar grondreinigingscentrum (GRC) ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"10.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume"]
[1,"10.",{"$nulls":5},"Morph",null,"Net Volume"]
[1,"10.","10.43.40.","grondverzet - afvoer uitgegraven bodem/naar erkende stortplaats"]
[1,"10.","10.43.41.","grondverzet - afvoer uitgegraven bodem/naar erkende stortplaats - klasse I ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"10.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume"]
[1,"10.",{"$nulls":5},"Morph",null,"Net Volume"]
[1,"10.","10.43.42.","grondverzet - afvoer uitgegraven bodem/naar erkende stortplaats - klasse II ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"10.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume"]
[1,"10.",{"$nulls":5},"Morph",null,"Net Volume"]
[1,"10.","10.43.43.","grondverzet - afvoer uitgegraven bodem/naar erkende stortplaats - klasse III ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"10.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume"]
[1,"10.",{"$nulls":5},"Morph",null,"Net Volume"]
[1,"10.","10.44.","grondverzet - fysische scheiding"]
[1,"10.","10.44.10.","grondverzet - fysische scheiding/uitzeving ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"10.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume"]
[1,"10.",{"$nulls":5},"Morph",null,"Net Volume"]
[1,"10.","10.44.20.","grondverzet - fysische scheiding/afvoer steenachtige materialen ","VH","ton","TYPE 3","Slab","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"10.",{"$nulls":4},"TYPE 5","Mesh","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet"]
[1,"10.",{"$nulls":5},"Morph","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet"]
[1,"10.",{"$nulls":5},"Object","Meetstaat Manager 22 KM","ARCHICAD Property: Grondverzet"]
[1,"10.",{"$nulls":6},"ARCHICAD property koppelen aan object KM","ARCHICAD Property: Grondverzet"]
[1,"10.","10.44.30.","grondverzet - fysische scheiding/afvoer bodemvreemde materialen ","VH","ton","TYPE 3","Slab","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"10.",{"$nulls":4},"TYPE 5","Mesh","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet"]
[1,"10.",{"$nulls":5},"Morph","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet"]
[1,"10.",{"$nulls":5},"Object","Meetstaat Manager 22 KM of ARCHICAD property koppelen aan object KM","ARCHICAD Property: Grondverzet"]
[1,"10.","10.50.","verwijdering massieven - algemeen ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"10.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume"]
[1,"10.",{"$nulls":5},"Morph",null,"Net Volume"]
[1,"10.","10.60.","bronbemaling - algemeen ","SOG"]
[1,"10.","10.70.","aanvullingen - algemeen"]
[1,"10.","10.71.","aanvullingen - wederaanvullingen"]
[1,"10.","10.71.10.","aanvullingen - wederaanvullingen/grond van uitgravingen ","PM"]
[1,"10.","10.71.20.","aanvullingen - wederaanvullingen/aangevoerde grond ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume"]
[1,"10.",{"$nulls":5},"Morph",null,"Net Volume"]
[1,"10.","10.71.30.","aanvullingen - wederaanvullingen/gestabiliseerd zand ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume"]
[1,"10.",{"$nulls":5},"Morph",null,"Net Volume"]
[1,"10.","10.71.40.","aanvullingen - wederaanvullingen/kunststeenslag ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume"]
[1,"10.",{"$nulls":5},"Morph",null,"Net Volume"]
[1,"10.","10.71.50.","aanvullingen - wederaanvullingen/natuursteenslag ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume"]
[1,"10.",{"$nulls":5},"Morph",null,"Net Volume"]
[1,"10.","10.72.","aanvullingen - ophoging terrein"]
[1,"10.","10.72.10.","aanvullingen - ophoging terrein/grond van afgravingen ","PM"]
[1,"10.","10.72.20","aanvullingen - ophoging terrein/aangevoerde grond ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume"]
[1,"10.",{"$nulls":5},"Morph",null,"Net Volume"]
[1,"10.","10.72.30.","aanvullingen - ophoging terrein/gestabiliseerd zand ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume"]
[1,"10.",{"$nulls":5},"Morph",null,"Net Volume"]
[1,"10.","10.80.","grondbehandeling - algemeen"]
[1,"10.","10.81.","grondbehandeling - kalk ","VH","m3","TYPE 5","Mesh",null,"Net Volume"]
[1,"10.",{"$nulls":5},"Morph",null,"Net Volume"]
[1,"10.","10.82.","grondbehandeling - cement ","VH","m3","TYPE 5","Mesh",null,"Net Volume"]
[1,"11.","11.","STUT- & ONDERVANGINGSWERKEN"]
[1,"11.","11.00.","stut- & ondervangingswerken - algemeen"]
[1,"11.","11.10.","beschoeiing bouwputten - algemeen"]
[1,"11.","11.11.","beschoeiing bouwputten - damplanken"]
[1,"11.","11.11.10.","beschoeiing bouwputten - damplanken/aanvoer & installatie machine ","SOG"]
[1,"11.","11.11.20.","beschoeiing bouwputten - damplanken/materialen & verwerking ","FH/VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[1,"11.",{"$nulls":5},"Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[1,"11.",{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (m2) in bij de Object Settings"]
[1,"11.","11.12.","beschoeiing bouwputten - berlinerwand"]
[1,"11.","11.12.10.","beschoeiing bouwputten - berlinerwand/ aanvoer & installatie machine ","SOG"]
[1,"11.","11.12.20.","beschoeiing bouwputten - berlinerwand/materialen & verwerking ","FH/VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[1,"11.",{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (m2) in bij de Object Settings"]
[1,"11.","11.13.","beschoeiing bouwputten - secanspalenwand"]
[1,"11.","11.13.10.","beschoeiing bouwputten - secanspalenwand/installatie palenmachine ","SOG"]
[1,"11.","11.13.20.","beschoeiing bouwputten - secanspalenwand/realisatie palenwand ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
[1,"11.","11.13.30.","beschoeiing bouwputten - secanspalenwand/verbindingsbalk ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[1,"11.","11.13.50.","beschoeiing bouwputten - secanspalenwand/horizontale verankering ","FH/VH","st","TYPE 5","Object",null,"Stuks"]
[1,"11.","11.13.60.","beschoeiing bouwputten - secanspalenwand/sonische integriteitstesten ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"11.","11.13.70.","beschoeiing bouwputten - secanspalenwand/afwerking als kelderwand ","FH","m3","TYPE 3","Wall",null,"Net Volume"]
[1,"11.","11.20.","onderschoeiingen - algemeen"]
[1,"11.","11.21.","onderschoeiingen - stortklaar beton ","VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[1,"11.",{"$nulls":5},"Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[1,"11.",null,null,null,"m3","TYPE 3","Beam",null,"Net Volume"]
[1,"11.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"11.","11.22.","onderschoeiingen - metselwerk ","VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[1,"11.",{"$nulls":5},"Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[1,"11.",null,null,null,"m3","TYPE 3","Beam",null,"Net Volume"]
[1,"11.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"11.","11.23.","onderschoeiingen - groutkolommen",{"$nulls":5},"Net Volume"]
[1,"11.","11.23.10.","onderschoeiingen - groutkolommen/aanvoer en installatie van de machine ","SOG"]
[1,"11.","11.23.20.","onderschoeiingen - groutkolommen/materialen en verwerking ","VH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"11.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[1,"11.","11.30.","keermuren - algemeen"]
[1,"11.","11.31.","keermuren - stortklaar beton ","VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[1,"11.",{"$nulls":5},"Wall",null,"Projected Area"]
[1,"11.",null,null,null,"m3","TYPE 3","Beam",null,"Net Volume"]
[1,"11.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"11."]
[1,"12.","12.","FUNDERINGEN OP STAAL"]
[1,"12.","12.00.","funderingen op staal - algemeen"]
[1,"12.","12.10.","funderingszolen en -stroken - algemeen"]
[1,"12.","12.11.","funderingszolen en -stroken - ongewapend beton ","VH","m3","TYPE 3","Beam",null,"Net Volume"]
[1,"12.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"12.","12.12.","funderingszolen en -stroken - gewapend beton ","VH","m3","TYPE 3","Beam",null,"Net Volume"]
[1,"12.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"12.","12.20.","ondergronds metselwerk - algemeen"]
[1,"12.","12.21.","ondergronds metselwerk - betonblokken"]
[1,"12.","12.21.10.","ondergronds metselwerk - betonblokken/muurdikte 35 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume"]
[1,"12.","12.21.20.","ondergronds metselwerk - betonblokken/muurdikte 40 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume"]
[1,"12.","12.21.30.","ondergronds metselwerk - betonblokken/muurdikte 45 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume"]
[1,"12.","12.22.","ondergronds metselwerk - snelbouw"]
[1,"12.","12.22.10.","ondergronds metselwerk - snelbouw/muurdikte 35 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume"]
[1,"12.","12.22.20.","ondergronds metselwerk - snelbouw/muurdikte 40 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume"]
[1,"12.","12.22.30.","ondergronds metselwerk - snelbouw/muurdikte 45 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume"]
[1,"12.","12.30.","doorbrekingen ondergronds metselwerk - algemeen"]
[1,"12.","12.31.","doorbrekingen ondergronds metselwerk - aansluitbocht ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"12.","12.40.","aardingslus - algemeen","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"12.",null,null,null,"st","TYPE 5","Object",null,"Stuks"]
[1,"12."]
[1,"13.","13.","SPECIALE FUNDERINGEN"]
[1,"13.","13.00.","speciale funderingen - algemeen"]
[1,"13.","13.01.","algemeen - diepsonderingsverslag"]
[1,"13.","13.10.","paalfundering - algemeen"]
[1,"13.","13.11.","paalfundering - schroefpalen"]
[1,"13.","13.11.10.","paalfundering - schroefpalen/enkele grondverdringing"]
[1,"13.","13.11.11.","paalfundering - schroefpalen/enkele grondverdringing - werfinstallatie ","SOG"]
[1,"13.","13.11.12.","paalfundering - schroefpalen/enkele grondverdringing - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks"]
[1,"13.","13.11.13.","paalfundering - schroefpalen/enkele grondverdringing - afkappen paalkoppen ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW paalfundering - Afkappen paalkoppen","Stuks"]
[1,"13.","13.11.14.","paalfundering - schroefpalen/enkele grondverdringing - sonische integriteitstesten  ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW paalfundering - Sonische integriteitstesten","Stuks"]
[1,"13.","13.11.20.","paalfundering - schroefpalen/dubbele grondverdringing"]
[1,"13.","13.11.21.","paalfundering - schroefpalen/dubbele grondverdringing - werfinstallatie ","SOG"]
[1,"13.","13.11.22.","paalfundering - schroefpalen/dubbele grondverdringing - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks"]
[1,"13.","13.11.23.","paalfundering - schroefpalen/dubbele grondverdringing - afkappen paalkoppen  ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW paalfundering - Afkappen paalkoppen","Stuks"]
[1,"13.","13.11.24.","paalfundering - schroefpalen/dubbele grondverdringing - sonische integriteitstesten  ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW paalfundering - Sonische integriteitstesten","Stuks"]
[1,"13.","13.12.","paalfundering - boorpalen"]
[1,"13.","13.12.10.","paalfundering - boorpalen/verbuisd"]
[1,"13.","13.12.11.","paalfundering - boorpalen/verbuisd - werfinstallatie ","SOG"]
[1,"13.","13.12.12.","paalfundering - boorpalen/verbuisd - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks"]
[1,"13.","13.12.13.","paalfundering - boorpalen/verbuisd - afkappen paalkoppen ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW paalfundering - Afkappen paalkoppen","Stuks"]
[1,"13.","13.12.14.","paalfundering - boorpalen/verbuisd - sonische integriteitstesten ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW paalfundering - Sonische integriteitstesten","Stuks"]
[1,"13.","13.12.20.","paalfundering - boorpalen/steunvloeistof"]
[1,"13.","13.12.21.","paalfundering - boorpalen/steunvloeistof - werfinstallatie ","SOG"]
[1,"13.","13.12.22.","paalfundering - boorpalen/steunvloeistof - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks"]
[1,"13.","13.12.23.","paalfundering - boorpalen/steunvloeistof - afkappen paalkoppen ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW paalfundering - Afkappen paalkoppen","Stuks"]
[1,"13.","13.12.24.","paalfundering - boorpalen steunvloeistof - sonische integriteitstesten ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW paalfundering - Sonische integriteitstesten","Stuks"]
[1,"13.","13.13.","paalfundering - kokerpalen"]
[1,"13.","13.13.10.","paalfundering - kokerpalen/geschroefd"]
[1,"13.","13.13.11.","paalfundering - kokerpalen/geschroefd - werfinstallatie ","SOG"]
[1,"13.","13.13.12.","paalfundering - kokerpalen/geschroefd - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks"]
[1,"13.","13.13.13.","paalfundering - kokerpalen geschroefd - afkappen paalkoppen ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW paalfundering - Afkappen paalkoppen","Stuks"]
[1,"13.","13.13.14.","paalfundering - kokerpalen/geschroefd - sonische integriteitstesten ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW paalfundering - Sonische integriteitstesten","Stuks"]
[1,"13.","13.13.20.","paalfundering - kokerpalen geheid"]
[1,"13.","13.13.21.","paalfundering - kokerpalen geheid - werfinstallatie ","SOG"]
[1,"13.","13.13.22.","paalfundering - kokerpalen/geheid - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks"]
[1,"13.","13.13.23.","paalfundering - kokerpalen/geheid - afkappen paalkoppen ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW paalfundering - Afkappen paalkoppen","Stuks"]
[1,"13.","13.13.24.","paalfundering - kokerpalen/geheid - sonische integriteitstesten ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW paalfundering - Sonische integriteitstesten","Stuks"]
[1,"13.","13.14.","paalfundering - heipalen"]
[1,"13.","13.14.10.","paalfundering - heipalen/in de grond gevormd"]
[1,"13.","13.14.11.","paalfundering - heipalen/in de grond gevormd - werfinstallatie ","SOG"]
[1,"13.","13.14.12.","paalfundering - heipalen/in de grond gevormd - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks"]
[1,"13.","13.14.13.","paalfundering - heipalen/in de grond gevormd - afkappen paalkoppen ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW paalfundering - Afkappen paalkoppen","Stuks"]
[1,"13.","13.14.14.","paalfundering - heipalen/in de grond gevormd - sonische integriteitstesten ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW paalfundering - Sonische integriteitstesten","Stuks"]
[1,"13.","13.14.20.","paalfundering - heipalen/prefab beton"]
[1,"13.","13.14.21.","paalfundering - heipalen/prefab beton - werfinstallatie ","SOG"]
[1,"13.","13.14.22.","paalfundering - heipalen/prefab beton - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks"]
[1,"13.","13.14.23.","paalfundering - heipalen/prefab beton - afkappen paalkoppen ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW paalfundering - Afkappen paalkoppen","Stuks"]
[1,"13.","13.14.24.","paalfundering - heipalen/prefab beton - sonische integriteitstesten ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW paalfundering - Sonische integriteitstesten","Stuks"]
[1,"13.","13.20.","fundering op valse putten - algemeen"]
[1,"13.","13.21.","fundering op valse putten - ongewapend stortklaar beton ","FH/VH","m","TYPE 3","Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen"]
[1,"13.",null,null,null,"m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"13.",null,null,null,"m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"13.","13.22.","fundering op valse putten - gewapend stortklaar beton ","FH/VH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"13.",{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen"]
[1,"13.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[1,"13.",null,null,null,"m2","TYPE 3","Column",null,"Net Area"]
[1,"13.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"13.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[1,"13.",null,null,null,"m3","TYPE 3","Column",null,"Net Volume"]
[1,"13.",{"$nulls":5},"Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"13.",{"$nulls":4},"TYPE 5","Morph",null,"Net Volume"]
[1,"13.","13.23.","fundering op valse putten - gestabiliseerd zand ","FH/VH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"13.",{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen"]
[1,"13.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[1,"13.",null,null,null,"m2","TYPE 3","Column",null,"Net Area"]
[1,"13.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"13.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[1,"13.",null,null,null,"m3","TYPE 3","Column",null,"Net Volume"]
[1,"13.",{"$nulls":5},"Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"13.",{"$nulls":4},"TYPE 5","Morph",null,"Net Volume"]
[1,"13.","13.24.","fundering op valse putten - steenslag ","FH/VH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"13.",{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen"]
[1,"13.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[1,"13.",null,null,null,"m2","TYPE 3","Column",null,"Net Area"]
[1,"13.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"13.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[1,"13.",null,null,null,"m3","TYPE 3","Column",null,"Net Volume"]
[1,"13.",{"$nulls":5},"Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"13.",{"$nulls":4},"TYPE 5","Morph",null,"Net Volume"]
[1,"13.","13.30.","funderingsbalken - algemeen"]
[1,"13.","13.31.","funderingsbalken - stortklaar beton ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[1,"13.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"13.","13.40.","plaat op putten - algemeen"]
[1,"13.","13.41.","plaat op putten - gewapend stortklaar beton ","FH","m3","TYPE 3","Beam ",null,"Net Volume"]
[1,"13.",{"$nulls":5},"Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"13.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"13.","13.42.","plaat op putten - gewapend & gepolierd stortklaar beton ","FH","m3","TYPE 3","Beam ",null,"Net Volume"]
[1,"13.",{"$nulls":5},"Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"13.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"13.","13.50.","plaatfunderingen - algemeen"]
[1,"13.","13.51.","plaatfunderingen - gewapend stortklaar beton ","FH","m3","TYPE 3","Beam ",null,"Net Volume"]
[1,"13.",{"$nulls":5},"Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"13.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"13.","13.52.","plaatfunderingen - gewapend en gepolierd stortklaar beton ","FH","m3","TYPE 3","Beam ",null,"Net Volume"]
[1,"13.",{"$nulls":5},"Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"13.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"13.","13.60.","liftputten - algemeen"]
[1,"13.","13.61.","liftputten - stortklaar beton ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"13.","13.70.","doorbrekingen speciale funderingen - algemeen"]
[1,"13.","13.71.","doorbrekingen speciale funderingen - aansluitbocht ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"13.","13.72.","doorbrekingen speciale funderingen - doorvoermoffen voor buizen en kabels ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"13."]
[1,"14.","14.","ONDERGRONDSE WANDEN"]
[1,"14.","14.00.","ondergrondse wanden - algemeen"]
[1,"14.","14.10.","funderingswanden - algemeen"]
[1,"14.","14.11.","funderingswanden - beton"]
[1,"14.","14.11.10.","funderingswanden - beton/ter plaatse gestort"]
[1,"14.","14.11.11.","funderingswanden - beton/ter plaatse gestort - dikte 20 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume"]
[1,"14.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"14.","14.11.12.","funderingswanden - beton/ter plaatse gestort - dikte 25 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume"]
[1,"14.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"14.","14.11.13.","funderingswanden - beton/ter plaatse gestort - dikte 30 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume"]
[1,"14.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"14.","14.11.14.","funderingswanden - beton/ter plaatse gestort - dikte 35 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume"]
[1,"14.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"14.","14.11.20.","funderingswanden - beton/holle wanden"]
[1,"14.","14.11.21.","funderingswanden - beton/holle wanden - prefabelementen ","FH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[1,"14.",{"$nulls":5},"Wall",null,"Projected Area"]
[1,"14.","14.11.22.","funderingswanden - beton/holle wanden - vulbeton ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[1,"14.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"14.","14.11.30.","funderingswanden - beton/injectie van onvermijdelijke scheuren ","VH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[1,"14.","14.12.","funderingswanden - metselwerk"]
[1,"14.","14.12.01.","funderingswanden - metselwerk/mortel ","PM"]
[1,"14.","14.12.02.","funderingswanden - metselwerk/wapening ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[1,"14.","14.12.10.","funderingswanden - metselwerk/betonblokken"]
[1,"14.","14.12.11.","funderingswanden - metselwerk/betonblokken - muurdikte 29 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume"]
[1,"14.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"14.","14.12.12.","funderingswanden - metselwerk/betonblokken - muurdikte 35 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume"]
[1,"14.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"14.","14.12.13.","funderingswanden - metselwerk/betonblokken - muurdikte 39 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume"]
[1,"14.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"14.","14.12.14.","funderingswanden - metselwerk/betonblokken - muurdikte 40 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume"]
[1,"14.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"14.","14.20.","dragende kelderwanden - algemeen"]
[1,"14.","14.21.","dragende kelderwanden - beton"]
[1,"14.","14.21.10.","dragende kelderwanden - beton/ter plaatse gestort"]
[1,"14.","14.21.11.","dragende kelderwanden - beton/ter plaatse gestort - dikte 20 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume"]
[1,"14.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"14.","14.21.12.","dragende kelderwanden - beton/ter plaatse gestort - dikte 25 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume"]
[1,"14.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"14.","14.21.13.","dragende kelderwanden - beton/ter plaatse gestort - dikte 30 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume"]
[1,"14.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"14.","14.21.20.","dragende kelderwanden - beton/holle wanden"]
[1,"14.","14.21.21.","dragende kelderwanden - beton/holle wanden - prefabelementen ","FH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[1,"14.",{"$nulls":5},"Wall",null,"Projected Area"]
[1,"14.","14.21.22.","dragende kelderwanden - beton/holle wanden - vulbeton ","FH","m3","TYPE 3","Wall",null,"Net Volume"]
[1,"14.","14.21.30.","dragende kelderwanden - beton/injectie van onvermijdelijke scheuren ","VH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[1,"14.","14.22.","dragende kelderwanden - metselwerk"]
[1,"14.","14.22.01.","dragende kelderwanden - metselwerk/mortel ","PM"]
[1,"14.","14.22.02.","dragende kelderwanden - metselwerk/wapening ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[1,"14.","14.22.03.","dragende kelderwanden - metselwerk/lateien ","PM"]
[1,"14.","14.22.10.","dragende kelderwanden - metselwerk/betonblokken"]
[1,"14.","14.22.11.","dragende kelderwanden - metselwerk/betonblokken - muurdikte 14 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume"]
[1,"14.","14.22.12.","dragende kelderwanden - metselwerk/betonblokken - muurdikte 19 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume"]
[1,"14.","14.22.13.","dragende kelderwanden - metselwerk/betonblokken - muurdikte 29 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume"]
[1,"14.","14.22.20.","dragende kelderwanden - metselwerk/baksteen"]
[1,"14.","14.22.21.","dragende kelderwanden - metselwerk/baksteen - muurdikte 14 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume"]
[1,"14.","14.22.22.","dragende kelderwanden - metselwerk/baksteen - muurdikte 19 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume"]
[1,"14.","14.22.30.","dragende kelderwanden - metselwerk/kalkzandsteen"]
[1,"14.","14.22.31.","dragende kelderwanden - metselwerk/kalkzandsteen - muurdikte 15 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume"]
[1,"14.","14.22.32.","dragende kelderwanden - metselwerk/kalkzandsteen - muurdikte 17,5 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume"]
[1,"14.","14.22.33.","dragende kelderwanden - metselwerk/kalkzandsteen - muurdikte 21,5 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume"]
[1,"14.","14.30.","geprefabriceerde kelders - algemeen"]
[1,"14.","14.31.","geprefabriceerde kelders - gedeeltelijke onderkeldering ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"14.",{"$nulls":5},"Wall",null,"Net Volume"]
[1,"14.",null,null,null,"st","TYPE 3","Slab",null,"Stuks"]
[1,"14.","14.40.","waterdichting ondergrondse wanden - algemeen"]
[1,"14.","14.41.","waterdichting ondergrondse wanden - mineraliserende mortel ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[1,"14.","14.42.","waterdichting ondergrondse wanden - gemodificeerde cementmortel ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[1,"14.","14.43.","waterdichting ondergrondse wanden - bitumenemulsie ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[1,"14.","14.44.","waterdichting ondergrondse wanden - noppenbanen ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[1,"14.","14.50.","doorbrekingen ondergrondse wanden - algemeen"]
[1,"14.","14.51.","doorbrekingen ondergrondse wanden - aansluitbocht ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"14.","14.52.","doorbrekingen ondergrondse wanden - doorvoermoffen buizen en kabels ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"14.","14.60.","verluchtingselementen ondergrondse wanden - algemeen"]
[1,"14.","14.61.","verluchtingselementen ondergrondse wanden - telescopische kokers ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"14.",null,null,"PM"]
[1,"14."]
[1,"15.","15.","VLOERLAGEN ONDERBOUW"]
[1,"15.","15.00.","vloerlagen onderbouw - algemeen"]
[1,"15.","15.10.","zuiverheidslagen - algemeen"]
[1,"15.","15.11.","zuiverheidslagen - stortklaar beton ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"15.",null,null,null,"m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"15.","15.20.","draagvloeren op volle grond - algemeen"]
[1,"15.","15.21.","draagvloeren op volle grond - stortklaar gewapend beton ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"15.","15.30.","vochtwerende lagen - algemeen"]
[1,"15.","15.31.","vochtwerende lagen - folies"]
[1,"15.","15.31.10.","vochtwerende lagen - folies/PE ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"15.",null,null,"PM",null,"Geen"]
[1,"15.","15.31.20.","vochtwerende lagen - folies/PVC ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"15.",null,null,"PM",null,"Geen"]
[1,"15.","15.31.30.","vochtwerende lagen - folies/PIB ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"15.",null,null,"PM",null,"Geen"]
[1,"15.","15.32.","vochtwerende lagen - banen"]
[1,"15.","15.32.10.","vochtwerende lagen - banen/HDPE ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"15.",null,null,"PM"]
[1,"15.","15.33.","vochtwerende lagen - bitumenglasvlies ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"15.",null,null,"PM"]
[1,"15."]
[1,"16.","16.","THERMISCHE ISOLATIE ONDERBOUW"]
[1,"16.","16.00.","thermische isolatie onderbouw - algemeen"]
[1,"16.","16.10.","isolatieplaten op volle grond - algemeen"]
[1,"16.","16.11.","isolatieplaten op volle grond - XPS"]
[1,"16.","16.11.10.","isolatieplaten op volle grond - XPS/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"16.","16.11.20.","isolatieplaten op volle grond - XPS/12 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"16.","16.12.","isolatieplaten op volle grond - PUR of PIR"]
[1,"16.","16.12.10.","isolatieplaten op volle grond - PUR of PIR/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"16.","16.12.20.","isolatieplaten op volle grond - PUR of PIR/12 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"16.","16.13.","isolatieplaten op volle grond - EPS"]
[1,"16.","16.13.10.","isolatieplaten op volle grond - EPS/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"16.","16.13.20.","isolatieplaten op volle grond - EPS/12 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[1,"16.","16.20.","perimeterisolatie - algemeen"]
[1,"16.","16.21.","perimeterisolatie - XPS"]
[1,"16.","16.21.10.","perimeterisolatie - XPS/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[1,"16.",{"$nulls":5},"Beam",null,"Oppervlakte middenas wand"]
[1,"16.","16.21.20.","perimeterisolatie - XPS/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[1,"16.",{"$nulls":5},"Beam",null,"Oppervlakte middenas wand"]
[1,"16.","16.22.","perimeterisolatie - PUR of PIR"]
[1,"16.","16.22.10.","perimeterisolatie - PUR of PIR/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[1,"16.",{"$nulls":5},"Beam",null,"Oppervlakte middenas wand"]
[1,"16.","16.22.20.","perimeterisolatie - PUR of PIR/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[1,"16.",{"$nulls":5},"Beam",null,"Oppervlakte middenas wand"]
[1,"16."]
[1,"17.","17.","ONDERGRONDSE LEIDINGEN"]
[1,"17.","17.00.","ondergrondse leidingen - algemeen"]
[1,"17.","17.10.","rioolbuizen - algemeen"]
[1,"17.","17.11.","rioolbuizen - beton"]
[1,"17.","17.11.10.","rioolbuizen - beton ongewapend"]
[1,"17.","17.11.11.","rioolbuizen - beton/ongewapend - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.11.12.","rioolbuizen - beton/ongewapend - diam 250 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.11.13.","rioolbuizen - beton/ongewapend - diam 300 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.11.14.","rioolbuizen - beton/ongewapend - diam 400 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.11.15.","rioolbuizen - beton/ongewapend - diam 500 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.11.16.","rioolbuizen - beton/ongewapend - diam 600 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.11.20.","rioolbuizen - beton gewapend"]
[1,"17.","17.11.21.","rioolbuizen - beton/gewapend - diam 300 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.11.22.","rioolbuizen - beton/gewapend - diam 400 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.11.23.","rioolbuizen - beton/gewapend - diam 500 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.11.24.","rioolbuizen - beton/gewapend - diam 600 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.11.25.","rioolbuizen - beton/gewapend - diam 800 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.","rioolbuizen - kunststof"]
[1,"17.","17.12.10.","rioolbuizen - kunststof/PVC"]
[1,"17.","17.12.11.","rioolbuizen - kunststof/PVC - diam 110 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.12.","rioolbuizen - kunststof/PVC - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.13.","rioolbuizen - kunststof/PVC - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.14.","rioolbuizen - kunststof/PVC - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.15.","rioolbuizen - kunststof/PVC - diam 315 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.16.","rioolbuizen - kunststof/PVC - diam 400 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.20.","rioolbuizen - kunststof/PE"]
[1,"17.","17.12.21.","rioolbuizen - kunststof/PE - diam 110 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.22.","rioolbuizen - kunststof/PE - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.23.","rioolbuizen - kunststof/PE - diam 140 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.24.","rioolbuizen - kunststof/PE - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.25.","rioolbuizen - kunststof/PE - diam 180 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.26.","rioolbuizen - kunststof/PE - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.27.","rioolbuizen - kunststof/PE - diam 225 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.28.","rioolbuizen - kunststof/PE - diam 250 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.30.","rioolbuizen - kunststof/PP"]
[1,"17.","17.12.31.","rioolbuizen - kunststof/PP - diam 110 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.32.","rioolbuizen - kunststof/PP - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.33.","rioolbuizen - kunststof/PP - diam 140 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.34.","rioolbuizen - kunststof/PP - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.35.","rioolbuizen - kunststof/PP - diam 180 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.36.","rioolbuizen - kunststof/PP - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.37.","rioolbuizen - kunststof/PP - diam 225 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.12.38.","rioolbuizen - kunststof/PP - diam 250 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.",{"$nulls":4},"TYPE 5","Object","MEP"]
[1,"17.","17.20.","draineerbuizen - algemeen"]
[1,"17.","17.21.","draineerbuizen - poreus beton"]
[1,"17.","17.21.10.","draineerbuizen - poreus beton/diam 80 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.21.20.","draineerbuizen - poreus beton/diam 100 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.21.30.","draineerbuizen - poreus beton/diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.21.40.","draineerbuizen - poreus beton/diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.21.50.","draineerbuizen - poreus beton/diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.22.","draineerbuizen - vezelcement"]
[1,"17.","17.22.10.","draineerbuizen - poreus beton/diam 80 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.22.20.","draineerbuizen - poreus beton/diam 100 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.22.30.","draineerbuizen - poreus beton/diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.22.40.","draineerbuizen - poreus beton/diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.22.50.","draineerbuizen - poreus beton/diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.23.","draineerbuizen - kunststof"]
[1,"17.","17.23.10.","draineerbuizen - kunststof/PVC"]
[1,"17.","17.23.11.","draineerbuizen - kunststof/PVC - diam 50 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.23.12.","draineerbuizen - kunststof/PVC - diam 65 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.23.13.","draineerbuizen - kunststof/PVC - diam 80 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.23.14.","draineerbuizen - kunststof/PVC - diam 100 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.23.15.","draineerbuizen - kunststof/PVC - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.23.16.","draineerbuizen - kunststof/PVC - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.23.17.","draineerbuizen - kunststof/PVC - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.23.20.","draineerbuizen - kunststof/PE"]
[1,"17.","17.23.21.","draineerbuizen - kunststof/PE - diam 50 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.23.22.","draineerbuizen - kunststof/PE - diam 60 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.23.23.","draineerbuizen - kunststof/PE - diam 80 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.23.24.","draineerbuizen - kunststof/PE - diam 100 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.23.25.","draineerbuizen - kunststof/PE - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.23.26.","draineerbuizen - kunststof/PE - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.23.27.","draineerbuizen - kunststof/PE - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.30.","toezichtputten - algemeen"]
[1,"17.","17.31.","toezichtputten - metselwerk ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.32.","toezichtsputten - beton"]
[1,"17.","17.32.10.","toezichtsputten - beton/stortklaar ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.32.20.","toezichtsputten - beton/prefab ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.33.","toezichtputten - vezelcement ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.34.","toezichtsputten - kunststof"]
[1,"17.","17.34.10.","toezichtputten - kunststof/PVC ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.34.20.","toezichtputten - kunststof/PE ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.34.30.","toezichtputten - kunststof/polyester ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.40.","ontvangtoestellen - algemeen"]
[1,"17.","17.41.","ontvangtoestellen - buitenontvanger"]
[1,"17.","17.41.10.","ontvangtoestellen - buitenontvanger/met klok ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.41.20.","ontvangtoestellen - buitenontvanger/met korf ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.42.","ontvangtoestellen - geulen"]
[1,"17.","17.42.10.","ontvangtoestellen - geulen/beton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.42.20.","ontvangtoestellen - geulen/glasvezelbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.42.30.","ontvangtoestellen - geulen/polyesterbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[1,"17.","17.43.","ontvangtoestellen - straatkolken ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.44.","ontvangtoestellen - prefab pompputten ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.50.","putdeksels en roosters - algemeen"]
[1,"17.","17.51.","putdeksels en roosters - enkel deksel ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.52.","putdeksels en roosters - dubbel deksel ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.53.","putdeksels en roosters - geulroosters ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[1,"17.","17.60.","afvalwaterbehandeling - algemeen"]
[1,"17.","17.61.","afvalwaterbehandeling - septische putten ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.70.","regenwaterbehandeling - algemeen"]
[1,"17.","17.71.","regenwaterbehandeling - regenwaterputten"]
[1,"17.","17.71.10.","regenwaterbehandeling - regenwaterputten/beton ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.71.20.","regenwaterbehandeling - regenwaterputten/HDPE ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.71.30.","regenwaterbehandeling - regenwaterputten/polyester ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.71.40.","regenwaterbehandeling - regenwaterputten/metselwerk ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.72.","regenwaterbehandeling - hergebruik regenwater ","PM"]
[1,"17.","17.73.","regenwaterbehandeling - voorfilters ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.74.","regenwaterbehandeling - overloop en terugslagklep ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.75.","regenwaterbehandeling - infiltratievoorzieningen"]
[1,"17.","17.75.10.","regenwaterbehandeling - infiltratievoorzieningen/infiltratieputten ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.75.20.","regenwaterbehandeling - infiltratievoorzieningen/infiltratieblokken ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.75.30.","regenwaterbehandeling - infiltratievoorzieningen/infiltratiebuizen ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.80.","aansluitingen - algemeen"]
[1,"17.","17.81.","aansluitingen - openbare riolering ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17.","17.82.","aansluitingen - doorvoer- en wachtbuizen ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[1,"17.",null,null,"PM"]
[1,"17.","17.83.","aansluitingen - wachtput ","FH","st","TYPE 5","Object",null,"Stuks"]
[1,"17."]
[2,"20.","20.","METSELWERK"]
[2,"20.","20.00.","metselwerken - algemeen"]
[2,"20.","20.01.","metselwerken - ter plaatse gemetst"]
[2,"20.","20.02.","metselwerken - prefab"]
[2,"20.","20.10.","materialen - algemeen"]
[2,"20.","20.11.","materialen - metselmortel"]
[2,"20.","20.11.10.","materialen - metselmortel/voor algemene toepassing (G) ","PM"]
[2,"20.","20.11.20.","materialen - metselmortel/lijmmortel (T) ","PM"]
[2,"20.","20.11.30.","materialen - metselmortel/lichtgewicht metselmortel (L) ","PM"]
[2,"20.","20.12.","materialen - hulpstukken"]
[2,"20.","20.12.10.","materialen - hulpstukken/spouwankers"]
[2,"20.","20.12.11.","materialen - hulpstukken/spouwankers - gewone spouwankers ","PM"]
[2,"20.","20.12.12.","materialen - hulpstukken/spouwankers - slag- en schroefankers met isolatieplug ","PM"]
[2,"20.","20.12.13.","materialen - hulpstukken/spouwankers - akoestisch spouwanker ","PM"]
[2,"20.","20.12.20.","materialen - hulpstukken/lateien"]
[2,"20.","20.12.21.","materialen - hulpstukken/lateien - beton ","PM"]
[2,"20.","20.12.22.","materialen - hulpstukken/lateien - staal ","PM"]
[2,"20.","20.12.23.","materialen - hulpstukken/lateien - bekistingsmetselstenen ","PM"]
[2,"20.","20.12.30.","materialen - hulpstukken/waterkering ","PM"]
[2,"20.","20.12.40.","materialen - hulpstukken/wapening ","FH","m","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Lengte (cm) in bij de Object settings"]
[2,"20.","20.12.50.","materialen - hulpstukken/akoestische stroken ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"20.",{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Lengte (cm) in bij de Object settings"]
[2,"20.","20.13.","materialen - kimblokken"]
[2,"20.","20.13.10.","materialen - kimblokken/cellenbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"20.",{"$nulls":5},"Wall",null,"Lengte volgens eigen middenas"]
[2,"20.","20.13.20.","materialen - kimblokken/samengestelde blok ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"20.",{"$nulls":5},"Wall",null,"Lengte volgens eigen middenas"]
[2,"20.","20.13.30.","materialen - kimblokken/thermisch verbeterde steen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"20.",{"$nulls":5},"Wall",null,"Lengte volgens eigen middenas"]
[2,"20.","20.13.40.","materialen - kimblokken/cellenglas ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"20.",{"$nulls":5},"Wall",null,"Lengte volgens eigen middenas"]
[2,"20.","20.20.","binnenspouwblad - algemeen"]
[2,"20.","20.21.","binnenspouwblad - snelbouw"]
[2,"20.","20.21.10.","binnenspouwblad - snelbouw/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.21.20.","binnenspouwblad - snelbouw/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.22.","binnenspouwblad - kalkzandsteen"]
[2,"20.","20.22.10.","binnenspouwblad - kalkzandsteen/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.22.20.","binnenspouwblad - kalkzandsteen/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.22.30.","binnenspouwblad - kalkzandsteen/dikte 21,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.22.40.","binnenspouwblad - kalkzandsteen/dikte 30 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.23.","binnenspouwblad - betonsteen met gewone granulaten"]
[2,"20.","20.23.10.","binnenspouwblad - betonsteen met gewone granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.23.20.","binnenspouwblad - betonsteen met gewone granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.24.","binnenspouwblad - betonsteen met lichte granulaten"]
[2,"20.","20.24.10.","binnenspouwblad - betonsteen met lichte granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.24.20.","binnenspouwblad - betonsteen met lichte granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.25.","binnenspouwblad - cellenbeton"]
[2,"20.","20.25.10.","binnenspouwblad - cellenbeton/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.25.20.","binnenspouwblad - cellenbeton/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.25.30.","binnenspouwblad - cellenbeton/dikte 20 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.25.40.","binnenspouwblad - cellenbeton/dikte 24 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.25.50.","binnenspouwblad - cellenbeton/dikte 30 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.25.60.","binnenspouwblad - cellenbeton/dikte 36,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.25.70.","binnenspouwblad - cellenbeton/dikte 40 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.25.80.","binnenspouwblad - cellenbeton/dikte 50 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.30.","woningscheidende wand - algemeen"]
[2,"20.","20.31.","woningscheidende wand - snelbouw"]
[2,"20.","20.31.10.","woningscheidende wand - snelbouw/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.31.20.","woningscheidende wand - snelbouw/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.32.","woningscheidende wand - kalkzandsteen"]
[2,"20.","20.32.10.","woningscheidende wand - kalkzandsteen/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.32.20.","woningscheidende wand - kalkzandsteen/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.32.30.","woningscheidende wand - kalkzandsteen/dikte 21,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.32.40.","woningscheidende wand - kalkzandsteen/dikte 30 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.33.","woningscheidende wand - betonsteen met gewone granulaten"]
[2,"20.","20.33.10.","woningscheidende wand - betonsteen met gewone granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.33.20.","woningscheidende wand - betonsteen met gewone granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.34.","woningscheidende wand - betonsteen met lichte granulaten"]
[2,"20.","20.34.10.","woningscheidende wand - betonsteen met lichte granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.34.20.","woningscheidende wand - betonsteen met lichte granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.35.","woningscheidende wand - cellenbeton"]
[2,"20.","20.35.10.","woningscheidende wand - cellenbeton/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.35.20.","woningscheidende wand - cellenbeton/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.35.30.","woningscheidende wand - cellenbeton/dikte 20 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.35.40.","woningscheidende wand - cellenbeton/dikte 24 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.40.","dragende binnenmuur - algemeen"]
[2,"20.","20.41.","dragende binnenmuur - snelbouw"]
[2,"20.","20.41.10.","dragende binnenmuur - snelbouw/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.41.20.","dragende binnenmuur - snelbouw/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.42.","dragende binnenmuur - kalkzandsteen"]
[2,"20.","20.42.10.","dragende binnenmuur - kalkzandsteen/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.42.20.","dragende binnenmuur - kalkzandsteen/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.42.30.","dragende binnenmuur - kalkzandsteen/dikte 21,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.43.","dragende binnenmuur - betonsteen met gewone granulaten"]
[2,"20.","20.43.10.","dragende binnenmuur - betonsteen met gewone granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.43.20.","dragende binnenmuur - betonsteen met gewone granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.44.","dragende binnenmuur - betonsteen met lichte granulaten"]
[2,"20.","20.44.10.","dragende binnenmuur - betonsteen met lichte granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.44.20.","dragende binnenmuur - betonsteen met lichte granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.45.","dragende binnenmuur - cellenbeton"]
[2,"20.","20.45.10.","dragende binnenmuur - cellenbeton/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.45.20.","dragende binnenmuur - cellenbeton/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.45.30.","dragende binnenmuur - cellenbeton/dikte 20 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.45.40.","dragende binnenmuur - cellenbeton/dikte 24 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.50.","niet-dragende binnenmuur - algemeen"]
[2,"20.","20.51.","niet-dragende binnenmuur - snelbouw"]
[2,"20.","20.51.10.","niet-dragende binnenmuur - snelbouw/dikte 9 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.51.20.","niet-dragende binnenmuur - snelbouw/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.52.","niet-dragende binnenmuur - kalkzandsteen"]
[2,"20.","20.52.10.","niet-dragende binnenmuur - kalkzandsteen/dikte 10 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.52.20.","niet-dragende binnenmuur - kalkzandsteen/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.53.","niet-dragende binnenmuur - betonsteen met lichte granulaten"]
[2,"20.","20.53.10.","niet-dragende binnenmuur - betonsteen met lichte granulaten/dikte 9 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.53.20.","niet-dragende binnenmuur - betonsteen met lichte granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.54.","niet-dragende binnenmuur - cellenbeton"]
[2,"20.","20.54.10.","niet-dragende binnenmuur - cellenbeton/dikte 7 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.54.20.","niet-dragende binnenmuur - cellenbeton/dikte 10 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.54.30.","niet-dragende binnenmuur - cellenbeton/dikte 11,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.55.","niet-dragende binnenmuur - gipsblokken"]
[2,"20.","20.55.10.","niet-dragende binnenmuur - gipsblokken/dikte 6 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.55.20.","niet-dragende binnenmuur - gipsblokken/dikte 7 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.55.30.","niet-dragende binnenmuur - gipsblokken/dikte 8 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.55.40.","niet-dragende binnenmuur - gipsblokken/dikte 10 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume"]
[2,"20.","20.60.","renovatiewerken - algemeen"]
[2,"20.","20.61.","renovatiewerken - behandeling tegen opstijgend vocht"]
[2,"20.","20.61.10.","renovatiewerken - behandeling tegen opstijgend vocht/injecteren ","FH/VH","m","TYPE 3","Wall",null,"Reference line length"]
[2,"20.",{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Lengte (cm) in bij de Object settings"]
[2,"20.","20.61.20.","renovatiewerken - behandeling tegen opstijgend vocht/plaatsen dichtingsmembraan ","FH/VH","m","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Lengte (cm) in bij de Object settings"]
[2,"20.",null,null,null,"m","TYPE 3","Wall",null,"Reference line length"]
[2,"20."]
[2,"21.","21.","SPOUWMUURISOLATIE"]
[2,"21.","21.00.","spouwmuurisolatie - algemeen"]
[2,"21.","21.10.","spouwmuurisolatie buitenspouwblad - algemeen"]
[2,"21.","21.11.","spouwmuurisolatie buitenspouwblad - MW"]
[2,"21.","21.11.10.","spouwmuurisolatie buitenspouwblad - MW / 12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[2,"21.","21.11.20.","spouwmuurisolatie buitenspouwblad - MW / 14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[2,"21.","21.12.","spouwmuurisolatie buitenspouwblad - PUR of PIR"]
[2,"21.","21.12.10.","spouwmuurisolatie buitenspouwblad - PUR of PIR/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[2,"21.","21.12.20.","spouwmuurisolatie buitenspouwblad - PUR of PIR/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[2,"21.","21.13.","spouwmuurisolatie buitenspouwblad - PF"]
[2,"21.","21.13.10.","spouwmuurisolatie buitenspouwblad - PF/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[2,"21.","21.13.20.","spouwmuurisolatie buitenspouwblad - PF/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[2,"21.","21.14.","spouwmuurisolatie buitenspouwblad - XPS"]
[2,"21.","21.14.10.","spouwmuurisolatie buitenspouwblad - XPS/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[2,"21.","21.14.20.","spouwmuurisolatie buitenspouwblad - XPS/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[2,"21.","21.15.","spouwmuurisolatie buitenspouwblad - EPS"]
[2,"21.","21.15.10.","spouwmuurisolatie buitenspouwblad - EPS/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[2,"21.","21.15.20.","spouwmuurisolatie buitenspouwblad - EPS/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[2,"21.","21.20.","spouwmuurisolatie woningscheidende wand - algemeen"]
[2,"21.","21.21.","spouwmuurisolatie woningscheidende wand - MW"]
[2,"21.","21.21.10.","spouwmuurisolatie woningscheidende wand - MW/4 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[2,"21.","21.21.20.","spouwmuurisolatie woningscheidende wand - MW/5 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[2,"21.","21.22.","spouwmuurisolatie woningscheidende wand - XPS"]
[2,"21.","21.22.10.","spouwmuurisolatie woningscheidende wand - XPS/2 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[2,"21.","21.22.20.","spouwmuurisolatie woningscheidende wand - XPS/3 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[2,"21.","21.23.","spouwmuurisolatie woningscheidende wand - PUR of PIR"]
[2,"21.","21.23.10.","spouwmuurisolatie woningscheidende wand - PUR of PIR/3 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[2,"21.","21.23.20.","spouwmuurisolatie woningscheidende wand - PUR of PIR/4 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[2,"21.","21.30.","spouwmuurisolatie navulling - algemeen"]
[2,"21.","21.31.","spouwmuurisolatie navulling - MW ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[2,"21.","21.32.","spouwmuurisolatie navulling - PUR ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[2,"21.","21.33.","spouwmuurisolatie navulling - EPS ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[2,"21."]
[2,"22.","22.","GEVELMETSELWERK"]
[2,"22.","22.00.","gevelmetselwerken - algemeen"]
[2,"22.","22.01.","algemeen - ter plaatse gemetst gevelmetselwerk"]
[2,"22.","22.02.","algemeen - prefab gevelmetselwerk"]
[2,"22.","22.10.","materialen - algemeen"]
[2,"22.","22.11.","materialen - mortel"]
[2,"22.","22.11.10.","materialen - mortel/metselmortel"]
[2,"22.","22.11.11.","materialen - mortel/metselmortel - voor algemene toepassing ","PM"]
[2,"22.","22.11.12.","materialen - mortel/metselmortel - dunbedmortel ","PM"]
[2,"22.","22.11.13.","materialen - mortel/metselmortel - lijmmortel ","PM"]
[2,"22.","22.11.20.","materialen - mortel/voegmortel"]
[2,"22.","22.12.","materialen - spouwankers ","PM"]
[2,"22.","22.13.","materialen - waterkering ","PM"]
[2,"22.","22.14.","materialen - wapening ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[2,"22.","22.20.","gevelstenen - algemeen"]
[2,"22.","22.21.","gevelstenen - baksteen"]
[2,"22.","22.21.10.","gevelstenen - baksteen/strengpersstenen ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[2,"22.","22.21.20.","gevelstenen - bakstenen/handvorm- en vormbakstenen ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[2,"22.","22.22.","gevelstenen - betonsteen ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[2,"22.","22.30.","renovatiewerken - algemeen"]
[2,"22.","22.31.","renovatiewerken - herstelling en aanpassing bestaand gevelmetselwerk ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[2,"22."]
[2,"23.","23.","DORPELS, PLINTEN EN DEKSTENEN"]
[2,"23.","23.00.","dorpels, plinten en dekstenen - algemeen"]
[2,"23.","23.01.","algemeen - blauwe hardsteen"]
[2,"23.","23.02.","algemeen - beton"]
[2,"23.","23.03.","algemeen - vezelcement"]
[2,"23.","23.10.","raam- en deurdorpels - algemeen"]
[2,"23.","23.11.","raam- en deurdorpels - blauwe hardsteen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"23.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel"]
[2,"23.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel"]
[2,"23.",null,null,null,"m2","TYPE 3","Beam",null,"Net Area"]
[2,"23.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","breedte dagkant * diepte dorpel"]
[2,"23.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Area"]
[2,"23.",null,null,null,"m3","TYPE 3","Beam",null,"Net Volume"]
[2,"23.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","breedte dagkant * diepte dorpel * dikte dorpel"]
[2,"23.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume"]
[2,"23.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[2,"23.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Stuks"]
[2,"23.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Stuks"]
[2,"23.","23.12.","raam- en deurdorpels - prefabbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"23.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel"]
[2,"23.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel"]
[2,"23.",null,null,null,"m3","TYPE 3","Beam",null,"Net Volume"]
[2,"23.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","breedte dagkant * diepte dorpel * dikte dorpel"]
[2,"23.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume"]
[2,"23.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[2,"23.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Stuks"]
[2,"23.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Stuks"]
[2,"23.","23.13.","raam- en deurdorpels - vezelcement ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"23.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel"]
[2,"23.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel"]
[2,"23.","23.14.","raam- en deurdorpels - gevelsteen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"23.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel"]
[2,"23.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel"]
[2,"23.",null,null,null,"m3","TYPE 3","Beam",null,"Net Volume"]
[2,"23.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","breedte dagkant * diepte dorpel * dikte dorpel"]
[2,"23.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume"]
[2,"23.","23.20.","garagepoortdorpels - algemeen"]
[2,"23.","23.21.","garagepoortdorpels - blauwe hardsteen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"23.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel"]
[2,"23.",null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","breedte dagkant * diepte dorpel"]
[2,"23.",null,null,null,"m3","TYPE 3","Beam",null,"Net Volume"]
[2,"23.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","breedte dagkant * diepte dorpel * dikte dorpel"]
[2,"23.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[2,"23.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","Stuks"]
[2,"23.",null,null,null,"        ","TYPE 3","Beam",null,"Net Area"]
[2,"23.","23.22.","garagepoortdorpels - prefabbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"23.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel"]
[2,"23.",null,null,null,"m3","TYPE 3","Beam",null,"Net Volume"]
[2,"23.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","breedte dagkant * diepte dorpel * dikte dorpel"]
[2,"23.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[2,"23.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","Stuks"]
[2,"23.","23.30.","gevelplinten - algemeen"]
[2,"23.","23.31.","gevelplinten - blauwe hardsteen ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[2,"23.",{"$nulls":5},"Wall",null,"Net Volume"]
[2,"23.","23.32.","gevelplinten - sierbeton ","FH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[2,"23.",{"$nulls":5},"Wall",null,"Projected Area"]
[2,"23.","23.33.","gevelplinten - vezelcement ","FH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[2,"23.",{"$nulls":5},"Wall ",null,"Projected Area"]
[2,"23.","23.40.","omkaderingselementen - algemeen"]
[2,"23.","23.41.","omkaderingselementen - blauwe steen ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[2,"23.",{"$nulls":5},"Column",null,"Net Volume"]
[2,"23.",{"$nulls":4},"TYPE 5","Morph",null,"Net Volume"]
[2,"23.","23.50.","muurdekstenen - algemeen"]
[2,"23.","23.51.","muurdekstenen - blauwe steen ","FH","m3","TYPE 3","Beam",null,"Net Volume","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"23.",{"$nulls":5},"Slab",null,"Net Volume "]
[2,"23.","23.52.","muurdekstenen - prefabbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"23.",{"$nulls":5},"Slab",null,"Omtrek vloer zonder openingen"]
[2,"23.","23.53.","muurdekstenen - vezelcement ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"23.",{"$nulls":5},"Slab",null,"Omtrek vloer zonder openingen"]
[2,"23.","23.60.","schoorsteendekplaten - algemeen"]
[2,"23.","23.61.","schoorsteendekplaten - blauwe steen ","FH","st","TYPE 3","Beam",null,"Stuks"]
[2,"23.",{"$nulls":5},"Slab",null,"Stuks"]
[2,"23.","23.62.","schoorsteendekplaten - beton ","FH","st","TYPE 3","Beam",null,"Stuks"]
[2,"23.",{"$nulls":5},"Slab",null,"Stuks"]
[2,"23.","23.63.","schoorsteendekplaten - vezelcement ","FH","st","TYPE 3","Beam",null,"Stuks"]
[2,"23.",{"$nulls":5},"Slab",null,"Stuks"]
[2,"23."]
[2,"24.","24.","RUWBOUWKANALEN"]
[2,"24.","24.00.","ruwbouw kanalen - algemeen"]
[2,"24.","24.10.","modulaire ruwbouwkanalen - algemeen"]
[2,"24.","24.11.","modulaire ruwbouwkanalen - beton "]
[2,"24.","24.11.10.","modulaire ruwbouwkanalen - beton/rookgasafvoer ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"24.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[2,"24.",null,null,null,"st","TYPE 3","Column",null,"Stuks"]
[2,"24.",{"$nulls":4},"TYPE 5","Object",null,"Stuks"]
[2,"24.","24.11.20.","modulaire ruwbouwkanalen - beton/ventilatie ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"24.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[2,"24.",null,null,null,"st","TYPE 3","Column",null,"Stuks"]
[2,"24.",{"$nulls":4},"TYPE 5","Object",null,"Stuks"]
[2,"24.","24.12.","modulaire ruwbouwkanalen - keramische blokken"]
[2,"24.","24.12.10.","modulaire ruwbouwkanalen - keramische blokken/rookgasafvoer ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"24.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[2,"24.",null,null,null,"st","TYPE 3","Column",null,"Stuks"]
[2,"24.",{"$nulls":4},"TYPE 5","Object",null,"Stuks"]
[2,"24.","24.12.20.","modulaire ruwbouwkanalen - keramische blokken/ventilatie ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"24.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[2,"24.",null,null,null,"st","TYPE 3","Column",null,"Stuks"]
[2,"24.",{"$nulls":4},"TYPE 5","Object",null,"Stuks"]
[2,"24."]
[2,"25.","25.","STRUCTUURELEMENTEN HOUT"]
[2,"25.","25.00.","structuurelementen hout - algemeen"]
[2,"25.","25.01.","algemeen - stabiliteitsstudie ","PM"]
[2,"25.","25.02.","algemeen - opleg- en bevestigingsmaterialen"]
[2,"25.","25.02.10.","algemeen - opleg- en bevestigingsmaterialen/metalen schoenen ","PM"]
[2,"25.","25.02.20.","algemeen - opleg- en bevestigingsmaterialen/schroeven, nagels en nieten ","PM"]
[2,"25.","25.02.30.","algemeen - opleg- en bevestigingsmaterialen/lijmen ","PM"]
[2,"25.","25.02.40.","algemeen - opleg- en bevestigingsmaterialen/metalen hechtplaten ","PM"]
[2,"25.","25.10.","balken - algemeen"]
[2,"25.","25.11.","balken - massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[2,"25.","25.12.","balken - LVL ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[2,"25.","25.13.","balken - lichte samengestelde liggers ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[2,"25.","25.14.","balken - gelijmd gelamineerd hout (GL) ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[2,"25.","25.20.","kolommen - algemeen"]
[2,"25.","25.21.","kolommen - massief hout ","FH","m3","TYPE 3","Column",null,"Net Volume"]
[2,"25.","25.22.","kolommen - LVL ","FH","m3","TYPE 3","Column",null,"Net Volume"]
[2,"25.","25.23.","kolommen - gelijmd gelamineerd hout"]
[2,"25.","25.30.","vloeren - algemeen"]
[2,"25.","25.31.","vloeren - roostering met beplating"]
[2,"25.","25.31.10.","vloeren - roostering met beplating/balken"]
[2,"25.","25.31.11.","vloeren - roostering met beplating/balken - massief hout ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"25.","25.31.12.","vloeren - roostering met beplating/balken - LVL ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"25.","25.31.13.","vloeren - roostering met beplating/balken - lichte samengestelde liggers ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"25.","25.31.14.","vloeren - roostering met beplating/balken - gelijmd gelamineerd hout ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"25.","25.31.20.","vloeren - roostering met beplating/beplating"]
[2,"25.","25.31.21.","vloeren - roostering met beplating/beplating - OSB ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"25.","25.31.22.","vloeren - roostering met beplating/beplating - spaanplaat ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"25.","25.31.23.","vloeren - roostering met beplating/beplating - LVL ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"25."]
[2,"26.","26.","STRUCTUURELEMENTEN BETON"]
[2,"26.","26.00.","structuurelementen gewapend beton - algemeen"]
[2,"26.","26.01.","algemeen - stabiliteitsstudie ","PM"]
[2,"26.","26.10.","materialen - algemeen"]
[2,"26.","26.11.","materialen - wapening"]
[2,"26.","26.11.10.","materialen - wapening/staven en netten"]
[2,"26.","26.11.11.","materialen - wapening/staven en netten - staven ","FH","kg","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Gewicht (kg) in bij Settings van het Object"]
[2,"26.","26.11.12.","materialen - wapening/staven en netten - netten ","FH","kg","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Gewicht (kg) in bij Settings van het Object"]
[2,"26.","26.11.20.","materialen - wapening/vezels"]
[2,"26.","26.11.21.","materialen - wapening/vezels - staalvezels ","VH of FH","kg","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Gewicht (kg) in bij Settings van het Object"]
[2,"26.","26.11.30.","materialen - wapening/voorspanstaal ","PM"]
[2,"26.","26.12.","materialen - beton"]
[2,"26.","26.12.10.","materialen - beton/stortklaar beton"]
[2,"26.","26.12.11.","materialen - beton/stortklaar beton - met staaf- en netwapening ","PM"]
[2,"26.","26.12.12.","materialen - beton/stortklaar beton - met vezelwapening ","PM"]
[2,"26.","26.12.13.","materialen - beton/stortklaar beton - zichtbeton ","FH","m2","TYPE 3","Column",null,"Core surface"]
[2,"26.",{"$nulls":4},"TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW Zichtbeton  ","Net Area"]
[2,"26.",{"$nulls":5},"Slab","Gebruik ARCHICAD Property: VMSW Zichtbeton  ","Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"26.",{"$nulls":5},"Wall","Gebruik ARCHICAD Property: VMSW Zichtbeton  ","ARCHICAD Property: Oppervlakte middenas wand"]
[2,"26.",null,null,"PM"]
[2,"26.","26.12.20.","materialen - beton/geprefabriceerd beton ","PM"]
[2,"26.","26.12.30.","materialen - beton/architectonisch beton ","PM"]
[2,"26.","26.13.","materialen - bekistingen ","PM"]
[2,"26.","26.14.","materialen - nabehandeling"]
[2,"26.","26.15.","materialen - chemische verankering ","FH of VH","st","TYPE 5","Object",null,"Stuks"]
[2,"26.",null,null,"PM "]
[2,"26.","26.16.","materialen - thermische onderbreking ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[2,"26.",null,null,"PM "]
[2,"26.","26.20.","ter plaatse gestorte elementen - algemeen"]
[2,"26.","26.21.","ter plaatse gestorte elementen - wanden"]
[2,"26.","26.21.10.","ter plaatse gestorte elementen - wanden/traditionele bekisting ","FH","m3","TYPE 3","Wall",null,"Net Volume"]
[2,"26.","26.21.20.","ter plaatse gestorte elementen - wanden/holle wanden"]
[2,"26.","26.21.21.","ter plaatse gestorte elementen - wanden/holle wanden - prefab elementen ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[2,"26.","26.21.22.","ter plaatse gestorte elementen - wanden/holle wanden - vulbeton ","FH","m3","TYPE 3","Wall",null,"Net Volume"]
[2,"26.","26.22.","ter plaatse gestorte elementen - kolommen ","FH","m3","TYPE 3","Column",null,"Net Volume"]
[2,"26.","26.23.","ter plaatse gestorte elementen - balken ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[2,"26.","26.24.","ter plaatse gestorte elementen - balken met afwijkend bekistingsprofiel ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[2,"26.","26.25.","ter plaatse gestorte elementen - trappen en bordessen ","FH","trede","TYPE 5","Stair",null,"Totaal aantal treden"]
[2,"26.","26.26.","ter plaatse gestorte elementen - draagvloeren"]
[2,"26.","26.26.10.","ter plaatse gestorte elementen - draagvloeren/traditionele bekisting ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"26.","26.26.20.","ter plaatse gestorte elementen - draagvloeren/verloren bekisting ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"26.","26.26.30.","ter plaatse gestorte elementen - draagvloeren/breedplaatvloeren"]
[2,"26.","26.26.31.","ter plaatse gestorte elementen - draagvloeren/breedplaatvloeren - prefab breedplaten ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"26.","26.26.32.","ter plaatse gestorte elementen - draagvloeren/breedplaatvloeren - opstort ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"26.","26.27.","ter plaatse gestorte elementen - uitkragende elementen"]
[2,"26.","26.27.10.","ter plaatse gestorte elementen - uitkragende elementen/balkons ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"26.","26.27.20.","ter plaatse gestorte elementen - uitkragende elementen/galerijen ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"26.","26.27.30.","ter plaatse gestorte elementen - uitkragende elementen/luifels ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"26.","26.27.40.","ter plaatse gestorte elementen - uitkragende elementen/kroonlijsten ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[2,"26.","26.30.","prefab elementen - algemeen"]
[2,"26.","26.31.","prefab elementen - wanden ","FH","m3","TYPE 3","Wall",null,"Net Volume"]
[2,"26.","26.32.","prefab elementen - kolommen ","FH","m3","TYPE 3","Column",null,"Net Volume"]
[2,"26.","26.33.","prefab elementen - balken ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[2,"26.","26.34.","prefab elementen - deur- en raamlateien ","PM"]
[2,"26.","26.35.","prefab elementen - trappen en bordessen ","FH","st","TYPE 5","Stair",null,"Stuks"]
[2,"26.","26.36.","prefab elementen - draagvloeren"]
[2,"26.","26.36.10.","prefab elementen - draagvloeren/welfsels"]
[2,"26.","26.36.11.","prefab elementen - draagvloeren/welfsels - zonder druklaag ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"26.","26.36.12.","prefab elementen - draagvloeren/welfsels - met druklaag ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"26.","26.36.20.","prefab elementen - draagvloeren/voorgespannen welfsels"]
[2,"26.","26.36.21.","prefab elementen - draagvloeren/voorgespannen welfsels - zonder druklaag ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"26.","26.36.22.","prefab elementen - draagvloeren/voorgespannen welfsels - met druklaag ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"26.","26.36.30.","prefab elementen - draagvloeren/cellenbeton ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"26.","26.36.40.","prefab elementen - draagvloeren/balken en vulblokken"]
[2,"26.","26.36.41.","prefab elementen - draagvloeren/balken en vulblokken - vulblokken beton ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"26.","26.36.42.","prefab elementen - draagvloeren/balken en vulblokken - vulblokken gebakken klei  ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"26.","26.36.43.","prefab elementen - draagvloeren/balken en vulblokken - vulblokken EPS ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"26.","26.37.","prefab elementen - uitkragende elementen"]
[2,"26.","26.37.10.","prefab elementen - uitkragende elementen/balkons ","FH","st","TYPE 3","Slab",null,"Stuks"]
[2,"26.","26.37.20.","prefab elementen - uitkragende elementen/galerijen ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"26.","26.37.30.","prefab elementen - uitkragende elementen/luifels ","FH","st","TYPE 3","Slab",null,"Stuks"]
[2,"26.",null,null,null,"m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"26.","26.37.40.","prefab elementen - uitkragende elementen/kroonlijsten ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"26.","26.40.","betonrenovatie - algemeen"]
[2,"26.","26.41.","betonrenovatie - passivatie van vrijgemaakte wapeningsstaven ","VH","m","TYPE 4","Object","Gebruik ARCHICAD Property: VMSW betonrenovatie  ","ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"26.",null,null,null,"m","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW betonrenovatie  ","ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"26.","26.42.","betonrenovatie - vervangen van wapening ","VH","kg","TYPE 3","Beam",null,"ARCHICAD property: Gewicht materiaal"]
[2,"26.","26.43.","betonrenovatie - handmatig te plaatsen mortel"]
[2,"26.","26.43.10.","betonrenovatie - handmatig te plaatsen mortel/ gemodificeerde hydraulische mortel  ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings"]
[2,"26.","26.43.20.","betonrenovatie - handmatig te plaatsen mortel/ harsgebonden mortel ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings"]
[2,"26.","26.44.","betonrenovatie - gietmortel"]
[2,"26.","26.44.10.","betonrenovatie - gietmortel/ gemodificeerde hydraulische mortel ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings"]
[2,"26.",null,null,null,"dm3","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Volume (dm3) in bij Settings van het Object"]
[2,"26.","26.44.20.","betonrenovatie - gietmortel/ beton ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings"]
[2,"26.",null,null,null,"dm3","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Volume (dm3) in bij Settings van het Object"]
[2,"26.","26.45.","betonrenovatie - spuitbeton ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings"]
[2,"26.",null,null,null,"dm3","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Volume (dm3) in bij Settings van het Object"]
[2,"26.","26.46.","betonrenovatie - injecteren van scheuren ","VH","m","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Lengte (cm) in bij de Object settings"]
[2,"26.","26.47.","betonrenovatie - coating ","FH of VH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[2,"26.",{"$nulls":5},"Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (m2) in bij de Object Settings"]
[2,"26."]
[2,"27.","27.","STRUCTUURELEMENTEN STAAL"]
[2,"27.","27.00.","structuurelementen staal - algemeen"]
[2,"27.","27.01.","algemeen - verbindingen ","PM"]
[2,"27.","27.02.","algemeen - stabiliteitsstudie ","PM"]
[2,"27.","27.10.","balken - algemeen"]
[2,"27.","27.11.","balken - blank profielstaal ","FH","kg","TYPE 3","Beam",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.","27.12.","balken - gemetalliseerd profielstaal ","FH","kg","TYPE 3","Beam",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.","27.13.","balken - thermisch verzinkt profielstaal ","FH","kg","TYPE 3","Beam",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.","27.14.","balken - thermisch verzinkt profielstaal met coating ","FH","kg","TYPE 3","Beam",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.","27.15.","balken - roestvast profielstaal (RVS) ","FH","kg","TYPE 3","Beam",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.","27.20.","lateien - algemeen"]
[2,"27.","27.21.","lateien - blank profielstaal ","PM"]
[2,"27.","27.22.","lateien - gemetalliseerd profielstaal ","PM"]
[2,"27.","27.23.","lateien - thermisch verzinkt profielstaal ","PM"]
[2,"27.","27.24.","lateien - thermisch verzinkt profielstaal met coating ","PM"]
[2,"27.","27.25.","lateien - roestvast profielstaal (RVS) ","PM"]
[2,"27.","27.26.","lateien - regelbare consoles"]
[2,"27.","27.26.10.","lateien - regelbare consoles/zichtbaar"]
[2,"27.","27.26.11.","lateien - regelbare consoles/zichtbaar - gemetalliseerd ","PM"]
[2,"27.","27.26.12.","lateien - regelbare consoles/zichtbaar - thermisch verzinkt ","PM"]
[2,"27.","27.26.13.","lateien - regelbare consoles/zichtbaar - thermisch verzinkt + coating ","PM"]
[2,"27.","27.26.14.","lateien - regelbare consoles/zichtbaar - roestvast staal (RVS) ","PM"]
[2,"27.","27.26.20.","lateien - regelbare consoles/niet-zichtbaar"]
[2,"27.","27.26.21.","lateien - regelbare consoles/niet-zichtbaar - gemetalliseerd ","PM"]
[2,"27.","27.26.22.","lateien - regelbare consoles/niet-zichtbaar - thermisch verzinkt ","PM"]
[2,"27.","27.26.23.","lateien - regelbare consoles/niet-zichtbaar - roestvast staal (RVS) ","PM"]
[2,"27.","27.30.","kolommen - algemeen"]
[2,"27.","27.31.","kolommen - blank profielstaal ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.","27.32.","kolommen - gemetalliseerd profielstaal ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.","27.33.","kolommen - thermisch verzinkt profielstaal ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.","27.34.","kolommen - thermisch verzinkt profielstaal met coating ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.","27.35.","kolommen - roestvast profielstaal (RVS) ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.","27.40.","vlakke spanten - algemeen","FH"]
[2,"27.","27.41.","vlakke spanten - blank profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.",null,null,null,"st","TYPE 5","Beam",null,"Stuks"]
[2,"27.",{"$nulls":5},"Object",null,"Stuks"]
[2,"27.","27.42.","vlakke spanten - gemetalliseerd profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.",null,null,null,"st","TYPE 5","Beam",null,"Stuks"]
[2,"27.",{"$nulls":5},"Object",null,"Stuks"]
[2,"27.","27.43.","vlakke spanten - thermisch verzinkt profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.",null,null,null,"st","TYPE 5","Beam",null,"Stuks"]
[2,"27.",{"$nulls":5},"Object",null,"Stuks"]
[2,"27.","27.44.","vlakke spanten - thermisch verzinkt profielstaal met coating ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.",null,null,null,"st","TYPE 5","Beam",null,"Stuks"]
[2,"27.",{"$nulls":5},"Object",null,"Stuks"]
[2,"27.","27.50.","hulpstukken - algemeen"]
[2,"27.","27.51.","hulpstukken - oplegstukken"]
[2,"27.","27.51.10.","hulpstukken - oplegstukken/thermisch verzinkt ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.",null,null,"PM"]
[2,"27.","27.51.20.","hulpstukken - oplegstukken/roestvast staal (RVS) ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal"]
[2,"27.",null,null,"PM"]
[2,"27.","27.52.","hulpstukken - spankabels ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[2,"27.",null,null,null,"st","TYPE 5","Object",null,"Stuks"]
[2,"27.",null,null,"SOG"]
[2,"27.","27.53.","hulpstukken - geveldragers"]
[2,"27.","27.53.10.","hulpstukken - geveldragers/gemetalliseerd ","PM"]
[2,"27.","27.53.20.","hulpstukken - geveldragers/thermisch verzinkt ","PM"]
[2,"27.","27.53.30.","hulpstukken - geveldragers/roestvast staal ","PM"]
[2,"27.","27.54.","hulpstukken - verhandelingsysteem liften"]
[2,"27.","27.60.","corrosiebescherming - algemeen"]
[2,"27.","27.61.","corrosiebescherming - metallisatie"]
[2,"27.","27.61.10.","corrosiebescherming - metallisatie/zonder bijkomende afwerkingslaag ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",null,null,"PM"]
[2,"27.","27.61.20.","corrosiebescherming - metallisatie/metallisatie + natlak ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",null,null,"PM"]
[2,"27.","27.61.30.","corrosiebescherming - metallisatie/metallisatie + poederlak ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",null,null,"PM"]
[2,"27.","27.62.","corrosiebescherming - thermisch verzinken ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",null,null,"PM"]
[2,"27.","27.63.","corrosiebescherming - duplexsysteem ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",null,null,"PM"]
[2,"27.","27.64.","corrosiebescherming - roestwerende verfsystemen ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",null,null,"PM"]
[2,"27.","27.70.","brandbeveiliging - algemeen"]
[2,"27.","27.71.","brandbeveiliging - brandwerend verfsysteem ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",null,null,"PM"]
[2,"27.","27.72.","brandbeveiliging - spuitmortel ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",null,null,"PM"]
[2,"27.","27.80.","renovatie stalen constructie-elementen - algemeen"]
[2,"27.","27.81.","renovatie stalen constructie-elementen - ontroesten ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",{"$nulls":5},"Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal"]
[2,"27.",null,null,"PM"]
[2,"27."]
[2,"28.","28.","HOUTSKELETBOUW"]
[2,"28.","28.00.","houtskeletbouw - algemeen"]
[2,"28.","28.01.","algemeen - stabiliteitsstudie ","PM"]
[2,"28.","28.02.","algemeen - prestaties ","PM"]
[2,"28.","28.10.","materialen - algemeen"]
[2,"28.","28.11.","materialen - onderdelen regelwerk"]
[2,"28.","28.11.10.","materialen - onderdelen regelwerk/stijlen"]
[2,"28.","28.11.11.","materialen - onderdelen regelwerk /stijlen - massief hout ","PM"]
[2,"28.","28.11.12.","materialen - onderdelen regelwerk /stijlen - I-vormige stijlen ","PM"]
[2,"28.","28.11.20.","materialen - onderdelen regelwerk/regels"]
[2,"28.","28.11.21.","materialen - onderdelen regelwerk /regels - onder- en bovenregels ","PM"]
[2,"28.","28.11.22.","materialen - onderdelen regelwerk /regels - grondregels ","PM"]
[2,"28.","28.11.23.","materialen - onderdelen regelwerk /regels - stelregels ","PM"]
[2,"28.","28.11.24.","materialen - onderdelen regelwerk /regels - koppelregels ","PM"]
[2,"28.","28.11.30.","materialen - onderdelen regelwerk/lateien ","PM"]
[2,"28.","28.12.","materialen - beplating"]
[2,"28.","28.12.10.","materialen - beplating/houtachtige platen"]
[2,"28.","28.12.11.","materialen - beplating/houtachtige platen - OSB ","PM"]
[2,"28.","28.12.12.","materialen - beplating/houtachtige platen - spaanplaat ","PM"]
[2,"28.","28.12.13.","materialen - beplating/houtachtige platen - multiplex ","PM"]
[2,"28.","28.12.14.","materialen - beplating/houtachtige platen - MDF ","PM"]
[2,"28.","28.12.15.","materialen - beplating/houtachtige platen - LVL ","PM"]
[2,"28.","28.12.16.","materialen - beplating/houtachtige platen - houtvezelisolatieplaat ","PM"]
[2,"28.","28.12.17.","materialen - beplating/houtachtige platen - houtvezelcementplaat ","PM"]
[2,"28.","28.12.20.","materialen - beplating/gipsachtige platen"]
[2,"28.","28.12.21.","materialen - beplating/gipsachtige platen - gipskartonplaten ","PM"]
[2,"28.","28.12.22.","materialen - beplating/gipsachtige platen - gipsvezelplaten ","PM"]
[2,"28.","28.12.30.","materialen - beplating/vezelcementplaten ","PM"]
[2,"28.","28.12.40.","materialen - beplating/calciumsilicaatplaten ","PM"]
[2,"28.","28.13.","materialen - isolatie"]
[2,"28.","28.13.10.","materialen - isolatie/minerale wol ","PM"]
[2,"28.","28.13.20.","materialen - isolatie/cellulosevlokken ","PM"]
[2,"28.","28.13.30.","materialen - isolatie/houtwol ","PM"]
[2,"28.","28.14.","materialen - folies"]
[2,"28.","28.14.10.","materialen - folies/buitenfolies"]
[2,"28.","28.14.11.","materialen - folies/buitenfolies - wanden ","PM"]
[2,"28.","28.14.12.","materialen - folies/buitenfolies - hellende daken ","PM"]
[2,"28.","28.14.20.","materialen - folies/binnenfolies"]
[2,"28.","28.14.21.","materialen - folies/binnenfolies - wanden ","PM"]
[2,"28.","28.14.22.","materialen - folies/binnenfolies - hellende daken ","PM"]
[2,"28.","28.14.23.","materialen - folies/binnenfolies - platte daken ","PM"]
[2,"28.","28.15.","materialen - regelstructuur voor binnenafwerking"]
[2,"28.","28.15.10.","materialen - regelstructuur voor binnenafwerking/hout ","PM"]
[2,"28.","28.15.20.","materialen - regelstructuur voor binnenafwerking/metaal ","PM"]
[2,"28.","28.16.","materialen - opleg- en bevestigingsmaterialen"]
[2,"28.","28.16.10.","materialen - opleg- en bevestigingsmaterialen/metalen schoenen ","PM"]
[2,"28.","28.16.20.","materialen - opleg- en bevestigingsmaterialen/tie-downs ","FH","st","TYPE 5","Object",null,"Stuks"]
[2,"28.","28.16.30.","materialen - opleg- en bevestigingsmaterialen/schroeven ","PM"]
[2,"28.","28.16.40.","materialen - opleg- en bevestigingsmaterialen/nagels ","PM"]
[2,"28.","28.16.50.","materialen - opleg- en bevestigingsmaterialen/nieten ","PM"]
[2,"28.","28.16.60.","materialen - opleg- en bevestigingsmaterialen/lijmen ","PM"]
[2,"28.","28.16.70.","materialen - opleg- en bevestigingsmaterialen/metalen hechtplaten ","PM"]
[2,"28.","28.20.","structuurelementen - algemeen"]
[2,"28.","28.21.","structuurelementen - vloerbalken"]
[2,"28.","28.21.10.","structuurelementen - vloerbalken/massief hout ","PM"]
[2,"28.","28.21.20.","structuurelementen - vloerbalken/LVL ","PM"]
[2,"28.","28.21.30.","structuurelementen - vloerbalken/lichte samengestelde liggers ","PM"]
[2,"28.","28.21.40.","structuurelementen - vloerbalken/gelijmd gelamineerd hout (GL) ","PM"]
[2,"28.","28.22.","structuurelementen - balken"]
[2,"28.","28.22.10.","structuurelementen - balken/massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[2,"28.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[2,"28.","28.22.20.","structuurelementen - balken/LVL ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[2,"28.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[2,"28.","28.22.30.","structuurelementen - balken/lichte samengestelde liggers ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[2,"28.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[2,"28.","28.22.40.","structuurelementen - balken/gelijmd gelamineerd hout (GL) ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[2,"28.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[2,"28.","28.22.50.","structuurelementen - balken/staal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal"]
[2,"28.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[2,"28.","28.23.","structuurelementen - lateien"]
[2,"28.","28.23.10.","structuurelementen - lateien/massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[2,"28.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[2,"28.","28.23.20.","structuurelementen - lateien/LVL ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[2,"28.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[2,"28.","28.23.30.","structuurelementen - lateien/gelijmd gelamineerd hout ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[2,"28.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[2,"28.","28.23.40.","structuurelementen - lateien/staal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal"]
[2,"28.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[2,"28.","28.24.","structuurelementen - kolommen"]
[2,"28.","28.24.10.","structuurelementen - kolommen/massief hout ","FH","m3","TYPE 3","Column",null,"Net Volume"]
[2,"28.",null,null,null,"st","TYPE 3","Column",null,"Stuks"]
[2,"28.","28.24.20.","structuurelementen - kolommen/LVL ","FH","m3","TYPE 3","Column",null,"Net Volume"]
[2,"28.",null,null,null,"st","TYPE 3","Column",null,"Stuks"]
[2,"28.","28.24.30.","structuurelementen - kolommen/gelijmd gelamineerd hout (GL) ","FH","m3","TYPE 3","Column",null,"Net Volume"]
[2,"28.",null,null,null,"st","TYPE 3","Column",null,"Stuks"]
[2,"28.","28.24.40.","structuurelementen - kolommen/staal ","FH","kg","TYPE 3","Column",null,"ARCHICAD property: Gewicht materiaal"]
[2,"28.",null,null,null,"st","TYPE 3","Column",null,"Stuks"]
[2,"28.","28.25.","structuurelementen - onderdelen hellend dak"]
[2,"28.","28.25.10.","structuurelementen - onderdelen hellend dak/gordingen"]
[2,"28.","28.25.11.","structuurelementen - onderdelen hellend dak/gordingen - massief hout ","PM"]
[2,"28.","28.25.12.","structuurelementen - onderdelen hellend dak/gordingen - gelamineerd hout ","PM"]
[2,"28.","28.25.20.","structuurelementen - onderdelen hellend dak/keperwerk"]
[2,"28.","28.25.21.","structuurelementen - onderdelen hellend dak/keperwerk - massief hout ","PM"]
[2,"28.","28.25.30.","structuurelementen - onderdelen hellend dak/spanten"]
[2,"28.","28.25.31.","structuurelementen - onderdelen hellend dak/spanten - massief hout","PM"]
[2,"28.","28.25.40.","structuurelementen - onderdelen hellend dak/scharnierdak ","PM"]
[2,"28.","28.25.50.","structuurelementen - onderdelen hellend dak/bakgootconstructies"]
[2,"28.","28.25.51.","structuurelementen - onderdelen hellend dak/bakgootconstructies - massief hout ","PM"]
[2,"28.","28.25.60.","structuurelementen - onderdelen hellend dak/dakrandoversteken"]
[2,"28.","28.25.61.","structuurelementen - onderdelen hellend dak/dakrandoversteken - massief hout ","PM"]
[2,"28.","28.25.70.","structuurelementen - onderdelen hellend dak/tengel- en panlatten ","PM"]
[2,"28.","28.30.","wanden - algemeen"]
[2,"28.","28.31.","wanden - buitenwanden "]
[2,"28.","28.31.10.","wanden - buitenwanden/type I ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[2,"28.",{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[2,"28.","28.31.20.","wanden - buitenwanden/type II ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[2,"28.",{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[2,"28.","28.31.30.","wanden - buitenwanden/type III ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[2,"28.",{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[2,"28.","28.32.","wanden - binnenwanden "]
[2,"28.","28.32.10.","wanden - binnenwanden/type I ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[2,"28.",{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[2,"28.","28.32.20.","wanden - binnenwanden/type II ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[2,"28.",{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[2,"28.","28.33.","wanden - woningscheidende wanden ","FH","m2","TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[2,"28.","28.34.","wanden - dakopstanden ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"28.",{"$nulls":5},"Wall",null,"Lengte volgens eigen middenas"]
[2,"28.","28.40.","vloeren - algemeen"]
[2,"28.","28.41.","vloeren - roostering met beplating ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"28.","28.42.","vloeren - geprefabriceerde houten vloeren"]
[2,"28.","28.42.10.","vloeren - geprefabriceerde houten vloeren/roostering met beplating ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"28.","28.42.20.","vloeren - geprefabriceerde houten vloeren/kokervormige vloeren ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"28.","28.42.30.","vloeren - geprefabriceerde houten vloeren/massieve houten vloeren ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"28.","28.43.","vloeren - hout-betonvloeren ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"28.","28.50.","hellende daken - algemeen"]
[2,"28.","28.51.","hellende daken - spanten ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[2,"28.",{"$nulls":5},"Shell",null,"Top Surface"]
[2,"28.","28.52.","hellende daken - gordingen ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[2,"28.",{"$nulls":5},"Shell",null,"Top Surface"]
[2,"28.","28.53.","hellende daken - scharnierdaken ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[2,"28.",{"$nulls":5},"Shell",null,"Top Surface"]
[2,"28.","28.60.","platte daken - algemeen"]
[2,"28.","28.61.","platte daken - roostering met beplating ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[2,"28.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"28.","28.62.","platte daken - geprefabriceerde houten vloeren"]
[2,"28.","28.62.10.","platte daken - geprefabriceerde houten vloeren/roostering met beplating ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[2,"28.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"28.","28.62.20.","platte daken - geprefabriceerde houten vloeren/kokervormige vloeren ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[2,"28.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"28.","28.62.30.","platte daken - geprefabriceerde houten vloeren/massieve houten vloeren ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[2,"28.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"28.","28.63.","platte daken - hout-betonvloeren ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[2,"28.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[2,"28.","28.64.","platte daken - randisolatie ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[2,"28.",{"$nulls":5},"Roof",null,"Omtrek "]
[2,"28.",{"$nulls":5},"Slab",null,"Omtrek "]
[2,"28."]
[3,"30.","30.","DAKOPBOUW HELLEND DAK"]
[3,"30.","30.00.","dakopbouw hellend dak - algemeen"]
[3,"30.","30.01.","dakopbouw hellend dak - stabiliteitsstudie ","PM"]
[3,"30.","30.10.","houten dakstructuur - algemeen ","FH","m3","TYPE 3","Roof",null,"Net Volume"]
[3,"30.",{"$nulls":5},"Shell",null,"Net Volume"]
[3,"30.",null,null,null,"st","TYPE 3","Roof",null,"Stuks"]
[3,"30.",{"$nulls":5},"Shell",null,"Stuks"]
[3,"30.",null,null,"PM"]
[3,"30.","30.11.","houten dakstructuur - muurplaten ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[3,"30.",null,null,"PM"]
[3,"30.","30.12.","houten dakstructuur - gordingen"]
[3,"30.","30.12.10.","houten dakstructuur - gordingen/massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[3,"30.",{"$nulls":4},"TYPE 5","Morph",null,"Net Volume"]
[3,"30.",{"$nulls":5},"Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing"]
[3,"30.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[3,"30.",{"$nulls":4},"TYPE 5","Morph",null,"Stuks"]
[3,"30.",{"$nulls":5},"Object",null,"Stuks"]
[3,"30.",null,null,"PM"]
[3,"30.","30.12.20.","houten dakstructuur - gordingen/gelamineerd hout ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[3,"30.",{"$nulls":4},"TYPE 5","Morph",null,"Net Volume"]
[3,"30.",{"$nulls":5},"Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing"]
[3,"30.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[3,"30.",{"$nulls":4},"TYPE 5","Morph",null,"Stuks"]
[3,"30.",{"$nulls":5},"Object",null,"Stuks"]
[3,"30.",null,null,"PM"]
[3,"30.","30.13.","houten dakstructuur - keperwerk ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[3,"30.",{"$nulls":4},"TYPE 5","Morph",null,"Net Volume"]
[3,"30.",{"$nulls":5},"Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing"]
[3,"30.",null,null,"PM"]
[3,"30.","30.14.","houten dakstructuur - keperspanten ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[3,"30.",{"$nulls":4},"TYPE 5","Morph",null,"Net Volume"]
[3,"30.",{"$nulls":5},"Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing"]
[3,"30.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[3,"30.",{"$nulls":4},"TYPE 5","Morph",null,"Stuks"]
[3,"30.",{"$nulls":5},"Object",null,"Stuks"]
[3,"30.",null,null,"PM"]
[3,"30.","30.15.","houten dakstructuur - prefabspanten ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[3,"30.",{"$nulls":4},"TYPE 5","Morph",null,"Net Volume"]
[3,"30.",{"$nulls":5},"Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing"]
[3,"30.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[3,"30.",{"$nulls":4},"TYPE 5","Morph",null,"Stuks"]
[3,"30.",{"$nulls":5},"Object",null,"Stuks"]
[3,"30.",null,null,"PM"]
[3,"30.","30.16.","houten dakstructuur - bakgootconstructies ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"30.","30.17.","houten dakstructuur - dakrandoversteken ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"30.","30.18.","houten dakstructuur - boordplanken"]
[3,"30.","30.18.10.","houten dakstructuur - boordplanken/massief hout ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"30.","30.18.20.","houten dakstructuur - boordplanken/multiplex ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"30.","30.20.","onderdak - algemeen"]
[3,"30.","30.21.","onderdak - soepele membranen ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"30.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"30.","30.22.","onderdak - platen"]
[3,"30.","30.22.10.","onderdak - platen/vezelcement ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"30.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"30.","30.22.20.","onderdak - platen/houtvezelplaten ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"30.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"30.","30.30.","tengel- & panlatten - algemeen ","PM"]
[3,"30."]
[3,"31.","31.","THERMISCHE ISOLATIE HELLEND DAK"]
[3,"31.","31.00.","thermische isolatie hellend dak - algemeen"]
[3,"31.","31.10.","isolatieplaten tussen dakstructuur - algemeen"]
[3,"31.","31.11.","isolatieplaten tussen dakstructuur - MW"]
[3,"31.","31.11.10.","isolatieplaten tussen dakstructuur - MW/18 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface"]
[3,"31.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"31.","31.11.20.","isolatieplaten tussen dakstructuur - MW/20 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface"]
[3,"31.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"31.","31.12.","isolatieplaten tussen dakstructuur - houtwol (WW)"]
[3,"31.","31.12.10.","isolatieplaten tussen dakstructuur - houtwol (WW)/18 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface"]
[3,"31.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"31.","31.12.20.","isolatieplaten tussen dakstructuur - houtwol (WW)/20 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface"]
[3,"31.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"31.","31.13.","isolatieplaten tussen dakstructuur - cellulose"]
[3,"31.","31.13.10.","isolatieplaten tussen dakstructuur - cellulose/18 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface"]
[3,"31.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"31.","31.13.20.","isolatieplaten tussen dakstructuur - cellulose/20 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface"]
[3,"31.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"31.","31.20.","isolatieplaten op dakstructuur (sarking) - algemeen"]
[3,"31.","31.21.","isolatieplaten op dakstructuur (sarking) - PUR of PIR"]
[3,"31.","31.21.10.","isolatieplaten op dakstructuur (sarking) - PUR of PIR/14 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface"]
[3,"31.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"31.","31.21.20.","isolatieplaten op dakstructuur (sarking) - PUR of PIR/16 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface"]
[3,"31.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"31.","31.22.","isolatieplaten op dakstructuur (sarking) - PF"]
[3,"31.","31.22.10.","isolatieplaten op dakstructuur (sarking) - PF/14 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface"]
[3,"31.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"31.","31.22.20.","isolatieplaten op dakstructuur (sarking) - PF/16 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface"]
[3,"31.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"31.","31.23.","isolatieplaten op dakstructuur (sarking) - XPS"]
[3,"31.","31.23.10.","isolatieplaten op dakstructuur (sarking) - XPS/14 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface"]
[3,"31.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"31.","31.23.20.","isolatieplaten op dakstructuur (sarking) - XPS/16 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface"]
[3,"31.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"31.","31.30.","ingeblazen isolatie - algemeen"]
[3,"31.","31.31.","ingeblazen isolatie - cellulose"]
[3,"31.","31.31.10.","ingeblazen isolatie - cellulose/18 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface"]
[3,"31.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"31.","31.31.20.","ingeblazen isolatie - cellulose/23 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface"]
[3,"31.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"31.","31.40.","binnenfolie - algemeen"]
[3,"31.","31.41.","binnenfolie - damprem ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"31.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"31.","31.42.","binnenfolie - dampscherm ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"31.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"31.","31.50.","isolerende dakelementen - algemeen"]
[3,"31.","31.51.","isolerende dakelementen - tweeschalig ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"31.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"31."]
[3,"32.","32.","DAKBEDEKKING HELLEND DAK"]
[3,"32.","32.00.","dakbedekking hellend dak - algemeen"]
[3,"32.","32.01.","dakbedekking hellend dak - prestaties"]
[3,"32.","32.10.","pannen - algemeen"]
[3,"32.","32.11.","pannen - gebakken aarde ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"32.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"32.",null,null,"PM"]
[3,"32.","32.11.10.","pannen - gebakken aarde/dakvlak ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"32.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"32.","32.11.20.","pannen - gebakken aarde/vormstukken ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[3,"32."]
[3,"32.","32.11.30.","pannen - gebakken aarde/toebehoren ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"32.","32.12.","pannen - beton ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"32.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"32.",null,null,"PM"]
[3,"32.","32.12.10.","pannen - beton/dakvlak ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"32.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"32.","32.12.20.","pannen - beton/vormstukken ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[3,"32.","32.12.30.","pannen - beton/toebehoren ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"32.","32.13.","pannen - metaal ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"32.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"32.",null,null,"PM"]
[3,"32.","32.13.10.","pannen - gecoat staal/dakvlak ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"32.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"32.","32.13.20.","pannen - gecoat staal/vormstukken ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[3,"32.","32.13.30.","pannen - gecoat staal/toebehoren ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"32.","32.20.","leien - algemeen"]
[3,"32.","32.21.","leien - vezelcement ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"32.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"32.","32.22.","leien - natuurleien ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"32.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"32.","32.30.","golfplaten - algemeen"]
[3,"32.","32.31.","golfplaten - vezelcement ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"32.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"32.",null,null,"PM"]
[3,"32.","32.31.10.","golfplaten - vezelcement/dakvlakken ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"32.",null,null,null,"m2","TYPE 3","Shell",null,"Top Surface"]
[3,"32.","32.31.20.","golfplaten - vezelcement/vormstukken ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[3,"32.","32.31.30.","golfplaten - vezelcement/toebehoren ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"32.","32.40.","geprofileerde metaalplaten - algemeen"]
[3,"32.","32.41.","geprofileerde metaalplaten - gecoat staal ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"32.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"32.","32.42.","geprofileerde metaalplaten - aluminium ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"32.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"32.","32.43.","geprofileerde metaalplaten - RVS ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"32.",{"$nulls":5},"Shell",null,"Top Surface"]
[3,"32.","32.50.","toebehoren hellend dak - algemeen"]
[3,"32.","32.51.","toebehoren hellend dak - dakdoorvoeren ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"32.",null,null,"PM"]
[3,"32.","32.52.","toebehoren hellend dak - verankeringssystemen ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"32.",null,null,"PM"]
[3,"32.","32.53.","toebehoren hellend dak - valbeveiliging"]
[3,"32.","32.53.10.","toebehoren hellend dak - valbeveiliging / ankerpunten ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"32.","32.53.20.","toebehoren hellend dak - valbeveiliging / lijnsysteem ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie"]
[3,"32.","32.54.","toebehoren hellend dak - ladderhaken ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"32.",null,null,"PM"]
[3,"32."]
[3,"33.","33.","DAKVLOER PLAT DAK"]
[3,"33.","33.00.","dakvloer plat dak - algemeen"]
[3,"33.","33.01.","algemeen - stabiliteitsstudie"]
[3,"33.","33.10.","houten roostering - algemeen"]
[3,"33.","33.11.","houten roostering - muurplaten ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"33.",null,null,null,"m3","TYPE 3","Beam",null,"Net Volume"]
[3,"33.","33.12.","houten roostering - balken"]
[3,"33.","33.12.10.","houten roostering - balken/massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume"]
[3,"33.",{"$nulls":4},"TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing"]
[3,"33.","33.12.20.","houten roostering - balken/LVL ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"33.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[3,"33.",null,null,null,"m3","TYPE 3","Beam",null,"Net Volume"]
[3,"33.",{"$nulls":4},"TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing"]
[3,"33.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[3,"33.",{"$nulls":4},"TYPE 5","Object",null,"Stuks"]
[3,"33.","33.12.30.","houten roostering - balken/lichte samengestelde liggers ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"33.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[3,"33.",null,null,null,"m3","TYPE 3","Beam",null,"Net Volume"]
[3,"33.",{"$nulls":4},"TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing"]
[3,"33.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[3,"33.",{"$nulls":4},"TYPE 5","Object",null,"Stuks"]
[3,"33.","33.20.","beplating op houten roostering - algemeen"]
[3,"33.","33.21.","beplating op houten roostering - multiplex ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"33.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"33.","33.22.","beplating op houten roostering - OSB ","FH","m2","TYPE 3","Roof",null,"Top Surface"]
[3,"33.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"33.","33.23.","beplating op houten roostering - spaanplaat ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"33.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"33.","33.24.","beplating op houten roostering - cementgebonden spaanplaat ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"33.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"33.","33.30.","zelfdragende elementen - algemeen"]
[3,"33.","33.31.","zelfdragende elementen - profielplaten staal"]
[3,"33.","33.31.10.","zelfdragende elementen - profielplaten staal/enkelvoudig ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"33.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"33.","33.32.","zelfdragende elementen - sandwichplaten hout ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"33.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"33.","33.40.","hellingsbeton - algemeen"]
[3,"33.","33.41.","hellingsbeton - niet isolerend"]
[3,"33.","33.41.10.","hellingsbeton - niet isolerend/mager beton ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"33.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"33.","33.41.20.","hellingsbeton - niet isolerend/zandcement dekvloer ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"33.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"33.","33.52.","hellingsbeton - licht isolerend"]
[3,"33.","33.52.10.","hellingsbeton - licht isolerend/granulaten ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"33.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"33.","33.52.20.","hellingsbeton - licht isolerend/schuimbeton ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"33.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"33."]
[3,"34.","34.","THERMISCHE ISOLATIE PLAT DAK"]
[3,"34.","34.00.","thermische isolatie plat dak - algemeen"]
[3,"34.","34.10.","isolatieplaten plat dak - algemeen"]
[3,"34.","34.11.","isolatieplaten plat dak - MW"]
[3,"34.","34.11.10.","isolatieplaten plat dak - MW/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area"]
[3,"34.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"34.","34.11.20.","isolatieplaten plat dak - MW/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area"]
[3,"34.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"34.","34.12.","isolatieplaten plat dak - PUR of PIR"]
[3,"34.","34.12.10.","isolatieplaten plat dak - PUR of PIR/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area"]
[3,"34.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"34.","34.12.20.","isolatieplaten plat dak - PUR of PIR/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area"]
[3,"34.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"34.","34.13.","isolatieplaten plat dak - EPS"]
[3,"34.","34.13.10.","isolatieplaten plat dak - EPS/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area"]
[3,"34.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"34.","34.13.20.","isolatieplaten plat dak - EPS/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area"]
[3,"34.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"34.","34.14.","isolatieplaten plat dak - CG"]
[3,"34.","34.14.10.","isolatieplaten plat dak - CG/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area"]
[3,"34.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"34.","34.14.20.","isolatieplaten plat dak - CG/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area"]
[3,"34.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"34.","34.15.","isolatieplaten omkeerdak - XPS"]
[3,"34.","34.15.10.","isolatieplaten omkeerdak - XPS/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area"]
[3,"34.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"34.","34.15.20.","isolatieplaten omkeerdak - XPS/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area"]
[3,"34.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"34.","34.20.","dampscherm - algemeen"]
[3,"34.","34.21.","dampscherm - gewapend bitumen ","PM"]
[3,"34."]
[3,"35.","35.","AFDICHTING & AFWERKING PLAT DAK"]
[3,"35.","35.00.","afdichting & afwerking plat dak - algemeen"]
[3,"35.","35.01.","afdichting & afwerking plat dak - waterdichtheidsproeven ","PM"]
[3,"35.","35.02.","afdichting & afwerking plat dak - waarborgen & attesten ","PM"]
[3,"35.","35.03.","afdichting & afwerking plat dak - renovatie bestaande daken ","PM"]
[3,"35.","35.10.","bitumineuze dakafdichting - algemeen"]
[3,"35.","35.11.","bitumineuze dakafdichting - SBS"]
[3,"35.","35.11.10.","bitumineuze dakafdichting - SBS/losliggend (L) ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.11.20.","bitumineuze dakafdichting - SBS/deelgekleefd (P) ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.11.30.","bitumineuze dakafdichting - SBS/volgekleefd (T) ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.11.40.","bitumineuze dakafdichting - SBS/mechanisch (M) ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.12.","bitumineuze dakafdichting - APP","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.","35.12.10.","bitumineuze dakafdichting - APP/losliggend (L) ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.12.20.","bitumineuze dakafdichting - APP/deelgekleefd (P) ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.12.30.","bitumineuze dakafdichting - APP/volgekleefd (T) ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.12.40.","bitumineuze dakafdichting - APP/mechanisch (M) ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.13.","bitumineuze dakafdichting - PBE"]
[3,"35.","35.20.","kunststof dakafdichting - algemeen"]
[3,"35.","35.21.","kunststof dakafdichting - EPDM"]
[3,"35.","35.21.10.","kunststof dakafdichting - EPDM/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.21.20.","kunststof dakafdichting - EPDM/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.21.30.","kunststof dakafdichting - EPDM/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.22.","kunststof dakafdichting - TPO"]
[3,"35.","35.22.10.","kunststof dakafdichting - TPO/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.22.20.","kunststof dakafdichting - TPO/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.22.30.","kunststof dakafdichting - TPO/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.23.","kunststof dakafdichting - PVC"]
[3,"35.","35.23.10.","kunststof dakafdichting - PVC/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.23.20.","kunststof dakafdichting - PVC/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.23.30.","kunststof dakafdichting - PVC/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.24.","kunststof dakafdichting - CPE"]
[3,"35.","35.24.10.","kunststof dakafdichting - CPE/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.24.20.","kunststof dakafdichting - CPE/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.24.30.","kunststof dakafdichting - CPE/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.25.","kunststof dakafdichting - PIB"]
[3,"35.","35.25.10.","kunststof dakafdichting - PIB/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.25.20.","kunststof dakafdichting - PIB/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.25.30.","kunststof dakafdichting - PIB/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.26.","kunststof dakafdichting - ECB"]
[3,"35.","35.26.10.","kunststof dakafdichting - ECB/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.26.20.","kunststof dakafdichting - ECB/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.26.30.","kunststof dakafdichting - ECB/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.30.","ballastlaag - algemeen"]
[3,"35.","35.31.","ballastlaag - grind ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.32.","ballastlaag - tegels ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.33.","ballastlaag - geotextiel ","PM"]
[3,"35.","35.40.","groendak - algemeen"]
[3,"35.","35.41.","groendak - extensief ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.42.","groendak - intensief ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[3,"35.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"35.","35.50.","toebehoren plat dak - algemeen"]
[3,"35.","35.51.","toebehoren plat dak - dakdoorvoeren ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"35.",null,null,"PM"]
[3,"35.","35.52.","toebehoren plat dak - verankeringssystemen ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"35.",null,null,"PM"]
[3,"35.","35.53.","toebehoren plat dak - valbeveiliging"]
[3,"35.","35.53.10.","toebehoren plat dak - valbeveiliging/doodgewicht ankers ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"35.","35.53.20.","toebehoren plat dak - valbeveiliging/vaste ankerpunten ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"35.","35.53.30.","toebehoren plat dak - valbeveiliging/lijnsysteem ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"35.",{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie"]
[3,"35."]
[3,"36.","36.","DAKLICHTOPENINGEN"]
[3,"36.","36.00.","daklichtopeningen - algemeen"]
[3,"36.","36.10.","dakvlakramen - algemeen"]
[3,"36.","36.11.","dakvlakramen - hout"]
[3,"36.","36.11.10.","dakvlakramen - hout/wentel ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"36.",{"$nulls":5},"Skylight",null,"Stuks"]
[3,"36.","36.11.20.","dakvlakramen - hout/uitzet en wentel ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"36.",{"$nulls":5},"Skylight",null,"Stuks"]
[3,"36.","36.11.30.","dakvlakramen - hout/uitzet ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"36.",{"$nulls":5},"Skylight",null,"Stuks"]
[3,"36.","36.11.40.","dakvlakramen - hout/rook- & warmteafvoer ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"36.",{"$nulls":5},"Skylight",null,"Stuks"]
[3,"36.","36.12.","dakvlakramen - kunststof"]
[3,"36.","36.12.10.","dakvlakramen - kunststof/wentel ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"36.",{"$nulls":5},"Skylight",null,"Stuks"]
[3,"36.","36.12.20.","dakvlakramen - kunststof/uitzet-wentel ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"36.",{"$nulls":5},"Skylight",null,"Stuks"]
[3,"36.","36.12.30.","dakvlakramen - kunststof/uitzet ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"36.",{"$nulls":5},"Skylight",null,"Stuks"]
[3,"36.","36.12.40.","dakvlakramen - kunststof/rook- en warmteafvoer ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"36.",{"$nulls":5},"Skylight",null,"Stuks"]
[3,"36.","36.13.","dakvlakramen - zolderraam ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"36.",{"$nulls":5},"Skylight",null,"Stuks"]
[3,"36.","36.20.","platdakramen - algemeen"]
[3,"36.","36.21.","platdakramen - kunststof"]
[3,"36.","36.21.10.","platdakramen - kunststof/vast ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"36.",{"$nulls":5},"Skylight",null,"Stuks"]
[3,"36.","36.21.20.","platdakramen - kunststof/opengaand ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"36.",{"$nulls":5},"Skylight",null,"Stuks"]
[3,"36.","36.21.30.","platdakramen - kunststof/rook- en warmteafvoer ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"36.",{"$nulls":5},"Skylight",null,"Stuks"]
[3,"36.","36.30.","koepels - algemeen"]
[3,"36.","36.31.","koepels - kunststof acrylaat (PMMA)"]
[3,"36.","36.31.10.","koepels - kunststof acrylaat (PMMA)/vast ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"36.",{"$nulls":5},"Skylight",null,"Stuks"]
[3,"36.","36.31.20.","koepels - kunststof acrylaat (PMMA)/opengaand ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"36.",{"$nulls":5},"Skylight",null,"Stuks"]
[3,"36.","36.31.30.","koepels - kunststof acrylaat (PMMA)/rook en warmteafvoer ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"36.",{"$nulls":5},"Skylight",null,"Stuks"]
[3,"36.","36.32.","koepels - kunststof polycarbonaat (PC) ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"36.",{"$nulls":5},"Skylight",null,"Stuks"]
[3,"36.","36.40.","daglichtreflectiebuizen - algemeen"]
[3,"36.","36.41.","daglichtreflectiebuizen - plat dak ","FH","m2","TYPE 5","Object",null,"Net Area"]
[3,"36.",{"$nulls":5},"Skylight",null,"Net Area"]
[3,"36.","36.42.","daglichtreflectiebuizen - hellend dak ","FH","m2","TYPE 5","Object",null,"Net Area"]
[3,"36.",{"$nulls":5},"Skylight",null,"Net Area"]
[3,"36.","36.50.","lichtstraten - algemeen"]
[3,"36.","36.51.","lichtstraten - profielen hout"]
[3,"36.","36.51.10.","lichtstraten - profielen hout/met beglazing ","FH","m2","TYPE 5","Object",null,"Net Area"]
[3,"36.",{"$nulls":5},"Skylight",null,"Net Area"]
[3,"36.","36.52.","lichtstraten - profielen aluminium"]
[3,"36.","36.52.10.","lichtstraten - profielen aluminium met beglazing ","FH","m2","TYPE 5","Object",null,"Net Area"]
[3,"36.",{"$nulls":5},"Skylight",null,"Net Area"]
[3,"36.","36.60.","dakkapellen - algemeen"]
[3,"36.","36.61.","dakkapellen - traditioneel ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"36."]
[3,"37.","37.","DAKRANDEN EN KROONLIJSTEN"]
[3,"37.","37.00.","dakranden en kroonlijsten - algemeen"]
[3,"37.","37.10.","slabben, loketten en aansluitbanden - algemeen"]
[3,"37.","37.11.","slabben, loketten en aansluitbanden - metaal"]
[3,"37.","37.11.10.","slabben, loketten en aansluitbanden - metaal/lood ","FH of VH","kg","TYPE 3","Beam",null,"ARCHICAD property: Gewicht materiaal"]
[3,"37.",{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","Vul Gewicht (kg) in bij Settings van het Object"]
[3,"37.",null,null,null,"m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"37.",null,null,"PM"]
[3,"37.","37.11.20.","slabben, loketten en aansluitbanden - metaal/aluminium ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"37.",null,null,"PM"]
[3,"37.","37.11.30.","slabben, loketten en aansluitbanden - metaal/zink ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"37.",null,null,"PM"]
[3,"37.","37.11.40.","slabben, loketten en aansluitbanden - metaal/koper ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[{"$nulls":4},"PM"]
[3,"37.","37.12.","slabben, loketten en aansluitbanden - membranen"]
[3,"37.","37.12.10.","slabben, loketten en aansluitbanden - membraan/EPDM ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"37.",null,null,"PM"]
[3,"37.","37.12.20.","slabben, loketten en aansluitbanden - membraan/PIB ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"37.",null,null,"PM"]
[3,"37.","37.12.30.","slabben, loketten en aansluitbanden - membraan/bitumen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"37.",null,null,"PM"]
[3,"37.","37.20.","dakrandprofielen - algemeen"]
[3,"37.","37.21.","dakrandprofielen - metaal"]
[3,"37.","37.21.10.","dakrandprofielen - metaal/zink ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"37.",{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen"]
[3,"37.",null,null,"PM"]
[3,"37.","37.21.20.","dakrandprofielen - metaal/aluminium ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"37.",{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen"]
[3,"37.",null,null,"PM"]
[3,"37.","37.21.30.","dakrandprofielen - metaal/metaalfolieplaten ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"37.",{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen"]
[3,"37.",null,null,"PM"]
[3,"37.","37.22.","dakrandprofielen - kunststof"]
[3,"37.","37.22.10.","dakrandprofielen - kunststof/polyester ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"37.",{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen"]
[{"$nulls":4},"PM"]
[3,"37.","37.30.","muurkappen - algemeen"]
[3,"37.","37.31.","muurkappen - metaal"]
[3,"37.","37.31.10.","muurkappen - metaal/zink ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"37.",{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen"]
[3,"37.","37.31.20.","muurkappen - metaal/aluminium ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"37.",{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen"]
[3,"37.","37.32.","muurkappen - kunststof ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"37.",{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen"]
[3,"37.","37.40.","uitbekleding kroonlijsten en luifels - algemeen"]
[3,"37.","37.41.","uitbekleding kroonlijsten en luifels - planchetten"]
[3,"37.","37.41.10.","uitbekleding kroonlijsten en luifels - planchetten/massief hout ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[3,"37.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"37.",{"$nulls":5},"Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[3,"37.","37.41.20.","uitbekleding kroonlijsten en luifels - planchetten/kunststof ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[3,"37.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"37.","37.41.30.","uitbekleding kroonlijsten en luifels - planchetten/vezelcement ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[3,"37.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"37.","37.42.","uitbekleding kroonlijsten en luifels - platen"]
[3,"37.","37.42.10.","uitbekleding kroonlijsten en luifels - platen/multiplex ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[3,"37.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"37.","37.42.20.","uitbekleding kroonlijsten en luifels - platen/kunststof ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[3,"37.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"37.","37.42.30.","uitbekleding kroonlijsten en luifels - platen/vezelcement ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[3,"37.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"37.","37.42.40.","uitbekleding kroonlijsten en luifels - platen/kunsthars ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[3,"37.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"37.","37.42.50.","uitbekleding kroonlijsten en luifels - platen/minerale vezels ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[3,"37.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"37.","37.43.","uitbekleding kroonlijsten en luifels - leien"]
[3,"37.","37.43.10.","uitbekleding kroonlijsten en luifels - leien/vezelcement ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[3,"37.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"37.","37.43.20.","uitbekleding kroonlijsten en luifels - leien hout ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[3,"37.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[3,"37.","37.50.","toebehoren dakranden - algemeen"]
[3,"37.","37.51.","toebehoren dakranden - valbeveiliging"]
[3,"37.","37.51.10.","toebehoren dakranden - valbeveiliging/lijn- of railsysteem ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie"]
[3,"37.","37.51.20.","toebehoren dakranden - valbeveiliging/permanente leuning ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie"]
[3,"37.","37.52.","toebehoren dakranden - gevelonderhoudsinstallaties"]
[3,"37.","37.52.10.","toebehoren dakranden - gevelonderhoud/railsysteem ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie"]
[3,"37.","37.53.","toebehoren dakranden - verhuisbalk ","FH","st","TYPE 3","Beam",null,"Stuks"]
[3,"37."]
[3,"38.","38.","DAKWATERAFVOER"]
[3,"38.","38.00.","dakwaterafvoer - algemeen"]
[3,"38.","38.10.","bakgootdichtingen - algemeen"]
[3,"38.","38.11.","bakgootdichtingen - metaalbladen"]
[3,"38.","38.11.10.","bakgootdichtingen - metaalbladen/zink ","FH","m2","TYPE 3","Beam","complex profile","Component Area"]
[3,"38.","38.11.20.","bakgootdichtingen - metaalbladen/koper ","FH","m2","TYPE 3","Beam","complex profile","Component Area"]
[3,"38.","38.12.","bakgootdichtingen - bitumen"]
[3,"38.","38.12.10.","bakgootdichtingen - bitumen/SBS ","FH","m2","TYPE 3","Beam","complex profile","Component Area"]
[3,"38.","38.12.20.","bakgootdichtingen - bitumen/APP ","FH","m2","TYPE 3","Beam","complex profile","Component Area"]
[3,"38.","38.13.","bakgootdichtingen - hoog polymeermembranen"]
[3,"38.","38.13.10.","bakgootdichtingen - hoog polymeermembranen/EPDM ","FH","m2","TYPE 3","Beam","complex profile","Component Area"]
[3,"38.","38.13.20.","bakgootdichtingen - hoog polymeermembranen/TPO ","FH","m2","TYPE 3","Beam","complex profile","Component Area"]
[3,"38.","38.13.30.","bakgootdichtingen - hoog polymeermembranen/PVC ","FH","m2","TYPE 3","Beam","complex profile","Component Area"]
[3,"38.","38.20.","hanggoten - algemeen"]
[3,"38.","38.21.","hanggoten - kunststof"]
[3,"38.","38.21.10.","hanggoten - kunststof/PVC ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"38.","38.21.20.","hanggoten - kunststof/polyesterhars ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"38.","38.22.","hanggoten - metaal"]
[3,"38.","38.22.10.","hanggoten - metaal/zink ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"38.","38.22.20.","hanggoten - metaal/aluminium ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"38.","38.22.30.","hanggoten - metaal/koper ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"38.","38.22.40.","hanggoten - metaal/gecoat staal ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"38.","38.22.50.","hanggoten - metaal/roestvast staal ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"38.","38.30.","afvoerpijpen - algemeen"]
[3,"38.","38.31.","afvoerpijpen - kunststof"]
[3,"38.","38.31.10.","afvoerpijpen - kunststof/PVC ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"38.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[3,"38.","38.31.20.","afvoerpijpen - kunststof/HDPE ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"38.","38.32.","afvoerpijpen - metaal","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[3,"38.","38.32.10.","afvoerpijpen - metaal/zink ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"38.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[3,"38.","38.32.20.","afvoerpijpen - metaal/koper ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"38.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[3,"38.","38.32.30.","afvoerpijpen - metaal/aluminium ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"38.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[3,"38.","38.32.40.","afvoerpijpen - metaal/gecoat staal ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[3,"38.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[3,"38.","38.32.50.","afvoerpijpen - metaal/roestvast staal ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[{"$nulls":6},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[3,"38.","38.40.","eindstukken - algemeen"]
[3,"38.","38.41.","eindstukken - slagvast kunststof ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"38.",null,null,"PM"]
[3,"38.","38.42.","eindstukken - behandeld gietijzer ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"38.",null,null,"PM"]
[3,"38.","38.43.","eindstukken - gegoten aluminium ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"38.",null,null,"PM"]
[3,"38.","38.50.","toebehoren - algemeen"]
[3,"38.","38.51.","toebehoren - dakkolken en tapbuizen ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"38.",null,null,"PM"]
[3,"38.","38.52.","toebehoren - draad- en bolroosters ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"38.",null,null,"PM"]
[3,"38.","38.53.","toebehoren - balkonafvoerputjes ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"38.",null,null,"PM"]
[3,"38.","38.54.","toebehoren - noodspuwers ","FH","st","TYPE 5","Object",null,"Stuks"]
[3,"38.",null,null,"PM"]
[3,"38."]
[4,"40.","40.","BUITENSCHRIJNWERK"]
[4,"40.","40.00.","buitenschrijnwerk - algemeen"]
[4,"40.","40.01.","buitenschrijnwerk - prestaties"]
[4,"40.","40.02.","buitenschrijnwerk - proeven"]
[4,"40.","40.02.10.","buitenschrijnwerk - proeven/op kosten ongelijk ","PM"]
[4,"40.","40.02.20.","buitenschrijnwerk - proeven/op kosten aannemer ","VH","st","TYPE 5","Object",null,"Stuks"]
[4,"40.","40.03.","buitenschrijnwerk - montage"]
[4,"40.","40.03.10.","buitenschrijnwerk - montage/spouwconstructie en dorpel ","PM"]
[4,"40.","40.03.20.","buitenschrijnwerk - montage/buitengevelisolatiesysteem ","PM"]
[4,"40.","40.03.30.","buitenschrijnwerk - montage/gevelbekledingsysteem ","PM"]
[4,"40.","40.03.40.","buitenschrijnwerk - montage/houtskeletbouw ","PM"]
[4,"40.","40.03.50.","buitenschrijnwerk - montage/vervanging schrijnwerk ","PM"]
[4,"40.","40.04.","buitenschrijnwerk - borderel"]
[4,"40.","40.10.","profielsystemen - algemeen"]
[4,"40.","40.11.","profielsysteem - hout"]
[4,"40.","40.11.10.","profielsysteem - hout/vaste ramen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side"]
[4,"40.",null,null,"PM"]
[4,"40.","40.11.20.","profielsysteem - hout/draairamen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side"]
[4,"40.",null,null,"PM"]
[4,"40.","40.11.30.","profielsysteem - hout/schuiframen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side"]
[4,"40.",null,null,"PM"]
[4,"40.",null,null,null,"m2","TYPE 5","Door",null,"W/D opening nominal surface area"]
[4,"40.","40.11.40.","profielsysteem - hout/buitendeuren ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area"]
[4,"40.",null,null,"PM"]
[4,"40.","40.12.","profielsysteem - aluminium"]
[4,"40.","40.12.10.","profielsysteem - aluminium/vaste ramen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side"]
[4,"40.",null,null,"PM"]
[4,"40.","40.12.20.","profielsysteem - aluminium/draairamen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side"]
[4,"40.",null,null,"PM"]
[4,"40.","40.12.30.","profielsysteem - aluminium/schuiframen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side"]
[4,"40.",null,null,"PM"]
[4,"40.",null,null,null,"m2","TYPE 5","Door",null,"W/D opening nominal surface area"]
[4,"40.","40.12.40.","profielsysteem - aluminium/buitendeuren ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area"]
[4,"40.","40.13.","profielsysteem - pvc"]
[4,"40.","40.13.10.","profielsysteem - pvc/vaste ramen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side"]
[4,"40.",null,null,"PM"]
[4,"40.","40.13.20.","profielsysteem - pvc/draairamen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side"]
[4,"40.",null,null,"PM"]
[4,"40.",null,null,null,"m2","TYPE 5","Door",null,"W/D opening nominal surface area"]
[4,"40.","40.13.30.","profielsysteem - pvc/schuiframen ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area"]
[4,"40.",null,null,"PM"]
[4,"40.","40.13.40.","profielsysteem - pvc/buitendeuren ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side"]
[4,"40.","40.14.","profielsysteem - staal"]
[4,"40.","40.14.10.","profielsysteem - staal/vaste ramen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side"]
[4,"40.",null,null,"PM"]
[4,"40.","40.14.20.","profielsysteem - staal/buitendeuren ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area"]
[4,"40.",null,null,"PM"]
[4,"40.","40.20.","hang- en sluitwerk - algemeen"]
[4,"40.","40.21.","hang- en sluitwerk - standaard beslag ","PM"]
[4,"40.","40.22.","hang- en sluitwerk - scharnieren en paumellen ","PM"]
[4,"40.","40.23.","hang- en sluitwerk - sloten ","PM"]
[4,"40.","40.23.10.","hang- en sluitwerk - sloten/manueel ","PM"]
[4,"40.","40.23.20.","hang- en sluitwerk - sloten/elektromagnetisch ","PM"]
[4,"40.","40.23.30.","hang- en sluitwerk - sloten/schuifdeurslot ","PM"]
[4,"40.","40.23.40.","hang- en sluitwerk - sloten/glasdeurslot ","PM"]
[4,"40.","40.23.50.","hang- en sluitwerk - sloten/sleutelplan ","PM"]
[4,"40.","40.24.","hang- en sluitwerk - deurdrangers ","PM"]
[4,"40.","40.24.10.","hang- en sluitwerk - deurdrangers/manueel ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurdranger","Stuks"]
[4,"40.",null,null,"PM"]
[4,"40.","40.24.20.","hang- en sluitwerk - deurdrangers/gemotoriseerd ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurdranger","Stuks"]
[4,"40.",null,null,"PM"]
[4,"40.","40.25.","hang- en sluitwerk - panieksluitingen ","PM"]
[4,"40.","40.26.","hang- en sluitwerk - raamkrukken ","PM"]
[4,"40.","40.27.","hang- en sluitwerk - deurkrukken ","PM"]
[4,"40.","40.28.","hang- en sluitwerk - vaste handgrepen ","PM"]
[4,"40.","40.29.","hang- en sluitwerk - toebehoren"]
[4,"40.","40.30.","ventilatieroosters - algemeen"]
[4,"40.","40.31.","ventilatieroosters - op glas"]
[4,"40.","40.31.10.","ventilatieroosters - op glas/kleprooster ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW ventilatierooster","ARCHICAD property: Lengte dorpel"]
[4,"40.",null,null,"PM"]
[4,"40.","40.32.","ventilatieroosters - op profiel"]
[4,"40.","40.32.10.","ventilatieroosters - op profiel/kleprooster ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW ventilatierooster","ARCHICAD property: Lengte dorpel"]
[{"$nulls":4},"PM"]
[4,"40.","40.40","beglazing - algemeen"]
[4,"40.","40.40.10.","beglazing - prestaties"]
[4,"40.","40.41.","beglazing - enkel glas"]
[4,"40.","40.41.10.","beglazing - enkel glas/type 1 ","PM"]
[4,"40.","40.42.","beglazing - dubbele beglazing"]
[4,"40.","40.42.10.","beglazing - dubbele beglazing/type 1 ","PM"]
[4,"40.","40.42.20.","beglazing - dubbele beglazing/type 2 ","PM"]
[4,"40.","40.43.","beglazing - drievoudige beglazing"]
[4,"40.","40.43.10.","beglazing - drievoudige beglazing/type 1 ","PM"]
[4,"40.","40.43.20.","beglazing - driedubbele beglazing/type 2 ","PM"]
[4,"40.","40.44.","beglazing - bijzondere beglazing"]
[4,"40.","40.44.10.","beglazing - bijzondere beglazing/dun monumentenglas ","PM"]
[4,"40.","40.50.","vulelementen - algemeen"]
[4,"40.","40.51.","vulelementen - kunststof ","PM"]
[4,"40.","40.52.","vulelementen - aluminium ","PM"]
[4,"40.","40.53.","vulelementen - kunsthars ","PM"]
[4,"40.","40.54.","vulelementen - vezelcement ","PM"]
[4,"40.","40.55.","vulelementen - multiplexplaten  ","PM"]
[4,"40.","40.56.","vulelementen - massief houten beplanking ","PM"]
[4,"40.","40.60.","raamdorpels - algemeen"]
[4,"40.","40.61.","raamdorpels - aluminium ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW raamdorpels","ARCHICAD property: Lengte dorpel"]
[4,"40.","40.62.","raamdorpels - staal ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW raamdorpels","ARCHICAD property: Lengte dorpel"]
[4,"40.","40.63.","raamdorpels - kunststof ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW raamdorpels","ARCHICAD property: Lengte dorpel"]
[4,"40.","40.70.","omkaderingselementen - algemeen"]
[4,"40.","40.71.","omkaderingselementen - hout ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[4,"40.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[4,"40.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten","omtrek dagkanten (2x hoogte + 1x breedte)"]
[4,"40.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten","Lengte omkaderingselement"]
[4,"40.",null,null,"PM"]
[4,"40.","40.72.","omkaderingselementen - aluminium ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[4,"40.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[4,"40.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten","omtrek dagkant uitgezonderd lengte dorpel"]
[4,"40.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten","Lengte omkaderingselement"]
[4,"40.",null,null,"PM"]
[4,"40.","40.80.","toebehoren - algemeen"]
[4,"40.","40.81.","toebehoren - brievenkleppen ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks"]
[4,"40.",null,null,"PM"]
[4,"40.","40.82.","toebehoren - deurspionnen ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks"]
[4,"40.",null,null,"PM"]
[4,"40.","40.83.","toebehoren - beschermplaten ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks"]
[4,"40.",null,null,"PM"]
[4,"40.","40.84.","toebehoren - deurstoppen ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks"]
[4,"40.",null,null,"PM"]
[4,"40.","40.85.","toebehoren - huisnummers ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks"]
[4,"40.",null,null,"PM"]
[4,"40.","40.86.","toebehoren - deur- en naambordjes ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks"]
[4,"40.",null,null,"PM"]
[4,"40.","40.87.","toebehoren - doorvalbeveiliging"]
[4,"40.","40.87.10.","toebehoren - doorvalbeveiliging/kokerprofiel ","FH","m ","TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
[4,"40.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[4,"40.",null,null,"PM"]
[4,"40.","40.87.20.","toebehoren - doorvalbeveiliging/glasplaat ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[4,"40.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[4,"40.",null,null,"PM"]
[4,"40."]
[4,"41.","41.","POORTEN & EXTERNE ZONWERING"]
[4,"41.","41.00.","poorten & externe zonwering - algemeen"]
[4,"41.","41.10.","kantelpoorten - algemeen"]
[4,"41.","41.11.","kantelpoorten - poortblad staal"]
[4,"41.","41.11.10.","kantelpoorten - poortblad staal/manueel ","FH","st","TYPE 5","Door",null,"Stuks"]
[4,"41.","41.11.20.","kantelpoorten - poortblad staal/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks"]
[4,"41.","41.12.","kantelpoorten - poortblad hout"]
[4,"41.","41.12.10.","kantelpoorten - poortblad hout/manueel ","FH","st","TYPE 5","Door",null,"Stuks"]
[4,"41.","41.12.20.","kantelpoorten - poortblad hout/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks"]
[4,"41.","41.13.","kantelpoorten - poortblad kunststof"]
[4,"41.","41.13.10.","kantelpoorten - poortblad kunststof/manueel ","FH","st","TYPE 5","Door",null,"Stuks"]
[4,"41.","41.13.20.","kantelpoorten - poortblad kunststof/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks"]
[4,"41.","41.20.","sectionaalpoorten - algemeen"]
[4,"41.","41.21.","sectionaalpoorten - staal"]
[4,"41.","41.21.10.","sectionaalpoorten - staal/manueel ","FH","st","TYPE 5","Door",null,"Stuks"]
[4,"41.","41.21.20.","sectionaalpoorten - staal/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks"]
[4,"41.","41.22.","sectionaalpoorten - aluminium"]
[4,"41.","41.22.10.","sectionaalpoorten - aluminium/manueel ","FH","st","TYPE 5","Door",null,"Stuks"]
[4,"41.","41.22.20.","sectionaalpoorten - aluminium/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks"]
[4,"41.","41.30.","Externe zonnewering - algemeen",{"$nulls":6},"Uitbreiding op de basis VMSW artikellijst"]
[4,"41.","41.31.","Externe zonnewering - rolluiken","FH","m2","TYPE 4","Window","ARCHICAD property: VMSW zonnewering","W/D Opening Surface on the Reveal Side","Uitbreiding op de basis VMSW artikellijst"]
[4,"41.","41.32.","Externe zonnewering - screens","FH","m2","TYPE 4","Window","ARCHICAD property: VMSW zonnewering","W/D Opening Surface on the Reveal Side","Uitbreiding op de basis VMSW artikellijst"]
[4,"41."]
[4,"42.","42.","GEVELBEKLEDINGEN"]
[4,"42.","42.00.","gevelbekledingen - algemeen"]
[4,"42.","42.10.","regelstructuur - algemeen"]
[4,"42.","42.11.","regelstructuur - hout ","PM"]
[4,"42.","42.12.","regelstructuur - aluminium ","PM"]
[4,"42.","42.20.","thermische isolatie voorhanggevel - algemeen"]
[4,"42.","42.21.","thermische isolatie voorhanggevel - MW"]
[4,"42.","42.21.10.","thermische isolatie voorhanggevel - MW/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[4,"42.","42.21.20.","thermische isolatie voorhanggevel - MW/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[4,"42.","42.22.","thermische isolatie voorhanggevel - PUR of PIR"]
[4,"42.","42.22.10.","thermische isolatie voorhanggevel - PUR of PIR/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[4,"42.","42.22.20.","thermische isolatie voorhanggevel - PUR of PIR/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[4,"42.","42.23.","thermische isolatie voorhanggevel - PF"]
[4,"42.","42.23.10.","thermische isolatie voorhanggevel - PF/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[4,"42.","42.23.20.","thermische isolatie voorhanggevel - PF/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[4,"42.","42.24.","thermische isolatie voorhanggevel - EPS"]
[4,"42.","42.24.10.","thermische isolatie voorhanggevel - EPS/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[4,"42.","42.24.20.","thermische isolatie voorhanggevel - EPS/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[4,"42.","42.25.","thermische isolatie voorhanggevel - XPS"]
[4,"42.","42.25.10.","thermische isolatie voorhanggevel - XPS/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[4,"42.","42.25.20.","thermische isolatie voorhanggevel - XPS/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[4,"42.","42.30.","buitenfolie - algemeen"]
[4,"42.","42.31.","buitenfolie - gevelfolie ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[4,"42.","42.40.","bekledingspanelen - algemeen"]
[4,"42.","42.41.","bekledingspanelen - HPL ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[4,"42.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[4,"42.",{"$nulls":5},"Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[4,"42.","42.42.","bekledingspanelen - vezelcement ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[4,"42.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[4,"42.",{"$nulls":5},"Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[4,"42.","42.43.","bekledingspanelen - minerale vezels ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[4,"42.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[4,"42.",{"$nulls":5},"Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[4,"42.","42.50.","bekledingsplanchetten - algemeen"]
[4,"42.","42.51.","bekledingsplanchetten - massief hout ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[4,"42.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[4,"42.",{"$nulls":5},"Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[4,"42.","42.52.","bekledingsplanchetten - kunststof ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[4,"42.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[4,"42.",{"$nulls":5},"Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[4,"42.","42.53.","bekledingsplanchetten - vezelcement ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[4,"42.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[4,"42.",{"$nulls":5},"Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[4,"42.","42.60.","gevelleien - algemeen"]
[4,"42.","42.61.","gevelleien - vezelcementleien ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[4,"42.","42.70.","geprofileerde metaalplaten - algemeen"]
[4,"42.","42.71.","geprofileerde metaalplaten - gecoat staal ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[4,"42.","42.72.","geprofileerde metaalplaten - aluminium ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[4,"42."]
[4,"43.","43.","BUITENBEPLEISTERING"]
[4,"43.","43.00.","buitenbepleistering - algemeen"]
[4,"43.","43.10.","sierpleisters op metselwerk - algemeen"]
[4,"43.","43.11.","sierpleisters op metselwerk - minerale pleister ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[4,"43.","43.20.","buitengevelisolatiesystemen met pleister - algemeen"]
[4,"43.","43.21.","buitengevelisolatiesystemen met pleister - EPS"]
[4,"43.","43.21.10.","buitengevelisolatiesystemen met pleister - EPS/isolatie"]
[4,"43.","43.21.11.","buitengevelisolatiesystemen met pleister - EPS/isolatie - 14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[4,"43.","43.21.12.","buitengevelisolatiesystemen met pleister - EPS/isolatie - 16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[4,"43.","43.21.20.","buitengevelisolatiesystemen met pleister - EPS/pleister ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[4,"43.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","omtrek dagkanten (2x hoogte + 1x breedte)"]
[4,"43.",{"$nulls":5},"Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[4,"43.","43.22.","buitengevelisolatiesystemen met pleister - MW"]
[4,"43.","43.22.10.","buitengevelisolatiesystemen met pleister - MW/isolatie"]
[4,"43.","43.22.11.","buitengevelisolatiesystemen met pleister - MW/isolatie - 14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[4,"43.","43.22.12.","buitengevelisolatiesystemen met pleister - MW/isolatie - 16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area"]
[4,"43.","43.22.20.","buitengevelisolatiesystemen met pleister - MW/pleister ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[4,"43.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","omtrek dagkanten (2x hoogte + 1x breedte)"]
[4,"43.",{"$nulls":5},"Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[4,"43."]
[4,"44.","44.","BUITENTRAPPEN & BORSTWERINGEN"]
[4,"44.","44.00.","buitentrappen en borstweringen - algemeen"]
[4,"44.","44.10.","trappen - algemeen"]
[4,"44.","44.11.","trappen - staal ","FH","st","TYPE 5","Stair",null,"Stuks"]
[4,"44.",null,null,"SOG"]
[4,"44.","44.20.","borstweringen - algemeen"]
[4,"44.","44.21.","borstweringen - staal ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie"]
[4,"44.",null,null,null,"st","TYPE 5","Railing",null,"Stuks"]
[4,"44.","44.22.","borstweringen - roestvast staal (RVS) ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie"]
[4,"44.","44.23.","borstweringen - aluminium ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie"]
[4,"44.","44.24.","borstweringen - veiligheidsglas ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie"]
[4,"44.","44.30.","trapleuningen - algemeen ","PM"]
[4,"44.","44.40.","vulpanelen en -roosters - algemeen ","PM"]
[4,"44.","44.50.","handgrepen - algemeen ","PM"]
[4,"44.","44.60.","brandladders - algemeen"]
[4,"44.","44.61.","brandladders - verzinkt staal ","FH","st","TYPE 5","Object",null,"Stuks"]
[4,"44.",{"$nulls":5},"Stair",null,"Stuks"]
[4,"44.","44.62.","brandladders - aluminium ","FH","st","TYPE 5","Object",null,"Stuks"]
[4,"44.",{"$nulls":5},"Stair",null,"Stuks"]
[4,"44."]
[5,"50.","50.","BINNENPLEISTERWERKEN"]
[5,"50.","50.00.","binnenpleisterwerken - algemeen"]
[5,"50.","50.10.","wandbepleistering - algemeen"]
[5,"50.","50.11.","wandbepleistering - gipspleisters"]
[5,"50.","50.11.10.","wandbepleistering - gipspleisters/dikpleister op metselwerk"]
[5,"50.","50.11.11.","wandbepleistering - gipspleisters/dikpleisters op metselwerk - wandvlakken ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[5,"50.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[5,"50.","50.11.12.","wandbepleistering - gipspleisters/dikpleisters op metselwerk - dagkanten ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","omtrek dagkanten (2x hoogte + 1x breedte)"]
[5,"50.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk"]
[5,"50.","50.11.20.","wandbepleistering - gipspleisters/dunpleister op lijmblokken"]
[5,"50.","50.11.21.","wandbepleistering - gipspleisters/dunpleister op lijmblokken - wandvlakken ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[5,"50.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[5,"50.","50.11.22.","wandbepleistering - gipspleisters/dunpleister op lijmblokken - dagkanten ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","omtrek dagkanten (2x hoogte + 1x breedte)"]
[5,"50.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk"]
[5,"50.","50.11.30.","wandbepleistering - gipspleisters/pleister op beplating"]
[5,"50.","50.11.31.","wandbepleistering - gipspleisters/pleister op beplating - wandvlakken ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[5,"50.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[5,"50.","50.11.32.","wandbepleistering - gipspleisters/pleister op beplating - dagkanten ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","omtrek dagkanten (2x hoogte + 1x breedte)"]
[5,"50.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk"]
[5,"50.","50.11.40.","wandbepleistering - gipspleisters/pleister op gaas"]
[5,"50.","50.11.41.","wandbepleistering - gipspleisters/pleister op gaas - wandvlakken ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[5,"50.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[5,"50.","50.11.42.","wandbepleistering - gipspleisters/pleister op gaas - dagkanten ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","omtrek dagkanten (2x hoogte + 1x breedte)"]
[5,"50.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk"]
[5,"50.","50.12.","wandbepleistering - cementpleisters"]
[5,"50.","50.12.10.","wandbepleistering - cementpleisters/te betegelen ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[5,"50.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[5,"50.","50.12.20.","wandbepleistering - cementpleisters/afwerksysteem ","FH","m2","TYPE 3","Wall",null,"Projected Area"]
[5,"50.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[5,"50.","50.20.","plafondbepleistering - algemeen"]
[5,"50.","50.21.","plafondbepleistering - gipspleisters"]
[5,"50.","50.21.10.","plafondbepleistering - gipspleisters/dikpleister op welfsels"]
[5,"50.","50.21.11.","plafondbepleistering - gipspleisters/dikpleister op welfsels - plafondoppervlakte ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[5,"50.",{"$nulls":5},"Shell",null,"Top Surface"]
[5,"50.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"50.","50.21.12.","plafondbepleistering - gipspleisters/dikpleister op welfsels - zijkanten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
[5,"50.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[5,"50.","50.21.20.","plafondbepleistering - gipspleisters/dunpleister op breedplaatvloeren "]
[5,"50.","50.21.21.","plafondbepleistering - gipspleisters/dunpleister op breedplaatvloeren - plafondoppervlakte ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[5,"50.",{"$nulls":5},"Shell",null,"Top Surface"]
[5,"50.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"50.","50.21.22.","plafondbepleistering - gipspleisters/dunpleister op breedplaatvloeren - zijkanten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
[5,"50.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[5,"50.","50.21.30.","plafondbepleistering - gipspleisters/pleister op beplating "]
[5,"50.","50.21.31.","plafondbepleistering - gipspleisters/pleister op beplating - plafondoppervlakte ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[5,"50.",{"$nulls":5},"Shell",null,"Top Surface"]
[5,"50.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"50.","50.21.32.","plafondbepleistering - gipspleisters/pleister op beplating - zijkanten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
[5,"50.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[5,"50.","50.21.40.","plafondbepleistering - gipspleisters/pleister op pleisterdrager "]
[5,"50.","50.21.41.","plafondbepleistering - gipspleisters/pleister op pleisterdrager - plafondoppervlakte ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[5,"50.",{"$nulls":5},"Shell",null,"Top Surface"]
[5,"50.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"50.","50.21.42.","plafondbepleistering - gipspleisters/pleister op pleisterdrager - zijkanten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
[5,"50.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[5,"50.","50.30.","renovatie pleisterwerk - algemeen ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[5,"50.",{"$nulls":5},"Shell",null,"Top Surface"]
[5,"50.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"50.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[5,"50."]
[5,"51.","51.","BINNENPLAATAFWERKINGEN"]
[5,"51.","51.00.","binnenplaatafwerkingen - algemeen"]
[5,"51.","51.10.","lichte scheidingswanden - algemeen"]
[5,"51.","51.11.","lichte scheidingswanden - gipskartonplaten ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[5,"51.",{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[5,"51.","51.12.","lichte scheidingswanden - gipsvezelplaten ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[5,"51.",{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[5,"51.","51.13.","lichte scheidingswanden - vezelcementplaten ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[5,"51.",{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[5,"51.","51.14.","lichte scheidingswanden - calciumsilicaatplaten ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[5,"51.",{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[5,"51.","51.15.","lichte scheidingswanden - multiplexplaten ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[5,"51.",{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[5,"51.","51.16.","lichte scheidingswanden - OSB-platen ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[5,"51.",{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[5,"51.","51.17.","lichte scheidingswanden - MDF-platen","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[5,"51.",{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand"]
[5,"51.","51.20.","voorzetwanden - algemeen"]
[5,"51.","51.21.","voorzetwanden - gipskartonplaten"]
[5,"51.","51.21.10.","voorzetwanden - gipskartonplaten/op regelstructuur ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand"]
[5,"51.","51.21.20.","voorzetwanden - gipskartonplaten/gekleefd ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand"]
[5,"51.","51.22.","voorzetwanden - gipsvezelplaten"]
[5,"51.","51.22.10.","voorzetwanden - gipsvezelplaten/op regelstructuur ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand"]
[5,"51.","51.22.20.","voorzetwanden - gipsvezelplaten/gekleefd ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand"]
[5,"51.","51.23.","voorzetwanden - vezelcementplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand"]
[5,"51.","51.24.","voorzetwanden - calciumsilicaatplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand"]
[5,"51.","51.25.","voorzetwanden - multiplex ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand"]
[5,"51.","51.26.","voorzetwanden - OSB-platen ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand"]
[5,"51.","51.27.","voorzetwanden - MDF-platen","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand"]
[5,"51.","51.30.","schachtwanden - algemeen"]
[5,"51.","51.31.","schachtwanden - gipskartonplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand"]
[5,"51.","51.32.","schachtwanden - gipsvezelplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand"]
[5,"51.","51.33.","schachtwanden - vezelcementplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand"]
[5,"51.","51.34.","schachtwanden - calciumsilicaatplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand"]
[5,"51.","51.35.","schachtwanden - multiplexplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand"]
[5,"51.","51.36.","schachtwanden - OSB-platen ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand"]
[5,"51.","51.37.","schachtwanden - MDF-platen","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand"]
[5,"51.","51.38.","schachtwanden - kunstharsplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand"]
[5,"51.","51.40.","toegangsluiken - algemeen"]
[5,"51.","51.41.","toegangsluiken - hout ","FH","st","TYPE 5","Door",null,"Stuks"]
[5,"51.",{"$nulls":5},"Window",null,"Stuks"]
[5,"51.",null,null,"PM"]
[5,"51.","51.42.","toegangsluiken - kunsthars ","FH","st","TYPE 5","Door",null,"Stuks"]
[5,"51.",{"$nulls":5},"Window",null,"Stuks"]
[5,"51.",null,null,"PM"]
[5,"51.","51.43.","toegangsluiken - vezelcement ","FH","st","TYPE 5","Door",null,"Stuks"]
[5,"51.",{"$nulls":5},"Window",null,"Stuks"]
[5,"51.",null,null,"PM"]
[5,"51.","51.44.","toegangsluiken - metalen kader ","FH","st","TYPE 5","Door",null,"Stuks"]
[5,"51.",{"$nulls":5},"Window",null,"Stuks"]
[5,"51.",null,null,"PM"]
[5,"51.","51.50.","plafondafwerking - algemeen"]
[5,"51.","51.51.","plafondafwerking - uitbekleding plafond"]
[5,"51.","51.51.10.","plafondafwerking - uitbekleding plafond/gipskartonplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[5,"51.",{"$nulls":5},"Shell",null,"Top Surface"]
[5,"51.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"51.",{"$nulls":5},"Wall",null,"Netto oppervlak binnenkant wand"]
[5,"51.","51.51.20.","plafondafwerking - uitbekleding plafond/gipsvezelplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[5,"51.",{"$nulls":5},"Shell",null,"Top Surface"]
[5,"51.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"51.","51.51.30.","plafondafwerking - uitbekleding plafond/vezelcementplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[5,"51.",{"$nulls":5},"Shell",null,"Top Surface"]
[5,"51.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"51.","51.51.40.","plafondafwerking - uitbekleding plafond/calciumsilicaatplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[5,"51.",{"$nulls":5},"Shell",null,"Top Surface"]
[5,"51.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"51.","51.51.50.","plafondafwerking - uitbekleding plafond/OSB","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[5,"51.",{"$nulls":5},"Shell",null,"Top Surface"]
[5,"51.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"51."]
[5,"51.","51.52.","plafondafwerking - uitbekleding daklichtopeningen ","FH","m","TYPE 3","Wall"]
[5,"51.",{"$nulls":4},"TYPE 4","Object","gebruik ARCHICAD property: VMSW uitbekleding daglichtopeningen "]
[5,"51.",{"$nulls":5},"Skylight","gebruik ARCHICAD property: VMSW uitbekleding daglichtopeningen "]
[5,"51.",null,null,null,"m2","TYPE 3","Wall",null,"Projected Area"]
[5,"51.",{"$nulls":4},"TYPE 4","Object","gebruik ARCHICAD property: VMSW uitbekleding daglichtopeningen "]
[5,"51.",{"$nulls":5},"Skylight","gebruik ARCHICAD property: VMSW uitbekleding daglichtopeningen ","Oppervlakte volgens openingshoogte daklicht en dikte dak"]
[5,"51.",null,null,"PM"]
[5,"51.","51.53.","plafondafwerking - verlaagd plafond"]
[5,"51.","51.53.10.","plafondafwerking - verlaagd plafond/gipskartonplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[5,"51.",{"$nulls":5},"Shell",null,"Top Surface"]
[5,"51.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"51.","51.53.20.","plafondafwerking - verlaagd plafond/gipsvezelplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[5,"51.",{"$nulls":5},"Shell",null,"Top Surface"]
[5,"51.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"51.","51.53.30.","plafondafwerking - verlaagd plafond/vezelcementplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[5,"51.",{"$nulls":5},"Shell",null,"Top Surface"]
[5,"51.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"51.","51.53.40.","plafondafwerking - verlaagd plafond/calciumsilicaatplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area"]
[5,"51.",{"$nulls":5},"Shell",null,"Top Surface"]
[5,"51.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"51.","51.60.","uitbekleding buitenramen en -deuren - algemeen"]
[5,"51.","51.61.","uitbekleding buitenramen en -deuren - isolatieplaten voor bepleistering ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)"]
[5,"51.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk"]
[5,"51.",null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[5,"51.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[5,"51.","51.62.","uitbekleding buitenramen en -deuren - multiplex ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)"]
[5,"51.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk"]
[5,"51.",null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[5,"51.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[5,"51.","51.63.","uitbekleding buitenramen en -deuren - MDF ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)"]
[5,"51.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk"]
[5,"51.",null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[5,"51.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[5,"51.","51.64.","uitbekleding buitenramen en -deuren - massief hout ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)"]
[5,"51.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk"]
[5,"51.",null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[5,"51.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[5,"51.","51.65.","uitbekleding buitenramen en -deuren - PVC ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)"]
[5,"51.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk"]
[5,"51.",null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[5,"51.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[5,"51.","51.66.","uitbekleding buitenramen en -deuren - gipskarton ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)"]
[5,"51.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk"]
[5,"51.",null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[5,"51.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[5,"51.","51.70.","uitbekleding sanitaire toestellen - algemeen"]
[5,"51.","51.71.","uitbekleding sanitaire toestellen - te betegelen plaat"]
[5,"51.","51.71.10.","uitbekleding sanitaire toestellen - te betegelen plaat/gipskarton ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW uitbeelden sanitaire toestellen","Stuks"]
[5,"51.","51.71.20.","uitbekleding sanitaire toestellen - te betegelen plaat/gipsvezel ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW uitbeelden sanitaire toestellen","Stuks"]
[5,"51.","51.71.30.","uitbekleding sanitaire toestellen - te betegelen plaat/hardschuim ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW uitbeelden sanitaire toestellen","Stuks"]
[5,"51.","51.72.","uitbekleding sanitaire toestellen - plaat als eindafwerking"]
[5,"51.","51.72.10.","uitbekleding sanitaire toestellen - plaat als eindafwerking/kunsthars ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW uitbeelden sanitaire toestellen","Stuks"]
[5,"51.","51.72.20.","uitbekleding sanitaire toestellen - plaat als eindafwerking/multiplex + kunststof ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW uitbeelden sanitaire toestellen","Stuks"]
[5,"51.","51.72.30.","uitbekleding sanitaire toestellen - plaat als eindafwerking/vezelcement ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW uitbeelden sanitaire toestellen","Stuks"]
[5,"51."]
[5,"52.","52.","DEK- EN BEDRIJFSVLOEREN"]
[5,"52.","52.00.","dek- en bedrijfsvloeren - algemeen"]
[5,"52.","52.10.","isolerende uitvullagen - algemeen"]
[5,"52.","52.11.","isolerende uitvullagen - cementgebonden ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.12.","isolerende uitvullagen - schuimbeton ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.13.","isolerende uitvullagen - gespoten polyurethaan ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.14.","isolerende uitvullagen - droge granulaten ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.20.","vochtwerende lagen - algemeen"]
[5,"52.","52.21.","vochtwerende lagen - PE-folie ","PM"]
[5,"52.","52.30.","thermische isolatie vloer - algemeen"]
[5,"52.","52.31.","thermische isolatie vloer - MW"]
[5,"52.","52.31.10.","thermische isolatie vloer - MW/8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.31.20.","thermische isolatie vloer - MW/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.32.","thermische isolatie vloer - PUR of PIR"]
[5,"52.","52.32.10.","thermische isolatie vloer - PUR of PIR 8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.32.20.","thermische isolatie vloer - PUR of PIR/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.33.","thermische isolatie vloer - PF"]
[5,"52.","52.33.10.","thermische isolatie vloer - PF/8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.33.20.","thermische isolatie vloer - PF/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.34.","thermische isolatie vloer - XPS"]
[5,"52.","52.34.10.","thermische isolatie vloer - XPS/8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.34.20.","thermische isolatie vloer - XPS/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.35.","thermische isolatie vloer - EPS"]
[5,"52.","52.35.10.","thermische isolatie vloer - EPS/8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.35.20.","thermische isolatie vloer - EPS/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.40.","akoestische isolatie vloer - algemeen"]
[5,"52.","52.41.","akoestische isolatie vloer - kunststofschuim ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.42.","akoestische isolatie vloer - kokosvezels ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.50.","cementgebonden dekvloeren - algemeen"]
[5,"52.","52.51.","cementgebonden dekvloeren - hechtend ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.52.","cementgebonden dekvloeren - niet hechtend ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.53.","cementgebonden dekvloeren - zwevend ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.54.","cementgebonden dekvloeren - zwevend en gepolierd ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.60.","calciumsulfaatgebonden dekvloeren - algemeen"]
[5,"52.","52.61.","calciumsulfaatgebonden dekvloeren - niet hechtend ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.62.","calciumsulfaatgebonden dekvloeren - zwevend ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.70.","bedrijfsvloeren - algemeen"]
[5,"52.","52.71.","bedrijfsvloeren - gepolierd beton ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52.","52.72.","bedrijfsvloeren - epoxymortel ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"52."]
[5,"53.","53.","BINNENVLOERAFWERKINGEN"]
[5,"53.","53.00.","binnenvloerafwerkingen - algemeen"]
[5,"53.","53.10.","tegelvloeren - algemeen"]
[5,"53.","53.11.","tegelvloeren - keramisch"]
[5,"53.","53.11.10.","tegelvloeren - keramisch/getrokken tegels ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"53.",{"$nulls":4},"TYPE 4","Zone",null,"Calculated Area"]
[5,"53.","53.11.20.","tegelvloeren - keramisch/geperste tegels ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"53.",{"$nulls":4},"TYPE 4","Zone",null,"Calculated Area"]
[5,"53.","53.12.","tegelvloeren - marmermozaiek ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"53.",{"$nulls":4},"TYPE 4","Zone",null,"Calculated Area"]
[5,"53.","53.13.","tegelvloeren - natuursteen"]
[5,"53.","53.13.10.","tegelvloeren - natuursteen/blauwe hardsteen ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"53.",{"$nulls":4},"TYPE 4","Zone",null,"Calculated Area"]
[5,"53.","53.13.20.","tegelvloeren - natuursteen/travertijn ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"53.",{"$nulls":4},"TYPE 4","Zone",null,"Calculated Area"]
[5,"53.","53.13.30.","tegelvloeren - natuursteen/jura ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"53.",{"$nulls":4},"TYPE 4","Zone",null,"Calculated Area"]
[5,"53.","53.14.","tegelvloeren - betontegels ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"53.",{"$nulls":4},"TYPE 4","Zone",null,"Calculated Area"]
[5,"53.","53.20.","soepele vloerbekledingen - algemeen"]
[5,"53.","53.21.","soepele vloerbekledingen - linoleum ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"53.",{"$nulls":4},"TYPE 4","Zone",null,"Calculated Area"]
[5,"53.","53.22.","soepele vloerbekledingen - vinyl (PVC) ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"53.",{"$nulls":4},"TYPE 4","Zone",null,"Calculated Area"]
[5,"53.","53.23.","soepele vloerbekledingen - rubber ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"53.",{"$nulls":4},"TYPE 4","Zone",null,"Calculated Area"]
[5,"53.","53.24.","soepele vloerbekledingen - douchecellen ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"53.",{"$nulls":4},"TYPE 4","Zone",null,"Calculated Area"]
[5,"53.","53.30.","houten vloerbekledingen - algemeen"]
[5,"53.","53.31.","houten vloerbekledingen - laminaat ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"53.",{"$nulls":4},"TYPE 4","Zone",null,"Calculated Area"]
[5,"53.","53.32.","houten vloerbekledingen - opschuren bij renovatie ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"53.",{"$nulls":4},"TYPE 4","Zone",null,"Calculated Area"]
[5,"53.","53.40.","plinten - algemeen"]
[5,"53.","53.41.","plinten - steen"]
[5,"53.","53.41.10.","plinten - steen/keramisch ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[5,"53.",{"$nulls":5},"Wall",null,"Reference line length"]
[5,"53.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[5,"53.","53.41.20.","plinten - steen/marmermozaiek ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[5,"53.",{"$nulls":5},"Wall",null,"Reference line length"]
[5,"53.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[5,"53.","53.41.30.","plinten - steen/natuursteen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[5,"53.",{"$nulls":5},"Wall",null,"Reference line length"]
[5,"53.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[5,"53.","53.42.","plinten - hout"]
[5,"53.","53.42.10.","plinten - hout/massief hout ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[5,"53.",{"$nulls":5},"Wall",null,"Reference line length"]
[5,"53.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[5,"53.","53.42.20.","plinten - hout/MDF ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[5,"53.",{"$nulls":5},"Wall",null,"Reference line length"]
[5,"53.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[5,"53.","53.43.","plinten - soepel"]
[5,"53.","53.43.10.","plinten - soepel/linoleum ","FH\n","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[5,"53.",{"$nulls":5},"Wall",null,"Reference line length"]
[5,"53.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[5,"53.","53.43.20.","plinten - soepel/PVC ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[5,"53.",{"$nulls":5},"Wall",null,"Reference line length"]
[5,"53.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[5,"53.","53.43.30.","plinten - soepel/rubber ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[5,"53.",{"$nulls":5},"Wall",null,"Reference line length"]
[5,"53.",{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[5,"53.","53.50.","tussendorpels - algemeen"]
[5,"53.","53.51.","tussendorpels - steen"]
[5,"53.","53.51.10.","tussendorpels - steen/natuursteen ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[5,"53.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW tussendorpel binnendeur","breedte deuropening * muurdikte"]
[5,"53.","53.51.20.","tussendorpels - steen/marmermozaiek ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[5,"53.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW tussendorpel binnendeur","breedte deuropening * muurdikte"]
[5,"53.","53.51.30.","tussendorpels - steen/composiet ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[5,"53.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW tussendorpel binnendeur","breedte deuropening * muurdikte"]
[5,"53.","53.60.","trapbekledingen - algemeen"]
[5,"53.","53.61.","trapbekledingen - steen"]
[5,"53.","53.61.10.","trapbekledingen - steen/keramisch ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks"]
[5,"53.","53.61.20.","trapbekledingen - steen/marmermozaiek ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks"]
[5,"53.","53.61.30.","trapbekledingen - steen/natuursteen ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks"]
[5,"53.","53.62.","trapbekledingen - hout"]
[5,"53.","53.62.10.","trapbekledingen - hout/massief ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks"]
[5,"53.","53.62.20.","trapbekledingen - hout/gelamineerd ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks"]
[5,"53.","53.63.","trapbekledingen - soepel"]
[5,"53.","53.63.10.","trapbekledingen - soepel/rubber ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks"]
[5,"53.","53.70.","toebehoren - algemeen"]
[5,"53.","53.71.","toebehoren - scheidingsprofielen ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[5,"53.",{"$nulls":5},"Wall",null,"Reference line length"]
[5,"53.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[5,"53.","53.72.","toebehoren - vloermatkaders ","FH","st","TYPE 3","Beam",null,"Stuks"]
[5,"53.",{"$nulls":5},"Wall",null,"Stuks"]
[5,"53.",{"$nulls":4},"TYPE 5","Morph",null,"Stuks"]
[5,"53.",{"$nulls":5},"Object",null,"Stuks"]
[5,"53.","53.73.","toebehoren - vloermatten ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[5,"53.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[5,"53.",{"$nulls":5},"Object",null,"Net Area"]
[5,"53.",null,null,null,"st","TYPE 3","Slab",null,"Stuks"]
[5,"53.",{"$nulls":4},"TYPE 5","Morph",null,"Stuks"]
[5,"53.",{"$nulls":5},"Object",null,"Stuks"]
[5,"53.","53.74.","toebehoren - vloerdeksels "]
[5,"53.","53.74.10.","toebehoren - vloerdeksels/metaal","FH","st","TYPE 5","Morph",null,"Stuks"]
[5,"53.",{"$nulls":5},"Object",null,"Stuks"]
[5,"53.","53.74.20.","toebehoren - vloerdeksels/betegelbaar","FH","st","TYPE 5","Morph",null,"Stuks"]
[5,"53.",{"$nulls":5},"Object",null,"Stuks"]
[5,"53.","53.75.","toebehoren - vloerroosters ","FH","st","TYPE 3","Beam",null,"Stuks"]
[5,"53.",{"$nulls":4},"TYPE 5","Morph",null,"Stuks"]
[5,"53.",{"$nulls":5},"Object",null,"Stuks"]
[5,"53.",{"$nulls":5},"Wall",null,"Stuks"]
[5,"53.","53.76.","toebehoren - zettingsprofielen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[5,"53.",{"$nulls":5},"Wall",null,"Reference line length"]
[5,"53.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[5,"53."]
[5,"54.","54.","BINNENDEUREN en -RAMEN"]
[5,"54.","54.00.","binnendeuren en -ramen - algemeen"]
[5,"54.","54.01.","binnendeuren en -ramen - prestaties"]
[5,"54.","54.02.","binnendeuren en -ramen - keuring en proeven"]
[5,"54.","54.03.","binnendeuren en -ramen - proefopstelling"]
[5,"54.","54.10.","deurkozijnen - algemeen"]
[5,"54.","54.11.","deurkozijnen - hout"]
[5,"54.","54.11.10.","deurkozijnen - hout/massief ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks"]
[5,"54.","54.11.20.","deurkozijnen - hout/multiplex ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks"]
[5,"54.","54.11.30.","deurkozijnen - hout/MDF ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks"]
[5,"54.","54.12.","deurkozijnen - staal"]
[5,"54.","54.12.10.","deurkozijnen - staal/montagekozijn ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks"]
[5,"54.","54.12.20.","deurkozijnen - staal/inbouwkozijn ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks"]
[5,"54.","54.20.","deurbladen - algemeen"]
[5,"54.","54.21.","deurbladen - hout met holle kern"]
[5,"54.","54.21.10.","deurbladen - hout met holle kern/celrooster ","FH","st","TYPE 4","Door ","Gebruik ARCHICAD property: VMSW deurblad","Stuks"]
[5,"54.","54.21.20.","deurbladen - hout met holle kern/tubespaan ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurblad","Stuks"]
[5,"54.","54.22.","deurbladen - hout met volle kern"]
[5,"54.","54.22.10.","deurbladen - hout met volle kern/spaan ","FH","st","TYPE 4","Door ","Gebruik ARCHICAD property: VMSW deurblad","Stuks"]
[5,"54.","54.22.20.","deurbladen - hout met volle kern/multiplex ","FH","st","TYPE 4","Door ","Gebruik ARCHICAD property: VMSW deurblad","Stuks"]
[5,"54.","54.30.","deurgehelen - algemeen"]
[5,"54.","54.31.","deurgehelen - kozijnen hout"]
[5,"54.","54.31.10.","deurgehelen - kozijnen hout/brandwerend ","FH","st","TYPE 5","Door",null,"Stuks"]
[5,"54.","54.31.20.","deurgehelen - kozijnen hout/inbraakwerend ","FH","st","TYPE 5","Door",null,"Stuks"]
[5,"54.","54.31.30.","deurgehelen - kozijnen hout/passiefdeur ","FH","st","TYPE 5","Door",null,"Stuks"]
[5,"54.","54.32.","deurgehelen - kozijnen staal"]
[5,"54.","54.32.10.","deurgehelen - kozijnen staal/brandwerend ","FH","st","TYPE 5","Door",null,"Stuks"]
[5,"54.","54.32.20.","deurgehelen - kozijnen staal/inbraakwerend ","FH","st","TYPE 5","Door",null,"Stuks"]
[5,"54.","54.40.","schuif- en vouwdeuren - algemeen"]
[5,"54.","54.41.","schuif- en vouwdeuren - schuifsystemen"]
[5,"54.","54.41.10.","schuif- en vouwdeuren - schuifsystemen/voorbouw ","FH","st","TYPE 5","Door ",null,"Stuks"]
[5,"54.",{"$nulls":5},"Window ",null,"Stuks"]
[5,"54.","54.41.20.","schuif- en vouwdeuren - schuifsystemen/inbouwmodule ","FH","st","TYPE 5","Door ",null,"Stuks"]
[5,"54.",{"$nulls":5},"Window ",null,"Stuks"]
[5,"54.","54.42.","schuif- en vouwdeuren - vouwsystemen"]
[5,"54.","54.42.10.","schuif- en vouwdeuren - vouwsystemen/kunststof ","FH","st","TYPE 5","Door",null,"Stuks"]
[5,"54.",{"$nulls":5},"Window",null,"Stuks"]
[5,"54.","54.50.","glazen deuren - algemeen"]
[5,"54.","54.51.","glazen deuren - opendraaiend ","FH","st","TYPE 5","Door",null,"Stuks"]
[5,"54.","54.52.","glazen deuren - openschuivend ","FH","st","TYPE 5","Door",null,"Stuks"]
[5,"54.","54.60.","hang- en sluitwerk - algemeen"]
[5,"54.","54.61.","hang- en sluitwerk - scharnieren en paumellen"]
[5,"54.","54.61.10.","hang- en sluitwerk - scharnieren en paumellen/aluminium ","PM"]
[5,"54.","54.61.20.","hang- en sluitwerk - scharnieren en paumellen/vernikkeld staal ","PM"]
[5,"54.","54.61.30.","hang- en sluitwerk - scharnieren en paumellen/roestvast staal ","PM"]
[5,"54.","54.62.","hang- en sluitwerk - deursloten"]
[5,"54.","54.62.10.","hang- en sluitwerk - deursloten/klaviersloten ","PM"]
[5,"54.","54.62.20.","hang- en sluitwerk - deursloten/veiligheidssloten ","PM"]
[5,"54.","54.62.30.","hang- en sluitwerk - deursloten/elektromagnetisch ","PM"]
[5,"54.","54.62.40.","hang- en sluitwerk - deursloten/kantschuiven ","PM"]
[5,"54.","54.62.50.","hang- en sluitwerk - deursloten/panieksluitingen ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW panieksluiting","Stuks"]
[5,"54.","54.63.","hang- en sluitwerk - deurkrukken"]
[5,"54.","54.63.10.","hang- en sluitwerk - deurkrukken/aluminium ","PM"]
[5,"54.","54.63.20.","hang- en sluitwerk - deurkrukken/RVS ","PM"]
[5,"54.","54.63.30.","hang- en sluitwerk - deurkrukken/kunststof ","PM"]
[5,"54.","54.64.","hang- en sluitwerk - vaste handgrepen ","PM"]
[5,"54.","54.65.","hang- en sluitwerk - deurdrangers ","PM"]
[5,"54.","54.70.","vaste binnenramen - algemeen"]
[5,"54.","54.71.","vaste binnenramen - hout ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side"]
[5,"54.","54.80.","toebehoren - algemeen"]
[5,"54.","54.81.","toebehoren - deurroosters"]
[5,"54.","54.81.10.","toebehoren - deurroosters/inbouw ","FH","st","TYPE 4","Door ","Gebruik ARCHICAD property: VMSW toebehoren binnendeuren","Stuks"]
[5,"54.","54.81.20.","toebehoren - deurroosters/opbouw ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren binnendeuren","Stuks"]
[5,"54.","54.82.","toebehoren - beschermplaten"]
[5,"54.","54.82.10.","toebehoren - beschermplaten/aluminium ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren binnendeuren","Stuks"]
[5,"54.",null,null,"PM"]
[5,"54.","54.82.20.","toebehoren - beschermplaten/RVS ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren binnendeuren","Stuks"]
[5,"54.","54.83.","toebehoren - deurspionnen ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren binnendeuren","Stuks"]
[5,"54.","54.84.","toebehoren - deurnummers ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren binnendeuren","Stuks"]
[5,"54.","54.85.","toebehoren - naamplaathouders ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren binnendeuren","Stuks"]
[5,"54.","54.86.","toebehoren - deurstoppen ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren binnendeuren","Stuks"]
[5,"54."]
[5,"55.","55.","BINNENTRAPPEN EN LEUNINGEN"]
[5,"55.","55.00.","binnentrappen en leuningen - algemeen"]
[5,"55.","55.10.","trappen - algemeen"]
[5,"55.","55.11.","trappen - hout"]
[5,"55.","55.11.10.","trappen - hout/rechte treden ","FH","st","TYPE 5","Stair",null,"Stuks"]
[5,"55.","55.11.20.","trappen - hout/verdreven treden ","FH","st","TYPE 5","Stair",null,"Stuks"]
[5,"55.","55.12.","trappen - staal"]
[5,"55.","55.12.10.","trappen - staal/rechte treden ","FH","st","TYPE 5","Stair",null,"Stuks"]
[5,"55.","55.12.20.","trappen - staal/verdreven treden ","FH","st","TYPE 5","Stair",null,"Stuks"]
[5,"55.","55.20.","borstweringen - algemeen"]
[5,"55.","55.21.","borstweringen - hout ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
[5,"55.",{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie"]
[5,"55.","55.22.","borstweringen - staal ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
[5,"55.",{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie"]
[5,"55.","55.23.","borstweringen - roestvast staal ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
[5,"55.",{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie"]
[5,"55.","55.24.","borstweringen - aluminium ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
[5,"55.",{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie"]
[5,"55.","55.25.","borstweringen - veiligheidsglas ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
[5,"55.",{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie"]
[5,"55.","55.30.","handgrepen - algemeen"]
[5,"55.","55.31.","handgrepen - hout ","PM"]
[5,"55.","55.32.","handgrepen - staal ","PM"]
[5,"55.","55.33.","handgrepen - roestvast staal ","PM"]
[5,"55.","55.34.","handgrepen - aluminium ","PM"]
[5,"55.","55.40.","zoldertrappen en -luiken - algemeen"]
[5,"55.","55.41.","zoldertrappen en -luiken - hout ","FH","st","TYPE 5","Object",null,"Stuks"]
[5,"55.","55.42.","zoldertrappen en -luiken - aluminium ","FH","st","TYPE 5","Object",null,"Stuks"]
[5,"55."]
[5,"56.","56.","VAST BINNENMEUBILAIR",{"$nulls":5},"wat met samengestelde onderdelen?"]
[5,"56.","56.00.","vast binnenmeubilair - algemeen"]
[5,"56.","56.10.","keukenmeubelen - algemeen"]
[5,"56.","56.11.","keukenmeubelen - onderdelen"]
[5,"56.","56.11.10.","keukenmeubelen - onderdelen/stelpoten en plintplaat ","PM"]
[5,"56.","56.11.20.","keukenmeubelen - onderdelen/corpus en leggers ","PM"]
[5,"56.","56.11.30.","keukenmeubelen - onderdelen/fronten en zichtwanden ","PM"]
[5,"56.","56.11.40.","keukenmeubelen - onderdelen/werkbladen ","PM"]
[5,"56.","56.11.50.","keukenmeubelen - onderdelen/beslag en handgrepen ","PM"]
[5,"56.","56.11.60.","keukenmeubelen - onderdelen/toebehoren ","PM"]
[5,"56.","56.12.","keukenmeubelen - type 1 ","FH","st","TYPE 5","Object",null,"Stuks"]
[5,"56.","56.13.","keukenmeubelen - type 2 ","FH","st","TYPE 5","Object",null,"Stuks"]
[5,"56.","56.14.","keukenmeubelen - type 3 ","FH","st","TYPE 5","Object",null,"Stuks"]
[5,"56.","56.20.","badkamermeubelen - algemeen"]
[5,"56.","56.21.","badkamermeubelen - onderdelen"]
[5,"56.","56.21.10.","badkamermeubelen - onderdelen/stelpoten en plintplaat ","PM"]
[5,"56.","56.21.20.","badkamermeubelen - onderdelen/corpus en leggers ","PM"]
[5,"56.","56.21.30.","badkamermeubelen - onderdelen/fronten en zichtwanden ","PM"]
[5,"56.","56.21.40.","badkamermeubelen - onderdelen/wastafeltabletten ","PM"]
[5,"56.","56.21.50.","badkamermeubelen - onderdelen/beslag en handgrepen ","PM"]
[5,"56.","56.21.60.","badkamermeubelen - onderdelen/toebehoren ","PM"]
[5,"56.","56.22.","badkamermeubelen - type 1 ","FH","st","TYPE 5","Object",null,"Stuks"]
[5,"56.","56.23.","badkamermeubelen - type 2 ","FH","st","TYPE 5","Object",null,"Stuks"]
[5,"56.","56.24.","badkamermeubelen - type 3 ","FH","st","TYPE 5","Object",null,"Stuks"]
[5,"56.","56.30.","inbouwkasten - algemeen"]
[5,"56.","56.31.","inbouwkasten - onderdelen"]
[5,"56.","56.31.10.","inbouwkasten - onderdelen/stelpoten en plintplaat ","PM"]
[5,"56.","56.31.20.","inbouwkasten - onderdelen/corpus en leggers ","PM"]
[5,"56.","56.31.30.","inbouwkasten - onderdelen/fronten en zichtwanden ","PM"]
[5,"56.","56.31.40.","inbouwkasten - onderdelen/tabletten en bureelbladen ","PM"]
[5,"56.","56.31.50.","inbouwkasten - onderdelen/beslag en handgrepen ","PM"]
[5,"56.","56.31.60.","inbouwkasten - onderdelen/toebehoren ","PM"]
[5,"56.","56.32.","inbouwkasten - kastgeheel type 1 ","FH","st","TYPE 5","Object",null,"Stuks"]
[5,"56.","56.33.","inbouwkasten - kastgeheel type 2 ","FH","st","TYPE 5","Object",null,"Stuks"]
[5,"56.","56.34.","inbouwkasten - kastgeheel type 3 ","FH","st","TYPE 5","Object",null,"Stuks"]
[5,"56.","56.40.","parlofoonconsoles - algemeen"]
[5,"56.","56.41.","parlofoonconsoles - multiplexplaat ","FH","st","TYPE 5","Morph",null,"Stuks"]
[5,"56.",{"$nulls":5},"Object",null,"Stuks"]
[5,"56.",null,null,"PM"]
[5,"56.","56.42.","parlofoonconsoles - kunstharsplaat ","FH","st","TYPE 5","Morph",null,"Stuks"]
[5,"56.",{"$nulls":5},"Object",null,"Stuks"]
[5,"56.",null,null,"PM"]
[5,"56.","56.43.","parlofoonconsoles - metaalplaat"]
[5,"56.","56.43.10.","parlofoonconsoles - metaalplaat/gemoffeld staal ","FH","st","TYPE 5","Morph",null,"Stuks"]
[5,"56.",{"$nulls":5},"Object",null,"Stuks"]
[5,"56.",null,null,"PM"]
[5,"56.","56.43.20.","parlofoonconsoles - metaalplaat/roestvast staal (RVS) ","FH","st","TYPE 5","Morph",null,"Stuks"]
[5,"56.",{"$nulls":5},"Object",null,"Stuks"]
[5,"56.",null,null,"PM"]
[5,"56.","56.43.30.","parlofoonconsoles - metaalplaat/aluminium ","FH","st","TYPE 5","Morph",null,"Stuks"]
[5,"56.",{"$nulls":5},"Object",null,"Stuks"]
[5,"56.",null,null,"PM"]
[5,"56.","56.50.","brievenbusgehelen - algemeen"]
[5,"56.","56.51.","brievenbusgehelen - multiplexplaat ","FH","st","TYPE 5","Morph",null,"Stuks"]
[5,"56.","56.52.","brievenbusgehelen - kunstharsplaat ","FH","st","TYPE 5","Morph",null,"Stuks"]
[5,"56.","56.53.","brievenbusgehelen - metaalplaat"]
[5,"56.","56.53.10.","brievenbusgehelen - metaalplaat/gemoffeld staal ","FH","st","TYPE 5","Morph",null,"Stuks"]
[5,"56.","56.53.20.","brievenbusgehelen - metaalplaat/roestvast staal (RVS) ","FH","st","TYPE 5","Morph",null,"Stuks"]
[5,"56.","56.53.30.","brievenbusgehelen - metaalplaat/gemoffeld aluminium ","FH","st","TYPE 5","Morph",null,"Stuks"]
[5,"56.","56.60.","gordijnkasten - algemeen"]
[5,"56.","56.61.","gordijnkasten - hout"]
[5,"56.","56.61.10.","gordijnkasten - hout/massief ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[5,"56.",{"$nulls":5},"Wall",null,"Reference line length"]
[5,"56.","56.61.20.","gordijnkasten - hout/houtspaanplaat ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[5,"56.",{"$nulls":5},"Wall",null,"Reference line length"]
[5,"56.","56.61.30.","gordijnkasten - hout/multiplex ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[5,"56.",{"$nulls":5},"Wall",null,"Reference line length"]
[5,"56.","56.61.40.","gordijnkasten - hout/MDF ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[5,"56.",{"$nulls":5},"Wall",null,"Reference line length"]
[5,"56.","56.62.","gordijnkasten - kunststof ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[5,"56."]
[5,"56."]
[5,"57.","57.","TABLET- EN WANDBEKLEDINGEN"]
[5,"57.","57.00.","tablet- en wandbekledingen - algemeen"]
[5,"57.","57.10.","venstertabletten - algemeen"]
[5,"57.","57.11.","venstertabletten - natuursteen"]
[5,"57.","57.11.10.","venstertabletten - natuursteen/marmer ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant"]
[5,"57.",null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)"]
[5,"57.","57.11.20.","venstertabletten - natuursteen/blauwe hardsteen ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant"]
[5,"57.",null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)"]
[5,"57.","57.11.30.","venstertabletten - natuursteen/leisteen ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant"]
[5,"57.",null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)"]
[5,"57.","57.11.40.","venstertabletten - natuursteen/volgens prestaties ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant"]
[5,"57.",null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)"]
[5,"57.","57.12.","venstertabletten - kunststeen"]
[5,"57.","57.12.10.","venstertabletten - kunststeen/marmermozaïek ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant"]
[5,"57.",null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)"]
[5,"57.","57.12.20.","venstertabletten - kunststeen/vezelcement ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant"]
[5,"57.",null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)"]
[5,"57.","57.12.30.","venstertabletten - kunststeen/composiet ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant"]
[5,"57.",null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)"]
[5,"57.","57.13.","venstertabletten - hout"]
[5,"57.","57.13.10.","venstertabletten - hout/massief ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant"]
[5,"57.",null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)"]
[5,"57.","57.13.20.","venstertabletten - hout/laminaat ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant"]
[5,"57.",null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)"]
[5,"57.","57.14.","venstertabletten - kunststof"]
[5,"57.","57.14.10.","venstertabletten - kunststof/PVC ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant"]
[5,"57.",null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)"]
[5,"57.","57.20.","wandbekledingen - algemeen"]
[5,"57.","57.21.","wandbekledingen - betegeling ","FH","m2","TYPE 3","Wall",null,"Netto oppervlakte binnenkant wand"]
[5,"57.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[5,"57.","57.21.10.","wandbekledingen - betegeling/keramisch ","FH","m2","TYPE 3","Wall",null,"Netto oppervlakte binnenkant wand"]
[5,"57.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[5,"57."]
[6,"60.","60.","SANITAIR LEIDINGNET"]
[6,"60.","60.00.","sanitair leidingnet - algemeen"]
[6,"60.","60.10.","afvoerbuizen - algemeen"]
[6,"60.","60.11.","afvoerbuizen - PVC ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"60.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"60.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"60.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"60.","60.12.","afvoerbuizen - PE ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"60.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"60.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"60.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"60.","60.13.","afvoerbuizen - PP ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"60.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"60.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"60.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"60.","60.20.","verluchtingsbuizen - algemeen"]
[6,"60.","60.21.","verluchtingsbuizen - PVC ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"60.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"60.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"60.",null,null,null,"st","TYPE 3","Column",null,"Stuks"]
[6,"60.",{"$nulls":4},"TYPE 5","Object","MEP","Stuks"]
[6,"60.",{"$nulls":5},"Object",null,"Stuks"]
[6,"60.",null,null,"PM"]
[6,"60.","60.22.","verluchtingsbuizen - PE ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"60.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"60.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"60.",null,null,null,"st","TYPE 3","Column",null,"Stuks"]
[6,"60.",{"$nulls":4},"TYPE 5","Object","MEP","Stuks"]
[6,"60.",{"$nulls":5},"Object",null,"Stuks"]
[6,"60.",null,null,"PM"]
[6,"60.","60.23.","verluchtingsbuizen - beluchtingsventielen ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"60.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"60.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"60.",null,null,null,"st","TYPE 3","Column",null,"Stuks"]
[6,"60.",{"$nulls":4},"TYPE 5","Object","MEP","Stuks"]
[6,"60.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"60.",null,null,"PM"]
[6,"60.","60.30.","klokroosters - intern - algemeen"]
[6,"60.","60.31.","klokroosters - gietijzer ","FH","st","TYPE 5","Object","MEP","Stuks"]
[6,"60.",{"$nulls":5},"Object",null,"Stuks"]
[6,"60.","60.32.","klokroosters - aluminium ","FH","st","TYPE 5","Object","MEP","Stuks"]
[6,"60.",{"$nulls":5},"Object",null,"Stuks"]
[6,"60.","60.33.","klokroosters - roestvast staal (RVS) ","FH","st","TYPE 5","Object","MEP","Stuks"]
[6,"60.",{"$nulls":5},"Object",null,"Stuks"]
[6,"60.","60.34.","klokroosters - kunststof ","FH","st","TYPE 5","Object","MEP","Stuks"]
[6,"60.",{"$nulls":5},"Object",null,"Stuks"]
[6,"60.","60.40.","putdeksels - algemeen"]
[6,"60.","60.41.","putdeksels - gietijzer ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"60.",null,null,"PM"]
[6,"60.","60.42.","putdeksels - aluminium ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"60.",null,null,"PM"]
[6,"60.","60.43.","putdeksels - roestvast staal ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"60.",null,null,"PM"]
[6,"60.","60.44.","putdeksels - kunststof ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"60.",null,null,"PM"]
[6,"60.","60.50.","sanitaire drukleidingen - algemeen"]
[6,"60.","60.51.","sanitaire drukleidingen - buizen"]
[6,"60.","60.51.10.","sanitaire drukleidingen - buizen/verzinkt staal ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"60.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"60.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"60.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"60.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[6,"60.",{"$nulls":5},"Column",null,"Stuks"]
[6,"60.",{"$nulls":4},"TYPE 5","Object","MEP","Stuks"]
[6,"60.",{"$nulls":5},"Object",null,"Stuks"]
[6,"60.","60.51.20.","sanitaire drukleidingen - buizen/koper ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"60.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"60.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"60.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"60.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[6,"60.",{"$nulls":5},"Column",null,"Stuks"]
[6,"60.",{"$nulls":4},"TYPE 5","Object","MEP","Stuks"]
[6,"60.",{"$nulls":5},"Object",null,"Stuks"]
[6,"60.","60.51.30.","sanitaire drukleidingen - buizen/kunststof ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"60.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"60.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"60.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"60.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[6,"60.",{"$nulls":5},"Column",null,"Stuks"]
[6,"60.",{"$nulls":4},"TYPE 5","Object","MEP","Stuks"]
[6,"60.",{"$nulls":5},"Object",null,"Stuks"]
[6,"60.","60.52.","sanitaire drukleidingen - collectoren ","FH","st","TYPE 5","Object","MEP","Stuks"]
[6,"60.",{"$nulls":5},"Object",null,"Stuks"]
[6,"60.",null,null,"PM"]
[6,"60.","60.53.","sanitaire drukleidingen - leidingisolatie ","FH","st","TYPE 3","Beam",null,"Stuks"]
[6,"60.",{"$nulls":5},"Column",null,"Stuks"]
[6,"60.",{"$nulls":4},"TYPE 5","Object","MEP","Stuks"]
[6,"60.",{"$nulls":5},"Object",null,"Stuks"]
[6,"60.",null,null,"PM"]
[6,"60.","60.54.","sanitaire drukleidingen - brandwerende doorvoeren ","FH","st","TYPE 5","Object","MEP","Stuks"]
[6,"60.",{"$nulls":5},"Object",null,"Stuks"]
[6,"60.",null,null,"PM"]
[6,"60.","60.55.","sanitaire drukleidingen - verwarmingslint ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"60.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"60.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"60.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"60.","60.56.","sanitaire drukleidingen - flexibele leidingen ","PM"]
[6,"60.","60.60.","aansluiting leidingnet - algemeen"]
[6,"60.","60.61.","aansluiting leidingnet - reglementaire meterstraat ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"60.","60.62.","aansluiting leidingnet - voedingsleidingen & tellers ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"60.","60.63.","aansluiting leidingnet - waterfilters ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"60.","60.70.","waterbehandeling - algemeen"]
[6,"60.","60.71.","waterbehandeling - ontharders ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"60.","60.72.","waterbehandeling - filters ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"60."]
[6,"61.","61.","SANITAIRE TOESTELLEN & TOEBEHOREN"]
[6,"61.","61.00.","sanitaire toestellen en toebehoren - algemeen"]
[6,"61.","61.10.","toiletpotten en toebehoren - algemeen"]
[6,"61.","61.11.","toiletpotten en toebehoren - staand ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"61.","61.12.","toiletpotten en toebehoren - hangend ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"61.","61.20.","handwastafels en toebehoren - algemeen"]
[6,"61.","61.21.","handwastafels & toebehoren - wandmodel"]
[6,"61.","61.21.10.","handwastafels & toebehoren - wandmodel/porselein ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"61.","61.22.","handwastafels en toebehoren - inbouwmodel ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"61.","61.30.","wastafels en toebehoren - algemeen"]
[6,"61.","61.31.","wastafels en toebehoren - wandmodel"]
[6,"61.","61.31.10.","wastafels en toebehoren - wandmodel/porselein ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"61.","61.32.","wastafels en toebehoren - inbouwmodel ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"61.","61.40.","baden - algemeen"]
[6,"61.","61.41.","baden - geëmailleerd staal ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"61.","61.42.","baden - acrylaat ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"61.","61.50.","douches - algemeen"]
[6,"61.","61.51.","douches - geëmailleerd staal ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"61.","61.52.","douches - acrylaat ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"61.","61.53.","douches - tegeldouche ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"61.","61.60.","speciale toebehoren - algemeen"]
[6,"61.","61.61.","speciale toebehoren - rail en douchegordijn ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"61.","61.62.","speciale toebehoren - douchedeuren en -wanden ","FH","st","TYPE 3","Wall",null,"Stuks"]
[6,"61.",{"$nulls":4},"TYPE 5","Door",null,"Stuks"]
[6,"61.",{"$nulls":5},"Object",null,"Stuks"]
[6,"61.",{"$nulls":5},"Window",null,"Stuks"]
[6,"61.","61.63.","speciale toebehoren - muurhandgrepen ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"61.","61.64.","speciale toebehoren - douchezitjes ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"61.","61.70.","afwastafels - algemeen"]
[6,"61.","61.71.","afwastafels - opbouwmodel"]
[6,"61.","61.71.10.","afwastafels - opbouwmodel/roestvast staal (RVS) ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"61.","61.72.","afwastafels - inbouwmodel"]
[6,"61.","61.72.10.","afwastafels - inbouwmodel/roestvast staal (RVS) ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"61.","61.80.","uitgietbakken - algemeen"]
[6,"61.","61.81.","uitgietbakken - sanitair porselein ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"61."]
[6,"62.","62.","SANITAIRE KRANEN & KLEPPEN"]
[6,"62.","62.00.","sanitaire kranen - kleppen - algemeen"]
[6,"62.","62.10.","terugslagkleppen - algemeen"]
[6,"62.","62.11.","terugslagkleppen - messing ","PM"]
[6,"62.","62.20.","installatieafsluitkranen - algemeen"]
[6,"62.","62.21.","installatieafsluitkranen - messing"]
[6,"62.","62.21.10.","installatieafsluitkranen - messing/zonder aftapkraan ","PM"]
[6,"62.","62.21.20.","installatieafsluitkranen - messing/met aftapkraan ","PM"]
[6,"62.","62.22.","installatieafsluitkranen - kunststof"]
[6,"62.","62.22.10.","installatieafsluitkranen - kunststof/zonder aftapkraan ","PM"]
[6,"62.","62.30.","wandafsluitkranen - algemeen"]
[6,"62.","62.31.","wandafsluitkranen - enkelvoudige stopkraan ","PM"]
[6,"62.","62.32.","wandafsluitkranen - stopkraan met dienstkraan ","PM"]
[6,"62.","62.40.","dienstkranen - algemeen"]
[6,"62.","62.41.","dienstkranen - enkele dienstkraan"]
[6,"62.","62.41.10.","dienstkranen - enkele dienstkraan/vaste uitloop ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"62.","62.41.20.","dienstkranen - enkele dienstkraan/draaibare uitloop ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"62.","62.42.","dienstkranen - dubbele dienstkraan"]
[6,"62.","62.42.10.","dienstkranen - dubbele dienstkraan/binnen ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"62.","62.42.20.","dienstkranen - dubbele dienstkraan/buiten ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"62.","62.50.","ééngatskranen - algemeen"]
[6,"62.","62.51.","ééngatskranen - handwastafelkraan ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"62.","62.52.","ééngatskranen - lavabomengkraan ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"62.","62.53.","ééngatskranen - afwastafelmengkraan ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"62.","62.60.","muurmengkranen - algemeen"]
[6,"62.","62.61.","muurmengkranen - badmengkraan & armatuur ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"62.","62.62.","muurmengkranen - douchemengkraan/armatuur ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"62.","62.63.","muurmengkranen - afwastafelmengkraan ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"62.","62.70.","regenwaterpompen - algemeen"]
[6,"62.","62.71.","regenwaterpompen - zelfaanzuigende hydrofoorgroep ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"62.","62.72.","regenwaterpompen - dompelpomp ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"62.","62.73.","regenwaterpompen - handpomp ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"62."]
[6,"63.","63.","SANITAIR WARM WATER"]
[6,"63.","63.00.","sanitair warm water - algemeen"]
[6,"63.","63.10.","doorstroomwaterverwarmers op gas - algemeen"]
[6,"63.","63.11.","doorstroomwaterverwarmers op gas - badgeisers"]
[6,"63.","63.11.10.","doorstroomwaterverwarmers op gas - badgeisers/type B11BS ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.","63.11.20.","doorstroomwaterverwarmers op gas - badgeisers/type C13-C33 ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.","63.12.","doorstroomwaterverwarmers op gas - keukengeisers"]
[6,"63.","63.12.10.","doorstroomwaterverwarmers op gas - keukengeisers/type AAS ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.","63.20.","voorraadtoestellen op gas ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.","63.30.","elektroboilers - algemeen"]
[6,"63.","63.31.","elektroboilers - kokend water toestellen ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.","63.32.","elektroboilers - inbouwmodel ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.","63.33.","elektroboilers - spaarboilers ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.","63.40.","voorraadboilers indirecte opwarming - algemeen"]
[6,"63.","63.41.","voorraadboilers indirecte opwarming - enkelvoudige warmtewisselaar ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.","63.42.","voorraadboilers indirecte opwarming - dubbelvoudige warmtewisselaar ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.","63.50.","zonneboilers - algemeen"]
[6,"63.","63.51.","zonneboilers - collectoren ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.","63.52.","zonneboilers - opslagvat ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.","63.53.","zonneboilers - leidingsysteem en toebehoren ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.","63.54.","zonneboilers - circulatoren ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.","63.55.","zonneboilers - expansiesysteem ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.","63.56.","zonneboilers - regelsystemen en beveiliging"]
[6,"63.","63.56.10.","zonneboilers - regelsystemen en beveiliging/aflaat- en vulkranen ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.",null,null,"PM"]
[6,"63.","63.56.20.","zonneboilers - regelsystemen en beveiliging/regelkranen ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.",null,null,"PM"]
[6,"63.","63.56.30.","zonneboilers - regelsystemen en beveiliging/ontluchters ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.",null,null,"PM"]
[6,"63.","63.56.40.","zonneboilers - regelsystemen en beveiliging/veiligheidskleppen ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.",null,null,"PM"]
[6,"63.","63.56.50.","zonneboilers - regelsystemen en beveiliging/keerkleppen ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.",null,null,"PM"]
[6,"63.","63.56.60.","zonneboilers - regelsystemen en beveiliging/mengventielen ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.",null,null,"PM"]
[6,"63.","63.60.","warmtepompboilers - algemeen"]
[6,"63.","63.70.","satellietsystemen - algemeen "]
[6,"63.","63.71.","satellietsystemen - voorraadboilers ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63.","63.72.","satellietsystemen - platenwisselaars ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"63."]
[6,"64.","64.","GASINSTALLATIES"]
[6,"64.","64.00.","gasinstallaties - algemeen"]
[6,"64.","64.10.","gasleidingen - algemeen"]
[6,"64.","64.11.","gasleidingen - staal ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"64.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"64.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"64.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"64.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[6,"64.",{"$nulls":5},"Column",null,"Stuks"]
[6,"64.",{"$nulls":4},"TYPE 5","Object","MEP","Stuks"]
[6,"64.",{"$nulls":5},"Object",null,"Stuks"]
[6,"64.","64.12.","gasleidingen - koper ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"64.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"64.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"64.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"64.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[6,"64.",{"$nulls":5},"Column",null,"Stuks"]
[6,"64.",{"$nulls":4},"TYPE 5","Object","MEP","Stuks"]
[6,"64.",{"$nulls":5},"Object",null,"Stuks"]
[6,"64.","64.13.","gasleidingen - PE ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"64.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"64.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"64.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"64.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[6,"64.",{"$nulls":5},"Column",null,"Stuks"]
[6,"64.",{"$nulls":4},"TYPE 5","Object","MEP","Stuks"]
[6,"64.",{"$nulls":5},"Object",null,"Stuks"]
[6,"64.","64.14.","gasleidingen - PLT-buissysteem ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"64.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"64.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"64.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"64.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[6,"64.",{"$nulls":5},"Column",null,"Stuks"]
[6,"64.",{"$nulls":4},"TYPE 5","Object","MEP","Stuks"]
[6,"64.",{"$nulls":5},"Object",null,"Stuks"]
[6,"64.","64.20.","gaskranen - algemeen"]
[6,"64.","64.21.","gaskranen - gasfilter ","PM"]
[6,"64.","64.22.","gaskranen - afsluitkranen ","PM"]
[6,"64.","64.30.","gasaansluiting ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"64.","64.40.","gastoestellen - algemeen ","PM"]
[6,"64."]
[6,"65.","65.","VERWARMING INDIVIDUELE INSTALLATIES"]
[6,"65.","65.00.","verwarming individuele installaties - algemeen"]
[6,"65.","65.01.","verwarming individuele installaties - proefopstelling ","PM"]
[6,"65.","65.02.","verwarming individuele installaties - grenzen van de aanneming ","PM"]
[6,"65.","65.10.","gasvloerketels - algemeen"]
[6,"65.","65.11.","gasvloerketels - open"]
[6,"65.","65.11.10.","gasvloerketels - open/enkel CV ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"65.","65.11.20.","gasvloerketels - open/CV & SWW (voorraad) ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"65.","65.12.","gasvloerketels - gesloten"]
[6,"65.","65.12.10.","gasvloerketels - gesloten/enkel CV ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"65.","65.12.20.","gasvloerketels - gesloten/CV & SWW (voorraad) ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"65.","65.20.","gaswandketels - algemeen"]
[6,"65.","65.21.","gaswandketels - gesloten"]
[6,"65.","65.21.10.","gaswandketels - gesloten/enkel CV ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"65.","65.21.20.","gaswandketels - gesloten/CV & SWW (doorstroom) ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"65.","65.21.30.","gaswandketels - gesloten/CV & SWW (voorraad) ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"65.","65.30.","leidingnet & toebehoren - algemeen"]
[6,"65.","65.31.","leidingnet & toebehoren - buizen"]
[6,"65.","65.31.10.","leidingnet & toebehoren - buizen/staal ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"65.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"65.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"65.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"65.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[6,"65.",{"$nulls":5},"Column",null,"Stuks"]
[6,"65.",{"$nulls":4},"TYPE 5","Object","MEP","Stuks"]
[6,"65.",{"$nulls":5},"Object",null,"Stuks"]
[6,"65.","65.31.20.","leidingnet & toebehoren - buizen/koper ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"65.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"65.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"65.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"65.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[6,"65.",{"$nulls":5},"Column",null,"Stuks"]
[6,"65.",{"$nulls":4},"TYPE 5","Object","MEP","Stuks"]
[6,"65.",{"$nulls":5},"Object",null,"Stuks"]
[6,"65.","65.31.30.","leidingnet & toebehoren - buizen/kunststof ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"65.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"65.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"65.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"65.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[6,"65.",{"$nulls":5},"Column",null,"Stuks"]
[6,"65.",{"$nulls":4},"TYPE 5","Object","MEP","Stuks"]
[6,"65.",{"$nulls":5},"Object",null,"Stuks"]
[6,"65.","65.31.40.","leidingnet & toebehoren - buizen/dunwandige verzinkte buis ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"65.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"65.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"65.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"65.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[6,"65.",{"$nulls":5},"Column",null,"Stuks"]
[6,"65.",{"$nulls":4},"TYPE 5","Object","MEP","Stuks"]
[6,"65.",{"$nulls":5},"Object",null,"Stuks"]
[6,"65.","65.32.","leidingnet & toebehoren - collectoren ","FH","st","TYPE 5","Object","MEP","Stuks"]
[6,"65.",{"$nulls":5},"Object",null,"Stuks"]
[6,"65.",null,null,"PM"]
[6,"65.","65.33.","leidingnet & toebehoren - leidingisolatie ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"65.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"65.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"65.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"65.",null,null,null,"st","TYPE 3","Beam",null,"Stuks"]
[6,"65.",{"$nulls":5},"Column",null,"Stuks"]
[6,"65.",{"$nulls":4},"TYPE 5","Object","MEP","Stuks"]
[6,"65.",{"$nulls":5},"Object",null,"Stuks"]
[6,"65.",null,null,"PM"]
[6,"65.","65.34.","leidingnet & toebehoren - brandwerende doorvoeren ","PM"]
[6,"65.","65.35.","leidingnet & toebehoren - verwarmingslint ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"65.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"65.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"65.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"65.","65.40.","installatieonderdelen - algemeen"]
[6,"65.","65.41.","installatieonderdelen - aflaatkranen ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"65.","65.42.","installatieonderdelen - regel- en afsluitkranen ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"65.","65.43.","installatieonderdelen - drukregelaars ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"65.","65.44.","installatieonderdelen - circulatoren ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"65.",null,null,"PM"]
[6,"65.","65.45.","installatieonderdelen - expansiesysteem ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"65.","65.46.","installatieonderdelen - vlotterontluchters ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"65.","65.47.","installatieonderdelen - microbellenafscheider ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"65.","65.50.","verwarmingselementen & toebehoren - algemeen"]
[6,"65.","65.51.","verwarmingselementen & toebehoren - plaatradiatoren ","FH","kW","TYPE 5","Object",null,"vul het vermogen in bij ARCHICAD property: Vermogen verwarmingselement"]
[6,"65.",null,null,null,"st","TYPE 5","Object",null,"Stuks"]
[6,"65.","65.52.","verwarmingselementen & toebehoren - wandconvectoren ","FH","kW","TYPE 5","Object",null,"vul het vermogen in bij ARCHICAD property: Vermogen verwarmingselement"]
[6,"65.",null,null,null,"st","TYPE 5","Object",null,"Stuks"]
[6,"65.","65.53.","verwarmingselementen & toebehoren - vloerverwarming ","FH","m2","TYPE 4","Slab","Gebruik ARCHICAD property: VMSW vloerverwarming","Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[6,"65.","65.60.","warmteregeling & toebehoren - algemeen"]
[6,"65.","65.61.","warmteregeling & toebehoren - radiatorkranen ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW warmteregeling en toebehoren","Stuks"]
[6,"65.","65.62.","warmteregeling & toebehoren - thermostaatkoppen ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW warmteregeling en toebehoren","Stuks"]
[6,"65.","65.63.","warmteregeling & toebehoren - kamerthermostaten ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW warmteregeling en toebehoren","Stuks"]
[6,"65.","65.64.","warmteregeling & toebehoren - weersafhankelijke regeling ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW warmteregeling en toebehoren","Stuks"]
[6,"65.","65.65.","warmteregeling & toebehoren - manometer ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW warmteregeling en toebehoren","Stuks"]
[6,"65.","65.66.","warmteregeling & toebehoren - thermometer ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW warmteregeling en toebehoren","Stuks"]
[6,"65."]
[6,"66.","66.","BIJZONDERE INSTALLATIES"]
[6,"66.","66.00.","bijzondere installaties - algemeen"]
[6,"66.","66.10.","warmtepompen - algemeen"]
[6,"66.","66.11.","warmtepompen - grond-water ","FH","st","TYPE 5","Morph",null,"Stuks"]
[6,"66.",{"$nulls":5},"Object",null,"Stuks"]
[6,"66.","66.12.","warmtepompen - water-water ","FH","st","TYPE 5","Morph",null,"Stuks"]
[6,"66.",{"$nulls":5},"Object",null,"Stuks"]
[6,"66.","66.13.","warmtepompen - lucht-water monoblok ","FH","st","TYPE 5","Morph",null,"Stuks"]
[6,"66.",{"$nulls":5},"Object",null,"Stuks"]
[6,"66.","66.14.","warmtepompen - lucht-water met binnen- en buitenunit (split-systeem) ","FH","st","TYPE 5","Morph",null,"Stuks"]
[6,"66.",{"$nulls":5},"Object",null,"Stuks"]
[6,"66.","66.15.","warmtepompen - gasabsorptiewarmtepompen"]
[6,"66.","66.16.","warmtepompen - verticale aardsondes ","SOG"]
[6,"66.","66.16.10.","warmtepompen - verticale aardsondes/warmtewisselaar ","FH","SOG"]
[6,"66.","66.16.20.","warmtepompen - verticale aardsondes/collector ","PM"]
[6,"66."]
[6,"67.","67.","BRANDBESTRIJDING"]
[6,"67.","67.00.","brandbestrijding - algemeen"]
[6,"67.","67.10.","brandblusapparaten - algemeen"]
[6,"67.","67.11.","brandblusapparaten - poedersnelblussers ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"67.","67.12.","brandblusapparaten - CO2-snelblussers ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"67.","67.13.","brandblusapparaten - schuimsnelblussers ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"67.","67.14.","brandblusapparaten - vast opgestelde poederblussers ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"67.","67.20.","externe bluswatervoorziening - algemeen ","SOG"]
[6,"67.","67.21.","externe bluswatervoorziening - leidingen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"67.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"67.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"67.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"67.","67.22.","externe bluswatervoorziening - buitenhydranten"]
[6,"67.","67.22.10.","externe bluswatervoorziening - buitenhydranten/bovengronds ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"67.","67.22.20.","externe bluswatervoorziening - buitenhydranten/ondergronds ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"67.","67.30.","interne bluswatervoorziening - algemeen ","SOG"]
[6,"67.","67.31.","interne bluswatervoorziening - leidingen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"67.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"67.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"67.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"67.","67.32.","interne bluswatervoorziening - brandkranen ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"67.","67.33.","interne bluswatervoorziening - muurhaspels zonder kast ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"67.","67.34.","interne bluswatervoorziening - kasten voor slanghaspels ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"67.","67.35.","interne bluswatervoorziening - manometers ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"67.","67.36.","interne bluswatervoorziening - pictogrammen ","PM"]
[6,"67.","67.40.","sprinklerinstallatie - algemeen ","SOG"]
[6,"67.","67.50.","brandwerende bescherming - algemeen ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"67.",null,null,"SOG"]
[6,"67."]
[6,"68.","68.","VENTILATIE"]
[6,"68.","68.00.","ventilatie - algemeen"]
[6,"68.","68.01.","ventilatie - proefopstelling ","PM"]
[6,"68.","68.02.","ventilatie - proeven"]
[6,"68.","68.02.10.","ventilatie - proeven/debietmeting ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"68.",null,null,"SOG"]
[6,"68.","68.02.20.","ventilatie - proeven/meting kanaaldichtheid ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"68.",null,null,"SOG"]
[6,"68.","68.02.30.","ventilatie - proeven/dichtheid collectieve kanalen ","SOG"]
[6,"68.","68.10.","ventilatiekanalen - algemeen"]
[6,"68.","68.11.","ventilatiekanalen - metaal"]
[6,"68.","68.11.10.","ventilatiekanalen - metaal/rond ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"68.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"68.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"68.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"68.",null,null,"SOG"]
[6,"68.","68.11.20.","ventilatiekanalen - metaal/rechthoekig ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"68.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"68.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"68.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"68.",null,null,"SOG"]
[6,"68.","68.12.","ventilatiekanalen - kunststof"]
[6,"68.","68.12.10.","ventilatiekanalen - kunststof/rond ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"68.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"68.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"68.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"68.",null,null,"SOG"]
[6,"68.","68.12.20.","ventilatiekanalen - kunststof/rechthoekig of ovaal ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"68.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"68.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"68.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"68.",null,null,"SOG"]
[6,"68.","68.13.","ventilatiekanalen - flexibele kanalen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"68.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"68.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"68.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"68.","68.14.","ventilatiekanalen - thermische isolatie ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"68.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[6,"68.",{"$nulls":4},"TYPE 5","Object","MEP","Lengte"]
[6,"68.",{"$nulls":5},"Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"68.","68.15.","ventilatiekanalen - ophanging en bevestiging ","PM"]
[6,"68.","68.20.","toebehoren ventilatiekanalen - algemeen"]
[6,"68.","68.21.","toebehoren ventilatiekanalen - brandkleppen ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW toebehoren ventilatiekanalen","Stuks"]
[6,"68.","68.22.","toebehoren ventilatiekanalen - brandmoffen ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW toebehoren ventilatiekanalen","Stuks"]
[6,"68.","68.23.","toebehoren ventilatiekanalen - regelkleppen ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW toebehoren ventilatiekanalen","Stuks"]
[6,"68.","68.24.","toebehoren ventilatiekanalen - meetstukken ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW toebehoren ventilatiekanalen","Stuks"]
[6,"68.","68.25.","toebehoren ventilatiekanalen - geluidsdempers ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW toebehoren ventilatiekanalen","Stuks"]
[6,"68.","68.26.","toebehoren ventilatiekanalen - filters ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW toebehoren ventilatiekanalen","Stuks"]
[6,"68.","68.27.","toebehoren ventilatiekanalen - terugslagkleppen ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW toebehoren ventilatiekanalen","Stuks"]
[6,"68.","68.28.","toebehoren ventilatiekanalen - inspectie- en reinigingsopeningen ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW toebehoren ventilatiekanalen","Stuks"]
[6,"68.","68.30.","woonhuisventilatoren - algemeen"]
[6,"68.","68.31.","woonhuisventilatoren - systeem C ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"68.","68.32.","woonhuisventilatoren - systeem D ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"68.","68.40.","ventilatoren - algemeen"]
[6,"68.","68.41.","ventilatoren - dakventilatoren ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"68.","68.42.","ventilatoren - kanaalventilatoren ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"68.","68.43.","ventilatoren - sanitaire ventilatoren ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"68.","68.50.","dampkappen - algemeen"]
[6,"68.","68.51.","dampkappen - inbouwmotor ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"68.","68.52.","dampkappen - motorloos ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"68.","68.60.","ventilatieventielen en -roosters - algemeen"]
[6,"68.","68.61.","ventilatiemonden - ventiel met regelbare conus ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"68.","68.62.","ventilatiemonden - zelfregelend ventiel ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"68.","68.63.","ventilatiemonden - gevelroosters ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"68.","68.64.","ventilatiemonden - dakventielen ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"68."]
[6,"69.","69.","OPBOUWKANALEN ROOKGAS EN VENTILATIE"]
[6,"69.","69.00.","opbouwkanalen rookgas en ventilatie - algemeen"]
[6,"69.","69.10.","schoorstenen - algemeen"]
[6,"69.","69.11.","schoorstenen - roestvast staal"]
[6,"69.","69.11.10.","schoorstenen - roestvast staal/CLV ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"69.",null,null,null,"st","TYPE 5","Object",null,"Stuks"]
[6,"69.","69.11.20.","schoorstenen - roestvast staal/enkelvoudig kanaal ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"69.",null,null,null,"st","TYPE 5","Object",null,"Stuks"]
[6,"69.","69.11.30.","schoorstenen - roestvast staal/buigzame kanaalvoering ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"69.",null,null,null,"st","TYPE 5","Object",null,"Stuks"]
[6,"69.","69.12.","schoorstenen - aluminium"]
[6,"69.","69.12.10.","schoorstenen - aluminium/CLV ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"69.",null,null,null,"st","TYPE 5","Object",null,"Stuks"]
[6,"69.","69.12.20.","schoorstenen - aluminium/enkelvoudig ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"69.",null,null,null,"st","TYPE 5","Object",null,"Stuks"]
[6,"69.","69.12.30.","schoorstenen - aluminium/buigzame kanaalvoering ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"69.",null,null,null,"st","TYPE 5","Object",null,"Stuks"]
[6,"69.","69.13.","schoorstenen - kunststof "]
[6,"69.","69.13.10.","schoorstenen - kunststof/CLV ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"69.",null,null,null,"st","TYPE 5","Object",null,"Stuks"]
[6,"69.","69.13.20.","schoorstenen - kunststof/enkelvoudig ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"69.",null,null,null,"st","TYPE 5","Object",null,"Stuks"]
[6,"69.","69.13.30.","schoorstenen - kunststof/buigzame kanaalvoering ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[6,"69.",null,null,null,"st","TYPE 5","Object",null,"Stuks"]
[6,"69.","69.20.","dakdoorgang - algemeen"]
[6,"69.","69.21.","dakdoorgang - enkelvoudig ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"69.","69.22.","dakdoorgang - multifunctioneel ","FH","st","TYPE 5","Object",null,"Stuks"]
[6,"69."]
[7,"70.","70.","ELEKTRICITEIT BINNENNET"]
[7,"70.","70.00.","elektriciteit binnennet - algemeen"]
[7,"70.","70.10.","aansluitingen - algemeen"]
[7,"70.","70.11.","aansluitingen - ondergrondse aansluiting ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"70.","70.12.","aansluitingen - aansluitbocht ","PM"]
[7,"70.","70.13.","aansluitingen - aansluitplaat ","FH","st","TYPE 5","Morph",null,"Stuks"]
[7,"70.",{"$nulls":5},"Object",null,"Stuks"]
[7,"70.","70.14.","aansluitingen - tellerkasten ","FH","st","TYPE 5","Morph",null,"Stuks"]
[7,"70.",{"$nulls":5},"Object",null,"Stuks"]
[7,"70.","70.15.","aansluitingen - verbindingskabels ","FH","st","TYPE 5","Morph",null,"Stuks"]
[7,"70.",{"$nulls":5},"Object",null,"Stuks"]
[7,"70.","70.20.","verdeelkasten - algemeen"]
[7,"70.","70.21.","verdeelkasten - hoofdverdeelborden ","FH","st","TYPE 5","Morph",null,"Stuks"]
[7,"70.",{"$nulls":5},"Object",null,"Stuks"]
[7,"70.","70.30.","stroombeveiliging - algemeen"]
[7,"70.","70.31.","stroombeveiliging - hoofdschakelaars ","PM"]
[7,"70.","70.32.","stroombeveiliging - differentieelschakelaars ","PM"]
[7,"70.","70.33.","stroombeveiliging - automatische schakelaars ","PM"]
[7,"70.","70.40.","aarding - algemeen"]
[7,"70.","70.41.","aarding - aardingslus ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"70.",null,null,null,"m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[7,"70.","70.42.","aarding - afzonderlijke aardverbindingen ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"70.","70.43.","aarding - aardingsonderbrekers ","PM"]
[7,"70.","70.44.","aarding - hoofdbeschermingsgeleiders ","PM"]
[7,"70.","70.45.","aarding - hoofdequipotentiaalverbindingen ","PM"]
[7,"70.","70.46.","aarding - bijkomende equipotentiaalverbindingen ","PM"]
[7,"70.","70.47.","aarding - bliksemafleidersinstalatie ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Bliksemafleiderinstallatie","Stuks"]
[7,"70.","70.50.","leidingen - algemeen"]
[7,"70.","70.51.","leidingen - ondergrondse kabels ","FH","m"]
[7,"70.","70.52.","leidingen - kabels in vrije buitenlucht ","FH","m"]
[7,"70.","70.53.","leidingen - inbouw kabelbuizen ","PM"]
[7,"70.","70.54.","leidingen - opbouw kabelbuizen ","PM"]
[7,"70.","70.55.","leidingen - plint- & wandkanalen ","PM"]
[7,"70.","70.56.","leidingen - kabelgoten en -ladders ","PM"]
[7,"70.","70.57.","leidingen - wachtbuizen ","PM"]
[7,"70.","70.60.","trek- en verbindingsdozen - algemeen"]
[7,"70.","70.61.","trek- en verbindingsdozen - inbouw metselwerk ","PM"]
[7,"70.","70.62.","trek- en verbindingsdozen - inbouw holle wanden ","PM"]
[7,"70.","70.63.","trek- en verbindingsdozen - inbouw verlaagde plafonds ","PM"]
[7,"70.","70.64.","trek- en verbindingsdozen - inbouw vloeren ","PM"]
[7,"70.","70.65.","trek- en verbindingsdozen - opbouw ","PM"]
[7,"70.","70.70.","bijzondere voorzieningen - algemeen"]
[7,"70.","70.71.","bijzondere voorzieningen - voeding liften ","PM"]
[7,"70."]
[7,"71.","71.","ELEKTRICITEIT SCHAKELAARS & CONTACTDOZEN"]
[7,"71.","71.00.","elektriciteit schakelaars & contactdozen - algemeen"]
[7,"71.","71.10.","stopcontacten - algemeen"]
[7,"71.","71.11.","stopcontacten - 10/16A ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"71.","71.12.","stopcontacten - 20/32A ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"71.","71.20.","aansluitdozen - algemeen"]
[7,"71.","71.21.","aansluitdozen - voeding elektrisch fornuis ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"71.","71.22.","aansluitdozen - voeding was- & vaatwasmachine ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"71.","71.23.","aansluitdozen - voeding HVAC en andere ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"71.","71.30.","schakelaars - algemeen"]
[7,"71.","71.31.","schakelaars - enkelpolig ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"71.","71.32.","schakelaars - dubbelpolig ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"71.","71.33.","schakelaars - wissel ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"71.","71.34.","schakelaars - kruis ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"71.","71.35.","schakelaars - timerschakelaars ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"71.","71.36.","schakelaars - teleruptoren ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"71.","71.37.","schakelaars - dimmers ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"71.","71.40.","speciale toebehoren - algemeen"]
[7,"71.","71.41.","speciale toebehoren - bewegingsdetectoren ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Schakelaar Toebehoren ","Stuks"]
[7,"71.","71.42.","speciale toebehoren - foto-elektrisch schakelaar ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Schakelaar Toebehoren ","Stuks"]
[7,"71.","71.43.","speciale toebehoren - schemerschakelaar ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Schakelaar Toebehoren ","Stuks"]
[7,"71."]
[7,"72.","72.","ELEKTRICITEIT LICHTARMATUREN"]
[7,"72.","72.00.","elektriciteit lichtarmaturen - algemeen"]
[7,"72.","72.10.","binnenarmaturen E27 - algemeen ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"72.","72.11.","binnenarmaturen E27 - met lenskap ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"72.","72.12.","binnenarmaturen E27 - andere ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"72.","72.20.","binnenarmaturen TL - algemeen"]
[7,"72.","72.21.","binnenarmaturen TL - opbouwarmatuur plafond"]
[7,"72.","72.21.10.","binnenarmaturen TL - opbouwarmatuur plafond - T8 ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"72.","72.21.20.","binnenarmaturen TL - opbouwarmatuur plafond - T5 ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"72.","72.22.","binnenarmaturen TL - lichtstrip keukenaanrecht ",null,null,"TYPE 5",null,null,"Stuks"]
[7,"72.","72.22.10.","binnenarmaturen TL - lichtstrip keukenaanrecht/T8 ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"72.","72.22.20.","binnenarmaturen TL - lichtstrip keukenaanrecht/T5 ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"72.","72.40.","binnenarmaturen halo - algemeen"]
[7,"72.","72.41.","binnenarmaturen halo - transfo ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"72.","72.42.","binnenarmaturen halo - inbouwspots ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"72.","72.43.","binnenarmaturen halo - opbouwspots ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"72.","72.50.","veiligheidsverlichting - algemeen"]
[7,"72.","72.51.","veiligheidsverlichting - autonoom niet-permanent ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"72.","72.52.","veiligheidsverlichting - autonoom permanent ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"72.","72.53.","veiligheidsverlichting - centrale noodvoeding ","SOG"]
[7,"72.","72.54.","veiligheidsverlichting - armaturen ","SOG"]
[7,"72.","72.55.","veiligheidsverlichting - signalisatie & pictogrammen ","PM"]
[7,"72.","72.60.","buitenarmaturen - algemeen"]
[7,"72.","72.70.","armaturen geleverd door het bestuur - algemeen"]
[7,"72."]
[7,"73.","73.","ELEKTRICITEIT BEL & PARLOFOON"]
[7,"73.","73.00.","elektriciteit bel & parlofoon - algemeen"]
[7,"73.","73.10.","individuele belinstallaties - algemeen"]
[7,"73.","73.11.","individuele belinstallaties - huisbel ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"73.","73.12.","individuele belinstallaties - beldrukknop ","PM"]
[7,"73.","73.13.","individuele belinstallaties - beltransfo ","PM"]
[7,"73.","73.14.","individuele belinstallaties - bedrading ","PM"]
[7,"73.","73.20.","parlofooninstallatie - algemeen"]
[7,"73.","73.21.","parlofooninstallatie - binnenposten ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"73.","73.22.","parlofooninstallatie - deurstation ","PM"]
[7,"73.","73.23.","parlofooninstallatie - beltransfo ","PM"]
[7,"73.","73.24.","parlofooninstallatie - verdeeldozen ","PM"]
[7,"73.","73.25.","parlofooninstallatie - bedrading ","PM"]
[7,"73.","73.26.","parlofooninstallatie - elektrisch deurslot ","PM"]
[7,"73.","73.30.","toegangscontrolesysteem - algemeen","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"73.",null,null,"SOG"]
[7,"73."]
[7,"74.","74.","ELEKTRICITEIT TELECOM & DOMOTICA"]
[7,"74.","74.00.","elektriciteit telecom & domotica - algemeen"]
[7,"74.","74.10.","telefoon - algemeen"]
[7,"74.","74.11.","telefoon - buitenbekabeling ","SOG"]
[7,"74.","74.12.","telefoon - basis aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"74.","74.13.","telefoon - extra aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"74.","74.14.","telefoon - binnenbekabeling ","PM"]
[7,"74.","74.20.","kabeldistributie - algemeen"]
[7,"74.","74.21.","kabeldistributie - buitenbekabeling ","SOG"]
[7,"74.","74.22.","kabeldistributie - basis aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"74.","74.23.","kabeldistributie - extra aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"74.","74.24.","kabeldistributie - binnenbekabeling ","PM"]
[7,"74.","74.30.","netwerkbekabeling - algemeen"]
[7,"74.","74.31.","netwerkbekabeling - buitenbekabeling ","SOG"]
[7,"74.","74.32.","netwerkbekabeling - basis aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"74.","74.33.","netwerkbekabeling - extra aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"74.","74.34.","netwerkbekabeling - binnenbekabeling ","PM"]
[7,"74.","74.40.","satelietontvangstsysteem - algemeen"]
[7,"74.","74.41.","satelietontvangstsysteem - centrale schotelantenne ","SOG"]
[7,"74.","74.42.","satelietontvangstsysteem - buitenbekabeling ","SOG"]
[7,"74.","74.43.","satelietontvangstsysteem - basis aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"74.","74.44.","satelietontvangstsysteem - extra aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"74.","74.45.","satelietontvangstsysteem - binnenbekabeling ","PM"]
[7,"74.","74.50.","alarmkabel - algemeen"]
[7,"74.","74.60.","luidsprekerkabel - algemeen"]
[7,"74.","74.70.","oproepsystemen ADL - algemeen"]
[7,"74.","74.80.","multimediakast","FH","st","TYPE 5","Morph",null,"Stuks"]
[7,"74.",{"$nulls":5},"Object",null,"Stuks"]
[7,"74."]
[7,"75.","75.","ELEKTRICITEIT VERWARMING"]
[7,"75.","75.00.","elektriciteit verwarming - algemeen"]
[7,"75.","75.10.","direct systeem - algemeen"]
[7,"75.","75.11.","direct systeem - gedecentraliseerd"]
[7,"75.","75.11.10.","direct systeem - gedecentraliseerd/wandconvectoren ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"75.","75.11.20.","direct systeem - gedecentraliseerd/plintconvectoren ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"75.","75.11.30.","direct systeem - gedecentraliseerd/stralingselementen ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"75.","75.20.","accumulatiesysteem - algemeen"]
[7,"75.","75.21.","accumulatiesysteem - gedecentraliseerd"]
[7,"75.","75.21.10.","accumulatiesysteem - gedecentraliseerd/dynamisch gemengd ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"75.","75.30.","meet- & regeltoestellen - algemeen"]
[7,"75.","75.31.","meet- & regeltoestellen - klokthermostaten "]
[7,"75.","75.31.10.","meet- & regeltoestellen - klokthermostaten/direct systeem ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"75.",null,null,"PM"]
[7,"75.","75.31.20.","meet- & regeltoestellen - klokthermostaten/accumulatie systeem ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"75.",null,null,"PM"]
[7,"75."]
[7,"76.","76.","ELEKTROMECHANICA LIFTEN"]
[7,"76.","76.00.","elektromechanica liften - algemeen"]
[7,"76.","76.01.","algemeen - grenzen van de aanneming ","PM"]
[7,"76.","76.02.","algemeen - controle op afmetingen ","PM"]
[7,"76.","76.03.","algemeen - documentatie en studie ","PM"]
[7,"76.","76.04.","algemeen - werfinstallatie en -organisatie ","PM"]
[7,"76.","76.05.","algemeen - onderhoud tijdens waarborgperiode ","PM"]
[7,"76.","76.10.","bestaande installaties - algemeen"]
[7,"76.","76.11.","bestaande installaties - afbraak ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Lift Bestaande installaties","Stuks"]
[7,"76.","76.12.","bestaande installaties - renovatie ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Lift Bestaande installaties","Stuks"]
[7,"76.","76.20.","elektrische liften - algemeen"]
[7,"76.","76.21.","elektrische liften - met machinekamer ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"76.","76.22.","elektrische liften - zonder machinekamer (gearless) ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"76.","76.30.","kooiuitrusting - algemeen"]
[7,"76.","76.31.","kooiuitrusting - personenlift ","PM"]
[7,"76.","76.32.","kooiuitrusting - goederenlift ","PM"]
[7,"76.","76.33.","kooiuitrusting - vandalismewerend ","PM"]
[7,"76.","76.40.","deuren & fronten - algemeen"]
[7,"76.","76.41.","deuren & fronten - personenlift ","PM"]
[7,"76.","76.50.","bedienings- & signalisatiepanelen - algemeen"]
[7,"76.","76.51.","bedienings- & signalisatiepanelen - personenlift ","PM"]
[7,"76."]
[7,"77.","77.","BRANDDETECTIE & ALARMSYSTEMEN"]
[7,"77.","77.00.","branddetectie & alarmsystemen - algemeen"]
[7,"77.","77.10.","centrale eenheid - algemeen ","SOG"]
[7,"77.","77.20.","energievoorziening - algemeen ","PM"]
[7,"77.","77.30.","bekabeling - algemeen ","PM"]
[7,"77.","77.40.","brandmelding - algemeen"]
[7,"77.","77.41.","brandmelding - branddetectoren ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"77.","77.42.","brandmelding - handmelders ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"77.","77.43.","brandmelding - gasdetectoren ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"77.","77.44.","brandmelding - autonome rookmelders ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"77.","77.50.","alarmsirenes - algemeen"]
[7,"77.","77.51.","alarmsirenes - signal fast sweep ","FH","st","TYPE 5","Object",null,"Stuks"]
[7,"77.","77.60.","evacuatietoebehoren - algemeen"]
[7,"77.","77.61.","evacuatietoebehoren - deurpomp met magneethouder ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurpomp","Stuks"]
[7,"77.","77.62.","evacuatietoebehoren - pictogrammen ","PM"]
[7,"77.","77.63.","evacuatietoebehoren - brandweersleutelkluis","FH","st","TYPE 5","Morph",null,"Stuks"]
[7,"77.",{"$nulls":5},"Object",null,"Stuks"]
[7,"77."]
[8,"80.","80.","BINNENSCHILDERWERKEN"]
[8,"80.","80.00.","schilderwerken - algemeen"]
[8,"80.","80.10.","binnenschilderwerken op pleisterwerk - algemeen"]
[8,"80.","80.11.","binnenschilderwerken op pleisterwerk - acrylaathars ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Zone"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.12.","binnenschilderwerken op pleisterwerk - acrylaatdispersie ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Zone"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.13.","binnenschilderwerken op pleisterwerk - vinyllatex ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Zone"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.14.","binnenschilderwerken op pleisterwerk - kwartshoudende structuurverf ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Zone"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.15.","binnenschilderwerken op pleisterwerk - meerkleurige effectverf ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Zone"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.20.","binnenschilderwerken op gipskartonplaten - algemeen"]
[8,"80.","80.21.","binnenschilderwerken op gipskartonplaten - acrylaathars ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Zone"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.22.","binnenschilderwerken op gipskartonplaten - acrylaatdispersie ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Zone"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.23.","binnenschilderwerken op gipskartonplaten - vinyllatex ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Zone"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.24.","binnenschilderwerken op gipskartonplaten - kwartshoudende structuurverf ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Zone"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.25.","binnenschilderwerken op gipskartonplaten - meerkleurige effectverf ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Zone"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.30.","binnenschilderwerken op beton - algemeen"]
[8,"80.","80.31.","binnenschilderwerken op beton - acrylaathars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"80.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Zone"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.32.","binnenschilderwerken op beton - acrylaatdispersie ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"80.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Zone"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.33.","binnenschilderwerken op beton - vinyllatex ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"80.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Zone"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.34.","binnenschilderwerken op beton - kwartshoudende structuurverf ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"80.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Zone"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.35.","binnenschilderwerken op beton - meerkleurig effectverf ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"80.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Zone"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.36.","binnenschilderwerken op beton - epoxyverf ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.40.","binnenschilderwerken op metselwerk - algemeen"]
[8,"80.","80.41.","binnenschilderwerken op metselwerk - acrylaathars ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.42.","binnenschilderwerken op metselwerk - acrylaatdispersie ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.43.","binnenschilderwerken op metselwerkwerk - vinyllatex ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.44.","binnenschilderwerken op metselwerk - kwartshoudende structuurverf ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.45.","binnenschilderwerken op metselwerk - meerkleurige effectverf ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.50.","binnenschilderwerken op hout en houtachtige platen - algemeen"]
[8,"80.","80.51.","binnenschilderwerken op hout en houtachtige platen - lak"]
[8,"80.","80.51.10.","op hout en houtachtige platen - lak/acryllaatdispersie ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"80.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.51.20.","op hout en houtachtige platen - lak/polyurethaan acrylaathars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"80.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.51.30.","op hout en houtachtige platen - lak/alkyd-urethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"80.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.51.40.","op hout en houtachtige platen - lak/alkydhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"80.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.52.","binnenschilderwerken op hout en houtachtige platen - vernis"]
[8,"80.","80.52.10.","op hout en houtachtige platen - vernis / acrylurethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"80.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.52.20.","op hout en houtachtige platen - vernis/polyurethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"80.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.52.30.","op hout en houtachtige platen - vernis/alkydurethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"80.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.53.","binnenschilderwerken op hout en houtachtige platen - beits ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"80.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"80.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"80.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"80.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"80.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"80.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"80.","80.60.","binnenschilderwerken op metaal - algemeen"]
[8,"80."]
[8,"81.","81.","BEHANGWERKEN"]
[8,"81.","81.00.","behangwerken - algemeen"]
[8,"81.","81.10.","verwijderen van behangpapier - algemeen ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"81.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"81.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"81.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"81.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"81.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"81.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"81.","81.20.","behangen met glasvezeldoek - algemeen"]
[8,"81.","81.21.","behangen met glasvezeldoek - op nieuw pleisterwerk ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"81.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"81.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"81.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"81.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"81.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"81.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"81.","81.22.","behangen met glasvezeldoek - op oud pleisterwerk ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"81.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"81.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"81.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"81.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"81.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"81.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"81.","81.23.","behangen met glasvezeldoek - op gipskartonplaten ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"81.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"81.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"81.",{"$nulls":5},"Wall",null,"Net Surface Area on the inside face"]
[8,"81.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"81.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)"]
[8,"81.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"81."]
[8,"82.","82.","BUITENSCHILDERWERKEN"]
[8,"82.","82.00.","buitenschilderwerken - algemeen"]
[8,"82.","82.10.","buitenschilderwerken op buitenbepleistering - algemeen"]
[8,"82.","82.11.","buitenschilderwerken op buitenbepleisteringen - acrylaatdispersie ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.12.","buitenschilderwerken op buitenbepleisteringen - siloxaan ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.13.","buitenschilderwerken op buitenbepleisteringen - silicaat ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.20.","buitenschilderwerken op beton - algemeen"]
[8,"82.","82.21.","buitenschilderwerken op beton - acrylaatdispersie ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.22.","buitenschilderwerken op beton - siloxaan ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.23.","buitenschilderwerken op beton - silicaat ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.24.","buitenschilderwerken op beton - kwartshoudende structuurverf ","FH","m2","TYPE 3","Beam",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.30.","buitenschilderwerken op gevelmetselwerk - algemeen"]
[8,"82.","82.31.","buitenschilderwerken op gevelmetselwerk - acrylaatdispersie ","FH","m2","TYPE 3","Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.32.","buitenschilderwerken op gevelmetselwerk - siloxaan ","FH","m2","TYPE 3","Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.33.","buitenschilderwerken op gevelmetselwerk - silicaat ","FH","m2","TYPE 3","Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.34.","buitenschilderwerken op gevelmetselwerk - kwartshoudende structuurverf ","FH","m2","TYPE 3","Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.40.","buitenschilderwerken op hout en houtachtige platen - algemeen"]
[8,"82.","82.41.","buitenschilderwerken op hout en houtachtige platen - lak"]
[8,"82.","82.41.10.","op hout en houtachtige platen - lak/acryllaatdispersie watergedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"82.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"82.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur buitenzijde"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"82.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.41.20.","op hout en houtachtige platen - lak/alkyd-urethaan watergedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"82.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"82.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur buitenzijde"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"82.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.41.30.","op hout en houtachtige platen - lak/alkydhars solventgedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"82.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"82.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur buitenzijde"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"82.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.41.40.","op hout en houtachtige platen - lak/urethaan-alkyd solventgedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"82.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"82.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur buitenzijde"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"82.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.42.","buitenschilderwerken op hout en houtachtige platen - vernis"]
[8,"82.","82.42.10.","op hout en houtachtige platen - vernis/alkyd-urethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"82.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"82.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur buitenzijde"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"82.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.43.","buitenschilderwerken op hout en houtachtige platen - beits"]
[8,"82.","82.43.10.","op hout en houtachtige platen - beits/alkydhars watergedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"82.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"82.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur buitenzijde"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"82.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.43.20.","op hout en houtachtige platen - beits/alkydhars solventgedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"82.",{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[8,"82.",{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur buitenzijde"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst"]
[8,"82.",null,null,null,"m2","TYPE 3","Beam",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.50.","nabehandelingen op metselwerk - algemeen"]
[8,"82.","82.51.","nabehandelingen op metselwerk - hydrofobering ","FH","m2","TYPE 3","Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.52.","nabehandelingen op metselwerk - antigraffiti ","FH","m2","TYPE 3","Column",null,"Top Surface"]
[8,"82.",{"$nulls":5},"Wall",null,"Net Surface Area on the outside face"]
[8,"82.",{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)"]
[8,"82.",{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area"]
[8,"82.","82.60.","buitenschilderwerken op metaal - algemeen"]
[8,"82."]
[9,"90.","90.","BUITENVERHARDINGEN"]
[9,"90.","90.00.","buitenverhardingen - algemeen"]
[9,"90.","90.10.","funderingen - algemeen"]
[9,"90.","90.11.","funderingen - steenslag"]
[9,"90.","90.11.10.","funderingen - steenslag/niet-continue korrelverdeling ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.11.20.","funderingen - steenslag/continue korrelverdeling zonder toevoegsels ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.11.30.","funderingen - steenslag/continue korrelverdeling met toevoegsels ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.12.","funderingen - ternair mengsel ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.13.","funderingen - zandcement ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.14.","funderingen - schraal beton"]
[9,"90.","90.14.10.","funderingen - schraal beton/ongewapend ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.14.20.","funderingen - schraal beton/gewapend ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.20.","verhardingen - algemeen"]
[9,"90.","90.21.","verhardingen - in rijen te leggen kasseien ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.22.","verhardingen - mozaïekkeien ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.23.","verhardingen - betonstraatstenen"]
[9,"90.","90.23.10.","verhardingen - betonstraatstenen/kleurvast ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.23.20.","verhardingen - betonstraatstenen/waterdoorlatend ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.24.","verhardingen - gebakken straatstenen ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.25.","verhardingen - betontegels"]
[9,"90.","90.25.10.","verhardingen - betontegels/kleurvast ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.25.20.","verhardingen - betontegels/waterdoorlatend ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.25.30.","verhardingen - betontegels/grasbetontegels ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.25.40.","verhardingen - betontegels/silexbetontegels ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.26.","verhardingen - tegels in natuursteen ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.27.","verhardingen - dolomiet ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.28.","verhardingen - gepolierd beton ","FH of VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume"]
[9,"90.",{"$nulls":5},"Morph",null,"Net Volume"]
[9,"90.","90.29.","verhardingen - tactiele oppervlakken ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"90.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"90.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"90.","90.30.","lijnvormige elementen - algemeen"]
[9,"90.","90.31.","lijnvormige elementen - boordstenen"]
[9,"90.","90.31.10.","lijnvormige elementen - boordstenen/beton"]
[9,"90.","90.31.11.","lijnvormige elementen - boordstenen/beton - prefab ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[9,"90.","90.31.12.","lijnvormige elementen - boordstenen/beton - ter plaatse gestort ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[9,"90.","90.31.20.","lijnvormige elementen - boordstenen/palissaden ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[9,"90.","90.31.30.","lijnvormige elementen - boordstenen/metaal ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[9,"90.","90.32.","lijnvormige elementen - watergreppels"]
[9,"90.","90.32.10.","lijnvormige elementen - watergreppels/beton"]
[9,"90.","90.32.11.","lijnvormige elementen - watergreppels/beton - prefab ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[9,"90."]
[9,"91.","91.","BUITENCONSTRUCTIES EN AFSLUITINGEN"]
[9,"91.","91.00.","buitenconstructies en afsluitingen - algemeen"]
[9,"91.","91.10.","tuinafsluitingspalen - algemeen"]
[9,"91.","91.11.","tuinafsluitingspalen - staal ","PM"]
[9,"91.","91.12.","tuinafsluitingspalen - hout ","PM"]
[9,"91.","91.13.","tuinafsluitingspalen - beton ","PM"]
[9,"91.","91.20.","draadafsluitingen - algemeen"]
[9,"91.","91.21.","draadafsluitingen - gladde draad ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
[9,"91.","91.22.","draadafsluitingen - draadgaas ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
[9,"91.","91.30.","tuinschermen - algemeen"]
[9,"91.","91.31.","tuinschermen - schapenhek ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
[9,"91.","91.32.","tuinschermen - houtschermen ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
[9,"91.","91.33.","tuinschermen - betonplaten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
[9,"91.","91.40.","tuinhekken - algemeen"]
[9,"91.","91.41.","tuinhekken - staal ","FH","st","TYPE 5","Door",null,"Stuks"]
[9,"91.","91.42.","tuinhekken - hout ","FH","st","TYPE 5","Door",null,"Stuks"]
[9,"91.","91.50.","terrassen tuinhout - algemeen"]
[9,"91.","91.51.","terrassen tuinhout - tegels ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"91.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"91.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"91.","91.52.","terrassen tuinhout - beplanking ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"91.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"91.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"91.","91.60.","constructies tuinhout - algemeen"]
[9,"91."]
[9,"92.","92.","BUITENMEUBILAIR EN UITRUSTINGSELEMENTEN"]
[9,"92.","92.00.","buitenmeubilair en uitrustingselementen - algemeen"]
[9,"92.","92.10.","brievenbussen - algemeen"]
[9,"92.","92.11.","brievenbussen - geleverd door het bestuur ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.12.","brievenbussen - prefab beton ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.13.","brievenbussen - staal ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.14.","brievenbussen - aluminium ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.20.","vuilnisbakken - algemeen"]
[9,"92.","92.21.","vuilnisbakken - geleverd door het bestuur ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.22.","vuilnisbakken - staal ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.23.","vuilnisbakken - kunststof ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.30.","fietsrekken - algemeen"]
[9,"92.","92.31.","fietsrekken - blokken beton ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.32.","fietsrekken - modules staal ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.33.","fietsrekken - aanleunbeugels staal ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.34.","fietsrekken - ophangelementen staal ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.35.","fietsrekken - klemmen staal ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.40.","parkingelementen - algemeen"]
[9,"92.","92.41.","parkingelementen - parkeerpalen ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.42.","parkingelementen - parkeerbeugels ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.50.","zitbanken - algemeen"]
[9,"92.","92.51.","zitbanken - geleverd door het bestuur ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.52.","zitbanken - zonder rugleuning ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.53.","zitbanken - met rugleuning ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.60.","boomomrandingen - algemeen"]
[9,"92.","92.61.","boomomrandingen - roosters beton ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.62.","boomomrandingen - roosters gietijzer ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.63.","boomomrandingen - roosters kunststof ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.64.","boomomrandingen - roosters staal ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.70.","plantbescherming - algemeen"]
[9,"92.","92.71.","plantbescherming - boombeugels staal ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.73.","plantbescherming - boomkorven staal ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92.","92.74.","plantbescherming - plantkorven staal ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"92."]
[9,"93.","93.","GROENAANLEG EN -ONDERHOUD"]
[9,"93.","93.00.","groenaanleg en -onderhoud - algemeen"]
[9,"93.","93.10.","grondbewerkingen - algemeen"]
[9,"93.","93.11.","grondbewerkingen - diepspitten ","PM"]
[9,"93.","93.12.","grondbewerkingen - egaliseren ","PM"]
[9,"93.","93.13.","grondbewerkingen - frezen ","PM"]
[9,"93.","93.20.","verwerking teelaarde - algemeen"]
[9,"93.","93.21.","verwerking teelaarde - afkomstig van afgraving ","FH/VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"93.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume"]
[9,"93.",{"$nulls":5},"Morph",null,"Net Volume"]
[9,"93.","93.22.","verwerking teelaarde - te leveren door de aannemer ","FH/VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"93.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume"]
[9,"93.",{"$nulls":5},"Morph",null,"Net Volume"]
[9,"93.","93.30.","verwerken van bodemverbeteringsmiddelen - algemeen ","FH/VH","kg","TYPE 4","Slab","vul de ARCHICAD property 'Soortelijk gewicht' in","ARCHICAD property: Gewicht materiaal"]
[9,"93.",{"$nulls":4},"TYPE 5","Mesh","vul de ARCHICAD property 'Soortelijk gewicht' in","ARCHICAD property: Gewicht materiaal"]
[9,"93.",{"$nulls":5},"Morph","vul de ARCHICAD property 'Soortelijk gewicht' in","ARCHICAD property: Gewicht materiaal"]
[9,"93.",null,null,null,"m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"93.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume"]
[9,"93.",{"$nulls":5},"Morph",null,"Net Volume"]
[9,"93.","93.40.","aanleg grasmatten - algemeen"]
[9,"93.","93.41.","aanleg grasmatten - door bezaaiing ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"93.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"93.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"93.","93.42.","aanleg grasmatten - door bezoding ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"93.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"93.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"93.","93.50.","aanplanting houtachtige vegetaties - algemeen"]
[9,"93.","93.51.","aanplanting houtachtige vegetaties - bomen ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"93.","93.52.","aanplanting houtachtige gewassen - hagen ","FH","st","TYPE 5","Morph",null,"Stuks"]
[9,"93.",{"$nulls":5},"Object",null,"Stuks"]
[9,"93.",{"$nulls":5},"Wall",null,"Stuks"]
[9,"93.","93.53.","aanplanting houtachtige gewassen - heesters ","FH","st","TYPE 5","Object",null,"Stuks"]
[9,"93.","93.60.","hulpmiddelen groenaanleg - algemeen"]
[9,"93.","93.61.","hulpmiddelen groenaanleg - boompaalconstructies ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW hulpmiddelen groenaanleg","Stuks"]
[9,"93.",{"$nulls":4},"TYPE 5","Object",null,"Stuks"]
[9,"93.","93.62.","hulpmiddelen groenaanleg - boomroosters ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW hulpmiddelen groenaanleg","Stuks"]
[9,"93.",{"$nulls":4},"TYPE 5","Object",null,"Stuks"]
[9,"93.","93.63.","hulpmiddelen groenaanleg - ondergrondse verankering van bomen ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW hulpmiddelen groenaanleg","Stuks"]
[9,"93.",{"$nulls":4},"TYPE 5","Object",null,"Stuks"]
[9,"93.","93.64.","hulpmiddelen groenaanleg - groeiplaatsverbetering van bomen (irrigatie) ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW hulpmiddelen groenaanleg","Stuks"]
[9,"93.",{"$nulls":4},"TYPE 5","Object",null,"Stuks"]
[9,"93.","93.65.","hulpmiddelen groenaanleg - haagsteun ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten"]
[9,"93.","93.70.","groenonderhoud - algemeen"]
[9,"93.","93.71.","groenonderhoud - maaien van grasmatten ","FH","m2","TYPE 4","Slab","Gebruik ARCHICAD property: VMSW maaien van grasmatten","Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig"]
[9,"93.",{"$nulls":4},"TYPE 5","Mesh",null,"Net Area"]
[9,"93.",{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area"]
[9,"93.","93.72.","groenonderhoud - bomen snoeien ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW bomen snoeien","Stuks"]
[9,"93.","93.73.","groenonderhoud - scheren van hagen en beplantingsmassieven ","FH","m2","TYPE 4","Morph","Gebruik ARCHICAD Property: VMSW_scheren van hagen en beplantingsmassieven","Surface Area"]
[9,"93.",{"$nulls":5},"Wall","Gebruik ARCHICAD Property: VMSW_scheren van hagen en beplantingsmassieven","Top Surface"]
[9,"93.","93.74.","groenonderhoud - snoeien van heesters ","FH","st","TYPE 5","Object",null,"Stuks"]