{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["Publicatie Art.NR en elementen","types"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Publicatie Art.NR en elementen","index":0,"n_rows":4098,"n_cols":10,"rows_kept":4098,"cut":false,"hidden":false,"merged":[]}
["Artikelnummer","Artikelomschrijving","AvO","Eenheid","Type","Element","Element specificatie","Wat rekent de Meetstaat Manager?","Aandachtspunten"]
[{"$nulls":9},"Totaal"]
["00.","ALGEMENE BEPALINGEN"]
["00.10.","projectgegevens"]
["00.20.","ontwerpteam"]
["00.21.","ontwerpteam - architecturaal ontwerp",null,null,"Geen",{"$nulls":4},1]
["00.22.","ontwerpteam - studie stabiliteit",null,null,"Geen",{"$nulls":4},1]
["00.23.","ontwerpteam - studie technieken",null,null,"Geen",{"$nulls":4},1]
["00.24.","ontwerpteam - veiligheidscoördinatie",null,null,"Geen",{"$nulls":4},1]
["00.25.","ontwerpteam - EPB verslaggeving",null,null,"Geen",{"$nulls":4},1]
["00.30.","documenten"]
["00.31.","documenten - architectuur",null,null,"Geen",{"$nulls":4},1]
["00.32.","documenten - stabiliteit",null,null,"Geen",{"$nulls":4},1]
["00.33.","documenten - technieken",null,null,"Geen",{"$nulls":4},1]
["00.34.","documenten - veiligheidscoördinatie",null,null,"Geen",{"$nulls":4},1]
["00.35.","documenten - EPB verslaggeving",null,null,"Geen",{"$nulls":4},1]
["00.36.","documenten - diepsonderingsverslag",null,null,"Geen",{"$nulls":4},1]
["00.37.","documenten - verslag milieutechnisch bodemonderzoek",null,null,"Geen",{"$nulls":4},1]
["01.","AANNEMINGSMODALITEITEN"]
["01.00.","aannemingsmodaliteiten - algemeen"]
["01.01.","aannemingsmodaliteiten - bestek ","PM",null,"Geen",{"$nulls":4},1]
["01.02.","aannemingsmodaliteiten - voorafgaand plaatsbezoek ","PM",null,"Geen",{"$nulls":4},1]
["01.03.","aannemingsmodaliteiten - burgerlijke aansprakelijkheid ","PM",null,"Geen",{"$nulls":4},1]
["01.04.","aannemingsmodaliteiten - volledigheid van inschrijving ","PM",null,"Geen",{"$nulls":4},1]
["01.05.","aannemingsmodaliteiten - onderaanneming ","PM",null,"Geen",{"$nulls":4},1]
["01.06.","aannemingsmodaliteiten - verrekeningen ","PM",null,"Geen",{"$nulls":4},1]
["01.07.","aannemingsmodaliteiten - keuringsattesten ","PM",null,"Geen",{"$nulls":4},1]
["01.08.","aannemingsmodaliteiten - materialenlijst ","PM",null,"Geen",{"$nulls":4},1]
["01.10.","plaatsbeschrijvingen - algemeen"]
["01.11.","plaatsbeschrijvingen - aangrenzende constructies"]
["01.11.10.","plaatsbeschrijvingen – aangrenzende constructies/bij aanvang van de werken","PM",null,"Geen",{"$nulls":4},1]
["01.11.20.","plaatsbeschrijvingen – aangrenzende constructies/staat van vergelijking","PM",null,"Geen",{"$nulls":4},1]
["01.12.","plaatsbeschrijvingen - te renoveren constructies",null,null,"Geen",{"$nulls":4},1]
["01.12.10.","plaatsbeschrijvingen – te renoveren constructies/bij aanvang van de werken","PM",null,"Geen",{"$nulls":4},1]
["01.12.20.","plaatsbeschrijvingen – te renoveren constructies/staat van vergelijking","PM",null,"Geen",{"$nulls":4},1]
["01.13.","plaatsbeschrijvingen - inboedel bij blijvende bewoning"]
["01.13.10.","plaatsbeschrijvingen – inboedel bij blijvende bewoning/bij aanvang van de werken","PM",null,"Geen",{"$nulls":4},1]
["01.13.20.","plaatsbeschrijvingen – inboedel bij blijvende bewoning/staat van vergelijking","PM",null,"Geen",{"$nulls":4},1]
["01.14.","plaatsbeschrijvingen - wegenis en voetpaden"]
["01.14.10.","plaatsbeschrijvingen – wegenis en voetpaden bij aanvang van de werken","PM",null,"Geen",{"$nulls":4},1]
["01.14.20.","plaatsbeschrijvingen – wegenis en voetpaden/staat van vergelijking","PM",null,"Geen",{"$nulls":4},1]
["01.15.","plaatsbeschrijvingen - beplanting"]
["01.15.10.","plaatsbeschrijvingen – beplanting/bij aanvang van de werken","PM",null,"Geen",{"$nulls":4},1]
["01.15.20.","plaatsbeschrijvingen – beplanting/staat van vergelijking","PM",null,"Geen",{"$nulls":4},1]
["01.20.","werfcoördinatie - algemeen"]
["01.21.","werfcoördinatie - planning van de werken ","PM",null,"Geen",{"$nulls":4},1]
["01.22.","werfcoördinatie - werfleiding en controle ","PM",null,"Geen",{"$nulls":4},1]
["01.23.","werfcoördinatie - werfvergaderingen ","PM",null,"Geen",{"$nulls":4},1]
["01.24.","werfcoördinatie - uitzetten bouwwerken ","PM",null,"Geen",{"$nulls":4},1]
["01.25.","werfcoördinatie - as-builtdossier ","PM",null,"Geen",{"$nulls":4},1]
["01.26.","werfcoördinatie - renovaties met blijvende bewoning ","PM",null,"Geen",{"$nulls":4},1]
["01.30.","werfcondities - algemeen"]
["01.31.","werfcondities - orde en netheid ","PM",null,"Geen",{"$nulls":4},1]
["01.32.","werfcondities - geluids- en stofhinder ","PM",null,"Geen",{"$nulls":4},1]
["01.33.","werfcondities - nazorg ","PM",null,"Geen",{"$nulls":4},1]
["01.40.","veiligheidsvoorschriften - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["02.","BOUWPLAATSVOORZIENINGEN"]
["02.00.","bouwplaatsvoorzieningen - algemeen"]
["02.10.","beschermingswerken - algemeen"]
["02.11.","beschermingwerken - openbare weg ","PM",null,"Geen",{"$nulls":4},1]
["02.12.","beschermingswerken - beplantingen"]
["02.12.10.","beschermingswerken – beplantingen/bomen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["02.12.20.","beschermingswerken – beplantingen/struiken en hagen","PM"]
["02.20.","opruiming beplantingen - algemeen"]
["02.21.","opruiming beplantingen - bomen ","PM ",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["02.22.","opruiming beplantingen - struiken en hagen ","PM",null,"Geen",{"$nulls":4},1]
["02.30.","toegangswegen - algemeen"]
["02.31.","toegangswegen - voorlopige verharding voor voetgangers ","PM",null,"Geen",{"$nulls":4},1]
["02.32.","toegangswegen - voorlopige verharding voor zware lasten ","PM",null,"Geen",{"$nulls":4},1]
["02.33.","toegangswegen - parkeerruimte voor laden en lossen ","PM",null,"Geen",{"$nulls":4},1]
["02.40.","voorlopige omheining - algemeen"]
["02.50.","aankondiging werf - algemeen"]
["02.51.","aankondiging werf - werfbord ","PM",null,"Geen",{"$nulls":4},1]
["02.52.","aankondiging werf - werfdoek ","PM",null,"Geen",{"$nulls":4},1]
["02.60.","werflokalen - algemeen"]
["02.61.","werflokalen - berging van materieel en bouwmaterialen ","PM",null,"Geen",{"$nulls":4},1]
["02.62.","werflokalen - kantoorruimte ","PM",null,"Geen",{"$nulls":4},1]
["02.63.","werflokalen - personeelslokaal ","PM",null,"Geen",{"$nulls":4},1]
["02.64.","werflokalen - sanitaire voorzieningen ","PM",null,"Geen",{"$nulls":4},1]
["02.70.","voorlopige aansluitingen - algemeen"]
["02.71.","voorlopige aansluitingen - stroomvoorziening ","PM",null,"Geen",{"$nulls":4},1]
["02.72.","voorlopige aansluitingen - watervoorziening ","PM",null,"Geen",{"$nulls":4},1]
["02.73.","voorlopige aansluitingen - waterafvoer ","PM",null,"Geen",{"$nulls":4},1]
["02.80.","arbeidsmiddelen - algemeen"]
["02.81.","arbeidsmiddelen - werken op hoogte"]
["02.81.10","arbeidsmiddelen - werken op hoogte/ladders","PM",null,"Geen",{"$nulls":4},1]
["02.81.20","arbeidsmiddelen - werken op hoogte/steigers","PM",null,"Geen",{"$nulls":4},1]
["02.82.","arbeidsmiddelen - hijsen en heffen van lasten ","PM",null,"Geen",{"$nulls":4},1]
["03.","AFBRAAKWERKEN"]
["03.00.","afbraakwerken - algemeen"]
["03.01.","afbraakwerken - asbestverwijdering"]
["03.02.","afbraakwerken - schoring"]
["03.03.","afbraakwerken - in bewoonde gebouwen"]
["03.10.","afbraak volledige constructie - algemeen"]
["03.11.","afbraak volledige constructie - vrijstaand"]
["03.11.10.","afbraak volledige constructie - vrijstaand/asbestverwijdering"]
["03.11.11.","afbraak volledige constructie – vrijstaand/asbestverwijdering - dakbedekking","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["03.11.12.","afbraak volledige constructie – vrijstaand/asbestverwijdering - onderdak","FH","m2","TYPE 3","Roof",null,"Top Surface",null,2]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["03.11.13.","afbraak volledige constructie – vrijstaand/asbestverwijdering - asbestcementbuizen","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["03.11.14.","afbraak volledige constructie – vrijstaand/asbestverwijdering - vloerafwerking","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.11.15.","afbraak volledige constructie – vrijstaand/asbestverwijdering - plaatmateriaal","FH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["03.11.16.","afbraak volledige constructie – vrijstaand/asbestverwijdering - buisisolatie","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.11.17.","afbraak volledige constructie – vrijstaand/asbestverwijdering - asbestkoord","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.11.18.","afbraak volledige constructie – vrijstaand/asbestverwijdering - raam- en deurkitten","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.11.20.","afbraak volledige constructie - vrijstaand/slopen gebouw","FH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.11.30.","afbraak volledige constructie - vrijstaand/ondergrondse massieven","VH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["03.11.40.","afbraak volledige constructie - vrijstaand/te behouden gevels","PM",null,"Geen",{"$nulls":4},1]
["03.12.","afbraak volledige constructie - grenzend aan andere gebouwen"]
["03.12.10.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering"]
["03.12.11.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - dakbedekking","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.12.12.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - onderdak","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.12.13.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - asbestcementbuizen","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["03.12.14.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - vloerafwerking","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.12.15.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - plaatmateriaal","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["03.12.16.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - buisisolatie","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.12.17.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - asbestkoord","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.12.18.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - raam- en deurkitten","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.12.20.","afbraak volledige constructie – grenzend aan andere gebouwen/slopen gebouw","FH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.12.30.","afbraak volledige constructie – grenzend aan andere gebouwen/ondergrondse massieven","VH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["03.12.40.","afbraak volledige constructie – grenzend aan andere gebouwen/te behouden gevels","PM",null,"Geen",{"$nulls":4},1]
["03.20.","afbraak ruwbouwelementen - algemeen"]
["03.21.","afbraak ruwbouwelementen - muren"]
["03.21.10.","afbraak ruwbouwelementen – muren/metselwerk","FH of VH","m3","TYPE 3","Wall",null,"Net Volume",null,1]
["03.21.20.","afbraak ruwbouwelementen – muren/beton","FH of VH","m3","TYPE 3","Wall",null,"Net Volume",null,1]
["03.21.30.","afbraak ruwbouwelementen – muren/houtskelet","FH of VH","m3","TYPE 3","Wall",null,"Net Volume",null,1]
["03.22.","afbraak ruwbouwelementen - vloeren"]
["03.22.10.","afbraak ruwbouwelementen – vloeren/potten en balken","FH of VH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.22.20.","afbraak ruwbouwelementen – vloeren/beton"]
["03.22.21.","afbraak ruwbouwelementen – vloeren/beton - verdiepingsvloer","FH of VH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.22.22.","afbraak ruwbouwelementen – vloeren/beton - vloer op volle grond","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.22.30.","afbraak ruwbouwelementen – vloeren/houten roostering","FH of VH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.30.","afbraak dakelementen - algemeen"]
["03.31.","afbraak dakelementen - hellend dak"]
["03.31.10.","afbraak dakelementen – hellend dak/asbestverwijdering"]
["03.31.11.","afbraak dakelementen – hellend dak/asbestverwijdering - dakbedekking","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["03.31.12.","afbraak dakelementen – hellend dak/asbestverwijdering - onderdak","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["03.31.13.","afbraak dakelementen – hellend dak/asbestverwijdering - asbestcement","FH","st","TYPE 3","Roof",null,"Stuks",null,1]
[{"$nulls":5},"Shell",null,"Stuks",null,1]
["03.31.20.","afbraak dakelementen – hellend dak/volledige dakopbouw","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.31.30.","afbraak dakelementen – hellend dak/dakbedekking","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["03.31.40.","afbraak dakelementen – hellend dak/dakisolatie","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.31.50.","afbraak dakelementen – hellend dak/daklichtelementen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.31.60.","afbraak dakelementen – hellend dak/dakdoorvoeren en schouwen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.32.","afbraak dakelementen - plat dak"]
["03.32.10.","afbraak dakelementen – plat dak/asbestverwijdering"]
["03.32.11.","afbraak dakelementen – plat dak/asbestverwijdering - asbestcement","FH","st","TYPE 3","Roof",null,"Stuks",null,1]
[{"$nulls":5},"Slab",null,"Stuks",null,1]
["03.32.20.","afbraak dakelementen – plat dak/volledige dakopbouw","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.32.30.","afbraak dakelementen – plat dak/dakdichting","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.32.40.","afbraak dakelementen – plat dak/dakisolatie","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.32.50.","afbraak dakelementen – plat dak/daklichtelementen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.32.60.","afbraak dakelementen – plat dak/dakdoorvoeren","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["03.40.","afbraak gevelelementen - algemeen"]
["03.41.","afbraak gevelelementen - gevelmetselwerk ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["03.42.","afbraak gevelelementen - leien"]
["03.42.10.","afbraak gevelelementen – leien/asbesthoudend","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["03.42.20.","afbraak gevelelementen – leien/niet-asbesthoudend","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["03.43.","afbraak gevelelementen - beplating ","FH","m2","TYPE 3","Wall",null,"Projected Area on the side opposite to the reference line",null,1]
["03.44.","afbraak gevelelementen - buitenschrijnwerk"]
["03.44.10.","afbraak gevelelementen – buitenschrijnwerk/asbestverwijdering"]
["03.44.11.","afbraak gevelelementen – buitenschrijnwerk/asbestverwijdering - kitten","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.44.20.","afbraak gevelelementen – buitenschrijnwerk/ramen, deuren en poorten","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
[{"$nulls":5},"Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.45.","afbraak gevelelementen - buitentrappen ","FH","m2","TYPE 5","Stair ","Tread total area","Net Area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.46.","afbraak gevelelementen - balustraden ","FH","st","TYPE 5","Railing",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.50.","afbraak binnenafwerking - algemeen"]
["03.51.","afbraak binnenafwerking - volledige ontmanteling ","SOG",null,"Geen",{"$nulls":4},1]
["03.52.","afbraak binnenafwerking - afkappen pleisterwerk ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["03.53.","afbraak binnenafwerking - plaatafwerking"]
["03.53.10.","afbraak binnenafwerking – plaatafwerking/asbestverwijdering","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["03.53.20.","afbraak binnenafwerking – plaatafwerking/lichte scheidingswanden","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.53.30.","afbraak binnenafwerking – plaatafwerking/plafondafwerking","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.53.40.","afbraak binnenafwerking – plaatafwerking/uitbekleding wanden","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.54.","afbraak binnenafwerking - dekvloer",{"$nulls":5},"Property: Oppervlakte middenas wand"]
["03.54.10.","afbraak binnenafwerking – dekvloer/asbestverwijdering","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.54.20.","afbraak binnenafwerking – dekvloer/tot op draagstructuur","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.55.","afbraak binnenafwerking - vloerafwerking"]
["03.55.10.","afbraak binnenafwerking – vloerafwerking/asbestverwijdering","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.55.20.","afbraak binnenafwerking – vloerafwerking/linoleum","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.55.30.","afbraak binnenafwerking – vloerafwerking/tegels"]
["03.55.31.","afbraak binnenafwerking – vloerafwerking/tegels - op dekvloer","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.55.32.","afbraak binnenafwerking – vloerafwerking/tegels - op zandbed","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.55.40.","afbraak binnenafwerking – vloerafwerking/houten vloer","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.56.","afbraak binnenafwerking - binnendeuren ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.57.","afbraak binnenafwerking - trappen en leuningen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Railing",null,"Stuks",null,1]
[{"$nulls":5},"Stair",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.58.","afbraak binnenafwerking - vast meubilair"]
["03.58.10.","afbraak binnenafwerking – vast meubilair/keukenmeubilair","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.58.20.","afbraak binnenafwerking – vast meubilair/badkamermeubilair","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.60.","afbraak technieken fluïda - algemeen"]
["03.61.","afbraak technieken fluïda - leidingen"]
["03.61.10.","afbraak technieken fluïda – leidingen/asbestverwijdering"]
["03.61.11.","afbraak technieken fluïda – leidingen/asbestverwijdering - asbestcement","FH of VH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["03.61.12.","afbraak technieken fluïda – leidingen/asbestverwijdering - leidingisolatie","FH of VH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["03.61.20.","afbraak technieken fluïda – leidingen/toevoer en afvoerleidingen","PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.62.","afbraak technieken fluïda - sanitaire toestellen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.63.","afbraak technieken fluïda - radiatoren & toebehoren","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.64.","afbraak technieken fluïda - gasleidingen & toebehoren","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.65.","afbraak technieken fluïda - CV-ketel & toebehoren","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.70.","afbraak technieken elektro - algemeen"]
["03.71.","afbraak technieken elektro - leidingnet ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["04.","GEBOUWPRESTATIES"]
["04.00.","gebouwprestaties - algemeen"]
["04.10.","energieprestatie en binnenklimaat (EPB) - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["04.20.","luchtdichtheid - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["04.30.","akoestiek - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["04.40.","brandveiligheid - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["05.","PROEVEN"]
["05.00.","proeven - algemeen"]
["05.10.","proeven - luchtdichtheidsmeting"]
["05.11.","proeven - luchtdichtheidsmeting / wooneenheid ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks",null,1]
["05.12.","proeven - luchtdichtheidsmeting / gebouw ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks",null,1]
["05.20.","proeven - akoestiek"]
["05.21.","proeven - akoestiek / luchtgeluidiolatie ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks",null,1]
["05.22.","proeven - akoestiek / contactgeluidiolatie ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks",null,1]
["05.23.","proeven - akoestiek / geluidisolatie van de gevel ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks",null,1]
["05.24.","proeven - akoestiek / geluid van technische installaties ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks",null,1]
["10.","GRONDWERKEN"]
["10.00.","grondwerken - algemeen"]
["10.10.","voorafgaande afgraving van het terrein - algemeen"]
["10.11.","voorafgaande afgraving terrein - ontzoden ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Projected Area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["10.12.","voorafgaande afgraving terrein - afgraven teelaarde ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Projected Area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["10.13.","voorafgaande afgraving terrein - machinale nivellering ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Projected Area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["10.20.","uitgraving bouwputten - algemeen"]
["10.21.","uitgraving bouwputten - gewone bouwputten ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
["10.22.","uitgraving bouwputten - prefabkelders ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["10.23.","uitgraving bouwputten - rioleringselementen ","PM",null,"Geen",{"$nulls":4},1]
["10.30.","uitgraving sleuven - algemeen"]
["10.31.","uitgraving sleuven - funderingssleuven ","FH/VH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
["10.32.","uitgraving sleuven - funderingsbalken ","FH/VH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
["10.33.","uitgraving sleuven - ondergrondse leidingen ","FH/VH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["10.40.","grondverzet - algemeen"]
["10.41.","grondverzet - projectopvolging ","SOG",null,"Geen",{"$nulls":4},1]
["10.42.","grondverzet - hergebruik uitgegraven grond op werf ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["10.43.","grondverzet - afvoer uitgegraven bodem"]
["10.43.10.","grondverzet - afvoer uitgegraven bodem/naar bestemming voor gebruik"]
["10.43.11.","grondverzet - afvoer uitgegraven bodem/naar bestemming voor gebruik - kwaliteit vrij gebruik ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["10.43.12.","grondverzet - afvoer uitgegraven bodem/naar bestemming voor gebruik - kwaliteit bouwkundig bodemgebruik ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["10.43.20.","grondverzet - afvoer uitgegraven bodem/naar tussentijdse opslagplaats (TOP) ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["10.43.30.","grondverzet - afvoer uitgegraven bodem/naar grondreinigingscentrum (GRC) ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["10.43.40.","grondverzet - afvoer uitgegraven bodem/naar erkende stortplaats"]
["10.43.41.","grondverzet - afvoer uitgegraven bodem/naar erkende stortplaats - klasse I ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["10.43.42.","grondverzet - afvoer uitgegraven bodem/naar erkende stortplaats - klasse II ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["10.43.43.","grondverzet - afvoer uitgegraven bodem/naar erkende stortplaats - klasse III ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["10.44.","grondverzet - fysische scheiding"]
["10.44.10.","grondverzet - fysische scheiding/uitzeving ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["10.44.20.","grondverzet - fysische scheiding/afvoer steenachtige materialen ","VH","ton","TYPE 3","Slab","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":4},"TYPE 5","Mesh","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":5},"Morph","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":5},"Object","Meetstaat Manager 22 KM","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":6},"ARCHICAD property koppelen aan object KM","ARCHICAD Property: Grondverzet",null,1]
["10.44.30.","grondverzet - fysische scheiding/afvoer bodemvreemde materialen ","VH","ton","TYPE 3","Slab","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":4},"TYPE 5","Mesh","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":5},"Morph","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":5},"Object","Meetstaat Manager 22 KM of ARCHICAD property koppelen aan object KM","ARCHICAD Property: Grondverzet",null,1]
["10.50.","verwijdering massieven - algemeen ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["10.60.","bronbemaling - algemeen ","SOG",null,"Geen",{"$nulls":4},1]
["10.70.","aanvullingen - algemeen"]
["10.71.","aanvullingen - wederaanvullingen"]
["10.71.10.","aanvullingen - wederaanvullingen/grond van uitgravingen ","PM",null,"Geen",{"$nulls":4},1]
["10.71.20.","aanvullingen - wederaanvullingen/aangevoerde grond ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["10.71.30.","aanvullingen - wederaanvullingen/gestabiliseerd zand ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["10.71.40.","aanvullingen - wederaanvullingen/kunststeenslag ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["10.71.50.","aanvullingen - wederaanvullingen/natuursteenslag ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["10.72.","aanvullingen - ophoging terrein"]
["10.72.10.","aanvullingen - ophoging terrein/grond van afgravingen ","PM",null,"Geen",{"$nulls":4},1]
["10.72.20","aanvullingen - ophoging terrein/aangevoerde grond ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["10.72.30.","aanvullingen - ophoging terrein/gestabiliseerd zand ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["10.80.","grondbehandeling - algemeen"]
["10.81.","grondbehandeling - kalk ","VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["10.82.","grondbehandeling - cement ","VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["11.","STUT- & ONDERVANGINGSWERKEN"]
["11.00.","stut- & ondervangingswerken - algemeen"]
["11.10.","beschoeiing bouwputten - algemeen"]
["11.11.","beschoeiing bouwputten - damplanken"]
["11.11.10.","beschoeiing bouwputten - damplanken/aanvoer & installatie machine ","SOG",null,"Geen",{"$nulls":4},1]
["11.11.20.","beschoeiing bouwputten - damplanken/materialen & verwerking ","FH/VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (m2) in bij de Object Settings",null,1]
["11.12.","beschoeiing bouwputten - berlinerwand"]
["11.12.10.","beschoeiing bouwputten - berlinerwand/ aanvoer & installatie machine ","SOG",null,"Geen",{"$nulls":4},1]
["11.12.20.","beschoeiing bouwputten - berlinerwand/materialen & verwerking ","FH/VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (m2) in bij de Object Settings",null,1]
["11.13.","beschoeiing bouwputten - secanspalenwand"]
["11.13.10.","beschoeiing bouwputten - secanspalenwand/installatie palenmachine ","SOG",null,"Geen",{"$nulls":4},1]
["11.13.20.","beschoeiing bouwputten - secanspalenwand/realisatie palenwand ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["11.13.30.","beschoeiing bouwputten - secanspalenwand/verbindingsbalk ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["11.13.50.","beschoeiing bouwputten - secanspalenwand/horizontale verankering ","FH/VH","st","TYPE 5","Object",null,"Stuks",null,1]
["11.13.60.","beschoeiing bouwputten - secanspalenwand/sonische integriteitstesten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["11.13.70.","beschoeiing bouwputten - secanspalenwand/afwerking als kelderwand ","FH","m3","TYPE 3","Wall",null,"Net Volume",null,1]
["11.20.","onderschoeiingen - algemeen"]
["11.21.","onderschoeiingen - stortklaar beton ","VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["11.22.","onderschoeiingen - metselwerk ","VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["11.23.","onderschoeiingen - groutkolommen",null,null,"TYPE 3",null,null,"Net Volume",null,1]
["11.23.10.","onderschoeiingen - groutkolommen/aanvoer en installatie van de machine ","SOG",null,"Geen",{"$nulls":4},1]
["11.23.20.","onderschoeiingen - groutkolommen/materialen en verwerking ","VH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["11.30.","keermuren - algemeen"]
["11.31.","keermuren - stortklaar beton ","VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":5},"Wall",null,"Projected Area",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["12.","FUNDERINGEN OP STAAL"]
["12.00.","funderingen op staal - algemeen"]
["12.10.","funderingszolen en -stroken - algemeen"]
["12.11.","funderingszolen en -stroken - ongewapend beton ","VH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["12.12.","funderingszolen en -stroken - gewapend beton ","VH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["12.20.","ondergronds metselwerk - algemeen"]
["12.21.","ondergronds metselwerk - betonblokken"]
["12.21.10.","ondergronds metselwerk - betonblokken/muurdikte 35 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["12.21.20.","ondergronds metselwerk - betonblokken/muurdikte 40 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["12.21.30.","ondergronds metselwerk - betonblokken/muurdikte 45 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["12.22.","ondergronds metselwerk - snelbouw"]
["12.22.10.","ondergronds metselwerk - snelbouw/muurdikte 35 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["12.22.20.","ondergronds metselwerk - snelbouw/muurdikte 40 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["12.22.30.","ondergronds metselwerk - snelbouw/muurdikte 45 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["12.30.","doorbrekingen ondergronds metselwerk - algemeen"]
["12.31.","doorbrekingen ondergronds metselwerk - aansluitbocht ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["12.40.","aardingslus - algemeen","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["13.","SPECIALE FUNDERINGEN"]
["13.00.","speciale funderingen - algemeen"]
["13.01.","algemeen - diepsonderingsverslag"]
["13.10.","paalfundering - algemeen"]
["13.11.","paalfundering - schroefpalen"]
["13.11.10.","paalfundering - schroefpalen/enkele grondverdringing"]
["13.11.11.","paalfundering - schroefpalen/enkele grondverdringing - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.11.12.","paalfundering - schroefpalen/enkele grondverdringing - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.11.20.","paalfundering - schroefpalen/dubbele grondverdringing"]
["13.11.21.","paalfundering - schroefpalen/dubbele grondverdringing - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.11.22.","paalfundering - schroefpalen/dubbele grondverdringing - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.12.","paalfundering - boorpalen"]
["13.12.10.","paalfundering - boorpalen/verbuisd"]
["13.12.11.","paalfundering - boorpalen/verbuisd - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.12.12.","paalfundering - boorpalen/verbuisd - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.12.20.","paalfundering - boorpalen/steunvloeistof"]
["13.12.21.","paalfundering - boorpalen/steunvloeistof - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.12.22.","paalfundering - boorpalen/steunvloeistof - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.13.","paalfundering - kokerpalen"]
["13.13.10.","paalfundering - kokerpalen/geschroefd"]
["13.13.11.","paalfundering - kokerpalen/geschroefd - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.13.12.","paalfundering - kokerpalen/geschroefd - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.13.20.","paalfundering - kokerpalen geheid"]
["13.13.21.","paalfundering - kokerpalen geheid - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.13.22.","paalfundering - kokerpalen/geheid - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.14.","paalfundering - heipalen"]
["13.14.10.","paalfundering - heipalen/in de grond gevormd"]
["13.14.11.","paalfundering - heipalen/in de grond gevormd - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.14.12.","paalfundering - heipalen/in de grond gevormd - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.14.20.","paalfundering - heipalen/prefab beton"]
["13.14.21.","paalfundering - heipalen/prefab beton - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.14.22.","paalfundering - heipalen/prefab beton - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.20.","fundering op valse putten - algemeen"]
["13.21.","fundering op valse putten - ongewapend stortklaar beton ","FH/VH","m","TYPE 3","Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
[null,null,null,"m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["13.22.","fundering op valse putten - gewapend stortklaar beton ","FH/VH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Column",null,"Net Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,null,"m3","TYPE 3","Column",null,"Net Volume",null,1]
[{"$nulls":5},"Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["13.23.","fundering op valse putten - gestabiliseerd zand ","FH/VH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Column",null,"Net Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,null,"m3","TYPE 3","Column",null,"Net Volume",null,1]
[{"$nulls":5},"Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["13.24.","fundering op valse putten - steenslag ","FH/VH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Column",null,"Net Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,null,"m3","TYPE 3","Column",null,"Net Volume",null,1]
[{"$nulls":5},"Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["13.30.","funderingsbalken - algemeen"]
["13.31.","funderingsbalken - stortklaar beton ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["13.40.","plaat op putten - algemeen"]
["13.41.","plaat op putten - gewapend stortklaar beton ","FH","m3","TYPE 3","Beam ",null,"Net Volume",null,1]
[{"$nulls":5},"Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["13.42.","plaat op putten - gewapend & gepolierd stortklaar beton ","FH","m3","TYPE 3","Beam ",null,"Net Volume",null,1]
[{"$nulls":5},"Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["13.50.","plaatfunderingen - algemeen"]
["13.51.","plaatfunderingen - gewapend stortklaar beton ","FH","m3","TYPE 3","Beam ",null,"Net Volume",null,1]
[{"$nulls":5},"Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["13.52.","plaatfunderingen - gewapend en gepolierd stortklaar beton ","FH","m3","TYPE 3","Beam ",null,"Net Volume",null,1]
[{"$nulls":5},"Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["13.60.","liftputten - algemeen"]
["13.61.","liftputten - stortklaar beton ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["13.70.","doorbrekingen speciale funderingen - algemeen"]
["13.71.","doorbrekingen speciale funderingen - aansluitbocht ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["13.72.","doorbrekingen speciale funderingen - doorvoermoffen voor buizen en kabels ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["14.","ONDERGRONDSE WANDEN"]
["14.00.","ondergrondse wanden - algemeen"]
["14.10.","funderingswanden - algemeen"]
["14.11.","funderingswanden - beton"]
["14.11.10.","funderingswanden - beton/ter plaatse gestort"]
["14.11.11.","funderingswanden - beton/ter plaatse gestort - dikte 20 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["14.11.12.","funderingswanden - beton/ter plaatse gestort - dikte 25 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["14.11.13.","funderingswanden - beton/ter plaatse gestort - dikte 30 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["14.11.14.","funderingswanden - beton/ter plaatse gestort - dikte 35 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["14.11.20.","funderingswanden - beton/holle wanden"]
["14.11.21.","funderingswanden - beton/holle wanden - prefabelementen ","FH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":5},"Wall",null,"Projected Area",null,1]
["14.11.22.","funderingswanden - beton/holle wanden - vulbeton ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["14.11.30.","funderingswanden - beton/injectie van onvermijdelijke scheuren ","VH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["14.12.","funderingswanden - metselwerk"]
["14.12.01.","funderingswanden - metselwerk/mortel ","PM",null,"Geen",{"$nulls":4},1]
["14.12.02.","funderingswanden - metselwerk/wapening ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["14.12.10.","funderingswanden - metselwerk/betonblokken"]
["14.12.11.","funderingswanden - metselwerk/betonblokken - muurdikte 29 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["14.12.12.","funderingswanden - metselwerk/betonblokken - muurdikte 35 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["14.12.13.","funderingswanden - metselwerk/betonblokken - muurdikte 39 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["14.12.14.","funderingswanden - metselwerk/betonblokken - muurdikte 40 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["14.20.","dragende kelderwanden - algemeen"]
["14.21.","dragende kelderwanden - beton"]
["14.21.10.","dragende kelderwanden - beton/ter plaatse gestort"]
["14.21.11.","dragende kelderwanden - beton/ter plaatse gestort - dikte 20 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["14.21.12.","dragende kelderwanden - beton/ter plaatse gestort - dikte 25 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["14.21.13.","dragende kelderwanden - beton/ter plaatse gestort - dikte 30 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["14.21.20.","dragende kelderwanden - beton/holle wanden"]
["14.21.21.","dragende kelderwanden - beton/holle wanden - prefabelementen ","FH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":5},"Wall",null,"Projected Area",null,1]
["14.21.22.","dragende kelderwanden - beton/holle wanden - vulbeton ","FH","m3","TYPE 3","Wall",null,"Net Volume",null,1]
["14.21.30.","dragende kelderwanden - beton/injectie van onvermijdelijke scheuren ","VH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["14.22.","dragende kelderwanden - metselwerk"]
["14.22.01.","dragende kelderwanden - metselwerk/mortel ","PM",null,"Geen",{"$nulls":4},1]
["14.22.02.","dragende kelderwanden - metselwerk/wapening ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["14.22.03.","dragende kelderwanden - metselwerk/lateien ","PM",null,"Geen",{"$nulls":4},1]
["14.22.10.","dragende kelderwanden - metselwerk/betonblokken"]
["14.22.11.","dragende kelderwanden - metselwerk/betonblokken - muurdikte 14 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.12.","dragende kelderwanden - metselwerk/betonblokken - muurdikte 19 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.13.","dragende kelderwanden - metselwerk/betonblokken - muurdikte 29 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.20.","dragende kelderwanden - metselwerk/baksteen"]
["14.22.21.","dragende kelderwanden - metselwerk/baksteen - muurdikte 14 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.22.","dragende kelderwanden - metselwerk/baksteen - muurdikte 19 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.30.","dragende kelderwanden - metselwerk/kalkzandsteen"]
["14.22.31.","dragende kelderwanden - metselwerk/kalkzandsteen - muurdikte 15 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.32.","dragende kelderwanden - metselwerk/kalkzandsteen - muurdikte 17,5 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.33.","dragende kelderwanden - metselwerk/kalkzandsteen - muurdikte 21,5 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.30.","geprefabriceerde kelders - algemeen"]
["14.31.","geprefabriceerde kelders - gedeeltelijke onderkeldering ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Slab",null,"Stuks",null,1]
["14.40.","waterdichting ondergrondse wanden - algemeen"]
["14.41.","waterdichting ondergrondse wanden - mineraliserende mortel ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["14.42.","waterdichting ondergrondse wanden - gemodificeerde cementmortel ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["14.43.","waterdichting ondergrondse wanden - bitumenemulsie ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["14.44.","waterdichting ondergrondse wanden - noppenbanen ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["14.50.","doorbrekingen ondergrondse wanden - algemeen"]
["14.51.","doorbrekingen ondergrondse wanden - aansluitbocht ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["14.52.","doorbrekingen ondergrondse wanden - doorvoermoffen buizen en kabels ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["14.60.","verluchtingselementen ondergrondse wanden - algemeen"]
["14.61.","verluchtingselementen ondergrondse wanden - telescopische kokers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["15.","VLOERLAGEN ONDERBOUW"]
["15.00.","vloerlagen onderbouw - algemeen"]
["15.10.","zuiverheidslagen - algemeen"]
["15.11.","zuiverheidslagen - stortklaar beton ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["15.20.","draagvloeren op volle grond - algemeen"]
["15.21.","draagvloeren op volle grond - stortklaar gewapend beton ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["15.30.","vochtwerende lagen - algemeen"]
["15.31.","vochtwerende lagen - folies"]
["15.31.10.","vochtwerende lagen - folies/PE ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["15.31.20.","vochtwerende lagen - folies/PVC ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["15.31.30.","vochtwerende lagen - folies/PIB ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["15.32.","vochtwerende lagen - banen"]
["15.32.10.","vochtwerende lagen - banen/HDPE ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["15.33.","vochtwerende lagen - bitumenglasvlies ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["16.","THERMISCHE ISOLATIE ONDERBOUW"]
["16.00.","thermische isolatie onderbouw - algemeen"]
["16.10.","isolatieplaten op volle grond - algemeen"]
["16.11.","isolatieplaten op volle grond - XPS"]
["16.11.10.","isolatieplaten op volle grond - XPS/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["16.11.20.","isolatieplaten op volle grond - XPS/12 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["16.12.","isolatieplaten op volle grond - PUR of PIR"]
["16.12.10.","isolatieplaten op volle grond - PUR of PIR/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["16.12.20.","isolatieplaten op volle grond - PUR of PIR/12 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["16.13.","isolatieplaten op volle grond - EPS"]
["16.13.10.","isolatieplaten op volle grond - EPS/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["16.13.20.","isolatieplaten op volle grond - EPS/12 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["16.20.","perimeterisolatie - algemeen"]
["16.21.","perimeterisolatie - XPS"]
["16.21.10.","perimeterisolatie - XPS/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 2","Beam",null,"Oppervlakte middenas wand",null,1]
["16.21.20.","perimeterisolatie - XPS/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 2","Beam",null,"Oppervlakte middenas wand",null,1]
["16.22.","perimeterisolatie - PUR of PIR"]
["16.22.10.","perimeterisolatie - PUR of PIR/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 2","Beam",null,"Oppervlakte middenas wand",null,1]
["16.22.20.","perimeterisolatie - PUR of PIR/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 2","Beam",null,"Oppervlakte middenas wand",null,1]
["17.","ONDERGRONDSE LEIDINGEN"]
["17.00.","ondergrondse leidingen - algemeen"]
["17.10.","rioolbuizen - algemeen"]
["17.11.","rioolbuizen - beton"]
["17.11.10.","rioolbuizen - beton ongewapend"]
["17.11.11.","rioolbuizen - beton/ongewapend - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.12.","rioolbuizen - beton/ongewapend - diam 250 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.13.","rioolbuizen - beton/ongewapend - diam 300 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.14.","rioolbuizen - beton/ongewapend - diam 400 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.15.","rioolbuizen - beton/ongewapend - diam 500 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.16.","rioolbuizen - beton/ongewapend - diam 600 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.20.","rioolbuizen - beton gewapend"]
["17.11.21.","rioolbuizen - beton/gewapend - diam 300 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,null,"m","TYPE 5","Object","MEP",null,null,1]
["17.11.22.","rioolbuizen - beton/gewapend - diam 400 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,null,"m","TYPE 5","Object","MEP",null,null,1]
["17.11.23.","rioolbuizen - beton/gewapend - diam 500 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.24.","rioolbuizen - beton/gewapend - diam 600 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.25.","rioolbuizen - beton/gewapend - diam 800 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.","rioolbuizen - kunststof"]
["17.12.10.","rioolbuizen - kunststof/PVC"]
["17.12.11.","rioolbuizen - kunststof/PVC - diam 110 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.12.","rioolbuizen - kunststof/PVC - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.13.","rioolbuizen - kunststof/PVC - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.14.","rioolbuizen - kunststof/PVC - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.15.","rioolbuizen - kunststof/PVC - diam 315 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.16.","rioolbuizen - kunststof/PVC - diam 400 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.20.","rioolbuizen - kunststof/PE"]
["17.12.21.","rioolbuizen - kunststof/PE - diam 110 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.22.","rioolbuizen - kunststof/PE - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.23.","rioolbuizen - kunststof/PE - diam 140 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.24.","rioolbuizen - kunststof/PE - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.25.","rioolbuizen - kunststof/PE - diam 180 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.26.","rioolbuizen - kunststof/PE - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.27.","rioolbuizen - kunststof/PE - diam 225 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.28.","rioolbuizen - kunststof/PE - diam 250 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.30.","rioolbuizen - kunststof/PP"]
["17.12.31.","rioolbuizen - kunststof/PP - diam 110 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.32.","rioolbuizen - kunststof/PP - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.33.","rioolbuizen - kunststof/PP - diam 140 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.34.","rioolbuizen - kunststof/PP - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.35.","rioolbuizen - kunststof/PP - diam 180 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.36.","rioolbuizen - kunststof/PP - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.37.","rioolbuizen - kunststof/PP - diam 225 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.38.","rioolbuizen - kunststof/PP - diam 250 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.20.","draineerbuizen - algemeen"]
["17.21.","draineerbuizen - poreus beton"]
["17.21.10.","draineerbuizen - poreus beton/diam 80 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.21.20.","draineerbuizen - poreus beton/diam 100 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.21.30.","draineerbuizen - poreus beton/diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.21.40.","draineerbuizen - poreus beton/diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.21.50.","draineerbuizen - poreus beton/diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.22.","draineerbuizen - vezelcement"]
["17.22.10.","draineerbuizen - poreus beton/diam 80 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.22.20.","draineerbuizen - poreus beton/diam 100 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.22.30.","draineerbuizen - poreus beton/diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.22.40.","draineerbuizen - poreus beton/diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.22.50.","draineerbuizen - poreus beton/diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.","draineerbuizen - kunststof"]
["17.23.10.","draineerbuizen - kunststof/PVC"]
["17.23.11.","draineerbuizen - kunststof/PVC - diam 50 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.12.","draineerbuizen - kunststof/PVC - diam 65 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.13.","draineerbuizen - kunststof/PVC - diam 80 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.14.","draineerbuizen - kunststof/PVC - diam 100 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.15.","draineerbuizen - kunststof/PVC - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.16.","draineerbuizen - kunststof/PVC - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.17.","draineerbuizen - kunststof/PVC - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.20.","draineerbuizen - kunststof/PE"]
["17.23.21.","draineerbuizen - kunststof/PE - diam 50 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.22.","draineerbuizen - kunststof/PE - diam 60 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.23.","draineerbuizen - kunststof/PE - diam 80 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.24.","draineerbuizen - kunststof/PE - diam 100 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.25.","draineerbuizen - kunststof/PE - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.26.","draineerbuizen - kunststof/PE - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.27.","draineerbuizen - kunststof/PE - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.30.","toezichtputten - algemeen"]
["17.31.","toezichtputten - metselwerk ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.32.","toezichtsputten - beton"]
["17.32.10.","toezichtsputten - beton/stortklaar ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.32.20.","toezichtsputten - beton/prefab ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.33.","toezichtputten - vezelcement ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.34.","toezichtsputten - kunststof"]
["17.34.10.","toezichtputten - kunststof/PVC ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.34.20.","toezichtputten - kunststof/PE ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.34.30.","toezichtputten - kunststof/polyester ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.40.","ontvangtoestellen - algemeen"]
["17.41.","ontvangtoestellen - buitenontvanger"]
["17.41.10.","ontvangtoestellen - buitenontvanger/met klok ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.41.20.","ontvangtoestellen - buitenontvanger/met korf ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.42.","ontvangtoestellen - geulen"]
["17.42.10.","ontvangtoestellen - geulen/beton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.42.20.","ontvangtoestellen - geulen/glasvezelbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.42.30.","ontvangtoestellen - geulen/polyesterbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.43.","ontvangtoestellen - straatkolken ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.44.","ontvangtoestellen - prefab pompputten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.50.","putdeksels en roosters - algemeen"]
["17.51.","putdeksels en roosters - enkel deksel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.52.","putdeksels en roosters - dubbel deksel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.53.","putdeksels en roosters - geulroosters ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["17.60.","afvalwaterbehandeling - algemeen"]
["17.61.","afvalwaterbehandeling - septische putten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.70.","regenwaterbehandeling - algemeen"]
["17.71.","regenwaterbehandeling - regenwaterputten"]
["17.71.10.","regenwaterbehandeling - regenwaterputten/beton ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.71.20.","regenwaterbehandeling - regenwaterputten/HDPE ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.71.30.","regenwaterbehandeling - regenwaterputten/polyester ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.71.40.","regenwaterbehandeling - regenwaterputten/metselwerk ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.72.","regenwaterbehandeling - hergebruik regenwater ","PM",null,"Geen",{"$nulls":4},1]
["17.73.","regenwaterbehandeling - voorfilters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.74.","regenwaterbehandeling - overloop en terugslagklep ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.75.","regenwaterbehandeling - infiltratievoorzieningen"]
["17.75.10.","regenwaterbehandeling - infiltratievoorzieningen/infiltratieputten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.75.20.","regenwaterbehandeling - infiltratievoorzieningen/infiltratieblokken ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.75.30.","regenwaterbehandeling - infiltratievoorzieningen/infiltratiebuizen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.80.","aansluitingen - algemeen"]
["17.81.","aansluitingen - openbare riolering ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.82.","aansluitingen - doorvoer- en wachtbuizen ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["17.83.","aansluitingen - wachtput ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["20.","METSELWERK"]
["20.00.","metselwerken - algemeen"]
["20.01.","metselwerken - ter plaatse gemetst"]
["20.02.","metselwerken - prefab"]
["20.10.","materialen - algemeen"]
["20.11.","materialen - metselmortel"]
["20.11.10.","materialen - metselmortel/voor algemene toepassing (G) ","PM",null,"Geen",{"$nulls":4},1]
["20.11.20.","materialen - metselmortel/lijmmortel (T) ","PM",null,"Geen",{"$nulls":4},1]
["20.11.30.","materialen - metselmortel/lichtgewicht metselmortel (L) ","PM",null,"Geen",{"$nulls":4},1]
["20.12.","materialen - hulpstukken"]
["20.12.10.","materialen - hulpstukken/spouwankers"]
["20.12.11.","materialen - hulpstukken/spouwankers - gewone spouwankers ","PM",null,"Geen",{"$nulls":4},1]
["20.12.12.","materialen - hulpstukken/spouwankers - slag- en schroefankers met isolatieplug ","PM",null,"Geen",{"$nulls":4},1]
["20.12.13.","materialen - hulpstukken/spouwankers - akoestisch spouwanker ","PM",null,"Geen",{"$nulls":4},1]
["20.12.20.","materialen - hulpstukken/lateien"]
["20.12.21.","materialen - hulpstukken/lateien - beton ","PM",null,"Geen",{"$nulls":4},1]
["20.12.22.","materialen - hulpstukken/lateien - staal ","PM",null,"Geen",{"$nulls":4},1]
["20.12.23.","materialen - hulpstukken/lateien - bekistingsmetselstenen ","PM",null,"Geen",{"$nulls":4},1]
["20.12.30.","materialen - hulpstukken/waterkering ","PM",null,"Geen",{"$nulls":4},1]
["20.12.40.","materialen - hulpstukken/wapening ","FH","m","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Lengte (cm) in bij de Object settings",null,1]
["20.12.50.","materialen - hulpstukken/akoestische stroken ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Lengte (cm) in bij de Object settings",null,1]
["20.13.","materialen - kimblokken"]
["20.13.10.","materialen - kimblokken/cellenbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Lengte volgens eigen middenas",null,1]
["20.13.20.","materialen - kimblokken/samengestelde blok ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Lengte volgens eigen middenas",null,1]
["20.13.30.","materialen - kimblokken/thermisch verbeterde steen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Lengte volgens eigen middenas",null,1]
["20.13.40.","materialen - kimblokken/cellenglas ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Lengte volgens eigen middenas",null,1]
["20.20.","binnenspouwblad - algemeen"]
["20.21.","binnenspouwblad - snelbouw"]
["20.21.10.","binnenspouwblad - snelbouw/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.21.20.","binnenspouwblad - snelbouw/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.22.","binnenspouwblad - kalkzandsteen"]
["20.22.10.","binnenspouwblad - kalkzandsteen/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.22.20.","binnenspouwblad - kalkzandsteen/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.22.30.","binnenspouwblad - kalkzandsteen/dikte 21,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.22.40.","binnenspouwblad - kalkzandsteen/dikte 30 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.23.","binnenspouwblad - betonsteen met gewone granulaten"]
["20.23.10.","binnenspouwblad - betonsteen met gewone granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.23.20.","binnenspouwblad - betonsteen met gewone granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.24.","binnenspouwblad - betonsteen met lichte granulaten"]
["20.24.10.","binnenspouwblad - betonsteen met lichte granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.24.20.","binnenspouwblad - betonsteen met lichte granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.","binnenspouwblad - cellenbeton"]
["20.25.10.","binnenspouwblad - cellenbeton/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.20.","binnenspouwblad - cellenbeton/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.30.","binnenspouwblad - cellenbeton/dikte 20 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.40.","binnenspouwblad - cellenbeton/dikte 24 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.50.","binnenspouwblad - cellenbeton/dikte 30 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.60.","binnenspouwblad - cellenbeton/dikte 36,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.70.","binnenspouwblad - cellenbeton/dikte 40 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.80.","binnenspouwblad - cellenbeton/dikte 50 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.30.","woningscheidende wand - algemeen"]
["20.31.","woningscheidende wand - snelbouw"]
["20.31.10.","woningscheidende wand - snelbouw/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.31.20.","woningscheidende wand - snelbouw/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.32.","woningscheidende wand - kalkzandsteen"]
["20.32.10.","woningscheidende wand - kalkzandsteen/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.32.20.","woningscheidende wand - kalkzandsteen/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.32.30.","woningscheidende wand - kalkzandsteen/dikte 21,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.32.40.","woningscheidende wand - kalkzandsteen/dikte 30 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.33.","woningscheidende wand - betonsteen met gewone granulaten"]
["20.33.10.","woningscheidende wand - betonsteen met gewone granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.33.20.","woningscheidende wand - betonsteen met gewone granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.34.","woningscheidende wand - betonsteen met lichte granulaten"]
["20.34.10.","woningscheidende wand - betonsteen met lichte granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.34.20.","woningscheidende wand - betonsteen met lichte granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.35.","woningscheidende wand - cellenbeton"]
["20.35.10.","woningscheidende wand - cellenbeton/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.35.20.","woningscheidende wand - cellenbeton/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.35.30.","woningscheidende wand - cellenbeton/dikte 20 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.35.40.","woningscheidende wand - cellenbeton/dikte 24 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.40.","dragende binnenmuur - algemeen"]
["20.41.","dragende binnenmuur - snelbouw"]
["20.41.10.","dragende binnenmuur - snelbouw/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.41.20.","dragende binnenmuur - snelbouw/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.42.","dragende binnenmuur - kalkzandsteen"]
["20.42.10.","dragende binnenmuur - kalkzandsteen/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.42.20.","dragende binnenmuur - kalkzandsteen/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.42.30.","dragende binnenmuur - kalkzandsteen/dikte 21,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.43.","dragende binnenmuur - betonsteen met gewone granulaten"]
["20.43.10.","dragende binnenmuur - betonsteen met gewone granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.43.20.","dragende binnenmuur - betonsteen met gewone granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.44.","dragende binnenmuur - betonsteen met lichte granulaten"]
["20.44.10.","dragende binnenmuur - betonsteen met lichte granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.44.20.","dragende binnenmuur - betonsteen met lichte granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.45.","dragende binnenmuur - cellenbeton"]
["20.45.10.","dragende binnenmuur - cellenbeton/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.45.20.","dragende binnenmuur - cellenbeton/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.45.30.","dragende binnenmuur - cellenbeton/dikte 20 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.45.40.","dragende binnenmuur - cellenbeton/dikte 24 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.50.","niet-dragende binnenmuur - algemeen"]
["20.51.","niet-dragende binnenmuur - snelbouw"]
["20.51.10.","niet-dragende binnenmuur - snelbouw/dikte 9 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.51.20.","niet-dragende binnenmuur - snelbouw/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.52.","niet-dragende binnenmuur - kalkzandsteen"]
["20.52.10.","niet-dragende binnenmuur - kalkzandsteen/dikte 10 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.52.20.","niet-dragende binnenmuur - kalkzandsteen/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.53.","niet-dragende binnenmuur - betonsteen met lichte granulaten"]
["20.53.10.","niet-dragende binnenmuur - betonsteen met lichte granulaten/dikte 9 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.53.20.","niet-dragende binnenmuur - betonsteen met lichte granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.54.","niet-dragende binnenmuur - cellenbeton"]
["20.54.10.","niet-dragende binnenmuur - cellenbeton/dikte 7 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.54.20.","niet-dragende binnenmuur - cellenbeton/dikte 10 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.54.30.","niet-dragende binnenmuur - cellenbeton/dikte 11,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.55.","niet-dragende binnenmuur - gipsblokken"]
["20.55.10.","niet-dragende binnenmuur - gipsblokken/dikte 6 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.55.20.","niet-dragende binnenmuur - gipsblokken/dikte 7 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.55.30.","niet-dragende binnenmuur - gipsblokken/dikte 8 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.55.40.","niet-dragende binnenmuur - gipsblokken/dikte 10 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.60.","renovatiewerken - algemeen"]
["20.61.","renovatiewerken - behandeling tegen opstijgend vocht"]
["20.61.10.","renovatiewerken - behandeling tegen opstijgend vocht/injecteren ","FH/VH","m","TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Lengte (cm) in bij de Object settings",null,1]
["20.61.20.","renovatiewerken - behandeling tegen opstijgend vocht/plaatsen dichtingsmembraan ","FH/VH","m","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Lengte (cm) in bij de Object settings",null,1]
[null,null,null,"m","TYPE 3","Wall",null,"Reference line length",null,1]
["21.","SPOUWMUURISOLATIE"]
["21.00.","spouwmuurisolatie - algemeen"]
["21.10.","spouwmuurisolatie buitenspouwblad - algemeen"]
["21.11.","spouwmuurisolatie buitenspouwblad - MW"]
["21.11.10.","spouwmuurisolatie buitenspouwblad - MW / 12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.11.20.","spouwmuurisolatie buitenspouwblad - MW / 14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.12.","spouwmuurisolatie buitenspouwblad - PUR of PIR"]
["21.12.10.","spouwmuurisolatie buitenspouwblad - PUR of PIR/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.12.20.","spouwmuurisolatie buitenspouwblad - PUR of PIR/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.13.","spouwmuurisolatie buitenspouwblad - PF"]
["21.13.10.","spouwmuurisolatie buitenspouwblad - PF/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.13.20.","spouwmuurisolatie buitenspouwblad - PF/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.14.","spouwmuurisolatie buitenspouwblad - XPS"]
["21.14.10.","spouwmuurisolatie buitenspouwblad - XPS/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.14.20.","spouwmuurisolatie buitenspouwblad - XPS/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.15.","spouwmuurisolatie buitenspouwblad - EPS"]
["21.15.10.","spouwmuurisolatie buitenspouwblad - EPS/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.15.20.","spouwmuurisolatie buitenspouwblad - EPS/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.20.","spouwmuurisolatie woningscheidende wand - algemeen"]
["21.21.","spouwmuurisolatie woningscheidende wand - MW"]
["21.21.10.","spouwmuurisolatie woningscheidende wand - MW/4 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.21.20.","spouwmuurisolatie woningscheidende wand - MW/5 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.22.","spouwmuurisolatie woningscheidende wand - XPS"]
["21.22.10.","spouwmuurisolatie woningscheidende wand - XPS/2 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.22.20.","spouwmuurisolatie woningscheidende wand - XPS/3 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.23.","spouwmuurisolatie woningscheidende wand - PUR of PIR"]
["21.23.10.","spouwmuurisolatie woningscheidende wand - PUR of PIR/3 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.23.20.","spouwmuurisolatie woningscheidende wand - PUR of PIR/4 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.30.","spouwmuurisolatie navulling - algemeen"]
["21.31.","spouwmuurisolatie navulling - MW ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["21.32.","spouwmuurisolatie navulling - PUR ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["21.33.","spouwmuurisolatie navulling - EPS ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["22.","GEVELMETSELWERK"]
["22.00.","gevelmetselwerken - algemeen"]
["22.01.","algemeen - ter plaatse gemetst gevelmetselwerk"]
["22.02.","algemeen - prefab gevelmetselwerk"]
["22.10.","materialen - algemeen"]
["22.11.","materialen - mortel"]
["22.11.10.","materialen - mortel/metselmortel"]
["22.11.11.","materialen - mortel/metselmortel - voor algemene toepassing ","PM",null,"Geen",{"$nulls":4},1]
["22.11.12.","materialen - mortel/metselmortel - dunbedmortel ","PM",null,"Geen",{"$nulls":4},1]
["22.11.13.","materialen - mortel/metselmortel - lijmmortel ","PM",null,"Geen",{"$nulls":4},1]
["22.11.20.","materialen - mortel/voegmortel"]
["22.12.","materialen - spouwankers ","PM",null,"Geen",{"$nulls":4},1]
["22.13.","materialen - waterkering ","PM",null,"Geen",{"$nulls":4},1]
["22.14.","materialen - wapening ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["22.20.","gevelstenen - algemeen"]
["22.21.","gevelstenen - baksteen"]
["22.21.10.","gevelstenen - baksteen/strengpersstenen ","FH","m2","TYPE 3","Wall",null,"Conditional surface area on the Inside Face\n\n",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
["22.21.20.","gevelstenen - bakstenen/handvorm- en vormbakstenen ","FH","m2","TYPE 3","Wall",null,"Conditional surface area on the Inside Face\n\n",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
["22.22.","gevelstenen - betonsteen ","FH","m2","TYPE 3","Wall",null,"Conditional surface area on the Inside Face\n\n",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
["22.30.","renovatiewerken - algemeen"]
["22.31.","renovatiewerken - herstelling en aanpassing bestaand gevelmetselwerk ","FH","m2","TYPE 3","Wall",null,"Conditional surface area on the Inside Face\n\n",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
["23.00.","dorpels, plinten en dekstenen - algemeen"]
["23.01.","algemeen - blauwe hardsteen"]
["23.02.","algemeen - beton"]
["23.03.","algemeen - vezelcement"]
["23.10.","raam- en deurdorpels - algemeen"]
["23.11.","raam- en deurdorpels - blauwe hardsteen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[null,null,null,"m2","TYPE 3","Beam",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","breedte dagkant * diepte dorpel",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Area",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","breedte dagkant * diepte dorpel * dikte dorpel",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Stuks",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Stuks",null,1]
["23.12.","raam- en deurdorpels - prefabbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","breedte dagkant * diepte dorpel * dikte dorpel",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Stuks",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Stuks",null,1]
["23.13.","raam- en deurdorpels - vezelcement ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
["23.14.","raam- en deurdorpels - gevelsteen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","breedte dagkant * diepte dorpel * dikte dorpel",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
["23.20.","garagepoortdorpels - algemeen"]
["23.21.","garagepoortdorpels - blauwe hardsteen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[null,null,null,"m2","TYPE 3","Beam",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","breedte dagkant * diepte dorpel",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","breedte dagkant * diepte dorpel * dikte dorpel",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","Stuks",null,1]
["23.22.","garagepoortdorpels - prefabbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","breedte dagkant * diepte dorpel * dikte dorpel",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","Stuks",null,1]
["23.30.","gevelplinten - algemeen"]
["23.31.","gevelplinten - blauwe hardsteen ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
["23.32.","gevelplinten - sierbeton ","FH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":5},"Wall",null,"Projected Area",null,1]
["23.33.","gevelplinten - vezelcement ","FH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":5},"Wall ",null,"Projected Area",null,1]
["23.40.","omkaderingselementen - algemeen"]
["23.41.","omkaderingselementen - blauwe steen ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Column",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["23.50.","muurdekstenen - algemeen"]
["23.51.","muurdekstenen - blauwe steen ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":5},"Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["23.52.","muurdekstenen - prefabbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Slab",null,"Omtrek vloer zonder openingen",null,1]
["23.53.","muurdekstenen - vezelcement ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Slab",null,"Omtrek vloer zonder openingen",null,1]
["23.60.","schoorsteendekplaten - algemeen"]
["23.61.","schoorsteendekplaten - blauwe steen ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Slab",null,"Stuks",null,1]
["23.62.","schoorsteendekplaten - beton ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Slab",null,"Stuks",null,1]
["23.63.","schoorsteendekplaten - vezelcement ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Slab",null,"Stuks",null,1]
["24.","RUWBOUWKANALEN"]
["24.00.","ruwbouw kanalen - algemeen"]
["24.10.","modulaire ruwbouwkanalen - algemeen"]
["24.11.","modulaire ruwbouwkanalen - beton "]
["24.11.10.","modulaire ruwbouwkanalen - beton/rookgasafvoer ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["24.11.20.","modulaire ruwbouwkanalen - beton/ventilatie ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["24.12.","modulaire ruwbouwkanalen - keramische blokken"]
["24.12.10.","modulaire ruwbouwkanalen - keramische blokken/rookgasafvoer ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["24.12.20.","modulaire ruwbouwkanalen - keramische blokken/ventilatie ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["25.","STRUCTUURELEMENTEN HOUT"]
["25.00.","structuurelementen hout - algemeen"]
["25.01.","algemeen - stabiliteitsstudie ","PM",null,"Geen",{"$nulls":4},1]
["25.02.","algemeen - opleg- en bevestigingsmaterialen"]
["25.02.10.","algemeen - opleg- en bevestigingsmaterialen/metalen schoenen ","PM",null,"Geen",{"$nulls":4},1]
["25.02.20.","algemeen - opleg- en bevestigingsmaterialen/schroeven, nagels en nieten ","PM",null,"Geen",{"$nulls":4},1]
["25.02.30.","algemeen - opleg- en bevestigingsmaterialen/lijmen ","PM",null,"Geen",{"$nulls":4},1]
["25.02.40.","algemeen - opleg- en bevestigingsmaterialen/metalen hechtplaten ","PM",null,"Geen",{"$nulls":4},1]
["25.10.","balken - algemeen"]
["25.11.","balken - massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["25.12.","balken - LVL ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["25.13.","balken - lichte samengestelde liggers ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["25.14.","balken - gelijmd gelamineerd hout (GL) ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["25.20.","kolommen - algemeen"]
["25.21.","kolommen - massief hout ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
["25.22.","kolommen - LVL ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
["25.23.","kolommen - gelijmd gelamineerd hout"]
["25.30.","vloeren - algemeen"]
["25.31.","vloeren - roostering met beplating"]
["25.31.10.","vloeren - roostering met beplating/balken"]
["25.31.11.","vloeren - roostering met beplating/balken - massief hout ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["25.31.12.","vloeren - roostering met beplating/balken - LVL ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["25.31.13.","vloeren - roostering met beplating/balken - lichte samengestelde liggers ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["25.31.14.","vloeren - roostering met beplating/balken - gelijmd gelamineerd hout ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["25.31.20.","vloeren - roostering met beplating/beplating"]
["25.31.21.","vloeren - roostering met beplating/beplating - OSB ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["25.31.22.","vloeren - roostering met beplating/beplating - spaanplaat ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["25.31.23.","vloeren - roostering met beplating/beplating - LVL ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.","STRUCTUURELEMENTEN BETON"]
["26.00.","structuurelementen gewapend beton - algemeen"]
["26.01.","algemeen - stabiliteitsstudie ","PM",null,"Geen",{"$nulls":4},1]
["26.10.","materialen - algemeen"]
["26.11.","materialen - wapening"]
["26.11.10.","materialen - wapening/staven en netten"]
["26.11.11.","materialen - wapening/staven en netten - staven ","FH","kg","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Gewicht (kg) in bij Settings van het Object",null,1]
["26.11.12.","materialen - wapening/staven en netten - netten ","FH","kg","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Gewicht (kg) in bij Settings van het Object",null,1]
["26.11.20.","materialen - wapening/vezels"]
["26.11.21.","materialen - wapening/vezels - staalvezels ","VH of FH","kg","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Gewicht (kg) in bij Settings van het Object",null,1]
["26.11.30.","materialen - wapening/voorspanstaal ","PM",null,"Geen",{"$nulls":4},1]
["26.12.","materialen - beton"]
["26.12.10.","materialen - beton/stortklaar beton"]
["26.12.11.","materialen - beton/stortklaar beton - met staaf- en netwapening ","PM",null,"Geen",{"$nulls":4},1]
["26.12.12.","materialen - beton/stortklaar beton - met vezelwapening ","PM",null,"Geen",{"$nulls":4},1]
["26.12.13.","materialen - beton/stortklaar beton - zichtbeton ","FH","m2","TYPE 3","Column",null,"Core surface",null,1]
[{"$nulls":4},"TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW Zichtbeton  ","Net Area",null,1]
[{"$nulls":5},"Slab","Gebruik ARCHICAD Property: VMSW Zichtbeton  ","Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall","Gebruik ARCHICAD Property: VMSW Zichtbeton  ","ARCHICAD Property: Oppervlakte middenas wand",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["26.12.20.","materialen - beton/geprefabriceerd beton ","PM",null,"Geen",{"$nulls":4},1]
["26.12.30.","materialen - beton/architectonisch beton ","PM",null,"Geen",{"$nulls":4},1]
["26.13.","materialen - bekistingen ","PM",null,"Geen",{"$nulls":4},1]
["26.14.","materialen - nabehandeling"]
["26.15.","materialen - chemische verankering ","FH of VH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM ",null,"Geen",{"$nulls":4},1]
["26.16.","materialen - thermische onderbreking ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,"PM ",null,"Geen",{"$nulls":4},1]
["26.20.","ter plaatse gestorte elementen - algemeen"]
["26.21.","ter plaatse gestorte elementen - wanden"]
["26.21.10.","ter plaatse gestorte elementen - wanden/traditionele bekisting ","FH","m3","TYPE 3","Wall",null,"Net Volume",null,1]
["26.21.20.","ter plaatse gestorte elementen - wanden/holle wanden"]
["26.21.21.","ter plaatse gestorte elementen - wanden/holle wanden - prefab elementen ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["26.21.22.","ter plaatse gestorte elementen - wanden/holle wanden - vulbeton ","FH","m3","TYPE 3","Wall",null,"Net Volume",null,1]
["26.22.","ter plaatse gestorte elementen - kolommen ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
["26.23.","ter plaatse gestorte elementen - balken ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["26.24.","ter plaatse gestorte elementen - balken met afwijkend bekistingsprofiel ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["26.25.","ter plaatse gestorte elementen - trappen en bordessen ","FH","trede","TYPE 5","Stair",null,"Totaal aantal treden",null,1]
["26.26.","ter plaatse gestorte elementen - draagvloeren"]
["26.26.10.","ter plaatse gestorte elementen - draagvloeren/traditionele bekisting ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.26.20.","ter plaatse gestorte elementen - draagvloeren/verloren bekisting ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.26.30.","ter plaatse gestorte elementen - draagvloeren/breedplaatvloeren"]
["26.26.31.","ter plaatse gestorte elementen - draagvloeren/breedplaatvloeren - prefab breedplaten ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.26.32.","ter plaatse gestorte elementen - draagvloeren/breedplaatvloeren - opstort ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.27.","ter plaatse gestorte elementen - uitkragende elementen"]
["26.27.10.","ter plaatse gestorte elementen - uitkragende elementen/balkons ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.27.20.","ter plaatse gestorte elementen - uitkragende elementen/galerijen ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.27.30.","ter plaatse gestorte elementen - uitkragende elementen/luifels ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.27.40.","ter plaatse gestorte elementen - uitkragende elementen/kroonlijsten ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["26.30.","prefab elementen - algemeen"]
["26.31.","prefab elementen - wanden ","FH","m3","TYPE 3","Wall",null,"Net Volume",null,1]
["26.32.","prefab elementen - kolommen ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
["26.33.","prefab elementen - balken ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["26.34.","prefab elementen - deur- en raamlateien ","PM",null,"Geen",{"$nulls":4},1]
["26.35.","prefab elementen - trappen en bordessen ","FH","st","TYPE 5","Stair",null,"Stuks",null,1]
["26.36.","prefab elementen - draagvloeren"]
["26.36.10.","prefab elementen - draagvloeren/welfsels"]
["26.36.11.","prefab elementen - draagvloeren/welfsels - zonder druklaag ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.12.","prefab elementen - draagvloeren/welfsels - met druklaag ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.20.","prefab elementen - draagvloeren/voorgespannen welfsels"]
["26.36.21.","prefab elementen - draagvloeren/voorgespannen welfsels - zonder druklaag ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.22.","prefab elementen - draagvloeren/voorgespannen welfsels - met druklaag ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.30.","prefab elementen - draagvloeren/cellenbeton ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.40.","prefab elementen - draagvloeren/balken en vulblokken"]
["26.36.41.","prefab elementen - draagvloeren/balken en vulblokken - vulblokken beton ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.42.","prefab elementen - draagvloeren/balken en vulblokken - vulblokken gebakken klei  ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.43.","prefab elementen - draagvloeren/balken en vulblokken - vulblokken EPS ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.37.","prefab elementen - uitkragende elementen"]
["26.37.10.","prefab elementen - uitkragende elementen/balkons ","FH","st","TYPE 3","Slab",null,"Stuks",null,1]
["26.37.20.","prefab elementen - uitkragende elementen/galerijen ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.37.30.","prefab elementen - uitkragende elementen/luifels ","FH","st","TYPE 3","Slab",null,"Stuks",null,1]
[null,null,null,"m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.37.40.","prefab elementen - uitkragende elementen/kroonlijsten ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["26.40.","betonrenovatie - algemeen"]
["26.41.","betonrenovatie - passivatie van vrijgemaakte wapeningsstaven ","VH","m","TYPE 4","Object","Gebruik ARCHICAD Property: VMSW betonrenovatie  ","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,null,"m","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW betonrenovatie  ","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["26.42.","betonrenovatie - vervangen van wapening ","VH","kg","TYPE 3","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
["26.43.","betonrenovatie - handmatig te plaatsen mortel"]
["26.43.10.","betonrenovatie - handmatig te plaatsen mortel/ gemodificeerde hydraulische mortel  ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings",null,1]
["26.43.20.","betonrenovatie - handmatig te plaatsen mortel/ harsgebonden mortel ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings",null,1]
["26.44.","betonrenovatie - gietmortel"]
["26.44.10.","betonrenovatie - gietmortel/ gemodificeerde hydraulische mortel ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings",null,1]
[null,null,null,"dm3","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Volume (dm3) in bij Settings van het Object",null,1]
["26.44.20.","betonrenovatie - gietmortel/ beton ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings",null,1]
[null,null,null,"dm3","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Volume (dm3) in bij Settings van het Object",null,1]
["26.45.","betonrenovatie - spuitbeton ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings",null,1]
[null,null,null,"dm3","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Volume (dm3) in bij Settings van het Object",null,1]
["26.46.","betonrenovatie - injecteren van scheuren ","VH","m","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Lengte (cm) in bij de Object settings",null,1]
["26.47.","betonrenovatie - coating ","FH of VH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[{"$nulls":5},"Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (m2) in bij de Object Settings",null,1]
["27.","STRUCTUURELEMENTEN STAAL"]
["27.00.","structuurelementen staal - algemeen"]
["27.01.","algemeen - verbindingen ","PM",null,"Geen",{"$nulls":4},1]
["27.02.","algemeen - stabiliteitsstudie ","PM",null,"Geen",{"$nulls":4},1]
["27.10.","balken - algemeen"]
["27.11.","balken - blank profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.12.","balken - gemetalliseerd profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.13.","balken - thermisch verzinkt profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.14.","balken - thermisch verzinkt profielstaal met coating ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.15.","balken - roestvast profielstaal (RVS) ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.20.","lateien - algemeen"]
["27.21.","lateien - blank profielstaal ","PM",null,"Geen",{"$nulls":4},1]
["27.22.","lateien - gemetalliseerd profielstaal ","PM",null,"Geen",{"$nulls":4},1]
["27.23.","lateien - thermisch verzinkt profielstaal ","PM",null,"Geen",{"$nulls":4},1]
["27.24.","lateien - thermisch verzinkt profielstaal met coating ","PM",null,"Geen",{"$nulls":4},1]
["27.25.","lateien - roestvast profielstaal (RVS) ","PM",null,"Geen",{"$nulls":4},1]
["27.26.","lateien - regelbare consoles"]
["27.26.10.","lateien - regelbare consoles/zichtbaar"]
["27.26.11.","lateien - regelbare consoles/zichtbaar - gemetalliseerd ","PM",null,"Geen",{"$nulls":4},1]
["27.26.12.","lateien - regelbare consoles/zichtbaar - thermisch verzinkt ","PM",null,"Geen",{"$nulls":4},1]
["27.26.13.","lateien - regelbare consoles/zichtbaar - thermisch verzinkt + coating ","PM",null,"Geen",{"$nulls":4},1]
["27.26.14.","lateien - regelbare consoles/zichtbaar - roestvast staal (RVS) ","PM",null,"Geen",{"$nulls":4},1]
["27.26.20.","lateien - regelbare consoles/niet-zichtbaar"]
["27.26.21.","lateien - regelbare consoles/niet-zichtbaar - gemetalliseerd ","PM",null,"Geen",{"$nulls":4},1]
["27.26.22.","lateien - regelbare consoles/niet-zichtbaar - thermisch verzinkt ","PM",null,"Geen",{"$nulls":4},1]
["27.26.23.","lateien - regelbare consoles/niet-zichtbaar - roestvast staal (RVS) ","PM",null,"Geen",{"$nulls":4},1]
["27.30.","kolommen - algemeen"]
["27.31.","kolommen - blank profielstaal ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.32.","kolommen - gemetalliseerd profielstaal ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.33.","kolommen - thermisch verzinkt profielstaal ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.34.","kolommen - thermisch verzinkt profielstaal met coating ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.35.","kolommen - roestvast profielstaal (RVS) ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.40.","vlakke spanten - algemeen","FH"]
["27.41.","vlakke spanten - blank profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 5","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["27.42.","vlakke spanten - gemetalliseerd profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 5","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["27.43.","vlakke spanten - thermisch verzinkt profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 5","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["27.44.","vlakke spanten - thermisch verzinkt profielstaal met coating ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 5","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["27.50.","hulpstukken - algemeen"]
["27.51.","hulpstukken - oplegstukken"]
["27.51.10.","hulpstukken - oplegstukken/thermisch verzinkt ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.51.20.","hulpstukken - oplegstukken/roestvast staal (RVS) ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.52.","hulpstukken - spankabels ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"SOG"]
["27.53.","hulpstukken - geveldragers"]
["27.53.10.","hulpstukken - geveldragers/gemetalliseerd ","PM",null,"Geen",{"$nulls":4},1]
["27.53.20.","hulpstukken - geveldragers/thermisch verzinkt ","PM",null,"Geen",{"$nulls":4},1]
["27.53.30.","hulpstukken - geveldragers/roestvast staal ","PM",null,"Geen",{"$nulls":4},1]
["27.54.","hulpstukken - verhandelingsysteem liften"]
["27.60.","corrosiebescherming - algemeen"]
["27.61.","corrosiebescherming - metallisatie"]
["27.61.10.","corrosiebescherming - metallisatie/zonder bijkomende afwerkingslaag ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.61.20.","corrosiebescherming - metallisatie/metallisatie + natlak ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.61.30.","corrosiebescherming - metallisatie/metallisatie + poederlak ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.62.","corrosiebescherming - thermisch verzinken ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.63.","corrosiebescherming - duplexsysteem ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.64.","corrosiebescherming - roestwerende verfsystemen ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.70.","brandbeveiliging - algemeen"]
["27.71.","brandbeveiliging - brandwerend verfsysteem ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.72.","brandbeveiliging - spuitmortel ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.80.","renovatie stalen constructie-elementen - algemeen"]
["27.81.","renovatie stalen constructie-elementen - ontroesten ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["28.","HOUTSKELETBOUW"]
["28.00.","houtskeletbouw - algemeen"]
["28.01.","algemeen - stabiliteitsstudie ","PM",null,"Geen",{"$nulls":4},1]
["28.02.","algemeen - prestaties ","PM",null,"Geen",{"$nulls":4},1]
["28.10.","materialen - algemeen"]
["28.11.","materialen - onderdelen regelwerk"]
["28.11.10.","materialen - onderdelen regelwerk/stijlen"]
["28.11.11.","materialen - onderdelen regelwerk /stijlen - massief hout ","PM",null,"Geen",{"$nulls":4},1]
["28.11.12.","materialen - onderdelen regelwerk /stijlen - I-vormige stijlen ","PM",null,"Geen",{"$nulls":4},1]
["28.11.20.","materialen - onderdelen regelwerk/regels"]
["28.11.21.","materialen - onderdelen regelwerk /regels - onder- en bovenregels ","PM",null,"Geen",{"$nulls":4},1]
["28.11.22.","materialen - onderdelen regelwerk /regels - grondregels ","PM",null,"Geen",{"$nulls":4},1]
["28.11.23.","materialen - onderdelen regelwerk /regels - stelregels ","PM",null,"Geen",{"$nulls":4},1]
["28.11.24.","materialen - onderdelen regelwerk /regels - koppelregels ","PM",null,"Geen",{"$nulls":4},1]
["28.11.30.","materialen - onderdelen regelwerk/lateien ","PM",null,"Geen",{"$nulls":4},1]
["28.12.","materialen - beplating"]
["28.12.10.","materialen - beplating/houtachtige platen"]
["28.12.11.","materialen - beplating/houtachtige platen - OSB ","PM",null,"Geen",{"$nulls":4},1]
["28.12.12.","materialen - beplating/houtachtige platen - spaanplaat ","PM",null,"Geen",{"$nulls":4},1]
["28.12.13.","materialen - beplating/houtachtige platen - multiplex ","PM",null,"Geen",{"$nulls":4},1]
["28.12.14.","materialen - beplating/houtachtige platen - MDF ","PM",null,"Geen",{"$nulls":4},1]
["28.12.15.","materialen - beplating/houtachtige platen - LVL ","PM",null,"Geen",{"$nulls":4},1]
["28.12.16.","materialen - beplating/houtachtige platen - houtvezelisolatieplaat ","PM",null,"Geen",{"$nulls":4},1]
["28.12.17.","materialen - beplating/houtachtige platen - houtvezelcementplaat ","PM",null,"Geen",{"$nulls":4},1]
["28.12.20.","materialen - beplating/gipsachtige platen"]
["28.12.21.","materialen - beplating/gipsachtige platen - gipskartonplaten ","PM",null,"Geen",{"$nulls":4},1]
["28.12.22.","materialen - beplating/gipsachtige platen - gipsvezelplaten ","PM",null,"Geen",{"$nulls":4},1]
["28.12.30.","materialen - beplating/vezelcementplaten ","PM",null,"Geen",{"$nulls":4},1]
["28.12.40.","materialen - beplating/calciumsilicaatplaten ","PM",null,"Geen",{"$nulls":4},1]
["28.13.","materialen - isolatie"]
["28.13.10.","materialen - isolatie/minerale wol ","PM",null,"Geen",{"$nulls":4},1]
["28.13.20.","materialen - isolatie/cellulosevlokken ","PM",null,"Geen",{"$nulls":4},1]
["28.13.30.","materialen - isolatie/houtwol ","PM",null,"Geen",{"$nulls":4},1]
["28.14.","materialen - folies"]
["28.14.10.","materialen - folies/buitenfolies"]
["28.14.11.","materialen - folies/buitenfolies - wanden ","PM",null,"Geen",{"$nulls":4},1]
["28.14.12.","materialen - folies/buitenfolies - hellende daken ","PM",null,"Geen",{"$nulls":4},1]
["28.14.20.","materialen - folies/binnenfolies"]
["28.14.21.","materialen - folies/binnenfolies - wanden ","PM",null,"Geen",{"$nulls":4},1]
["28.14.22.","materialen - folies/binnenfolies - hellende daken ","PM",null,"Geen",{"$nulls":4},1]
["28.14.23.","materialen - folies/binnenfolies - platte daken ","PM",null,"Geen",{"$nulls":4},1]
["28.15.","materialen - regelstructuur voor binnenafwerking"]
["28.15.10.","materialen - regelstructuur voor binnenafwerking/hout ","PM",null,"Geen",{"$nulls":4},1]
["28.15.20.","materialen - regelstructuur voor binnenafwerking/metaal ","PM",null,"Geen",{"$nulls":4},1]
["28.16.","materialen - opleg- en bevestigingsmaterialen"]
["28.16.10.","materialen - opleg- en bevestigingsmaterialen/metalen schoenen ","PM",null,"Geen",{"$nulls":4},1]
["28.16.20.","materialen - opleg- en bevestigingsmaterialen/tie-downs ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["28.16.30.","materialen - opleg- en bevestigingsmaterialen/schroeven ","PM",null,"Geen",{"$nulls":4},1]
["28.16.40.","materialen - opleg- en bevestigingsmaterialen/nagels ","PM",null,"Geen",{"$nulls":4},1]
["28.16.50.","materialen - opleg- en bevestigingsmaterialen/nieten ","PM",null,"Geen",{"$nulls":4},1]
["28.16.60.","materialen - opleg- en bevestigingsmaterialen/lijmen ","PM",null,"Geen",{"$nulls":4},1]
["28.16.70.","materialen - opleg- en bevestigingsmaterialen/metalen hechtplaten ","PM",null,"Geen",{"$nulls":4},1]
["28.20.","structuurelementen - algemeen"]
["28.21.","structuurelementen - vloerbalken"]
["28.21.10.","structuurelementen - vloerbalken/massief hout ","PM",null,"Geen",{"$nulls":4},1]
["28.21.20.","structuurelementen - vloerbalken/LVL ","PM",null,"Geen",{"$nulls":4},1]
["28.21.30.","structuurelementen - vloerbalken/lichte samengestelde liggers ","PM",null,"Geen",{"$nulls":4},1]
["28.21.40.","structuurelementen - vloerbalken/gelijmd gelamineerd hout (GL) ","PM",null,"Geen",{"$nulls":4},1]
["28.22.","structuurelementen - balken"]
["28.22.10.","structuurelementen - balken/massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.22.20.","structuurelementen - balken/LVL ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.22.30.","structuurelementen - balken/lichte samengestelde liggers ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.22.40.","structuurelementen - balken/gelijmd gelamineerd hout (GL) ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.22.50.","structuurelementen - balken/staal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.23.","structuurelementen - lateien"]
["28.23.10.","structuurelementen - lateien/massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.23.20.","structuurelementen - lateien/LVL ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.23.30.","structuurelementen - lateien/gelijmd gelamineerd hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.23.40.","structuurelementen - lateien/staal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.24.","structuurelementen - kolommen"]
["28.24.10.","structuurelementen - kolommen/massief hout ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
["28.24.20.","structuurelementen - kolommen/LVL ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
["28.24.30.","structuurelementen - kolommen/gelijmd gelamineerd hout (GL) ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
["28.24.40.","structuurelementen - kolommen/staal ","FH","kg","TYPE 3","Column",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
["28.25.","structuurelementen - onderdelen hellend dak"]
["28.25.10.","structuurelementen - onderdelen hellend dak/gordingen"]
["28.25.11.","structuurelementen - onderdelen hellend dak/gordingen - massief hout ","PM",null,"Geen",{"$nulls":4},1]
["28.25.12.","structuurelementen - onderdelen hellend dak/gordingen - gelamineerd hout ","PM",null,"Geen",{"$nulls":4},1]
["28.25.20.","structuurelementen - onderdelen hellend dak/keperwerk"]
["28.25.21.","structuurelementen - onderdelen hellend dak/keperwerk - massief hout ","PM",null,"Geen",{"$nulls":4},1]
["28.25.30.","structuurelementen - onderdelen hellend dak/spanten"]
["28.25.31.","structuurelementen - onderdelen hellend dak/spanten - massief hout"]
["28.25.40.","structuurelementen - onderdelen hellend dak/scharnierdak ","PM",null,"Geen",{"$nulls":4},1]
["28.25.50.","structuurelementen - onderdelen hellend dak/bakgootconstructies"]
["28.25.51.","structuurelementen - onderdelen hellend dak/bakgootconstructies - massief hout ","PM",null,"Geen",{"$nulls":4},1]
["28.25.60.","structuurelementen - onderdelen hellend dak/dakrandoversteken"]
["28.25.61.","structuurelementen - onderdelen hellend dak/dakrandoversteken - massief hout ","PM",null,"Geen",{"$nulls":4},1]
["28.25.70.","structuurelementen - onderdelen hellend dak/tengel- en panlatten ","PM",null,"Geen",{"$nulls":4},1]
["28.30.","wanden - algemeen"]
["28.31.","wanden - buitenwanden "]
["28.31.10.","wanden - buitenwanden/type I ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["28.31.20.","wanden - buitenwanden/type II ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["28.31.30.","wanden - buitenwanden/type III ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["28.32.","wanden - binnenwanden "]
["28.32.10.","wanden - binnenwanden/type I ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["28.32.20.","wanden - binnenwanden/type II ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["28.33.","wanden - woningscheidende wanden ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["28.34.","wanden - dakopstanden ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Lengte volgens eigen middenas",null,1]
["28.40.","vloeren - algemeen"]
["28.41.","vloeren - roostering met beplating ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.42.","vloeren - geprefabriceerde houten vloeren"]
["28.42.10.","vloeren - geprefabriceerde houten vloeren/roostering met beplating ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.42.20.","vloeren - geprefabriceerde houten vloeren/kokervormige vloeren ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.42.30.","vloeren - geprefabriceerde houten vloeren/massieve houten vloeren ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.43.","vloeren - hout-betonvloeren ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.50.","hellende daken - algemeen"]
["28.51.","hellende daken - spanten ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":5},"Shell",null,null,null,1]
["28.52.","hellende daken - gordingen ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":5},"Shell",null,null,null,1]
["28.53.","hellende daken - scharnierdaken ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":5},"Shell",null,null,null,1]
["28.60.","platte daken - algemeen"]
["28.61.","platte daken - roostering met beplating ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":5},"Slab",null,null,null,1]
["28.62.","platte daken - geprefabriceerde houten vloeren"]
["28.62.10.","platte daken - geprefabriceerde houten vloeren/roostering met beplating ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":5},"Slab",null,null,null,1]
["28.62.20.","platte daken - geprefabriceerde houten vloeren/kokervormige vloeren ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":5},"Slab",null,null,null,1]
["28.62.30.","platte daken - geprefabriceerde houten vloeren/massieve houten vloeren ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":5},"Slab",null,null,null,1]
["28.63.","platte daken - hout-betonvloeren ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":5},"Slab",null,null,null,1]
["28.64.","platte daken - randisolatie ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Roof",null,"Omtrek ",null,1]
[{"$nulls":5},"Slab",null,"Omtrek ",null,1]
["30.","DAKOPBOUW HELLEND DAK"]
["30.00.","dakopbouw hellend dak - algemeen"]
["30.01.","dakopbouw hellend dak - stabiliteitsstudie ","PM",null,"Geen",{"$nulls":4},1]
["30.10.","houten dakstructuur - algemeen ","FH","m3","TYPE 3","Roof",null,"Net Volume",null,1]
[{"$nulls":5},"Shell",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Roof",null,"Stuks",null,1]
[{"$nulls":5},"Shell",null,"Stuks",null,1]
[null,null,"PM"]
["30.11.","houten dakstructuur - muurplaten ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["30.12.","houten dakstructuur - gordingen"]
["30.12.10.","houten dakstructuur - gordingen/massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
[{"$nulls":5},"Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["30.12.20.","houten dakstructuur - gordingen/gelamineerd hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
[{"$nulls":5},"Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["30.13.","houten dakstructuur - keperwerk ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
[{"$nulls":5},"Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["30.14.","houten dakstructuur - keperspanten ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
[{"$nulls":5},"Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["30.15.","houten dakstructuur - prefabspanten ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
[{"$nulls":5},"Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["30.16.","houten dakstructuur - bakgootconstructies ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["30.17.","houten dakstructuur - dakrandoversteken ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["30.18.","houten dakstructuur - boordplanken"]
["30.18.10.","houten dakstructuur - boordplanken/massief hout ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["30.18.20.","houten dakstructuur - boordplanken/multiplex ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["30.20.","onderdak - algemeen"]
["30.21.","onderdak - soepele membranen ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
["30.22.","onderdak - platen"]
["30.22.10.","onderdak - platen/vezelcement ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["30.22.20.","onderdak - platen/houtvezelplaten ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["30.30.","tengel- & panlatten - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["31.","THERMISCHE ISOLATIE HELLEND DAK"]
["31.00.","thermische isolatie hellend dak - algemeen"]
["31.10.","isolatieplaten tussen dakstructuur - algemeen"]
["31.11.","isolatieplaten tussen dakstructuur - MW"]
["31.11.10.","isolatieplaten tussen dakstructuur - MW/18 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["31.11.20.","isolatieplaten tussen dakstructuur - MW/20 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["31.12.","isolatieplaten tussen dakstructuur - houtwol (WW)"]
["31.12.10.","isolatieplaten tussen dakstructuur - houtwol (WW)/18 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["31.12.20.","isolatieplaten tussen dakstructuur - houtwol (WW)/20 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["31.13.","isolatieplaten tussen dakstructuur - cellulose"]
["31.13.10.","isolatieplaten tussen dakstructuur - cellulose/18 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["31.13.20.","isolatieplaten tussen dakstructuur - cellulose/20 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["31.20.","isolatieplaten op dakstructuur (sarking) - algemeen"]
["31.21.","isolatieplaten op dakstructuur (sarking) - PUR of PIR"]
["31.21.10.","isolatieplaten op dakstructuur (sarking) - PUR of PIR/14 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["31.21.20.","isolatieplaten op dakstructuur (sarking) - PUR of PIR/16 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["31.22.","isolatieplaten op dakstructuur (sarking) - PF"]
["31.22.10.","isolatieplaten op dakstructuur (sarking) - PF/14 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["31.22.20.","isolatieplaten op dakstructuur (sarking) - PF/16 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["31.23.","isolatieplaten op dakstructuur (sarking) - XPS"]
["31.23.10.","isolatieplaten op dakstructuur (sarking) - XPS/14 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["31.23.20.","isolatieplaten op dakstructuur (sarking) - XPS/16 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["31.30.","ingeblazen isolatie - algemeen"]
["31.31.","ingeblazen isolatie - cellulose"]
["31.31.10.","ingeblazen isolatie - cellulose/18 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["31.31.20.","ingeblazen isolatie - cellulose/23 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["31.40.","binnenfolie - algemeen"]
["31.41.","binnenfolie - damprem ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["31.42.","binnenfolie - dampscherm ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["31.50.","isolerende dakelementen - algemeen"]
["31.51.","isolerende dakelementen - tweeschalig ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["32.","DAKBEDEKKING HELLEND DAK"]
["32.00.","dakbedekking hellend dak - algemeen"]
["32.01.","dakbedekking hellend dak - prestaties"]
["32.10.","pannen - algemeen"]
["32.11.","pannen - gebakken aarde ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["32.11.10.","pannen - gebakken aarde/dakvlak ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["32.11.20.","pannen - gebakken aarde/vormstukken ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[]
["32.11.30.","pannen - gebakken aarde/toebehoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["32.12.","pannen - beton ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["32.12.10.","pannen - beton/dakvlak ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["32.12.20.","pannen - beton/vormstukken ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["32.12.30.","pannen - beton/toebehoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["32.13.","pannen - metaal ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
["32.13.10.","pannen - gecoat staal/dakvlak ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["32.13.20.","pannen - gecoat staal/vormstukken ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["32.13.30.","pannen - gecoat staal/toebehoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["32.20.","leien - algemeen"]
["32.21.","leien - vezelcement ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["32.22.","leien - natuurleien ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["32.30.","golfplaten - algemeen"]
["32.31.","golfplaten - vezelcement ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
["32.31.10.","golfplaten - vezelcement/dakvlakken ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
["32.31.20.","golfplaten - vezelcement/vormstukken ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["32.31.30.","golfplaten - vezelcement/toebehoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["32.40.","geprofileerde metaalplaten - algemeen"]
["32.41.","geprofileerde metaalplaten - gecoat staal ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["32.42.","geprofileerde metaalplaten - aluminium ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["32.43.","geprofileerde metaalplaten - RVS ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["32.50.","toebehoren hellend dak - algemeen"]
["32.51.","toebehoren hellend dak - dakdoorvoeren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["32.52.","toebehoren hellend dak - verankeringssystemen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["32.53.","toebehoren hellend dak - valbeveiliging"]
["32.53.10.","toebehoren hellend dak - valbeveiliging / ankerpunten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["32.53.20.","toebehoren hellend dak - valbeveiliging / lijnsysteem ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["32.54.","toebehoren hellend dak - ladderhaken ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["33.","DAKVLOER PLAT DAK"]
["33.00.","dakvloer plat dak - algemeen"]
["33.01.","algemeen - stabiliteitsstudie"]
["33.10.","houten roostering - algemeen"]
["33.11.","houten roostering - muurplaten ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
["33.12.","houten roostering - balken"]
["33.12.10.","houten roostering - balken/massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
["33.12.20.",null,"FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,0,"FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"m3","TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["33.12.30.","houten roostering - balken/lichte samengestelde liggers ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["33.20.","beplating op houten roostering - algemeen",null,null,"TYPE 5",{"$nulls":4},1]
["33.21.","beplating op houten roostering - multiplex ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.22.","beplating op houten roostering - OSB ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.23.","beplating op houten roostering - spaanplaat ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.24.","beplating op houten roostering - cementgebonden spaanplaat ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.30.","zelfdragende elementen - algemeen"]
["33.31.","zelfdragende elementen - profielplaten staal"]
["33.31.10.","zelfdragende elementen - profielplaten staal/enkelvoudig ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.32.","zelfdragende elementen - sandwichplaten hout ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.40.","hellingsbeton - algemeen"]
["33.41.","hellingsbeton - niet isolerend"]
["33.41.10.","hellingsbeton - niet isolerend/mager beton ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.41.20.","hellingsbeton - niet isolerend/zandcement dekvloer ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.52.","hellingsbeton - licht isolerend"]
["33.52.10.","hellingsbeton - licht isolerend/granulaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.52.20.","hellingsbeton - licht isolerend/schuimbeton ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.","THERMISCHE ISOLATIE PLAT DAK"]
["34.00.","thermische isolatie plat dak - algemeen"]
["34.10.","isolatieplaten plat dak - algemeen"]
["34.11.","isolatieplaten plat dak - MW"]
["34.11.10.","isolatieplaten plat dak - MW/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.11.20.","isolatieplaten plat dak - MW/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.12.","isolatieplaten plat dak - PUR of PIR"]
["34.12.10.","isolatieplaten plat dak - PUR of PIR/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.12.20.","isolatieplaten plat dak - PUR of PIR/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.13.","isolatieplaten plat dak - EPS"]
["34.13.10.","isolatieplaten plat dak - EPS/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.13.20.","isolatieplaten plat dak - EPS/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.14.","isolatieplaten plat dak - CG"]
["34.14.10.","isolatieplaten plat dak - CG/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.14.20.","isolatieplaten plat dak - CG/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.15.","isolatieplaten omkeerdak - XPS"]
["34.15.10.","isolatieplaten omkeerdak - XPS/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.15.20.","isolatieplaten omkeerdak - XPS/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.20.","dampscherm - algemeen"]
["34.21.","dampscherm - gewapend bitumen ","PM",null,"Geen",{"$nulls":4},1]
["35.","AFDICHTING & AFWERKING PLAT DAK"]
["35.00.","afdichting & afwerking plat dak - algemeen"]
["35.01.","afdichting & afwerking plat dak - waterdichtheidsproeven ","PM",null,"Geen",{"$nulls":4},1]
["35.02.","afdichting & afwerking plat dak - waarborgen & attesten ","PM",null,"Geen",{"$nulls":4},1]
["35.03.","afdichting & afwerking plat dak - renovatie bestaande daken ","PM",null,"Geen",{"$nulls":4},1]
["35.10.","bitumineuze dakafdichting - algemeen"]
["35.11.","bitumineuze dakafdichting - SBS"]
["35.11.10.","bitumineuze dakafdichting - SBS/losliggend (L) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.11.20.","bitumineuze dakafdichting - SBS/deelgekleefd (P) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.11.30.","bitumineuze dakafdichting - SBS/volgekleefd (T) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.11.40.","bitumineuze dakafdichting - SBS/mechanisch (M) ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.12.","bitumineuze dakafdichting - APP","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
["35.12.10.","bitumineuze dakafdichting - APP/losliggend (L) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.12.20.","bitumineuze dakafdichting - APP/deelgekleefd (P) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.12.30.","bitumineuze dakafdichting - APP/volgekleefd (T) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.12.40.","bitumineuze dakafdichting - APP/mechanisch (M) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.13.","bitumineuze dakafdichting - PBE"]
["35.20.","kunststof dakafdichting - algemeen"]
["35.21.","kunststof dakafdichting - EPDM"]
["35.21.10.","kunststof dakafdichting - EPDM/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.21.20.","kunststof dakafdichting - EPDM/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.21.30.","kunststof dakafdichting - EPDM/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.22.","kunststof dakafdichting - TPO"]
["35.22.10.","kunststof dakafdichting - TPO/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.22.20.","kunststof dakafdichting - TPO/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.22.30.","kunststof dakafdichting - TPO/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.23.","kunststof dakafdichting - PVC"]
["35.23.10.","kunststof dakafdichting - PVC/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.23.20.","kunststof dakafdichting - PVC/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.23.30.","kunststof dakafdichting - PVC/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.24.","kunststof dakafdichting - CPE"]
["35.24.10.","kunststof dakafdichting - CPE/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.24.20.","kunststof dakafdichting - CPE/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.24.30.","kunststof dakafdichting - CPE/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.25.","kunststof dakafdichting - PIB"]
["35.25.10.","kunststof dakafdichting - PIB/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.25.20.","kunststof dakafdichting - PIB/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.25.30.","kunststof dakafdichting - PIB/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.26.","kunststof dakafdichting - ECB"]
["35.26.10.","kunststof dakafdichting - ECB/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.26.20.","kunststof dakafdichting - ECB/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.26.30.","kunststof dakafdichting - ECB/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.30.","ballastlaag - algemeen"]
["35.31.","ballastlaag - grind ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.32.","ballastlaag - tegels ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.33.","ballastlaag - geotextiel ","PM",null,"Geen",{"$nulls":4},1]
["35.40.","groendak - algemeen"]
["35.41.","groendak - extensief ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.42.","groendak - intensief ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.50.","toebehoren plat dak - algemeen"]
["35.51.","toebehoren plat dak - dakdoorvoeren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["35.52.","toebehoren plat dak - verankeringssystemen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["35.53.","toebehoren plat dak - valbeveiliging"]
["35.53.10.","toebehoren plat dak - valbeveiliging/doodgewicht ankers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["35.53.20.","toebehoren plat dak - valbeveiliging/vaste ankerpunten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["35.53.30.","toebehoren plat dak - valbeveiliging/lijnsysteem ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,null,"m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["36.","DAKLICHTOPENINGEN"]
["36.00.","daklichtopeningen - algemeen"]
["36.10.","dakvlakramen - algemeen"]
["36.11.","dakvlakramen - hout"]
["36.11.10.","dakvlakramen - hout/wentel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
["36.11.20.","dakvlakramen - hout/uitzet en wentel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
["36.11.30.","dakvlakramen - hout/uitzet ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
["36.11.40.","dakvlakramen - hout/rook- & warmteafvoer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
["36.12.","dakvlakramen - kunststof"]
["36.12.10.","dakvlakramen - kunststof/wentel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
["36.12.20.","dakvlakramen - kunststof/uitzet-wentel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
["36.12.30.","dakvlakramen - kunststof/uitzet ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
["36.12.40.","dakvlakramen - kunststof/rook- en warmteafvoer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
["36.13.","dakvlakramen - zolderraam ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
["36.20.","platdakramen - algemeen"]
["36.21.","platdakramen - kunststof"]
["36.21.10.","platdakramen - kunststof/vast ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
["36.21.20.","platdakramen - kunststof/opengaand ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
["36.21.30.","platdakramen - kunststof/rook- en warmteafvoer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
["36.30.","koepels - algemeen"]
["36.31.","koepels - kunststof acrylaat (PMMA)"]
["36.31.10.","koepels - kunststof acrylaat (PMMA)/vast ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
["36.31.20.","koepels - kunststof acrylaat (PMMA)/opengaand ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
["36.31.30.","koepels - kunststof acrylaat (PMMA)/rook en warmteafvoer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
["36.32.","koepels - kunststof polycarbonaat (PC) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Skylight",null,"Stuks",null,1]
["36.40.","daglichtreflectiebuizen - algemeen"]
["36.41.","daglichtreflectiebuizen - plat dak ","FH","m2","TYPE 5","Object",null,"Net Area",null,1]
[{"$nulls":5},"Skylight",null,"Net Area",null,1]
["36.42.","daglichtreflectiebuizen - hellend dak ","FH","m2","TYPE 5","Object",null,"Net Area",null,1]
[{"$nulls":5},"Skylight",null,"Net Area",null,1]
["36.50.","lichtstraten - algemeen"]
["36.51.","lichtstraten - profielen hout"]
["36.51.10.","lichtstraten - profielen hout/met beglazing ","FH","m2","TYPE 3","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Area",null,1]
[{"$nulls":5},"Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Skylight",null,"Net Area",null,1]
["36.52.","lichtstraten - profielen aluminium"]
["36.52.10.","lichtstraten - profielen aluminium met beglazing ","FH","m2","TYPE 3","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Area",null,1]
[{"$nulls":5},"Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Skylight",null,"Net Area",null,1]
["36.60.","dakkapellen - algemeen"]
["36.61.","dakkapellen - traditioneel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["37.","DAKRANDEN EN KROONLIJSTEN"]
["37.00.","dakranden en kroonlijsten - algemeen"]
["37.10.","slabben, loketten en aansluitbanden - algemeen"]
["37.11.","slabben, loketten en aansluitbanden - metaal"]
["37.11.10.","slabben, loketten en aansluitbanden - metaal/lood ","FH of VH","kg","TYPE 3","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,null,"kg","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Gewicht (kg) in bij Settings van het Object",null,1]
["37.11.20.","slabben, loketten en aansluitbanden - metaal/aluminium ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.11.30.","slabben, loketten en aansluitbanden - metaal/zink ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.11.40.","slabben, loketten en aansluitbanden - metaal/koper ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.12.","slabben, loketten en aansluitbanden - membranen"]
["37.12.10.","slabben, loketten en aansluitbanden - membraan/EPDM ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.12.20.","slabben, loketten en aansluitbanden - membraan/PIB ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.12.30.","slabben, loketten en aansluitbanden - membraan/bitumen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.20.","dakrandprofielen - algemeen"]
["37.21.","dakrandprofielen - metaal"]
["37.21.10.","dakrandprofielen - metaal/zink ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.21.20.","dakrandprofielen - metaal/aluminium ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.21.30.","dakrandprofielen - metaal/metaalfolieplaten ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.22.","dakrandprofielen - kunststof"]
["37.22.10.","dakrandprofielen - kunststof/polyester ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.30.","muurkappen - algemeen","FH","m","TYPE 3","Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
["37.31.","muurkappen - metaal"]
["37.31.10.","muurkappen - metaal/zink ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
["37.31.20.","muurkappen - metaal/aluminium ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
["37.32.","muurkappen - kunststof ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
["37.40.","uitbekleding kroonlijsten en luifels - algemeen"]
["37.41.","uitbekleding kroonlijsten en luifels - planchetten"]
["37.41.10.","uitbekleding kroonlijsten en luifels - planchetten/massief hout ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["37.41.20.","uitbekleding kroonlijsten en luifels - planchetten/kunststof ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.41.30.","uitbekleding kroonlijsten en luifels - planchetten/vezelcement ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.42.","uitbekleding kroonlijsten en luifels - platen"]
["37.42.10.","uitbekleding kroonlijsten en luifels - platen/multiplex ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.42.20.","uitbekleding kroonlijsten en luifels - platen/kunststof ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.42.30.","uitbekleding kroonlijsten en luifels - platen/vezelcement ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.42.40.","uitbekleding kroonlijsten en luifels - platen/kunsthars ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.42.50.","uitbekleding kroonlijsten en luifels - platen/minerale vezels ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.43.","uitbekleding kroonlijsten en luifels - leien"]
["37.43.10.","uitbekleding kroonlijsten en luifels - leien/vezelcement ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.43.20.","uitbekleding kroonlijsten en luifels - leien hout ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.50.","toebehoren dakranden - algemeen"]
["37.51.","toebehoren dakranden - valbeveiliging"]
["37.51.10.","toebehoren dakranden - valbeveiliging/lijn- of railsysteem ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["37.51.20.","toebehoren dakranden - valbeveiliging/permanente leuning ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["37.52.","toebehoren dakranden - gevelonderhoudsinstallaties"]
["37.52.10.","toebehoren dakranden - gevelonderhoud/railsysteem ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["37.53.","toebehoren dakranden - verhuisbalk ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
["38.","DAKWATERAFVOER"]
["38.00.","dakwaterafvoer - algemeen"]
["38.10.","bakgootdichtingen - algemeen"]
["38.11.","bakgootdichtingen - metaalbladen"]
["38.11.10.","bakgootdichtingen - metaalbladen/zink ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.11.20.","bakgootdichtingen - metaalbladen/koper ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.12.","bakgootdichtingen - bitumen"]
["38.12.10.","bakgootdichtingen - bitumen/SBS ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.12.20.","bakgootdichtingen - bitumen/APP ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.13.","bakgootdichtingen - hoog polymeermembranen"]
["38.13.10.","bakgootdichtingen - hoog polymeermembranen/EPDM ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.13.20.","bakgootdichtingen - hoog polymeermembranen/TPO ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.13.30.","bakgootdichtingen - hoog polymeermembranen/PVC ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.20.","hanggoten - algemeen"]
["38.21.","hanggoten - kunststof"]
["38.21.10.","hanggoten - kunststof/PVC ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.21.20.","hanggoten - kunststof/polyesterhars ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.22.","hanggoten - metaal"]
["38.22.10.","hanggoten - metaal/zink ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.22.20.","hanggoten - metaal/aluminium ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.22.30.","hanggoten - metaal/koper ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.22.40.","hanggoten - metaal/gecoat staal ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.22.50.","hanggoten - metaal/roestvast staal ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.30.","afvoerpijpen - algemeen"]
["38.31.","afvoerpijpen - kunststof"]
["38.31.10.","afvoerpijpen - kunststof/PVC ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.31.20.","afvoerpijpen - kunststof/HDPE ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.32.","afvoerpijpen - metaal","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.32.10.","afvoerpijpen - metaal/zink ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.32.20.","afvoerpijpen - metaal/koper ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.32.30.","afvoerpijpen - metaal/aluminium ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.32.40.","afvoerpijpen - metaal/gecoat staal ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.32.50.","afvoerpijpen - metaal/roestvast staal ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.40.","eindstukken - algemeen","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.41.","eindstukken - slagvast kunststof ","FH","st","TYPE 5","Object",null,"Stuks",null,2]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["38.42.","eindstukken - behandeld gietijzer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["38.43.","eindstukken - gegoten aluminium ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["38.50.","toebehoren - algemeen",null,null,"Geen",{"$nulls":4},1]
["38.51.","toebehoren - dakkolken en tapbuizen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["38.52.","toebehoren - draad- en bolroosters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["38.53.","toebehoren - balkonafvoerputjes ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["38.54.","toebehoren - noodspuwers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.","BUITENSCHRIJNWERK"]
["40.00.","buitenschrijnwerk - algemeen"]
["40.01.","buitenschrijnwerk - prestaties"]
["40.02.","buitenschrijnwerk - proeven"]
["40.02.10.","buitenschrijnwerk - proeven/op kosten ongelijk ","PM",null,"Geen",{"$nulls":4},1]
["40.02.20.","buitenschrijnwerk - proeven/op kosten aannemer ","VH","st","TYPE 5","Object",null,"Stuks",null,1]
["40.03.","buitenschrijnwerk - montage"]
["40.03.10.","buitenschrijnwerk - montage/spouwconstructie en dorpel ","PM",null,"Geen",{"$nulls":4},1]
["40.03.20.","buitenschrijnwerk - montage/buitengevelisolatiesysteem ","PM",null,"Geen",{"$nulls":4},1]
["40.03.30.","buitenschrijnwerk - montage/gevelbekledingsysteem ","PM",null,"Geen",{"$nulls":4},1]
["40.03.40.","buitenschrijnwerk - montage/houtskeletbouw ","PM",null,"Geen",{"$nulls":4},1]
["40.03.50.","buitenschrijnwerk - montage/vervanging schrijnwerk ","PM",null,"Geen",{"$nulls":4},1]
["40.04.","buitenschrijnwerk - borderel"]
["40.10.","profielsystemen - algemeen"]
["40.11.","profielsysteem - hout"]
["40.11.10.","profielsysteem - hout/vaste ramen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.11.20.","profielsysteem - hout/draairamen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.11.30.","profielsysteem - hout/schuiframen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,null,"m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
["40.11.40.","profielsysteem - hout/buitendeuren ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.12.","profielsysteem - aluminium"]
["40.12.10.","profielsysteem - aluminium/vaste ramen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.12.20.","profielsysteem - aluminium/draairamen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.12.30.","profielsysteem - aluminium/schuiframen ","FH of PM","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,null,"m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
["40.12.40.","profielsysteem - aluminium/buitendeuren ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
["40.13.","profielsysteem - pvc"]
["40.13.10.","profielsysteem - pvc/vaste ramen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.13.20.","profielsysteem - pvc/draairamen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,null,"m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
["40.13.30.","profielsysteem - pvc/schuiframen ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.13.40.","profielsysteem - pvc/buitendeuren ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
["40.14.","profielsysteem - staal"]
["40.14.10.","profielsysteem - staal/vaste ramen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.14.20.","profielsysteem - staal/buitendeuren ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
[]
["40.20.","hang- en sluitwerk - algemeen"]
["40.21.","hang- en sluitwerk - standaard beslag ","PM",null,"Geen",{"$nulls":4},1]
["40.22.","hang- en sluitwerk - scharnieren en paumellen ","PM",null,"Geen",{"$nulls":4},1]
["40.23.","hang- en sluitwerk - sloten ","PM",null,"Geen",{"$nulls":4},1]
["40.23.10.","hang- en sluitwerk - sloten/manueel ","PM",null,"Geen",{"$nulls":4},1]
["40.23.20.","hang- en sluitwerk - sloten/elektromagnetisch ","PM",null,"Geen",{"$nulls":4},1]
["40.23.30.","hang- en sluitwerk - sloten/schuifdeurslot ","PM",null,"Geen",{"$nulls":4},1]
["40.23.40.","hang- en sluitwerk - sloten/glasdeurslot ","PM",null,"Geen",{"$nulls":4},1]
["40.23.50.","hang- en sluitwerk - sloten/sleutelplan ","PM",null,"Geen",{"$nulls":4},1]
["40.24.","hang- en sluitwerk - deurdrangers ","PM",null,"Geen",{"$nulls":4},1]
["40.24.10.","hang- en sluitwerk - deurdrangers/manueel ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurdranger","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.24.20.","hang- en sluitwerk - deurdrangers/gemotoriseerd ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurdranger","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.25.","hang- en sluitwerk - panieksluitingen ","PM",null,"Geen",{"$nulls":4},1]
["40.26.","hang- en sluitwerk - raamkrukken ","PM",null,"Geen",{"$nulls":4},1]
["40.27.","hang- en sluitwerk - deurkrukken ","PM",null,"Geen",{"$nulls":4},1]
["40.28.","hang- en sluitwerk - vaste handgrepen ","PM",null,"Geen",{"$nulls":4},1]
["40.29.","hang- en sluitwerk - toebehoren"]
["40.30.","ventilatieroosters - algemeen"]
["40.31.","ventilatieroosters - op glas"]
["40.31.10.","ventilatieroosters - op glas/kleprooster ","PM",null,"Geen",{"$nulls":4},1]
["40.32.","ventilatieroosters - op profiel"]
["40.32.10.","ventilatieroosters - op profiel/kleprooster ","PM",null,"Geen",{"$nulls":4},1]
["40.40","beglazing - algemeen"]
["40.40.10.","beglazing - prestaties"]
["40.41.","beglazing - enkel glas"]
["40.41.10.","beglazing - enkel glas/type 1 ","PM",null,"Geen",{"$nulls":4},1]
["40.42.","beglazing - dubbele beglazing"]
["40.42.10.","beglazing - dubbele beglazing/type 1 ","PM",null,"Geen",{"$nulls":4},1]
["40.42.20.","beglazing - dubbele beglazing/type 2 ","PM",null,"Geen",{"$nulls":4},1]
["40.43.","beglazing - drievoudige beglazing"]
["40.43.10.","beglazing - drievoudige beglazing/type 1 ","PM",null,"Geen",{"$nulls":4},1]
["40.43.20.","beglazing - driedubbele beglazing/type 2 ","PM",null,"Geen",{"$nulls":4},1]
["40.44.","beglazing - bijzondere beglazing"]
["40.44.10.","beglazing - bijzondere beglazing/dun monumentenglas ","PM",null,"Geen",{"$nulls":4},1]
["40.50.","vulelementen - algemeen"]
["40.51.","vulelementen - kunststof ","PM",null,"Geen",{"$nulls":4},1]
["40.52.","vulelementen - aluminium ","PM",null,"Geen",{"$nulls":4},1]
["40.53.","vulelementen - kunsthars ","PM",null,"Geen",{"$nulls":4},1]
["40.54.","vulelementen - vezelcement ","PM",null,"Geen",{"$nulls":4},1]
["40.55.","vulelementen - multiplexplaten  ","PM",null,"Geen",{"$nulls":4},1]
["40.56.","vulelementen - massief houten beplanking ","PM",null,"Geen",{"$nulls":4},1]
["40.60.","raamdorpels - algemeen"]
["40.70.","omkaderingselementen - algemeen"]
["40.71.","omkaderingselementen - hout ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten","Lengte omkaderingselement",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.72.","omkaderingselementen - aluminium ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten","omtrek dagkant uitgezonderd lengte dorpel",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten","Lengte omkaderingselement",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.80.","toebehoren - algemeen"]
["40.81.","toebehoren - brievenkleppen ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.82.","toebehoren - deurspionnen ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.83.","toebehoren - beschermplaten ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.84.","toebehoren - deurstoppen ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.85.","toebehoren - huisnummers ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.86.","toebehoren - deur- en naambordjes ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.87.","toebehoren - doorvalbeveiliging"]
["40.87.10.","toebehoren - doorvalbeveiliging/kokerprofiel ","FH","m ","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.87.20.","toebehoren - doorvalbeveiliging/glasplaat ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["41.","POORTEN & EXTERNE ZONWERING"]
["41.00.","poorten & externe zonwering - algemeen"]
["41.10.","kantelpoorten - algemeen"]
["41.11.","kantelpoorten - poortblad staal"]
["41.11.10.","kantelpoorten - poortblad staal/manueel ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.11.20.","kantelpoorten - poortblad staal/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.12.","kantelpoorten - poortblad hout"]
["41.12.10.","kantelpoorten - poortblad hout/manueel ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.12.20.","kantelpoorten - poortblad hout/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.13.","kantelpoorten - poortblad kunststof"]
["41.13.10.","kantelpoorten - poortblad kunststof/manueel ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.13.20.","kantelpoorten - poortblad kunststof/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.20.","sectionaalpoorten - algemeen"]
["41.21.","sectionaalpoorten - staal"]
["41.21.10.","sectionaalpoorten - staal/manueel ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.21.20.","sectionaalpoorten - staal/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.22.","sectionaalpoorten - aluminium"]
["41.22.10.","sectionaalpoorten - aluminium/manueel ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.22.20.","sectionaalpoorten - aluminium/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.30.","Externe zonnewering - algemeen",{"$nulls":6},"Uitbreiding op de basis VMSW artikellijst"]
["41.31.","Externe zonnewering - rolluiken","FH","m2","TYPE 4","Window","ARCHICAD property: VMSW zonnewering","W/D Opening Surface on the Reveal Side","Uitbreiding op de basis VMSW artikellijst",1]
["41.32.","Externe zonnewering - screens","FH","m2","TYPE 4","Window","ARCHICAD property: VMSW zonnewering","W/D Opening Surface on the Reveal Side","Uitbreiding op de basis VMSW artikellijst",1]
["42.","GEVELBEKLEDINGEN"]
["42.00.","gevelbekledingen - algemeen"]
["42.10.","regelstructuur - algemeen"]
["42.11.","regelstructuur - hout ","PM",null,"Geen",{"$nulls":4},1]
["42.12.","regelstructuur - aluminium ","PM",null,"Geen",{"$nulls":4},1]
["42.20.","thermische isolatie voorhanggevel - algemeen"]
["42.21.","thermische isolatie voorhanggevel - MW"]
["42.21.10.","thermische isolatie voorhanggevel - MW/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.21.20.","thermische isolatie voorhanggevel - MW/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.22.","thermische isolatie voorhanggevel - PUR of PIR"]
["42.22.10.","thermische isolatie voorhanggevel - PUR of PIR/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.22.20.","thermische isolatie voorhanggevel - PUR of PIR/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.23.","thermische isolatie voorhanggevel - PF"]
["42.23.10.","thermische isolatie voorhanggevel - PF/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.23.20.","thermische isolatie voorhanggevel - PF/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.24.","thermische isolatie voorhanggevel - EPS"]
["42.24.10.","thermische isolatie voorhanggevel - EPS/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.24.20.","thermische isolatie voorhanggevel - EPS/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.25.","thermische isolatie voorhanggevel - XPS"]
["42.25.10.","thermische isolatie voorhanggevel - XPS/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.25.20.","thermische isolatie voorhanggevel - XPS/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.30.","buitenfolie - algemeen"]
["42.31.","buitenfolie - gevelfolie ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["42.40.","bekledingspanelen - algemeen"]
["42.41.","bekledingspanelen - HPL ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["42.42.","bekledingspanelen - vezelcement ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["42.43.","bekledingspanelen - minerale vezels ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["42.50.","bekledingsplanchetten - algemeen"]
["42.51.","bekledingsplanchetten - massief hout ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["42.52.","bekledingsplanchetten - kunststof ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["42.53.","bekledingsplanchetten - vezelcement ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["42.60.","gevelleien - algemeen"]
["42.61.","gevelleien - vezelcementleien ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["42.70.","geprofileerde metaalplaten - algemeen"]
["42.71.","geprofileerde metaalplaten - gecoat staal ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["42.72.","geprofileerde metaalplaten - aluminium ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["43.","BUITENBEPLEISTERING"]
["43.00.","buitenbepleistering - algemeen"]
["43.10.","sierpleisters op metselwerk - algemeen"]
["43.11.","sierpleisters op metselwerk - minerale pleister ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["43.20.","buitengevelisolatiesystemen met pleister - algemeen"]
["43.21.","buitengevelisolatiesystemen met pleister - EPS"]
["43.21.10.","buitengevelisolatiesystemen met pleister - EPS/isolatie"]
["43.21.11.","buitengevelisolatiesystemen met pleister - EPS/isolatie - 14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["43.21.12.","buitengevelisolatiesystemen met pleister - EPS/isolatie - 16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["43.21.20.","buitengevelisolatiesystemen met pleister - EPS/pleister ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["43.22.","buitengevelisolatiesystemen met pleister - MW"]
["43.22.10.","buitengevelisolatiesystemen met pleister - MW/isolatie"]
["43.22.11.","buitengevelisolatiesystemen met pleister - MW/isolatie - 14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["43.22.12.","buitengevelisolatiesystemen met pleister - MW/isolatie - 16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["43.22.20.","buitengevelisolatiesystemen met pleister - MW/pleister ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["44.","BUITENTRAPPEN & BORSTWERINGEN"]
["44.00.","buitentrappen en borstweringen - algemeen"]
["44.10.","trappen - algemeen"]
["44.11.","trappen - staal ","FH","st","TYPE 5","Stair",null,"Stuks",null,1]
[null,null,"SOG"]
["44.20.","borstweringen - algemeen"]
["44.21.","borstweringen - staal ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
[null,null,null,"st","TYPE 5","Railing",null,"Stuks",null,1]
["44.22.","borstweringen - roestvast staal (RVS) ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["44.23.","borstweringen - aluminium ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["44.24.","borstweringen - veiligheidsglas ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["44.30.","trapleuningen - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["44.40.","vulpanelen en -roosters - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["44.50.","handgrepen - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["44.60.","brandladders - algemeen"]
["44.61.","brandladders - verzinkt staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Stair",null,"Stuks",null,1]
["44.62.","brandladders - aluminium ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":5},"Stair",null,"Stuks",null,1]
["50.","BINNENPLEISTERWERKEN"]
["50.00.","binnenpleisterwerken - algemeen"]
["50.10.","wandbepleistering - algemeen"]
["50.11.","wandbepleistering - gipspleisters"]
["50.11.10.","wandbepleistering - gipspleisters/dikpleister op metselwerk"]
["50.11.11.","wandbepleistering - gipspleisters/dikpleisters op metselwerk - wandvlakken ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["50.11.12.","wandbepleistering - gipspleisters/dikpleisters op metselwerk - dagkanten ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
["50.11.20.","wandbepleistering - gipspleisters/dunpleister op lijmblokken"]
["50.11.21.","wandbepleistering - gipspleisters/dunpleister op lijmblokken - wandvlakken ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["50.11.22.","wandbepleistering - gipspleisters/dunpleister op lijmblokken - dagkanten ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
["50.11.30.","wandbepleistering - gipspleisters/pleister op beplating"]
["50.11.31.","wandbepleistering - gipspleisters/pleister op beplating - wandvlakken ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["50.11.32.","wandbepleistering - gipspleisters/pleister op beplating - dagkanten ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
["50.11.40.","wandbepleistering - gipspleisters/pleister op gaas"]
["50.11.41.","wandbepleistering - gipspleisters/pleister op gaas - wandvlakken ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["50.11.42.","wandbepleistering - gipspleisters/pleister op gaas - dagkanten ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
["50.12.","wandbepleistering - cementpleisters"]
["50.12.10.","wandbepleistering - cementpleisters/te betegelen ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["50.12.20.","wandbepleistering - cementpleisters/afwerksysteem ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["50.20.","plafondbepleistering - algemeen"]
["50.21.","plafondbepleistering - gipspleisters"]
["50.21.10.","plafondbepleistering - gipspleisters/dikpleister op welfsels"]
["50.21.11.","plafondbepleistering - gipspleisters/dikpleister op welfsels - plafondoppervlakte ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["50.21.12.","plafondbepleistering - gipspleisters/dikpleister op welfsels - zijkanten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["50.21.20.","plafondbepleistering - gipspleisters/dunpleister op breedplaatvloeren "]
["50.21.21.","plafondbepleistering - gipspleisters/dunpleister op breedplaatvloeren - plafondoppervlakte ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["50.21.22.","plafondbepleistering - gipspleisters/dunpleister op breedplaatvloeren - zijkanten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["50.21.30.","plafondbepleistering - gipspleisters/pleister op beplating "]
["50.21.31.","plafondbepleistering - gipspleisters/pleister op beplating - plafondoppervlakte ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["50.21.32.","plafondbepleistering - gipspleisters/pleister op beplating - zijkanten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["50.21.40.","plafondbepleistering - gipspleisters/pleister op pleisterdrager "]
["50.21.41.","plafondbepleistering - gipspleisters/pleister op pleisterdrager - plafondoppervlakte ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["50.21.42.","plafondbepleistering - gipspleisters/pleister op pleisterdrager - zijkanten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["50.30.","renovatie pleisterwerk - algemeen ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["51.","BINNENPLAATAFWERKINGEN"]
["51.00.","binnenplaatafwerkingen - algemeen"]
["51.10.","lichte scheidingswanden - algemeen"]
["51.11.","lichte scheidingswanden - gipskartonplaten ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.12.","lichte scheidingswanden - gipsvezelplaten ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.13.","lichte scheidingswanden - calciumsilicaatplaten ","FH","m2","TYPE 2","Wall",null,null,null,1]
[null,"lichte scheidingswanden - vezelcementplaten ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.14.","lichte scheidingswanden - calciumsilicaatplaten ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.15.","lichte scheidingswanden - multiplexplaten ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.16.","lichte scheidingswanden - OSB-platen ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.17.","lichte scheidingswanden - MDF-platen","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.20.","voorzetwanden - algemeen"]
["51.21.","voorzetwanden - gipskartonplaten"]
["51.21.10.","voorzetwanden - gipskartonplaten/op regelstructuur ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.21.20.","voorzetwanden - gipskartonplaten/gekleefd ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.22.","voorzetwanden - gipsvezelplaten"]
["51.22.10.","voorzetwanden - gipsvezelplaten/op regelstructuur ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.22.20.","voorzetwanden - gipsvezelplaten/gekleefd ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.23.","voorzetwanden - vezelcementplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.24.","voorzetwanden - calciumsilicaatplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.25.","voorzetwanden - multiplex ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.26.","voorzetwanden - OSB-platen ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.27.","voorzetwanden - MDF-platen","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.30.","schachtwanden - algemeen"]
["51.31.","schachtwanden - gipskartonplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.32.","schachtwanden - gipsvezelplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.33.","schachtwanden - vezelcementplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.34.","schachtwanden - calciumsilicaatplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.35.","schachtwanden - multiplexplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.36.","schachtwanden - OSB-platen ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.37.","schachtwanden - MDF-platen","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.38.","schachtwanden - kunstharsplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.40.","toegangsluiken - algemeen"]
["51.41.","toegangsluiken - hout ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
[{"$nulls":5},"Window",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["51.42.","toegangsluiken - kunsthars ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
[{"$nulls":5},"Window",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["51.43.","toegangsluiken - vezelcement ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
[{"$nulls":5},"Window",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["51.44.","toegangsluiken - metalen kader ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
[{"$nulls":5},"Window",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["51.50.","plafondafwerking - algemeen"]
["51.51.","plafondafwerking - uitbekleding plafond"]
["51.51.10.","plafondafwerking - uitbekleding plafond/gipskartonplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,2]
[{"$nulls":5},"Shell",null,"Top Surface",null,2]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",2]
[{"$nulls":5},"Wall",null,"Netto oppervlak binnenkant wand",null,2]
["51.51.20.","plafondafwerking - uitbekleding plafond/gipsvezelplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.51.30.","plafondafwerking - uitbekleding plafond/vezelcementplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.51.40.","plafondafwerking - uitbekleding plafond/calciumsilicaatplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.51.50.","plafondafwerking - uitbekleding plafond/OSB","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.52.","plafondafwerking - uitbekleding daklichtopeningen ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 4","Object","gebruik ARCHICAD property: VMSW uitbekleding daglichtopeningen ",null,null,1]
[{"$nulls":5},"Skylight","gebruik ARCHICAD property: VMSW uitbekleding daglichtopeningen ",null,null,1]
[null,null,null,"m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Object","gebruik ARCHICAD property: VMSW uitbekleding daglichtopeningen ",null,null,1]
[{"$nulls":5},"Skylight","gebruik ARCHICAD property: VMSW uitbekleding daglichtopeningen ","Oppervlakte volgens openingshoogte daklicht en dikte dak",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["51.53.","plafondafwerking - verlaagd plafond"]
["51.53.10.","plafondafwerking - verlaagd plafond/gipskartonplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.53.20.","plafondafwerking - verlaagd plafond/gipsvezelplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.53.30.","plafondafwerking - verlaagd plafond/vezelcementplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.53.40.","plafondafwerking - verlaagd plafond/calciumsilicaatplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.60.","uitbekleding buitenramen en -deuren - algemeen"]
["51.61.","uitbekleding buitenramen en -deuren - isolatieplaten voor bepleistering ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["51.62.","uitbekleding buitenramen en -deuren - multiplex ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["51.63.","uitbekleding buitenramen en -deuren - MDF ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["51.64.","uitbekleding buitenramen en -deuren - massief hout ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["51.65.","uitbekleding buitenramen en -deuren - PVC ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["51.66.","uitbekleding buitenramen en -deuren - gipskarton ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["51.70.","uitbekleding sanitaire toestellen - algemeen"]
["51.71.","uitbekleding sanitaire toestellen - te betegelen plaat"]
["51.72.","uitbekleding sanitaire toestellen - plaat als eindafwerking"]
["52.","DEK- EN BEDRIJFSVLOEREN"]
["52.00.","dek- en bedrijfsvloeren - algemeen"]
["52.10.","isolerende uitvullagen - algemeen"]
["52.11.","isolerende uitvullagen - cementgebonden ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.12.","isolerende uitvullagen - schuimbeton ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.13.","isolerende uitvullagen - gespoten polyurethaan ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.14.","isolerende uitvullagen - droge granulaten ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.20.","vochtwerende lagen - algemeen"]
["52.21.","vochtwerende lagen - PE-folie ","PM",null,"Geen",{"$nulls":4},1]
["52.30.","thermische isolatie vloer - algemeen"]
["52.31.","thermische isolatie vloer - MW"]
["52.31.10.","thermische isolatie vloer - MW/8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.31.20.","thermische isolatie vloer - MW/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.32.","thermische isolatie vloer - PUR of PIR"]
["52.32.10.","thermische isolatie vloer - PUR of PIR 8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.32.20.","thermische isolatie vloer - PUR of PIR/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.33.","thermische isolatie vloer - PF"]
["52.33.10.","thermische isolatie vloer - PF/8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.33.20.","thermische isolatie vloer - PF/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.34.","thermische isolatie vloer - XPS"]
["52.34.10.","thermische isolatie vloer - XPS/8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.34.20.","thermische isolatie vloer - XPS/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.35.","thermische isolatie vloer - EPS"]
["52.35.10.","thermische isolatie vloer - EPS/8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.35.20.","thermische isolatie vloer - EPS/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.40.","akoestische isolatie vloer - algemeen"]
["52.41.","akoestische isolatie vloer - kunststofschuim ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.42.","akoestische isolatie vloer - kokosvezels ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.50.","cementgebonden dekvloeren - algemeen"]
["52.51.","cementgebonden dekvloeren - hechtend ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.52.","cementgebonden dekvloeren - niet hechtend ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.53.","cementgebonden dekvloeren - zwevend ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.54.","cementgebonden dekvloeren - zwevend en gepolierd ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.60.","calciumsulfaatgebonden dekvloeren - algemeen"]
["52.61.","calciumsulfaatgebonden dekvloeren - niet hechtend ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.62.","calciumsulfaatgebonden dekvloeren - zwevend ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.70.","bedrijfsvloeren - algemeen"]
["52.71.","bedrijfsvloeren - gepolierd beton ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.72.","bedrijfsvloeren - epoxymortel ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.","BINNENVLOERAFWERKINGEN"]
["53.00.","binnenvloerafwerkingen - algemeen"]
["53.10.","tegelvloeren - algemeen"]
["53.11.","tegelvloeren - keramisch"]
["53.11.10.","tegelvloeren - keramisch/getrokken tegels ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.11.20.","tegelvloeren - keramisch/geperste tegels ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.12.","tegelvloeren - marmermozaiek ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.13.","tegelvloeren - natuursteen"]
["53.13.10.","tegelvloeren - natuursteen/blauwe hardsteen ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.13.20.","tegelvloeren - natuursteen/travertijn ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.13.30.","tegelvloeren - natuursteen/jura ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.14.","tegelvloeren - betontegels ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.20.","soepele vloerbekledingen - algemeen"]
["53.21.","soepele vloerbekledingen - linoleum ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.22.","soepele vloerbekledingen - vinyl (PVC) ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.23.","soepele vloerbekledingen - rubber ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.24.","soepele vloerbekledingen - douchecellen ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.30.","houten vloerbekledingen - algemeen"]
["53.31.","houten vloerbekledingen - laminaat ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.32.","houten vloerbekledingen - opschuren bij renovatie ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.40.","plinten - algemeen"]
["53.41.","plinten - steen"]
["53.41.10.","plinten - steen/keramisch ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["53.41.20.","plinten - steen/marmermozaiek ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["53.41.30.","plinten - steen/natuursteen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["53.42.","plinten - hout"]
["53.42.10.","plinten - hout/massief hout ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["53.42.20.","plinten - hout/MDF ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["53.43.","plinten - soepel"]
["53.43.10.","plinten - soepel/linoleum ","FH\n","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["53.43.20.","plinten - soepel/PVC ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["53.43.30.","plinten - soepel/rubber ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["53.50.","tussendorpels - algemeen"]
["53.51.","tussendorpels - steen"]
["53.51.10.","tussendorpels - steen/natuursteen ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW tussendorpel binnendeur","breedte deuropening * muurdikte",null,1]
["53.51.20.","tussendorpels - steen/marmermozaiek ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW tussendorpel binnendeur","breedte deuropening * muurdikte",null,1]
["53.51.30.","tussendorpels - steen/composiet ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW tussendorpel binnendeur","breedte deuropening * muurdikte",null,1]
["53.60.","trapbekledingen - algemeen"]
["53.61.","trapbekledingen - steen"]
["53.61.10.","trapbekledingen - steen/keramisch ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks",null,1]
["53.61.20.","trapbekledingen - steen/marmermozaiek ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks",null,1]
["53.61.30.","trapbekledingen - steen/natuursteen ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks",null,1]
["53.62.","trapbekledingen - hout"]
["53.62.10.","trapbekledingen - hout/massief ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks",null,1]
["53.62.20.","trapbekledingen - hout/gelamineerd ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks",null,1]
["53.63.","trapbekledingen - soepel"]
["53.63.10.","trapbekledingen - soepel/rubber ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks",null,1]
["53.70.","toebehoren - algemeen"]
["53.71.","toebehoren - scheidingsprofielen ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["53.72.","toebehoren - vloermatkaders ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
[{"$nulls":5},"Wall",null,"Stuks",null,1]
["53.73.","toebehoren - vloermatten ","FH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[{"$nulls":5},"Object",null,"Net Area",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"st","TYPE 3","Slab",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["53.74.","toebehoren - vloerdeksels "]
["53.74.10.","toebehoren - vloerdeksels/metaal","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["53.74.20.","toebehoren - vloerdeksels/betegelbaar","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["53.75.","toebehoren - vloerroosters ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
[{"$nulls":5},"Wall",null,"Stuks",null,1]
["53.76.","toebehoren - zettingsprofielen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["54.","BINNENDEUREN en -RAMEN"]
["54.00.","binnendeuren en -ramen - algemeen"]
["54.01.","binnendeuren en -ramen - prestaties"]
["54.02.","binnendeuren en -ramen - keuring en proeven"]
["54.03.","binnendeuren en -ramen - proefopstelling"]
["54.10.","deurkozijnen - algemeen"]
["54.11.","deurkozijnen - hout"]
["54.11.10.","deurkozijnen - hout/massief ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks",null,1]
["54.11.20.","deurkozijnen - hout/multiplex ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks",null,1]
["54.11.30.","deurkozijnen - hout/MDF ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks",null,1]
["54.12.","deurkozijnen - staal"]
["54.12.10.","deurkozijnen - staal/montagekozijn ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks",null,1]
["54.12.20.","deurkozijnen - staal/inbouwkozijn ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks",null,1]
["54.20.","deurbladen - algemeen"]
["54.21.","deurbladen - hout met holle kern"]
["54.21.10.","deurbladen - hout met holle kern/celrooster ","FH","st","TYPE 4","Door ","Gebruik ARCHICAD property: VMSW deurblad","Stuks",null,1]
["54.21.20.","deurbladen - hout met holle kern/tubespaan ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurblad","Stuks",null,1]
["54.22.","deurbladen - hout met volle kern"]
["54.22.10.","deurbladen - hout met volle kern/spaan ","FH","st","TYPE 4","Door ","Gebruik ARCHICAD property: VMSW deurblad","Stuks",null,1]
["54.22.20.","deurbladen - hout met volle kern/multiplex ","FH","st","TYPE 4","Door ","Gebruik ARCHICAD property: VMSW deurblad","Stuks",null,1]
["54.30.","deurgehelen - algemeen"]
["54.31.","deurgehelen - kozijnen hout"]
["54.31.10.","deurgehelen - kozijnen hout/brandwerend ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.31.20.","deurgehelen - kozijnen hout/inbraakwerend ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.31.30.","deurgehelen - kozijnen hout/passiefdeur ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.32.","deurgehelen - kozijnen staal"]
["54.32.10.","deurgehelen - kozijnen staal/brandwerend ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.32.20.","deurgehelen - kozijnen staal/inbraakwerend ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.40.","schuif- en vouwdeuren - algemeen"]
["54.41.","schuif- en vouwdeuren - schuifsystemen"]
["54.41.10.","schuif- en vouwdeuren - schuifsystemen/voorbouw ","FH","st","TYPE 5","Door ",null,"Stuks",null,1]
[{"$nulls":5},"Window ",null,"Stuks",null,1]
["54.41.20.","schuif- en vouwdeuren - schuifsystemen/inbouwmodule ","FH","st","TYPE 5","Door ",null,"Stuks",null,1]
[{"$nulls":5},"Window ",null,"Stuks",null,1]
["54.42.","schuif- en vouwdeuren - vouwsystemen"]
["54.42.10.","schuif- en vouwdeuren - vouwsystemen/kunststof ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
[{"$nulls":5},"Window",null,"Stuks",null,1]
["54.50.","glazen deuren - algemeen"]
["54.51.","glazen deuren - opendraaiend ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.52.","glazen deuren - openschuivend ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.60.","hang- en sluitwerk - algemeen"]
["54.61.","hang- en sluitwerk - scharnieren en paumellen"]
["54.61.10.","hang- en sluitwerk - scharnieren en paumellen/aluminium ","PM",null,"Geen",{"$nulls":4},1]
["54.61.20.","hang- en sluitwerk - scharnieren en paumellen/vernikkeld staal ","PM",null,"Geen",{"$nulls":4},1]
["54.61.30.","hang- en sluitwerk - scharnieren en paumellen/roestvast staal ","PM",null,"Geen",{"$nulls":4},1]
["54.62.","hang- en sluitwerk - deursloten"]
["54.62.10.","hang- en sluitwerk - deursloten/klaviersloten ","PM",null,"Geen",{"$nulls":4},1]
["54.62.20.","hang- en sluitwerk - deursloten/veiligheidssloten ","PM",null,"Geen",{"$nulls":4},1]
["54.62.30.","hang- en sluitwerk - deursloten/elektromagnetisch ","PM",null,"Geen",{"$nulls":4},1]
["54.62.40.","hang- en sluitwerk - deursloten/kantschuiven ","PM",null,"Geen",{"$nulls":4},1]
["54.62.50.","hang- en sluitwerk - deursloten/panieksluitingen ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW panieksluiting","Stuks",null,1]
["54.63.","hang- en sluitwerk - deurkrukken"]
["54.63.10.","hang- en sluitwerk - deurkrukken/aluminium ","PM",null,"Geen",{"$nulls":4},1]
["54.63.20.","hang- en sluitwerk - deurkrukken/RVS ","PM",null,"Geen",{"$nulls":4},1]
["54.63.30.","hang- en sluitwerk - deurkrukken/kunststof ","PM",null,"Geen",{"$nulls":4},1]
["54.64.","hang- en sluitwerk - vaste handgrepen ","PM",null,"Geen",{"$nulls":4},1]
["54.65.","hang- en sluitwerk - deurdrangers ","PM",null,"Geen",{"$nulls":4},1]
["54.70.","vaste binnenramen - algemeen"]
["54.71.","vaste binnenramen - hout ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
["54.80.","toebehoren - algemeen"]
["54.81.","toebehoren - deurroosters"]
["54.82.","toebehoren - beschermplaten"]
["54.82.10.","toebehoren - beschermplaten/aluminium ","PM",null,"Geen",{"$nulls":4},1]
["55.","BINNENTRAPPEN EN LEUNINGEN"]
["55.00.","binnentrappen en leuningen - algemeen"]
["55.10.","trappen - algemeen"]
["55.11.","trappen - hout"]
["55.11.10.","trappen - hout/rechte treden ","FH","st","TYPE 5","Stair",null,"Stuks",null,1]
["55.11.20.","trappen - hout/verdreven treden ","FH","st","TYPE 5","Stair",null,"Stuks",null,1]
["55.12.","trappen - staal"]
["55.12.10.","trappen - staal/rechte treden ","FH","st","TYPE 5","Stair",null,"Stuks",null,1]
["55.12.20.","trappen - staal/verdreven treden ","FH","st","TYPE 5","Stair",null,"Stuks",null,1]
["55.20.","borstweringen - algemeen"]
["55.21.","borstweringen - hout ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["55.22.","borstweringen - staal ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["55.23.","borstweringen - roestvast staal ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["55.24.","borstweringen - aluminium ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["55.25.","borstweringen - veiligheidsglas ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["55.30.","handgrepen - algemeen"]
["55.31.","handgrepen - hout ","PM",null,"Geen",{"$nulls":4},1]
["55.32.","handgrepen - staal ","PM",null,"Geen",{"$nulls":4},1]
["55.33.","handgrepen - roestvast staal ","PM",null,"Geen",{"$nulls":4},1]
["55.34.","handgrepen - aluminium ","PM",null,"Geen",{"$nulls":4},1]
["55.40.","zoldertrappen en -luiken - algemeen"]
["55.41.","zoldertrappen en -luiken - hout ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["55.42.","zoldertrappen en -luiken - aluminium ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.","VAST BINNENMEUBILAIR",{"$nulls":5},"wat met samengestelde onderdelen?"]
["56.00.","vast binnenmeubilair - algemeen"]
["56.10.","keukenmeubelen - algemeen"]
["56.11.","keukenmeubelen - onderdelen"]
["56.11.10.","keukenmeubelen - onderdelen/stelpoten en plintplaat ","PM",null,"Geen",{"$nulls":4},1]
["56.11.20.","keukenmeubelen - onderdelen/corpus en leggers ","PM",null,"Geen",{"$nulls":4},1]
["56.11.30.","keukenmeubelen - onderdelen/fronten en zichtwanden ","PM",null,"Geen",{"$nulls":4},1]
["56.11.40.","keukenmeubelen - onderdelen/werkbladen ","PM",null,"Geen",{"$nulls":4},1]
["56.11.50.","keukenmeubelen - onderdelen/beslag en handgrepen ","PM",null,"Geen",{"$nulls":4},1]
["56.11.60.","keukenmeubelen - onderdelen/toebehoren ","PM",null,"Geen",{"$nulls":4},1]
["56.12.","keukenmeubelen - type 1 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.13.","keukenmeubelen - type 2 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.14.","keukenmeubelen - type 3 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.20.","badkamermeubelen - algemeen"]
["56.21.","badkamermeubelen - onderdelen"]
["56.21.10.","badkamermeubelen - onderdelen/stelpoten en plintplaat ","PM",null,"Geen",{"$nulls":4},1]
["56.21.20.","badkamermeubelen - onderdelen/corpus en leggers ","PM",null,"Geen",{"$nulls":4},1]
["56.21.30.","badkamermeubelen - onderdelen/fronten en zichtwanden ","PM",null,"Geen",{"$nulls":4},1]
["56.21.40.","badkamermeubelen - onderdelen/wastafeltabletten ","PM",null,"Geen",{"$nulls":4},1]
["56.21.50.","badkamermeubelen - onderdelen/beslag en handgrepen ","PM",null,"Geen",{"$nulls":4},1]
["56.21.60.","badkamermeubelen - onderdelen/toebehoren ","PM",null,"Geen",{"$nulls":4},1]
["56.22.","badkamermeubelen - type 1 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.23.","badkamermeubelen - type 2 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.24.","badkamermeubelen - type 3 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.30.","inbouwkasten - algemeen"]
["56.31.","inbouwkasten - onderdelen"]
["56.31.10.","inbouwkasten - onderdelen/stelpoten en plintplaat ","PM",null,"Geen",{"$nulls":4},1]
["56.31.20.","inbouwkasten - onderdelen/corpus en leggers ","PM",null,"Geen",{"$nulls":4},1]
["56.31.30.","inbouwkasten - onderdelen/fronten en zichtwanden ","PM",null,"Geen",{"$nulls":4},1]
["56.31.40.","inbouwkasten - onderdelen/tabletten en bureelbladen ","PM",null,"Geen",{"$nulls":4},1]
["56.31.50.","inbouwkasten - onderdelen/beslag en handgrepen ","PM",null,"Geen",{"$nulls":4},1]
["56.31.60.","inbouwkasten - onderdelen/toebehoren ","PM",null,"Geen",{"$nulls":4},1]
["56.32.","inbouwkasten - kastgeheel type 1 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.33.","inbouwkasten - kastgeheel type 2 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.34.","inbouwkasten - kastgeheel type 3 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.40.","parlofoonconsoles - algemeen"]
["56.41.","parlofoonconsoles - multiplexplaat ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["56.42.","parlofoonconsoles - kunstharsplaat ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["56.43.","parlofoonconsoles - metaalplaat"]
["56.43.10.","parlofoonconsoles - metaalplaat/gemoffeld staal ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["56.43.20.","parlofoonconsoles - metaalplaat/roestvast staal (RVS) ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["56.43.30.","parlofoonconsoles - metaalplaat/aluminium ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["56.50.","brievenbusgehelen - algemeen"]
["56.51.","brievenbusgehelen - multiplexplaat ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
["56.52.","brievenbusgehelen - kunstharsplaat ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
["56.53.","brievenbusgehelen - metaalplaat"]
["56.53.10.","brievenbusgehelen - metaalplaat/gemoffeld staal ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
["56.53.20.","brievenbusgehelen - metaalplaat/roestvast staal (RVS) ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
["56.53.30.","brievenbusgehelen - metaalplaat/gemoffeld aluminium ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
["56.60.","gordijnkasten - algemeen"]
["56.61.","gordijnkasten - hout"]
["56.61.10.","gordijnkasten - hout/massief ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Reference line length",null,1]
["56.61.20.","gordijnkasten - hout/houtspaanplaat ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Reference line length",null,1]
["56.61.30.","gordijnkasten - hout/multiplex ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Reference line length",null,1]
["56.61.40.","gordijnkasten - hout/MDF ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"Reference line length",null,1]
["56.62.","gordijnkasten - kunststof ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[]
["57.","TABLET- EN WANDBEKLEDINGEN"]
["57.00.","tablet- en wandbekledingen - algemeen"]
["57.10.","venstertabletten - algemeen"]
["57.11.","venstertabletten - natuursteen"]
["57.11.10.","venstertabletten - natuursteen/marmer ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.11.20.","venstertabletten - natuursteen/blauwe hardsteen ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.11.30.","venstertabletten - natuursteen/leisteen ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.11.40.","venstertabletten - natuursteen/volgens prestaties ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.12.","venstertabletten - kunststeen"]
["57.12.10.","venstertabletten - kunststeen/marmermozaïek ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.12.20.","venstertabletten - kunststeen/vezelcement ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.12.30.","venstertabletten - kunststeen/composiet ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.13.","venstertabletten - hout"]
["57.13.10.","venstertabletten - hout/massief ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.13.20.","venstertabletten - hout/laminaat ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.14.","venstertabletten - kunststof"]
["57.14.10.","venstertabletten - kunststof/PVC ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.20.","wandbekledingen - algemeen"]
["57.21.","wandbekledingen - betegeling ","FH","m2","TYPE 3","Wall",null,"Netto oppervlakte binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["57.21.10.","wandbekledingen - betegeling/keramisch ","FH","m2","TYPE 3","Wall",null,"Netto oppervlakte binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["60.","SANITAIR LEIDINGNET"]
["60.00.","sanitair leidingnet - algemeen"]
["60.10.","afvoerbuizen - algemeen"]
["60.11.","afvoerbuizen - PVC ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["60.12.","afvoerbuizen - PE ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["60.13.","afvoerbuizen - PP ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["60.20.","verluchtingsbuizen - algemeen"]
["60.21.","verluchtingsbuizen - PVC ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.22.","verluchtingsbuizen - PE ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.23.","verluchtingsbuizen - beluchtingsventielen ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.30.","klokroosters - intern - algemeen"]
["60.31.","klokroosters - gietijzer ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.32.","klokroosters - aluminium ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.33.","klokroosters - roestvast staal (RVS) ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.34.","klokroosters - kunststof ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.40.","putdeksels - algemeen"]
["60.41.","putdeksels - gietijzer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.42.","putdeksels - aluminium ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.43.","putdeksels - roestvast staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.44.","putdeksels - kunststof ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.50.","sanitaire drukleidingen - algemeen"]
["60.51.","sanitaire drukleidingen - buizen"]
["60.51.10.","sanitaire drukleidingen - buizen/verzinkt staal ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.51.20.","sanitaire drukleidingen - buizen/koper ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.51.30.","sanitaire drukleidingen - buizen/kunststof ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.52.","sanitaire drukleidingen - collectoren ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.53.","sanitaire drukleidingen - leidingisolatie ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.54.","sanitaire drukleidingen - brandwerende doorvoeren ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.55.","sanitaire drukleidingen - verwarmingslint ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["60.56.","sanitaire drukleidingen - flexibele leidingen ","PM",null,"Geen",{"$nulls":4},1]
["60.60.","aansluiting leidingnet - algemeen"]
["60.61.","aansluiting leidingnet - reglementaire meterstraat ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["60.62.","aansluiting leidingnet - voedingsleidingen & tellers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["60.63.","aansluiting leidingnet - waterfilters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["60.70.","waterbehandeling - algemeen"]
["60.71.","waterbehandeling - ontharders ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["60.72.","waterbehandeling - filters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.","SANITAIRE TOESTELLEN & TOEBEHOREN"]
["61.00.","sanitaire toestellen en toebehoren - algemeen"]
["61.10.","toiletpotten en toebehoren - algemeen"]
["61.11.","toiletpotten en toebehoren - staand ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.12.","toiletpotten en toebehoren - hangend ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.20.","handwastafels en toebehoren - algemeen"]
["61.21.","handwastafels & toebehoren - wandmodel"]
["61.21.10.","handwastafels & toebehoren - wandmodel/porselein ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.22.","handwastafels en toebehoren - inbouwmodel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.30.","wastafels en toebehoren - algemeen"]
["61.31.","wastafels en toebehoren - wandmodel"]
["61.31.10.","wastafels en toebehoren - wandmodel/porselein ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.32.","wastafels en toebehoren - inbouwmodel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.40.","baden - algemeen"]
["61.41.","baden - geëmailleerd staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.42.","baden - acrylaat ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.50.","douches - algemeen"]
["61.51.","douches - geëmailleerd staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.52.","douches - acrylaat ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.53.","douches - tegeldouche ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.60.","speciale toebehoren - algemeen"]
["61.61.","speciale toebehoren - rail en douchegordijn ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.62.","speciale toebehoren - douchedeuren en -wanden ","FH","st","TYPE 3","Wall",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Door",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
[{"$nulls":5},"Window",null,"Stuks",null,1]
["61.63.","speciale toebehoren - muurhandgrepen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.64.","speciale toebehoren - douchezitjes ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.70.","afwastafels - algemeen"]
["61.71.","afwastafels - opbouwmodel"]
["61.71.10.","afwastafels - opbouwmodel/roestvast staal (RVS) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.72.","afwastafels - inbouwmodel"]
["61.72.10.","afwastafels - inbouwmodel/roestvast staal (RVS) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.80.","uitgietbakken - algemeen"]
["61.81.","uitgietbakken - sanitair porselein ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.","SANITAIRE KRANEN & KLEPPEN"]
["62.00.","sanitaire kranen - kleppen - algemeen"]
["62.10.","terugslagkleppen - algemeen"]
["62.11.","terugslagkleppen - messing ","PM",null,"Geen",{"$nulls":4},1]
["62.20.","installatieafsluitkranen - algemeen"]
["62.21.","installatieafsluitkranen - messing"]
["62.21.10.","installatieafsluitkranen - messing/zonder aftapkraan ","PM",null,"Geen",{"$nulls":4},1]
["62.21.20.","installatieafsluitkranen - messing/met aftapkraan ","PM",null,"Geen",{"$nulls":4},1]
["62.22.","installatieafsluitkranen - kunststof"]
["62.22.10.","installatieafsluitkranen - kunststof/zonder aftapkraan ","PM",null,"Geen",{"$nulls":4},1]
["62.30.","wandafsluitkranen - algemeen"]
["62.31.","wandafsluitkranen - enkelvoudige stopkraan ","PM",null,"Geen",{"$nulls":4},1]
["62.32.","wandafsluitkranen - stopkraan met dienstkraan ","PM",null,"Geen",{"$nulls":4},1]
["62.40.","dienstkranen - algemeen"]
["62.41.","dienstkranen - enkele dienstkraan"]
["62.41.10.","dienstkranen - enkele dienstkraan/vaste uitloop ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.41.20.","dienstkranen - enkele dienstkraan/draaibare uitloop ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.42.","dienstkranen - dubbele dienstkraan"]
["62.42.10.","dienstkranen - dubbele dienstkraan/binnen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.42.20.","dienstkranen - dubbele dienstkraan/buiten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.50.","ééngatskranen - algemeen"]
["62.51.","ééngatskranen - handwastafelkraan ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.52.","ééngatskranen - lavabomengkraan ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.53.","ééngatskranen - afwastafelmengkraan ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.60.","muurmengkranen - algemeen"]
["62.61.","muurmengkranen - badmengkraan & armatuur ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.62.","muurmengkranen - douchemengkraan/armatuur ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.63.","muurmengkranen - afwastafelmengkraan ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.70.","regenwaterpompen - algemeen"]
["62.71.","regenwaterpompen - zelfaanzuigende hydrofoorgroep ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.72.","regenwaterpompen - dompelpomp ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.73.","regenwaterpompen - handpomp ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.","SANITAIR WARM WATER"]
["63.00.","sanitair warm water - algemeen"]
["63.10.","doorstroomwaterverwarmers op gas - algemeen"]
["63.11.","doorstroomwaterverwarmers op gas - badgeisers"]
["63.11.10.","doorstroomwaterverwarmers op gas - badgeisers/type B11BS ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.11.20.","doorstroomwaterverwarmers op gas - badgeisers/type C13-C33 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.12.","doorstroomwaterverwarmers op gas - keukengeisers"]
["63.12.10.","doorstroomwaterverwarmers op gas - keukengeisers/type AAS ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.20.","voorraadtoestellen op gas ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.30.","elektroboilers - algemeen"]
["63.31.","elektroboilers - kokend water toestellen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.32.","elektroboilers - inbouwmodel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.33.","elektroboilers - spaarboilers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.40.","voorraadboilers indirecte opwarming - algemeen"]
["63.41.","voorraadboilers indirecte opwarming - enkelvoudige warmtewisselaar ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.42.","voorraadboilers indirecte opwarming - dubbelvoudige warmtewisselaar ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.50.","zonneboilers - algemeen"]
["63.51.","zonneboilers - collectoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.52.","zonneboilers - opslagvat ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.53.","zonneboilers - leidingsysteem en toebehoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.54.","zonneboilers - circulatoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.55.","zonneboilers - expansiesysteem ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.56.","zonneboilers - regelsystemen en beveiliging"]
["63.56.10.","zonneboilers - regelsystemen en beveiliging/aflaat- en vulkranen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["63.56.20.","zonneboilers - regelsystemen en beveiliging/regelkranen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["63.56.30.","zonneboilers - regelsystemen en beveiliging/ontluchters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["63.56.40.","zonneboilers - regelsystemen en beveiliging/veiligheidskleppen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["63.56.50.","zonneboilers - regelsystemen en beveiliging/keerkleppen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["63.56.60.","zonneboilers - regelsystemen en beveiliging/mengventielen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["63.60.","warmtepompboilers - algemeen"]
["63.70.","satellietsystemen - algemeen "]
["63.71.","satellietsystemen - voorraadboilers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.72.","satellietsystemen - platenwisselaars ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["64.","GASINSTALLATIES"]
["64.00.","gasinstallaties - algemeen"]
["64.10.","gasleidingen - algemeen"]
["64.11.","gasleidingen - staal ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["64.12.","gasleidingen - koper ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["64.13.","gasleidingen - PE ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["64.14.","gasleidingen - PLT-buissysteem ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["64.20.","gaskranen - algemeen"]
["64.21.","gaskranen - gasfilter ","PM",null,"Geen",{"$nulls":4},1]
["64.22.","gaskranen - afsluitkranen ","PM",null,"Geen",{"$nulls":4},1]
["64.30.","gasaansluiting ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["64.40.","gastoestellen - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["65.","VERWARMING INDIVIDUELE INSTALLATIES"]
["65.00.","verwarming individuele installaties - algemeen"]
["65.01.","verwarming individuele installaties - proefopstelling ","PM",null,"Geen",{"$nulls":4},1]
["65.02.","verwarming individuele installaties - grenzen van de aanneming ","PM",null,"Geen",{"$nulls":4},1]
["65.10.","gasvloerketels - algemeen"]
["65.11.","gasvloerketels - open"]
["65.11.10.","gasvloerketels - open/enkel CV ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.11.20.","gasvloerketels - open/CV & SWW (voorraad) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.12.","gasvloerketels - gesloten"]
["65.12.10.","gasvloerketels - gesloten/enkel CV ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.12.20.","gasvloerketels - gesloten/CV & SWW (voorraad) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.20.","gaswandketels - algemeen"]
["65.21.","gaswandketels - gesloten"]
["65.21.10.","gaswandketels - gesloten/enkel CV ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.21.20.","gaswandketels - gesloten/CV & SWW (doorstroom) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.21.30.","gaswandketels - gesloten/CV & SWW (voorraad) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.30.","leidingnet & toebehoren - algemeen"]
["65.31.","leidingnet & toebehoren - buizen"]
["65.31.10.","leidingnet & toebehoren - buizen/staal ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["65.31.20.","leidingnet & toebehoren - buizen/koper ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["65.31.30.","leidingnet & toebehoren - buizen/kunststof ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["65.31.40.","leidingnet & toebehoren - buizen/dunwandige verzinkte buis ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["65.32.","leidingnet & toebehoren - collectoren ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["65.33.","leidingnet & toebehoren - leidingisolatie ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":5},"Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["65.34.","leidingnet & toebehoren - brandwerende doorvoeren ","PM",null,"Geen",{"$nulls":4},1]
["65.35.","leidingnet & toebehoren - verwarmingslint ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["65.40.","installatieonderdelen - algemeen"]
["65.41.","installatieonderdelen - aflaatkranen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.42.","installatieonderdelen - regel- en afsluitkranen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.43.","installatieonderdelen - drukregelaars ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.44.","installatieonderdelen - circulatoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["65.45.","installatieonderdelen - expansiesysteem ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.46.","installatieonderdelen - vlotterontluchters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.47.","installatieonderdelen - microbellenafscheider ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.50.","verwarmingselementen & toebehoren - algemeen"]
["65.51.","verwarmingselementen & toebehoren - plaatradiatoren ","FH","kW","TYPE 5","Object",null,"vul het vermogen in bij ARCHICAD property: Vermogen verwarmingselement",null,1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["65.52.","verwarmingselementen & toebehoren - wandconvectoren ","FH","kW","TYPE 5","Object",null,"vul het vermogen in bij ARCHICAD property: Vermogen verwarmingselement",null,1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["65.60.","warmteregeling & toebehoren - algemeen"]
["65.63.","warmteregeling & toebehoren - kamerthermostaten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["66.","BIJZONDERE INSTALLATIES"]
["66.00.","bijzondere installaties - algemeen"]
["66.10.","warmtepompen - algemeen"]
["66.11.","warmtepompen - grond-water ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["66.12.","warmtepompen - water-water ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["66.13.","warmtepompen - lucht-water monoblok ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["66.14.","warmtepompen - lucht-water met binnen- en buitenunit (split-systeem) ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["66.15.","warmtepompen - gasabsorptiewarmtepompen"]
["66.16.","warmtepompen - verticale aardsondes ","SOG",null,"Geen",{"$nulls":4},1]
["66.16.10.","warmtepompen - verticale aardsondes/warmtewisselaar ","FH","SOG","Geen",{"$nulls":4},1]
["66.16.20.","warmtepompen - verticale aardsondes/collector ","PM",null,"Geen",{"$nulls":4},1]
["67.","BRANDBESTRIJDING"]
["67.00.","brandbestrijding - algemeen"]
["67.10.","brandblusapparaten - algemeen"]
["67.11.","brandblusapparaten - poedersnelblussers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.12.","brandblusapparaten - CO2-snelblussers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.13.","brandblusapparaten - schuimsnelblussers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.14.","brandblusapparaten - vast opgestelde poederblussers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.20.","externe bluswatervoorziening - algemeen ","SOG",null,"Geen",{"$nulls":4},1]
["67.21.","externe bluswatervoorziening - leidingen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["67.22.","externe bluswatervoorziening - buitenhydranten"]
["67.22.10.","externe bluswatervoorziening - buitenhydranten/bovengronds ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.22.20.","externe bluswatervoorziening - buitenhydranten/ondergronds ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.30.","interne bluswatervoorziening - algemeen ","SOG",null,"Geen",{"$nulls":4},1]
["67.31.","interne bluswatervoorziening - leidingen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["67.32.","interne bluswatervoorziening - brandkranen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.33.","interne bluswatervoorziening - muurhaspels zonder kast ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.34.","interne bluswatervoorziening - kasten voor slanghaspels ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.35.","interne bluswatervoorziening - manometers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.36.","interne bluswatervoorziening - pictogrammen ","PM",null,"Geen",{"$nulls":4},1]
["67.40.","sprinklerinstallatie - algemeen ","SOG",null,"Geen",{"$nulls":4},1]
["67.50.","brandwerende bescherming - algemeen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["68.","VENTILATIE"]
["68.00.","ventilatie - algemeen"]
["68.01.","ventilatie - proefopstelling ","PM",null,"Geen",{"$nulls":4},1]
["68.02.","ventilatie - proeven"]
["68.02.10.","ventilatie - proeven/debietmeting ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["68.02.20.","ventilatie - proeven/meting kanaaldichtheid ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["68.02.30.","ventilatie - proeven/dichtheid collectieve kanalen ","SOG",null,"Geen",{"$nulls":4},1]
["68.10.","ventilatiekanalen - algemeen"]
["68.11.","ventilatiekanalen - metaal"]
["68.11.10.","ventilatiekanalen - metaal/rond ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["68.11.20.","ventilatiekanalen - metaal/rechthoekig ","FH of SOG","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"Geen",{"$nulls":4},1]
["68.12.","ventilatiekanalen - kunststof"]
["68.12.10.","ventilatiekanalen - kunststof/rond ","FH of SOG","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"Geen",{"$nulls":4},1]
["68.12.20.","ventilatiekanalen - kunststof/rechthoekig of ovaal ","FH of SOG","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"Geen",{"$nulls":4},1]
["68.13.","ventilatiekanalen - flexibele kanalen ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["68.14.","ventilatiekanalen - thermische isolatie ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["68.15.","ventilatiekanalen - ophanging en bevestiging ","PM",null,"Geen",{"$nulls":4},1]
["68.20.","toebehoren ventilatiekanalen - algemeen"]
["68.30.","woonhuisventilatoren - algemeen"]
["68.31.","woonhuisventilatoren - systeem C ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.32.","woonhuisventilatoren - systeem D ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.40.","ventilatoren - algemeen"]
["68.41.","ventilatoren - dakventilatoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.42.","ventilatoren - kanaalventilatoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.43.","ventilatoren - sanitaire ventilatoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.50.","dampkappen - algemeen"]
["68.51.","dampkappen - inbouwmotor ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.52.","dampkappen - motorloos ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.60.","ventilatieventielen en -roosters - algemeen"]
["68.61.","ventilatiemonden - ventiel met regelbare conus ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.62.","ventilatiemonden - zelfregelend ventiel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.63.","ventilatiemonden - gevelroosters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.64.","ventilatiemonden - dakventielen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["69.","OPBOUWKANALEN ROOKGAS EN VENTILATIE"]
["69.00.","opbouwkanalen rookgas en ventilatie - algemeen"]
["69.10.","schoorstenen - algemeen"]
["69.11.","schoorstenen - roestvast staal"]
["69.11.10.","schoorstenen - roestvast staal/CLV ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.11.20.","schoorstenen - roestvast staal/enkelvoudig kanaal ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.11.30.","schoorstenen - roestvast staal/buigzame kanaalvoering ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.12.","schoorstenen - aluminium"]
["69.12.10.","schoorstenen - aluminium/CLV ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.12.20.","schoorstenen - aluminium/enkelvoudig ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.12.30.","schoorstenen - aluminium/buigzame kanaalvoering ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.13.","schoorstenen - kunststof "]
["69.13.10.","schoorstenen - kunststof/CLV ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.13.20.","schoorstenen - kunststof/enkelvoudig ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.13.30.","schoorstenen - kunststof/buigzame kanaalvoering ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.20.","dakdoorgang - algemeen"]
["69.21.","dakdoorgang - enkelvoudig ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["69.22.","dakdoorgang - multifunctioneel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["70.","ELEKTRICITEIT BINNENNET"]
["70.00.","elektriciteit binnennet - algemeen"]
["70.10.","aansluitingen - algemeen"]
["70.11.","aansluitingen - ondergrondse aansluiting ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["70.12.","aansluitingen - aansluitbocht ","PM",null,"Geen",{"$nulls":4},1]
["70.13.","aansluitingen - aansluitplaat ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["70.14.","aansluitingen - tellerkasten ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["70.15.","aansluitingen - verbindingskabels ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["70.20.","verdeelkasten - algemeen"]
["70.21.","verdeelkasten - hoofdverdeelborden ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["70.30.","stroombeveiliging - algemeen"]
["70.31.","stroombeveiliging - hoofdschakelaars ","PM",null,"Geen",{"$nulls":4},1]
["70.32.","stroombeveiliging - differentieelschakelaars ","PM",null,"Geen",{"$nulls":4},1]
["70.33.","stroombeveiliging - automatische schakelaars ","PM",null,"Geen",{"$nulls":4},1]
["70.40.","aarding - algemeen"]
["70.41.","aarding - aardingslus ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"v","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["70.42.","aarding - afzonderlijke aardverbindingen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["70.43.","aarding - aardingsonderbrekers ","PM",null,"Geen",{"$nulls":4},1]
["70.44.","aarding - hoofdbeschermingsgeleiders ","PM",null,"Geen",{"$nulls":4},1]
["70.45.","aarding - hoofdequipotentiaalverbindingen ","PM",null,"Geen",{"$nulls":4},1]
["70.46.","aarding - bijkomende equipotentiaalverbindingen ","PM",null,"Geen",{"$nulls":4},1]
["70.47.","aarding - bliksemafleidersinstalatie ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Bliksemafleiderinstallatie","Stuks",null,1]
["70.50.","leidingen - algemeen"]
["70.53.","leidingen - inbouw kabelbuizen ","PM",null,"Geen",{"$nulls":4},1]
["70.54.","leidingen - opbouw kabelbuizen ","PM",null,"Geen",{"$nulls":4},1]
["70.55.","leidingen - plint- & wandkanalen ","PM",null,"Geen",{"$nulls":4},1]
["70.56.","leidingen - kabelgoten en -ladders ","PM",null,"Geen",{"$nulls":4},1]
["70.57.","leidingen - wachtbuizen ","PM",null,"Geen",{"$nulls":4},1]
["70.60.","trek- en verbindingsdozen - algemeen"]
["70.61.","trek- en verbindingsdozen - inbouw metselwerk ","PM",null,"Geen",{"$nulls":4},1]
["70.62.","trek- en verbindingsdozen - inbouw holle wanden ","PM",null,"Geen",{"$nulls":4},1]
["70.63.","trek- en verbindingsdozen - inbouw verlaagde plafonds ","PM",null,"Geen",{"$nulls":4},1]
["70.64.","trek- en verbindingsdozen - inbouw vloeren ","PM",null,"Geen",{"$nulls":4},1]
["70.65.","trek- en verbindingsdozen - opbouw ","PM",null,"Geen",{"$nulls":4},1]
["70.70.","bijzondere voorzieningen - algemeen"]
["70.71.","bijzondere voorzieningen - voeding liften ","PM",null,"Geen",{"$nulls":4},1]
["71.","ELEKTRICITEIT SCHAKELAARS & CONTACTDOZEN"]
["71.00.","elektriciteit schakelaars & contactdozen - algemeen"]
["71.10.","stopcontacten - algemeen"]
["71.11.","stopcontacten - 10/16A ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.12.","stopcontacten - 20/32A ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.20.","aansluitdozen - algemeen"]
["71.21.","aansluitdozen - voeding elektrisch fornuis ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.22.","aansluitdozen - voeding was- & vaatwasmachine ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.23.","aansluitdozen - voeding HVAC en andere ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.30.","schakelaars - algemeen"]
["71.31.","schakelaars - enkelpolig ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.32.","schakelaars - dubbelpolig ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.33.","schakelaars - wissel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.34.","schakelaars - kruis ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.35.","schakelaars - timerschakelaars ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.36.","schakelaars - teleruptoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.37.","schakelaars - dimmers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.40.","speciale toebehoren - algemeen"]
["71.41.","speciale toebehoren - bewegingsdetectoren ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Schakelaar Toebehoren ","Stuks",null,1]
["71.42.","speciale toebehoren - foto-elektrisch schakelaar ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Schakelaar Toebehoren ","Stuks",null,1]
["71.43.","speciale toebehoren - schemerschakelaar ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Schakelaar Toebehoren ","Stuks",null,1]
["72.","ELEKTRICITEIT LICHTARMATUREN"]
["72.00.","elektriciteit lichtarmaturen - algemeen"]
["72.10.","binnenarmaturen E27 - algemeen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["72.11.","binnenarmaturen E27 - met lenskap ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["72.12.","binnenarmaturen E27 - andere ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["72.20.","binnenarmaturen TL - algemeen"]
["72.21.","binnenarmaturen TL - opbouwarmatuur plafond"]
["72.21.10.","binnenarmaturen TL - opbouwarmatuur plafond - T8 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["72.21.20.","binnenarmaturen TL - opbouwarmatuur plafond - T5 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["72.22.","binnenarmaturen TL - lichtstrip keukenaanrecht ",null,null,"TYPE 5",null,null,"Stuks",null,1]
["72.22.10.","binnenarmaturen TL - lichtstrip keukenaanrecht/T8 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["72.22.20.","binnenarmaturen TL - lichtstrip keukenaanrecht/T5 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["72.40.","binnenarmaturen halogeen - algemeen"]
["72.41.","binnenarmaturen halogeen - transfo ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["72.42.","binnenarmaturen halogeen - inbouwspots ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["72.43.","binnenarmaturen halogeen - opbouwspots ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["72.50.","veiligheidsverlichting - algemeen"]
["72.51.","veiligheidsverlichting - autonoom niet-permanent ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["72.52.","veiligheidsverlichting - autonoom permanent ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["72.53.","veiligheidsverlichting - centrale noodvoeding ","SOG",null,"Geen",{"$nulls":4},1]
["72.54.","veiligheidsverlichting - armaturen ","SOG",null,"Geen",{"$nulls":4},1]
["72.55.","veiligheidsverlichting - signalisatie & pictogrammen ","PM",null,"Geen",{"$nulls":4},1]
["72.60.","buitenarmaturen - algemeen"]
["72.70.","armaturen geleverd door het bestuur - algemeen"]
["73.","ELEKTRICITEIT BEL & PARLOFOON"]
["73.00.","elektriciteit bel & parlofoon - algemeen"]
["73.10.","individuele belinstallaties - algemeen"]
["73.11.","individuele belinstallaties - huisbel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["73.12.","individuele belinstallaties - beldrukknop ","PM",null,"Geen",{"$nulls":4},1]
["73.13.","individuele belinstallaties - beltransfo ","PM",null,"Geen",{"$nulls":4},1]
["73.14.","individuele belinstallaties - bedrading ","PM",null,"Geen",{"$nulls":4},1]
["73.20.","parlofooninstallatie - algemeen"]
["73.21.","parlofooninstallatie - binnenposten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["73.22.","parlofooninstallatie - deurstation ","PM",null,"Geen",{"$nulls":4},1]
["73.23.","parlofooninstallatie - beltransfo ","PM",null,"Geen",{"$nulls":4},1]
["73.24.","parlofooninstallatie - verdeeldozen ","PM",null,"Geen",{"$nulls":4},1]
["73.25.","parlofooninstallatie - bedrading ","PM",null,"Geen",{"$nulls":4},1]
["73.26.","parlofooninstallatie - elektrisch deurslot ","PM",null,"Geen",{"$nulls":4},1]
["73.30.","toegangscontrolesysteem - algemeen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["74.","ELEKTRICITEIT TELECOM & DOMOTICA"]
["74.00.","elektriciteit telecom & domotica - algemeen"]
["74.10.","telefoon - algemeen"]
["74.11.","telefoon - buitenbekabeling ","SOG",null,"Geen",{"$nulls":4},1]
["74.12.","telefoon - basis aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.13.","telefoon - extra aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.14.","telefoon - binnenbekabeling ","PM",null,"Geen",{"$nulls":4},1]
["74.20.","kabeldistributie - algemeen"]
["74.21.","kabeldistributie - buitenbekabeling ","SOG",null,"Geen",{"$nulls":4},1]
["74.22.","kabeldistributie - basis aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.23.","kabeldistributie - extra aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.24.","kabeldistributie - binnenbekabeling ","PM",null,"Geen",{"$nulls":4},1]
["74.30.","netwerkbekabeling - algemeen"]
["74.31.","netwerkbekabeling - buitenbekabeling ","SOG",null,"Geen",{"$nulls":4},1]
["74.32.","netwerkbekabeling - basis aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.33.","netwerkbekabeling - extra aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.34.","netwerkbekabeling - binnenbekabeling ","PM",null,"Geen",{"$nulls":4},1]
["74.40.","satelietontvangstsysteem - algemeen"]
["74.41.","satelietontvangstsysteem - centrale schotelantenne ","SOG",null,"Geen",{"$nulls":4},1]
["74.42.","satelietontvangstsysteem - buitenbekabeling ","SOG",null,"Geen",{"$nulls":4},1]
["74.43.","satelietontvangstsysteem - basis aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.44.","satelietontvangstsysteem - extra aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.45.","satelietontvangstsysteem - binnenbekabeling ","PM",null,"Geen",{"$nulls":4},1]
["74.50.","alarmkabel - algemeen"]
["74.60.","luidsprekerkabel - algemeen"]
["74.70.","oproepsystemen ADL - algemeen"]
["74.80.","multimediakast","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["75.","ELEKTRICITEIT VERWARMING"]
["75.00.","elektriciteit verwarming - algemeen"]
["75.10.","direct systeem - algemeen"]
["75.11.","direct systeem - gedecentraliseerd"]
["75.11.10.","direct systeem - gedecentraliseerd/wandconvectoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["75.11.20.","direct systeem - gedecentraliseerd/plintconvectoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["75.11.30.","direct systeem - gedecentraliseerd/stralingselementen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["75.20.","accumulatiesysteem - algemeen"]
["75.21.","accumulatiesysteem - gedecentraliseerd"]
["75.21.10.","accumulatiesysteem - gedecentraliseerd/dynamisch gemengd ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["75.30.","meet- & regeltoestellen - algemeen"]
["75.31.","meet- & regeltoestellen - klokthermostaten "]
["75.31.10.","meet- & regeltoestellen - klokthermostaten/direct systeem ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["75.31.20.","meet- & regeltoestellen - klokthermostaten/accumulatie systeem ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["76.","ELEKTROMECHANICA LIFTEN"]
["76.00.","elektromechanica liften - algemeen"]
["76.01.","algemeen - grenzen van de aanneming ","PM",null,"Geen",{"$nulls":4},1]
["76.02.","algemeen - controle op afmetingen ","PM",null,"Geen",{"$nulls":4},1]
["76.03.","algemeen - documentatie en studie ","PM",null,"Geen",{"$nulls":4},1]
["76.04.","algemeen - werfinstallatie en -organisatie ","PM",null,"Geen",{"$nulls":4},1]
["76.05.","algemeen - onderhoud tijdens waarborgperiode ","PM",null,"Geen",{"$nulls":4},1]
["76.10.","bestaande installaties - algemeen"]
["76.11.","bestaande installaties - afbraak ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Lift Bestaande installaties","Stuks",null,1]
["76.12.","bestaande installaties - renovatie ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Lift Bestaande installaties","Stuks",null,1]
["76.20.","elektrische liften - algemeen"]
["76.21.","elektrische liften - met machinekamer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["76.22.","elektrische liften - zonder machinekamer (gearless) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["76.30.","kooiuitrusting - algemeen"]
["76.31.","kooiuitrusting - personenlift ","PM",null,"Geen",{"$nulls":4},1]
["76.32.","kooiuitrusting - goederenlift ","PM",null,"Geen",{"$nulls":4},1]
["76.33.","kooiuitrusting - vandalismewerend ","PM",null,"Geen",{"$nulls":4},1]
["76.40.","deuren & fronten - algemeen"]
["76.41.","deuren & fronten - personenlift ","PM",null,"Geen",{"$nulls":4},1]
["76.50.","bedienings- & signalisatiepanelen - algemeen"]
["76.51.","bedienings- & signalisatiepanelen - personenlift ","PM",null,"Geen",{"$nulls":4},1]
["77.","BRANDDETECTIE & ALARMSYSTEMEN"]
["77.00.","branddetectie & alarmsystemen - algemeen"]
["77.10.","centrale eenheid - algemeen ","SOG",null,"Geen",{"$nulls":4},1]
["77.20.","energievoorziening - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["77.30.","bekabeling - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["77.40.","brandmelding - algemeen"]
["77.41.","brandmelding - branddetectoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["77.42.","brandmelding - handmelders ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["77.43.","brandmelding - gasdetectoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["77.44.","brandmelding - autonome rookmelders ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["77.50.","alarmsirenes - algemeen"]
["77.51.","alarmsirenes - signal fast sweep ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["77.60.","evacuatietoebehoren - algemeen"]
["77.61.","evacuatietoebehoren - deurpomp met magneethouder ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurpomp","Stuks",null,1]
["77.62.","evacuatietoebehoren - pictogrammen ","PM",null,"Geen",{"$nulls":4},1]
["77.63.","evacuatietoebehoren - brandweersleutelkluis","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["80.","BINNENSCHILDERWERKEN"]
["80.00.","schilderwerken - algemeen"]
["80.10.","binnenschilderwerken op pleisterwerk - algemeen"]
["80.11.","binnenschilderwerken op pleisterwerk - acrylaathars ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.12.","binnenschilderwerken op pleisterwerk - acrylaatdispersie ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.13.","binnenschilderwerken op pleisterwerk - vinyllatex ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.14.","binnenschilderwerken op pleisterwerk - kwartshoudende structuurverf ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.15.","binnenschilderwerken op pleisterwerk - meerkleurige effectverf ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.20.","binnenschilderwerken op gipskartonplaten - algemeen"]
["80.21.","binnenschilderwerken op gipskartonplaten - acrylaathars ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.22.","binnenschilderwerken op gipskartonplaten - acrylaatdispersie ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.23.","binnenschilderwerken op gipskartonplaten - vinyllatex ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.24.","binnenschilderwerken op gipskartonplaten - kwartshoudende structuurverf ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.25.","binnenschilderwerken op gipskartonplaten - meerkleurige effectverf ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.30.","binnenschilderwerken op beton - algemeen"]
["80.31.","binnenschilderwerken op beton - acrylaathars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.32.","binnenschilderwerken op beton - acrylaatdispersie ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.33.","binnenschilderwerken op beton - vinyllatex ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.34.","binnenschilderwerken op beton - kwartshoudende structuurverf ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.35.","binnenschilderwerken op beton - meerkleurig effectverf ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.36.","binnenschilderwerken op beton - epoxyverf ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.40.","binnenschilderwerken op metselwerk - algemeen"]
["80.41.","binnenschilderwerken op metselwerk - acrylaathars ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.42.","binnenschilderwerken op metselwerk - acrylaatdispersie ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.43.","binnenschilderwerken op metselwerkwerk - vinyllatex ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.44.","binnenschilderwerken op metselwerk - kwartshoudende structuurverf ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.45.","binnenschilderwerken op metselwerk - meerkleurige effectverf ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.50.","binnenschilderwerken op hout en houtachtige platen - algemeen"]
["80.51.","binnenschilderwerken op hout en houtachtige platen - lak"]
["80.51.10.","op hout en houtachtige platen - lak/acryllaatdispersie ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.51.20.","op hout en houtachtige platen - lak/polyurethaan acrylaathars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.51.30.","op hout en houtachtige platen - lak/alkyd-urethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.51.40.","op hout en houtachtige platen - lak/alkydhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.52.","binnenschilderwerken op hout en houtachtige platen - vernis"]
["80.52.10.","op hout en houtachtige platen - vernis / acrylurethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.52.20.","op hout en houtachtige platen - vernis/polyurethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.52.30.","op hout en houtachtige platen - vernis/alkydurethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.53.","binnenschilderwerken op hout en houtachtige platen - beits ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.60.","binnenschilderwerken op metaal - algemeen"]
["81.","BEHANGWERKEN"]
["81.00.","behangwerken - algemeen"]
["81.10.","verwijderen van behangpapier - algemeen ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["81.20.","behangen met glasvezeldoek - algemeen"]
["81.21.","behangen met glasvezeldoek - op nieuw pleisterwerk ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["81.22.","behangen met glasvezeldoek - op oud pleisterwerk ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["81.23.","behangen met glasvezeldoek - op gipskartonplaten ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.","BUITENSCHILDERWERKEN"]
["82.00.","buitenschilderwerken - algemeen"]
["82.10.","buitenschilderwerken op buitenbepleistering - algemeen"]
["82.11.","buitenschilderwerken op buitenbepleisteringen - acrylaatdispersie ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.12.","buitenschilderwerken op buitenbepleisteringen - siloxaan ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.13.","buitenschilderwerken op buitenbepleisteringen - silicaat ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.20.","buitenschilderwerken op beton - algemeen"]
["82.21.","buitenschilderwerken op beton - acrylaatdispersie ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.22.","buitenschilderwerken op beton - siloxaan ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.23.","buitenschilderwerken op beton - silicaat ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.24.","buitenschilderwerken op beton - kwartshoudende structuurverf ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.30.","buitenschilderwerken op gevelmetselwerk - algemeen"]
["82.31.","buitenschilderwerken op gevelmetselwerk - acrylaatdispersie ","FH","m2","TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.32.","buitenschilderwerken op gevelmetselwerk - siloxaan ","FH","m2","TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.33.","buitenschilderwerken op gevelmetselwerk - silicaat ","FH","m2","TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.34.","buitenschilderwerken op gevelmetselwerk - kwartshoudende structuurverf ","FH","m2","TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.40.","buitenschilderwerken op hout en houtachtige platen - algemeen"]
["82.41.","buitenschilderwerken op hout en houtachtige platen - lak"]
["82.41.10.","op hout en houtachtige platen - lak/acryllaatdispersie watergedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.41.20.","op hout en houtachtige platen - lak/alkyd-urethaan watergedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.41.30.","op hout en houtachtige platen - lak/alkydhars solventgedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.41.40.","op hout en houtachtige platen - lak/urethaan-alkyd solventgedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.42.","buitenschilderwerken op hout en houtachtige platen - vernis"]
["82.42.10.","op hout en houtachtige platen - vernis/alkyd-urethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.43.","buitenschilderwerken op hout en houtachtige platen - beits"]
["82.43.10.","op hout en houtachtige platen - beits/alkydhars watergedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.43.20.","op hout en houtachtige platen - beits/alkydhars solventgedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":5},"Column",null,"Top Surface",null,1]
[{"$nulls":5},"Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.50.","nabehandelingen op metselwerk - algemeen"]
["82.51.","nabehandelingen op metselwerk - hydrofobering ","FH","m2","TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.52.","nabehandelingen op metselwerk - antigraffiti ","FH","m2","TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":5},"Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.60.","buitenschilderwerken op metaal - algemeen"]
["90.","BUITENVERHARDINGEN"]
["90.00.","buitenverhardingen - algemeen"]
["90.10.","funderingen - algemeen"]
["90.11.","funderingen - steenslag"]
["90.11.10.","funderingen - steenslag/niet-continue korrelverdeling ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.11.20.","funderingen - steenslag/continue korrelverdeling zonder toevoegsels ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.11.30.","funderingen - steenslag/continue korrelverdeling met toevoegsels ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.12.","funderingen - ternair mengsel ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.13.","funderingen - zandcement ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.14.","funderingen - schraal beton"]
["90.14.10.","funderingen - schraal beton/ongewapend ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.14.20.","funderingen - schraal beton/gewapend ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.20.","verhardingen - algemeen"]
["90.21.","verhardingen - in rijen te leggen kasseien ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.22.","verhardingen - mozaïekkeien ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.23.","verhardingen - betonstraatstenen"]
["90.23.10.","verhardingen - betonstraatstenen/kleurvast ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.23.20.","verhardingen - betonstraatstenen/waterdoorlatend ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.24.","verhardingen - gebakken straatstenen ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.25.","verhardingen - betontegels"]
["90.25.10.","verhardingen - betontegels/kleurvast ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.25.20.","verhardingen - betontegels/waterdoorlatend ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.25.30.","verhardingen - betontegels/grasbetontegels ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.25.40.","verhardingen - betontegels/silexbetontegels ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.26.","verhardingen - tegels in natuursteen ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.27.","verhardingen - dolomiet ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.28.","verhardingen - gepolierd beton ","FH of VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["90.29.","verhardingen - tactiele oppervlakken ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.30.","lijnvormige elementen - algemeen"]
["90.31.","lijnvormige elementen - boordstenen"]
["90.31.10.","lijnvormige elementen - boordstenen/beton"]
["90.31.11.","lijnvormige elementen - boordstenen/beton - prefab ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["90.31.12.","lijnvormige elementen - boordstenen/beton - ter plaatse gestort ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["90.31.20.","lijnvormige elementen - boordstenen/palissaden ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["90.31.30.","lijnvormige elementen - boordstenen/metaal ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["90.32.","lijnvormige elementen - watergreppels"]
["90.32.10.","lijnvormige elementen - watergreppels/beton"]
["90.32.11.","lijnvormige elementen - watergreppels/beton - prefab ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["91.","BUITENCONSTRUCTIES EN AFSLUITINGEN"]
["91.00.","buitenconstructies en afsluitingen - algemeen"]
["91.10.","tuinafsluitingspalen - algemeen"]
["91.11.","tuinafsluitingspalen - staal ","PM",null,"Geen",{"$nulls":4},1]
["91.12.","tuinafsluitingspalen - hout ","PM",null,"Geen",{"$nulls":4},1]
["91.13.","tuinafsluitingspalen - beton ","PM",null,"Geen",{"$nulls":4},1]
["91.20.","draadafsluitingen - algemeen"]
["91.21.","draadafsluitingen - gladde draad ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["91.22.","draadafsluitingen - draadgaas ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["91.30.","tuinschermen - algemeen"]
["91.31.","tuinschermen - schapenhek ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["91.32.","tuinschermen - houtschermen ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["91.33.","tuinschermen - betonplaten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["91.40.","tuinhekken - algemeen"]
["91.41.","tuinhekken - staal ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["91.42.","tuinhekken - hout ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["91.50.","terrassen tuinhout - algemeen"]
["91.51.","terrassen tuinhout - tegels ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["91.52.","terrassen tuinhout - beplanking ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["91.60.","constructies tuinhout - algemeen"]
["92.","BUITENMEUBILAIR EN UITRUSTINGSELEMENTEN"]
["92.00.","buitenmeubilair en uitrustingselementen - algemeen"]
["92.10.","brievenbussen - algemeen"]
["92.11.","brievenbussen - geleverd door het bestuur ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.12.","brievenbussen - prefab beton ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.13.","brievenbussen - staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.14.","brievenbussen - aluminium ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.20.","vuilnisbakken - algemeen"]
["92.21.","vuilnisbakken - geleverd door het bestuur ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.22.","vuilnisbakken - staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.23.","vuilnisbakken - kunststof ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.30.","fietsrekken - algemeen"]
["92.31.","fietsrekken - blokken beton ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.32.","fietsrekken - modules staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.33.","fietsrekken - aanleunbeugels staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.34.","fietsrekken - ophangelementen staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.35.","fietsrekken - klemmen staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.40.","parkingelementen - algemeen"]
["92.41.","parkingelementen - parkeerpalen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.42.","parkingelementen - parkeerbeugels ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.50.","zitbanken - algemeen"]
["92.51.","zitbanken - geleverd door het bestuur ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.52.","zitbanken - zonder rugleuning ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.53.","zitbanken - met rugleuning ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.60.","boomomrandingen - algemeen"]
["92.61.","boomomrandingen - roosters beton ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.62.","boomomrandingen - roosters gietijzer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.63.","boomomrandingen - roosters kunststof ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.64.","boomomrandingen - roosters staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.70.","plantbescherming - algemeen"]
["92.71.","plantbescherming - boombeugels staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.73.","plantbescherming - boomkorven staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.74.","plantbescherming - plantkorven staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["93.","GROENAANLEG EN -ONDERHOUD"]
["93.00.","groenaanleg en -onderhoud - algemeen"]
["93.10.","grondbewerkingen - algemeen"]
["93.11.","grondbewerkingen - diepspitten ","PM",null,"Geen",{"$nulls":4},1]
["93.12.","grondbewerkingen - egaliseren ","PM",null,"Geen",{"$nulls":4},1]
["93.13.","grondbewerkingen - frezen ","PM",null,"Geen",{"$nulls":4},1]
["93.20.","verwerking teelaarde - algemeen"]
["93.21.","verwerking teelaarde - afkomstig van afgraving ","FH/VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["93.22.","verwerking teelaarde - te leveren door de aannemer ","FH/VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["93.30.","verwerken van bodemverbeteringsmiddelen - algemeen ","FH/VH","kg","TYPE 4","Slab","vul de ARCHICAD property 'Soortelijk gewicht' in","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Mesh","vul de ARCHICAD property 'Soortelijk gewicht' in","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":5},"Morph","vul de ARCHICAD property 'Soortelijk gewicht' in","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["93.40.","aanleg grasmatten - algemeen"]
["93.41.","aanleg grasmatten - door bezaaiing ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["93.42.","aanleg grasmatten - door bezoding ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["93.50.","aanplanting houtachtige vegetaties - algemeen"]
["93.51.","aanplanting houtachtige vegetaties - bomen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["93.52.","aanplanting houtachtige gewassen - hagen ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
[{"$nulls":5},"Wall",null,"Stuks",null,1]
["93.53.","aanplanting houtachtige gewassen - heesters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["93.60.","hulpmiddelen groenaanleg - algemeen"]
["93.61.","hulpmiddelen groenaanleg - boompaalconstructies ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW hulpmiddelen groenaanleg","Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["93.62.","hulpmiddelen groenaanleg - boomroosters ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW hulpmiddelen groenaanleg","Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["93.63.","hulpmiddelen groenaanleg - ondergrondse verankering van bomen ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW hulpmiddelen groenaanleg","Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["93.64.","hulpmiddelen groenaanleg - groeiplaatsverbetering van bomen (irrigatie) ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW hulpmiddelen groenaanleg","Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["93.65.","hulpmiddelen groenaanleg - haagsteun ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["93.70.","groenonderhoud - algemeen"]
["93.71.","groenonderhoud - maaien van grasmatten ","FH","m2","TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["93.72.","groenonderhoud - bomen snoeien ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW bomen snoeien","Stuks",null,1]
["93.73.","groenonderhoud - scheren van hagen en beplantingsmassieven ","FH","m2","TYPE 4","Morph","Gebruik ARCHICAD Property: VMSW_scheren van hagen en beplantingsmassieven","Surface Area",null,1]
[{"$nulls":5},"Wall","Gebruik ARCHICAD Property: VMSW_scheren van hagen en beplantingsmassieven","Top Surface",null,1]
["93.74.","groenonderhoud - snoeien van heesters ","FH","st","TYPE 5",null,null,"Stuks",null,1]
[]
["0","DEEL"]
[1,"DEEL"]
[2,"DEEL"]
[3,"DEEL"]
[4,"DEEL"]
[5,"DEEL"]
[6,"DEEL"]
[7,"DEEL"]
[8,"DEEL"]
[9,"DEEL"]
["23.","DORPELS, PLINTEN EN DEKSTENEN"]

{"sheet":"types","index":1,"n_rows":5,"n_cols":2,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
["TYPE 1","BUILDING MATERIAL CONVERSIE 20.XX.XX."]
["TYPE 2","BUILDING MATERIAL ONDERVERDELING NAAR DIKTES"]
["TYPE 3","BUILDING MATERIAL AS IT IS"]
["TYPE 4","ARCHICAD PROPERTY"]
["TYPE 5","CLASSIFICATION"]