{"text_format":"2","workbook":"xlsx","n_sheets":13,"sheets":["Overzicht","Types","00 Algem bepalingen","10 Onderbouw","20 Bovenbouw","30 Dak","40 Gevelsluiting","50 Afwerking (bi)","60 Installaties ","70 Electriciteit","80 Binnenschilderw","90 Buitenverhardingen","Volledige artikellijst"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Overzicht","index":0,"n_rows":32,"n_cols":4,"rows_kept":32,"cut":false,"hidden":false,"merged":[[2,1,2,3]]}
[]
[]
[null,"This document was exported from Numbers. Each table was converted to an Excel worksheet. All other objects on each Numbers sheet were placed on separate worksheets. Please be aware that formula calculations may differ in Excel."]
[]
[]
[]
[null,"Numbers Sheet Name","Numbers Table Name","Excel Worksheet Name"]
[]
[null,"00 Algemene bepalingen"]
[null,null,"Table 1","00 Algemene bepalingen"]
[null,"10 Onderbouw"]
[null,null,"Table 1","10 Onderbouw"]
[null,"20 Bovenbouw"]
[null,null,"Table 1","20 Bovenbouw"]
[null,"30 Dak"]
[null,null,"Table 1","30 Dak"]
[null,"40 Gevelsluiting"]
[null,null,"Table 1","40 Gevelsluiting"]
[null,"50 Afwerking (bi)"]
[null,null,"Table 1","50 Afwerking (bi)"]
[null,"60 Installaties "]
[null,null,"Table 1","60 Installaties "]
[null,"70 Electriciteit "]
[null,null,"Table 1","70 Electriciteit"]
[null,"80 Binnenschilderwerken"]
[null,null,"Table 1","80 Binnenschilderwerken"]
[null,"90 Volledige artikellijst"]
[null,null,"Table 1","90 Buitenverhardingen"]
[null,"Publicatie Art.NR en elementen"]
[null,null,"Table 1","Publicatie Art.NR en elementen"]
[null,"Types"]
[null,null,"Table 1","Types"]

{"sheet":"Types","index":1,"n_rows":5,"n_cols":2,"rows_kept":5,"cut":false,"hidden":false,"merged":[]}
["TYPE 1","BUILDING MATERIAL + layer + dikte >  CONVERSIE 20.XX.XX."]
["TYPE 2","BUILDING MATERIAL + dikte > ONDERVERDELING NAAR DIKTES 20.13.XX."]
["TYPE 3","BUILDING MATERIAL > Classificatie"]
["TYPE 4","Element/object > ARCHICAD PROPERTY"]
["TYPE 5","Element/object > Classificatie"]

{"sheet":"00 Algem bepalingen","index":2,"n_rows":333,"n_cols":10,"rows_kept":333,"cut":false,"hidden":false,"merged":[]}
["Artikelnummer","Artikelomschrijving","AvO","Eenheid","Type","Element","Element specificatie","Wat rekent de Meetstaat Manager?","Aandachtspunten","Column1"]
[{"$nulls":9},"Totaal"]
["00.","ALGEMENE BEPALINGEN"]
["00.10.","projectgegevens"]
["00.20.","ontwerpteam"]
["00.21.","ontwerpteam - architecturaal ontwerp",null,null,"Geen",{"$nulls":4},1]
["00.22.","ontwerpteam - studie stabiliteit",null,null,"Geen",{"$nulls":4},1]
["00.23.","ontwerpteam - studie technieken",null,null,"Geen",{"$nulls":4},1]
["00.24.","ontwerpteam - veiligheidscoördinatie",null,null,"Geen",{"$nulls":4},1]
["00.25.","ontwerpteam - EPB verslaggeving",null,null,"Geen",{"$nulls":4},1]
["00.30.","documenten"]
["00.31.","documenten - architectuur",null,null,"Geen",{"$nulls":4},1]
["00.32.","documenten - stabiliteit",null,null,"Geen",{"$nulls":4},1]
["00.33.","documenten - technieken",null,null,"Geen",{"$nulls":4},1]
["00.34.","documenten - veiligheidscoördinatie",null,null,"Geen",{"$nulls":4},1]
["00.35.","documenten - EPB verslaggeving",null,null,"Geen",{"$nulls":4},1]
["00.36.","documenten - diepsonderingsverslag",null,null,"Geen",{"$nulls":4},1]
["00.37.","documenten - verslag milieutechnisch bodemonderzoek",null,null,"Geen",{"$nulls":4},1]
["01.","AANNEMINGSMODALITEITEN"]
["01.00.","aannemingsmodaliteiten - algemeen"]
["01.01.","aannemingsmodaliteiten - bestek ","PM",null,"Geen",{"$nulls":4},1]
["01.02.","aannemingsmodaliteiten - voorafgaand plaatsbezoek ","PM",null,"Geen",{"$nulls":4},1]
["01.03.","aannemingsmodaliteiten - burgerlijke aansprakelijkheid ","PM",null,"Geen",{"$nulls":4},1]
["01.04.","aannemingsmodaliteiten - volledigheid van inschrijving ","PM",null,"Geen",{"$nulls":4},1]
["01.05.","aannemingsmodaliteiten - onderaanneming ","PM",null,"Geen",{"$nulls":4},1]
["01.06.","aannemingsmodaliteiten - verrekeningen ","PM",null,"Geen",{"$nulls":4},1]
["01.07.","aannemingsmodaliteiten - keuringsattesten ","PM",null,"Geen",{"$nulls":4},1]
["01.08.","aannemingsmodaliteiten - materialenlijst ","PM",null,"Geen",{"$nulls":4},1]
["01.10.","plaatsbeschrijvingen - algemeen"]
["01.11.","plaatsbeschrijvingen - aangrenzende constructies"]
["01.11.10.","plaatsbeschrijvingen – aangrenzende constructies/bij aanvang van de werken","PM",null,"Geen",{"$nulls":4},1]
["01.11.20.","plaatsbeschrijvingen – aangrenzende constructies/staat van vergelijking","PM",null,"Geen",{"$nulls":4},1]
["01.12.","plaatsbeschrijvingen - te renoveren constructies",null,null,"Geen",{"$nulls":4},1]
["01.12.10.","plaatsbeschrijvingen – te renoveren constructies/bij aanvang van de werken","PM",null,"Geen",{"$nulls":4},1]
["01.12.20.","plaatsbeschrijvingen – te renoveren constructies/staat van vergelijking","PM",null,"Geen",{"$nulls":4},1]
["01.13.","plaatsbeschrijvingen - inboedel bij blijvende bewoning"]
["01.13.10.","plaatsbeschrijvingen – inboedel bij blijvende bewoning/bij aanvang van de werken","PM",null,"Geen",{"$nulls":4},1]
["01.13.20.","plaatsbeschrijvingen – inboedel bij blijvende bewoning/staat van vergelijking","PM",null,"Geen",{"$nulls":4},1]
["01.14.","plaatsbeschrijvingen - wegenis en voetpaden"]
["01.14.10.","plaatsbeschrijvingen – wegenis en voetpaden bij aanvang van de werken","PM",null,"Geen",{"$nulls":4},1]
["01.14.20.","plaatsbeschrijvingen – wegenis en voetpaden/staat van vergelijking","PM",null,"Geen",{"$nulls":4},1]
["01.15.","plaatsbeschrijvingen - beplanting"]
["01.15.10.","plaatsbeschrijvingen – beplanting/bij aanvang van de werken","PM",null,"Geen",{"$nulls":4},1]
["01.15.20.","plaatsbeschrijvingen – beplanting/staat van vergelijking","PM",null,"Geen",{"$nulls":4},1]
["01.20.","werfcoördinatie - algemeen"]
["01.21.","werfcoördinatie - planning van de werken ","PM",null,"Geen",{"$nulls":4},1]
["01.22.","werfcoördinatie - werfleiding en controle ","PM",null,"Geen",{"$nulls":4},1]
["01.23.","werfcoördinatie - werfvergaderingen ","PM",null,"Geen",{"$nulls":4},1]
["01.24.","werfcoördinatie - uitzetten bouwwerken ","PM",null,"Geen",{"$nulls":4},1]
["01.25.","werfcoördinatie - as-builtdossier ","PM",null,"Geen",{"$nulls":4},1]
["01.26.","werfcoördinatie - renovaties met blijvende bewoning ","PM",null,"Geen",{"$nulls":4},1]
["01.30.","werfcondities - algemeen"]
["01.31.","werfcondities - orde en netheid ","PM",null,"Geen",{"$nulls":4},1]
["01.32.","werfcondities - geluids- en stofhinder ","PM",null,"Geen",{"$nulls":4},1]
["01.33.","werfcondities - nazorg ","PM",null,"Geen",{"$nulls":4},1]
["01.40.","veiligheidsvoorschriften - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["02.","BOUWPLAATSVOORZIENINGEN"]
["02.00.","bouwplaatsvoorzieningen - algemeen"]
["02.10.","beschermingswerken - algemeen"]
["02.11.","beschermingwerken - openbare weg ","PM",null,"Geen",{"$nulls":4},1]
["02.12.","beschermingswerken - beplantingen"]
["02.12.10.","beschermingswerken – beplantingen/bomen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["02.12.20.","beschermingswerken – beplantingen/struiken en hagen","PM"]
["02.20.","opruiming beplantingen - algemeen"]
["02.21.","opruiming beplantingen - bomen ","PM ",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["02.22.","opruiming beplantingen - struiken en hagen ","PM",null,"Geen",{"$nulls":4},1]
["02.30.","toegangswegen - algemeen"]
["02.31.","toegangswegen - voorlopige verharding voor voetgangers ","PM",null,"Geen",{"$nulls":4},1]
["02.32.","toegangswegen - voorlopige verharding voor zware lasten ","PM",null,"Geen",{"$nulls":4},1]
["02.33.","toegangswegen - parkeerruimte voor laden en lossen ","PM",null,"Geen",{"$nulls":4},1]
["02.40.","voorlopige omheining - algemeen"]
["02.50.","aankondiging werf - algemeen"]
["02.51.","aankondiging werf - werfbord ","PM",null,"Geen",{"$nulls":4},1]
["02.52.","aankondiging werf - werfdoek ","PM",null,"Geen",{"$nulls":4},1]
["02.60.","werflokalen - algemeen"]
["02.61.","werflokalen - berging van materieel en bouwmaterialen ","PM",null,"Geen",{"$nulls":4},1]
["02.62.","werflokalen - kantoorruimte ","PM",null,"Geen",{"$nulls":4},1]
["02.63.","werflokalen - personeelslokaal ","PM",null,"Geen",{"$nulls":4},1]
["02.64.","werflokalen - sanitaire voorzieningen ","PM",null,"Geen",{"$nulls":4},1]
["02.70.","voorlopige aansluitingen - algemeen"]
["02.71.","voorlopige aansluitingen - stroomvoorziening ","PM",null,"Geen",{"$nulls":4},1]
["02.72.","voorlopige aansluitingen - watervoorziening ","PM",null,"Geen",{"$nulls":4},1]
["02.73.","voorlopige aansluitingen - waterafvoer ","PM",null,"Geen",{"$nulls":4},1]
["02.80.","arbeidsmiddelen - algemeen"]
["02.81.","arbeidsmiddelen - werken op hoogte"]
["02.81.10","arbeidsmiddelen - werken op hoogte/ladders","PM",null,"Geen",{"$nulls":4},1]
["02.81.20","arbeidsmiddelen - werken op hoogte/steigers","PM",null,"Geen",{"$nulls":4},1]
["02.82.","arbeidsmiddelen - hijsen en heffen van lasten ","PM",null,"Geen",{"$nulls":4},1]
["03.","AFBRAAKWERKEN"]
["03.00.","afbraakwerken - algemeen"]
["03.01.","afbraakwerken - asbestverwijdering"]
["03.02.","afbraakwerken - schoring"]
["03.03.","afbraakwerken - in bewoonde gebouwen"]
["03.10.","afbraak volledige constructie - algemeen"]
["03.11.","afbraak volledige constructie - vrijstaand"]
["03.11.10.","afbraak volledige constructie - vrijstaand/asbestverwijdering"]
["03.11.11.","afbraak volledige constructie – vrijstaand/asbestverwijdering - dakbedekking","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["03.11.12.","afbraak volledige constructie – vrijstaand/asbestverwijdering - onderdak","FH","m2","TYPE 3","Roof",null,"Top Surface",null,2]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["03.11.13.","afbraak volledige constructie – vrijstaand/asbestverwijdering - asbestcementbuizen","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["03.11.14.","afbraak volledige constructie – vrijstaand/asbestverwijdering - vloerafwerking","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.11.15.","afbraak volledige constructie – vrijstaand/asbestverwijdering - plaatmateriaal","FH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["03.11.16.","afbraak volledige constructie – vrijstaand/asbestverwijdering - buisisolatie","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.11.17.","afbraak volledige constructie – vrijstaand/asbestverwijdering - asbestkoord","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.11.18.","afbraak volledige constructie – vrijstaand/asbestverwijdering - raam- en deurkitten","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.11.20.","afbraak volledige constructie - vrijstaand/slopen gebouw","FH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.11.30.","afbraak volledige constructie - vrijstaand/ondergrondse massieven","VH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["03.11.40.","afbraak volledige constructie - vrijstaand/te behouden gevels","PM",null,"Geen",{"$nulls":4},1]
["03.12.","afbraak volledige constructie - grenzend aan andere gebouwen"]
["03.12.10.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering"]
["03.12.11.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - dakbedekking","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.12.12.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - onderdak","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.12.13.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - asbestcementbuizen","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["03.12.14.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - vloerafwerking","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.12.15.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - plaatmateriaal","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["03.12.16.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - buisisolatie","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.12.17.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - asbestkoord","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.12.18.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - raam- en deurkitten","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.12.20.","afbraak volledige constructie – grenzend aan andere gebouwen/slopen gebouw","FH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.12.30.","afbraak volledige constructie – grenzend aan andere gebouwen/ondergrondse massieven","VH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["03.12.40.","afbraak volledige constructie – grenzend aan andere gebouwen/te behouden gevels","PM",null,"Geen",{"$nulls":4},1]
["03.20.","afbraak ruwbouwelementen - algemeen"]
["03.21.","afbraak ruwbouwelementen - muren"]
["03.21.10.","afbraak ruwbouwelementen – muren/metselwerk","FH of VH","m3","TYPE 3","Wall",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"Net Volume"]
[{"$nulls":4},"TYPE 5","Opening"]
["03.21.20.","afbraak ruwbouwelementen – muren/beton","FH of VH","m3","TYPE 3","Wall",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"Net Volume"]
[{"$nulls":4},"TYPE 5","Opening"]
["03.21.30.","afbraak ruwbouwelementen – muren/houtskelet","FH of VH","m3","TYPE 3","Wall",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"Net Volume"]
[{"$nulls":4},"TYPE 5","Opening"]
["03.22.","afbraak ruwbouwelementen - vloeren"]
["03.22.10.","afbraak ruwbouwelementen – vloeren/potten en balken","FH of VH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m3","TYPE 3","Roof",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Roof",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Shell",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Slab",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Opening"]
["03.22.20.","afbraak ruwbouwelementen – vloeren/beton"]
["03.22.21.","afbraak ruwbouwelementen – vloeren/beton - verdiepingsvloer","FH of VH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m3","TYPE 3","Roof",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Roof",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Shell",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Slab",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Opening"]
["03.22.22.","afbraak ruwbouwelementen – vloeren/beton - vloer op volle grond","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m3","TYPE 3","Slab",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Slab",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Opening"]
["03.22.30.","afbraak ruwbouwelementen – vloeren/houten roostering","FH of VH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m3","TYPE 3","Roof",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Roof",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Shell",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Slab",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Opening"]
["03.30.","afbraak dakelementen - algemeen"]
["03.31.","afbraak dakelementen - hellend dak"]
["03.31.10.","afbraak dakelementen – hellend dak/asbestverwijdering"]
["03.31.11.","afbraak dakelementen – hellend dak/asbestverwijdering - dakbedekking","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["03.31.12.","afbraak dakelementen – hellend dak/asbestverwijdering - onderdak","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["03.31.13.","afbraak dakelementen – hellend dak/asbestverwijdering - asbestcement","FH","st","TYPE 3","Roof",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Stuks",null,1]
["03.31.20.","afbraak dakelementen – hellend dak/volledige dakopbouw","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.31.30.","afbraak dakelementen – hellend dak/dakbedekking","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["03.31.40.","afbraak dakelementen – hellend dak/dakisolatie","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.31.50.","afbraak dakelementen – hellend dak/daklichtelementen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.31.60.","afbraak dakelementen – hellend dak/dakdoorvoeren en schouwen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.32.","afbraak dakelementen - plat dak"]
["03.32.10.","afbraak dakelementen – plat dak/asbestverwijdering"]
["03.32.11.","afbraak dakelementen – plat dak/asbestverwijdering - asbestcement","FH","st","TYPE 3","Roof",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Stuks",null,1]
["03.32.20.","afbraak dakelementen – plat dak/volledige dakopbouw","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"SOG",{"$nulls":6},1]
["03.32.30.","afbraak dakelementen – plat dak/dakdichting","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.32.40.","afbraak dakelementen – plat dak/dakisolatie","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.32.50.","afbraak dakelementen – plat dak/daklichtelementen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.32.60.","afbraak dakelementen – plat dak/dakdoorvoeren","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["03.40.","afbraak gevelelementen - algemeen"]
["03.41.","afbraak gevelelementen - gevelmetselwerk ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["03.42.","afbraak gevelelementen - leien"]
["03.42.10.","afbraak gevelelementen – leien/asbesthoudend","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["03.42.20.","afbraak gevelelementen – leien/niet-asbesthoudend","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["03.43.","afbraak gevelelementen - beplating ","FH","m2","TYPE 3","Wall",null,"Projected Area on the side opposite to the reference line",null,1]
["03.44.","afbraak gevelelementen - buitenschrijnwerk"]
["03.44.10.","afbraak gevelelementen – buitenschrijnwerk/asbestverwijdering"]
["03.44.11.","afbraak gevelelementen – buitenschrijnwerk/asbestverwijdering - kitten","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.44.20.","afbraak gevelelementen – buitenschrijnwerk/ramen, deuren en poorten","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
[{"$nulls":4},"TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.45.","afbraak gevelelementen - buitentrappen ","FH","m2","TYPE 5","Stair ","Tread total area","Net Area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.46.","afbraak gevelelementen - balustraden ","FH","st","TYPE 5","Railing",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.50.","afbraak binnenafwerking - algemeen"]
["03.51.","afbraak binnenafwerking - volledige ontmanteling ","SOG",null,"Geen",{"$nulls":4},1]
["03.52.","afbraak binnenafwerking - afkappen pleisterwerk ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["03.53.","afbraak binnenafwerking - plaatafwerking"]
["03.53.10.","afbraak binnenafwerking – plaatafwerking/asbestverwijdering","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["03.53.20.","afbraak binnenafwerking – plaatafwerking/lichte scheidingswanden","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.53.30.","afbraak binnenafwerking – plaatafwerking/plafondafwerking","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.53.40.","afbraak binnenafwerking – plaatafwerking/uitbekleding wanden","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.54.","afbraak binnenafwerking - dekvloer",{"$nulls":5},"Property: Oppervlakte middenas wand"]
["03.54.10.","afbraak binnenafwerking – dekvloer/asbestverwijdering","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.54.20.","afbraak binnenafwerking – dekvloer/tot op draagstructuur","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.55.","afbraak binnenafwerking - vloerafwerking"]
["03.55.10.","afbraak binnenafwerking – vloerafwerking/asbestverwijdering","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.55.20.","afbraak binnenafwerking – vloerafwerking/linoleum","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.55.30.","afbraak binnenafwerking – vloerafwerking/tegels"]
["03.55.31.","afbraak binnenafwerking – vloerafwerking/tegels - op dekvloer","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.55.32.","afbraak binnenafwerking – vloerafwerking/tegels - op zandbed","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.55.40.","afbraak binnenafwerking – vloerafwerking/houten vloer","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.56.","afbraak binnenafwerking - binnendeuren ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.57.","afbraak binnenafwerking - trappen en leuningen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Railing",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Stair",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.58.","afbraak binnenafwerking - vast meubilair"]
["03.58.10.","afbraak binnenafwerking – vast meubilair/keukenmeubilair","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.58.20.","afbraak binnenafwerking – vast meubilair/badkamermeubilair","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.60.","afbraak technieken fluïda - algemeen"]
["03.61.","afbraak technieken fluïda - leidingen"]
["03.61.10.","afbraak technieken fluïda – leidingen/asbestverwijdering"]
["03.61.11.","afbraak technieken fluïda – leidingen/asbestverwijdering - asbestcement","FH of VH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["03.61.12.","afbraak technieken fluïda – leidingen/asbestverwijdering - leidingisolatie","FH of VH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["03.61.20.","afbraak technieken fluïda – leidingen/toevoer en afvoerleidingen","PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.62.","afbraak technieken fluïda - sanitaire toestellen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.63.","afbraak technieken fluïda - radiatoren & toebehoren","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.64.","afbraak technieken fluïda - gasleidingen & toebehoren","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.65.","afbraak technieken fluïda - CV-ketel & toebehoren","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.70.","afbraak technieken elektro - algemeen"]
["03.71.","afbraak technieken elektro - leidingnet ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["04.","GEBOUWPRESTATIES"]
["04.00.","gebouwprestaties - algemeen"]
["04.10.","energieprestatie en binnenklimaat (EPB) - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["04.20.","luchtdichtheid - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["04.30.","akoestiek - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["04.40.","brandveiligheid - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["05.","PROEVEN"]
["05.00.","proeven - algemeen"]
["05.10.","proeven - luchtdichtheidsmeting"]
["05.11.","proeven - luchtdichtheidsmeting / wooneenheid ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks",null,1]
["05.12.","proeven - luchtdichtheidsmeting / gebouw ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks",null,1]
["05.20.","proeven - akoestiek"]
["05.21.","proeven - akoestiek / luchtgeluidiolatie ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks",null,1]
["05.22.","proeven - akoestiek / contactgeluidiolatie ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks",null,1]
["05.23.","proeven - akoestiek / geluidisolatie van de gevel ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks",null,1]
["05.24.","proeven - akoestiek / geluid van technische installaties ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks",null,1]

{"sheet":"10 Onderbouw","index":3,"n_rows":526,"n_cols":10,"rows_kept":526,"cut":false,"hidden":false,"merged":[]}
["Artikelnummer","Artikelomschrijving","AvO","Eenheid","Type","Element","Element specificatie","Wat rekent de Meetstaat Manager?","Aandachtspunten","Column3"]
["10.","GRONDWERKEN"]
["10.00.","grondwerken - algemeen"]
["10.10.","voorafgaande afgraving van het terrein - algemeen"]
["10.11.","voorafgaande afgraving terrein - ontzoden ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Projected Area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["10.12.","voorafgaande afgraving terrein - afgraven teelaarde ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Projected Area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["10.13.","voorafgaande afgraving terrein - machinale nivellering ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Projected Area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["10.20.","uitgraving bouwputten - algemeen"]
["10.21.","uitgraving bouwputten - gewone bouwputten ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
["10.22.","uitgraving bouwputten - prefabkelders ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["10.23.","uitgraving bouwputten - rioleringselementen ","PM",null,"Geen",{"$nulls":4},1]
["10.30.","uitgraving sleuven - algemeen"]
["10.31.","uitgraving sleuven - funderingssleuven ","FH/VH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
["10.32.","uitgraving sleuven - funderingsbalken ","FH/VH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
["10.33.","uitgraving sleuven - ondergrondse leidingen ","FH/VH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["10.40.","grondverzet - algemeen"]
["10.41.","grondverzet - projectopvolging ","SOG",null,"Geen",{"$nulls":4},1]
["10.42.","grondverzet - hergebruik uitgegraven grond op werf ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.43.","grondverzet - afvoer uitgegraven bodem"]
["10.43.10.","grondverzet - afvoer uitgegraven bodem/naar bestemming voor gebruik"]
["10.43.11.","grondverzet - afvoer uitgegraven bodem/naar bestemming voor gebruik - kwaliteit vrij gebruik ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.43.12.","grondverzet - afvoer uitgegraven bodem/naar bestemming voor gebruik - kwaliteit bouwkundig bodemgebruik ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.43.20.","grondverzet - afvoer uitgegraven bodem/naar tussentijdse opslagplaats (TOP) ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.43.30.","grondverzet - afvoer uitgegraven bodem/naar grondreinigingscentrum (GRC) ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.43.40.","grondverzet - afvoer uitgegraven bodem/naar erkende stortplaats"]
["10.43.41.","grondverzet - afvoer uitgegraven bodem/naar erkende stortplaats - klasse I ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.43.42.","grondverzet - afvoer uitgegraven bodem/naar erkende stortplaats - klasse II ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.43.43.","grondverzet - afvoer uitgegraven bodem/naar erkende stortplaats - klasse III ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.44.","grondverzet - fysische scheiding"]
["10.44.10.","grondverzet - fysische scheiding/uitzeving ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.44.20.","grondverzet - fysische scheiding/afvoer steenachtige materialen ","VH","ton","TYPE 3","Slab","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":4},"TYPE 5","Mesh","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":4},"TYPE 5","Morph","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":6},"ARCHICAD property koppelen aan object KM","ARCHICAD Property: Grondverzet",null,1]
["10.44.30.","grondverzet - fysische scheiding/afvoer bodemvreemde materialen ","VH","ton","TYPE 3","Slab","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":4},"TYPE 5","Mesh","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":4},"TYPE 5","Morph","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM of ARCHICAD property koppelen aan object KM","ARCHICAD Property: Grondverzet",null,1]
["10.50.","verwijdering massieven - algemeen ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.60.","bronbemaling - algemeen ","SOG",null,"Geen",{"$nulls":4},1]
["10.70.","aanvullingen - algemeen"]
["10.71.","aanvullingen - wederaanvullingen"]
["10.71.10.","aanvullingen - wederaanvullingen/grond van uitgravingen ","PM",null,"Geen",{"$nulls":4},1]
["10.71.20.","aanvullingen - wederaanvullingen/aangevoerde grond ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.71.30.","aanvullingen - wederaanvullingen/gestabiliseerd zand ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.71.40.","aanvullingen - wederaanvullingen/kunststeenslag ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.71.50.","aanvullingen - wederaanvullingen/natuursteenslag ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.72.","aanvullingen - ophoging terrein"]
["10.72.10.","aanvullingen - ophoging terrein/grond van afgravingen ","PM",null,"Geen",{"$nulls":4},1]
["10.72.20","aanvullingen - ophoging terrein/aangevoerde grond ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.72.30.","aanvullingen - ophoging terrein/gestabiliseerd zand ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.80.","grondbehandeling - algemeen"]
["10.81.","grondbehandeling - kalk ","VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.82.","grondbehandeling - cement ","VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["11.","STUT- & ONDERVANGINGSWERKEN"]
["11.00.","stut- & ondervangingswerken - algemeen"]
["11.10.","beschoeiing bouwputten - algemeen"]
["11.11.","beschoeiing bouwputten - damplanken"]
["11.11.10.","beschoeiing bouwputten - damplanken/aanvoer & installatie machine ","SOG",null,"Geen",{"$nulls":4},1]
["11.11.20.","beschoeiing bouwputten - damplanken/materialen & verwerking ","FH/VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (m2) in bij de Object Settings",null,1]
["11.12.","beschoeiing bouwputten - berlinerwand"]
["11.12.10.","beschoeiing bouwputten - berlinerwand/ aanvoer & installatie machine ","SOG",null,"Geen",{"$nulls":4},1]
["11.12.20.","beschoeiing bouwputten - berlinerwand/materialen & verwerking ","FH/VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (m2) in bij de Object Settings",null,1]
["11.13.","beschoeiing bouwputten - secanspalenwand"]
["11.13.10.","beschoeiing bouwputten - secanspalenwand/installatie palenmachine ","SOG",null,"Geen",{"$nulls":4},1]
["11.13.20.","beschoeiing bouwputten - secanspalenwand/realisatie palenwand ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["11.13.30.","beschoeiing bouwputten - secanspalenwand/verbindingsbalk ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["11.13.50.","beschoeiing bouwputten - secanspalenwand/horizontale verankering ","FH/VH","st","TYPE 5","Object",null,"Stuks",null,1]
["11.13.60.","beschoeiing bouwputten - secanspalenwand/sonische integriteitstesten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["11.13.70.","beschoeiing bouwputten - secanspalenwand/afwerking als kelderwand ","FH","m3","TYPE 3","Wall",null,"Net Volume (heel element)",null,1]
["11.20.","onderschoeiingen - algemeen"]
["11.21.","onderschoeiingen - stortklaar beton ","VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume (heel element)",null,1]
["11.22.","onderschoeiingen - metselwerk ","VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume",null,1]
["11.23.","onderschoeiingen - groutkolommen",{"$nulls":7},1]
["11.23.10.","onderschoeiingen - groutkolommen/aanvoer en installatie van de machine ","SOG",null,"Geen",{"$nulls":4},1]
["11.23.20.","onderschoeiingen - groutkolommen/materialen en verwerking ","VH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["11.30.","keermuren - algemeen"]
["11.31.","keermuren - stortklaar beton ","VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Projected Area",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume (heel element)",null,1]
["12.","FUNDERINGEN OP STAAL"]
["12.00.","funderingen op staal - algemeen"]
["12.10.","funderingszolen en -stroken - algemeen"]
["12.11.","funderingszolen en -stroken - ongewapend beton ","VH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume (heel element)",null,1]
["12.12.","funderingszolen en -stroken - gewapend beton ","VH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume (heel element)",null,1]
["12.20.","ondergronds metselwerk - algemeen"]
["12.21.","ondergronds metselwerk - betonblokken"]
["12.21.10.","ondergronds metselwerk - betonblokken/muurdikte 35 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["12.21.20.","ondergronds metselwerk - betonblokken/muurdikte 40 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["12.21.30.","ondergronds metselwerk - betonblokken/muurdikte 45 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["12.22.","ondergronds metselwerk - snelbouw"]
["12.22.10.","ondergronds metselwerk - snelbouw/muurdikte 35 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["12.22.20.","ondergronds metselwerk - snelbouw/muurdikte 40 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["12.22.30.","ondergronds metselwerk - snelbouw/muurdikte 45 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["12.30.","doorbrekingen ondergronds metselwerk - algemeen"]
["12.31.","doorbrekingen ondergronds metselwerk - aansluitbocht ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["12.40.","aardingslus - algemeen","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"FH","st","TYPE 5","Object",null,"Stuks",null,1]
["13.","SPECIALE FUNDERINGEN"]
["13.00.","speciale funderingen - algemeen"]
["13.01.","algemeen - diepsonderingsverslag"]
["13.10.","paalfundering - algemeen"]
["13.11.","paalfundering - schroefpalen"]
["13.11.10.","paalfundering - schroefpalen/enkele grondverdringing"]
["13.11.11.","paalfundering - schroefpalen/enkele grondverdringing - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.11.12.","paalfundering - schroefpalen/enkele grondverdringing - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.11.20.","paalfundering - schroefpalen/dubbele grondverdringing"]
["13.11.21.","paalfundering - schroefpalen/dubbele grondverdringing - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.11.22.","paalfundering - schroefpalen/dubbele grondverdringing - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.12.","paalfundering - boorpalen"]
["13.12.10.","paalfundering - boorpalen/verbuisd"]
["13.12.11.","paalfundering - boorpalen/verbuisd - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.12.12.","paalfundering - boorpalen/verbuisd - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.12.20.","paalfundering - boorpalen/steunvloeistof"]
["13.12.21.","paalfundering - boorpalen/steunvloeistof - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.12.22.","paalfundering - boorpalen/steunvloeistof - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.13.","paalfundering - kokerpalen"]
["13.13.10.","paalfundering - kokerpalen/geschroefd"]
["13.13.11.","paalfundering - kokerpalen/geschroefd - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.13.12.","paalfundering - kokerpalen/geschroefd - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.13.20.","paalfundering - kokerpalen geheid"]
["13.13.21.","paalfundering - kokerpalen geheid - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.13.22.","paalfundering - kokerpalen/geheid - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.14.","paalfundering - heipalen"]
["13.14.10.","paalfundering - heipalen/in de grond gevormd"]
["13.14.11.","paalfundering - heipalen/in de grond gevormd - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.14.12.","paalfundering - heipalen/in de grond gevormd - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.14.20.","paalfundering - heipalen/prefab beton"]
["13.14.21.","paalfundering - heipalen/prefab beton - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.14.22.","paalfundering - heipalen/prefab beton - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.20.","fundering op valse putten - algemeen"]
["13.21.","fundering op valse putten - ongewapend stortklaar beton ","FH/VH","m","TYPE 2","Column",null,"diepte / hoogte kolom",null,1]
[null,null,"FH/VH","m","TYPE 3","Slab",null,null,null,1]
[null,null,"FH/VH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"FH/VH","m","TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,"FH/VH","m2","TYPE 2","Column",null,"Top Surface <> rekent momenteel core uit",null,1]
[null,null,"FH/VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"FH/VH","m2","TYPE 3","Column",null,"Net Area",null,1]
[null,null,"FH/VH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,"FH/VH","m3","TYPE 2","Column",null,"Net Volume",null,1]
[null,null,"FH/VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"FH/VH","m3","TYPE 3","Column",null,"Net Volume",null,1]
[null,null,"FH/VH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
["13.22.","fundering op valse putten - gewapend stortklaar beton ","FH/VH","m","TYPE 2","Column",null,"diepte / hoogte kolom",null,1]
[null,null,"FH/VH","m","TYPE 3","Slab",null,null,null,1]
[null,null,"FH/VH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"FH/VH","m","TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,"FH/VH","m2","TYPE 2","Column",null,"Top Surface <> rekent momenteel core uit",null,1]
[null,null,"FH/VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"FH/VH","m2","TYPE 3","Column",null,"Net Area",null,1]
[null,null,"FH/VH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,"FH/VH","m3","TYPE 2","Column",null,"Net Volume",null,1]
[null,null,"FH/VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"FH/VH","m3","TYPE 3","Column",null,"Net Volume",null,1]
[null,null,"FH/VH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
["13.23.","fundering op valse putten - gestabiliseerd zand ","FH/VH","m","TYPE 2","Column",null,"diepte / hoogte kolom",null,1]
[null,null,"FH/VH","m","TYPE 3","Slab",null,null,null,1]
[null,null,"FH/VH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"FH/VH","m","TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,"FH/VH","m2","TYPE 2","Column",null,"Top Surface <> rekent momenteel core uit",null,1]
[null,null,"FH/VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"FH/VH","m2","TYPE 3","Column",null,"Net Area",null,1]
[null,null,"FH/VH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,"FH/VH","m3","TYPE 2","Column",null,"Net Volume",null,1]
[null,null,"FH/VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"FH/VH","m3","TYPE 3","Column",null,"Net Volume",null,1]
[null,null,"FH/VH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
["13.24.","fundering op valse putten - steenslag ","FH/VH","m","TYPE 2","Column",null,"diepte / hoogte kolom",null,1]
[null,null,"FH/VH","m","TYPE 3","Slab",null,null,null,1]
[null,null,"FH/VH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"FH/VH","m","TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,"FH/VH","m2","TYPE 2","Column",null,"Top Surface <> rekent momenteel core uit",null,1]
[null,null,"FH/VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"FH/VH","m2","TYPE 3","Column",null,"Net Area",null,1]
[null,null,"FH/VH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,"FH/VH","m3","TYPE 2","Column",null,"Net Volume",null,1]
[null,null,"FH/VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"FH/VH","m3","TYPE 3","Column",null,"Net Volume",null,1]
[null,null,"FH/VH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
["13.30.","funderingsbalken - algemeen"]
["13.31.","funderingsbalken - stortklaar beton ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume",null,1]
["13.40.","plaat op putten - algemeen"]
["13.41.","plaat op putten - gewapend stortklaar beton ","FH","m3","TYPE 3","Beam ",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume",null,1]
["13.42.","plaat op putten - gewapend & gepolierd stortklaar beton ","FH","m3","TYPE 3","Beam ",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume",null,1]
["13.50.","plaatfunderingen - algemeen"]
["13.51.","plaatfunderingen - gewapend stortklaar beton ","FH","m3","TYPE 3","Beam ",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume",null,1]
["13.52.","plaatfunderingen - gewapend en gepolierd stortklaar beton ","FH","m3","TYPE 3","Beam ",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume",null,1]
["13.60.","liftputten - algemeen"]
["13.61.","liftputten - stortklaar beton ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["13.70.","doorbrekingen speciale funderingen - algemeen"]
["13.71.","doorbrekingen speciale funderingen - aansluitbocht ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["13.72.","doorbrekingen speciale funderingen - doorvoermoffen voor buizen en kabels ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["14.","ONDERGRONDSE WANDEN"]
["14.00.","ondergrondse wanden - algemeen"]
["14.10.","funderingswanden - algemeen"]
["14.11.","funderingswanden - beton"]
["14.11.10.","funderingswanden - beton/ter plaatse gestort"]
["14.11.11.","funderingswanden - beton/ter plaatse gestort - dikte 20 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.11.12.","funderingswanden - beton/ter plaatse gestort - dikte 25 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.11.13.","funderingswanden - beton/ter plaatse gestort - dikte 30 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.11.14.","funderingswanden - beton/ter plaatse gestort - dikte 35 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.11.20.","funderingswanden - beton/holle wanden"]
["14.11.21.","funderingswanden - beton/holle wanden - prefabelementen ","FH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Projected Area",null,1]
["14.11.22.","funderingswanden - beton/holle wanden - vulbeton ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume",null,1]
["14.11.30.","funderingswanden - beton/injectie van onvermijdelijke scheuren ","VH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["14.12.","funderingswanden - metselwerk"]
["14.12.01.","funderingswanden - metselwerk/mortel ","PM",null,"Geen",{"$nulls":4},1]
["14.12.02.","funderingswanden - metselwerk/wapening ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["14.12.10.","funderingswanden - metselwerk/betonblokken"]
["14.12.11.","funderingswanden - metselwerk/betonblokken - muurdikte 29 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.12.12.","funderingswanden - metselwerk/betonblokken - muurdikte 35 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.12.13.","funderingswanden - metselwerk/betonblokken - muurdikte 39 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.12.14.","funderingswanden - metselwerk/betonblokken - muurdikte 40 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.20.","dragende kelderwanden - algemeen"]
["14.21.","dragende kelderwanden - beton"]
["14.21.10.","dragende kelderwanden - beton/ter plaatse gestort"]
["14.21.11.","dragende kelderwanden - beton/ter plaatse gestort - dikte 20 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.21.12.","dragende kelderwanden - beton/ter plaatse gestort - dikte 25 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.21.13.","dragende kelderwanden - beton/ter plaatse gestort - dikte 30 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.21.20.","dragende kelderwanden - beton/holle wanden"]
["14.21.21.","dragende kelderwanden - beton/holle wanden - prefabelementen ","FH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Projected Area",null,1]
["14.21.22.","dragende kelderwanden - beton/holle wanden - vulbeton ","FH","m3","TYPE 3","Wall",null,"Net Volume",null,1]
["14.21.30.","dragende kelderwanden - beton/injectie van onvermijdelijke scheuren ","VH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["14.22.","dragende kelderwanden - metselwerk"]
["14.22.01.","dragende kelderwanden - metselwerk/mortel ","PM",null,"Geen",{"$nulls":4},1]
["14.22.02.","dragende kelderwanden - metselwerk/wapening ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["14.22.03.","dragende kelderwanden - metselwerk/lateien ","PM",null,"Geen",{"$nulls":4},1]
["14.22.10.","dragende kelderwanden - metselwerk/betonblokken"]
["14.22.11.","dragende kelderwanden - metselwerk/betonblokken - muurdikte 14 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.12.","dragende kelderwanden - metselwerk/betonblokken - muurdikte 19 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.13.","dragende kelderwanden - metselwerk/betonblokken - muurdikte 29 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.20.","dragende kelderwanden - metselwerk/baksteen"]
["14.22.21.","dragende kelderwanden - metselwerk/baksteen - muurdikte 14 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.22.","dragende kelderwanden - metselwerk/baksteen - muurdikte 19 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.30.","dragende kelderwanden - metselwerk/kalkzandsteen"]
["14.22.31.","dragende kelderwanden - metselwerk/kalkzandsteen - muurdikte 15 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.32.","dragende kelderwanden - metselwerk/kalkzandsteen - muurdikte 17,5 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.33.","dragende kelderwanden - metselwerk/kalkzandsteen - muurdikte 21,5 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.30.","geprefabriceerde kelders - algemeen"]
["14.31.","geprefabriceerde kelders - gedeeltelijke onderkeldering ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Slab",null,"Stuks",null,1]
["14.40.","waterdichting ondergrondse wanden - algemeen"]
["14.41.","waterdichting ondergrondse wanden - mineraliserende mortel ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["14.42.","waterdichting ondergrondse wanden - gemodificeerde cementmortel ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["14.43.","waterdichting ondergrondse wanden - bitumenemulsie ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["14.44.","waterdichting ondergrondse wanden - noppenbanen ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["14.50.","doorbrekingen ondergrondse wanden - algemeen"]
["14.51.","doorbrekingen ondergrondse wanden - aansluitbocht ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["14.52.","doorbrekingen ondergrondse wanden - doorvoermoffen buizen en kabels ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["14.60.","verluchtingselementen ondergrondse wanden - algemeen"]
["14.61.","verluchtingselementen ondergrondse wanden - telescopische kokers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["15.","VLOERLAGEN ONDERBOUW"]
["15.00.","vloerlagen onderbouw - algemeen"]
["15.10.","zuiverheidslagen - algemeen"]
["15.11.","zuiverheidslagen - stortklaar beton ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m3","TYPE 2","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["15.20.","draagvloeren op volle grond - algemeen"]
["15.21.","draagvloeren op volle grond - stortklaar gewapend beton ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["15.30.","vochtwerende lagen - algemeen"]
["15.31.","vochtwerende lagen - folies"]
["15.31.10.","vochtwerende lagen - folies/PE ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["15.31.20.","vochtwerende lagen - folies/PVC ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["15.31.30.","vochtwerende lagen - folies/PIB ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["15.32.","vochtwerende lagen - banen"]
["15.32.10.","vochtwerende lagen - banen/HDPE ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["15.33.","vochtwerende lagen - bitumenglasvlies ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["16.","THERMISCHE ISOLATIE ONDERBOUW"]
["16.00.","thermische isolatie onderbouw - algemeen"]
["16.10.","isolatieplaten op volle grond - algemeen"]
["16.11.","isolatieplaten op volle grond - XPS"]
["16.11.10.","isolatieplaten op volle grond - XPS/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["16.11.20.","isolatieplaten op volle grond - XPS/12 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["16.12.","isolatieplaten op volle grond - PUR of PIR"]
["16.12.10.","isolatieplaten op volle grond - PUR of PIR/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["16.12.20.","isolatieplaten op volle grond - PUR of PIR/12 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["16.13.","isolatieplaten op volle grond - EPS"]
["16.13.10.","isolatieplaten op volle grond - EPS/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["16.13.20.","isolatieplaten op volle grond - EPS/12 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["16.20.","perimeterisolatie - algemeen"]
["16.21.","perimeterisolatie - XPS"]
["16.21.10.","perimeterisolatie - XPS/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 2","Beam",null,"Oppervlakte middenas wand",null,1]
["16.21.20.","perimeterisolatie - XPS/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 2","Beam",null,"Oppervlakte middenas wand",null,1]
["16.22.","perimeterisolatie - PUR of PIR"]
["16.22.10.","perimeterisolatie - PUR of PIR/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 2","Beam",null,"Oppervlakte middenas wand",null,1]
["16.22.20.","perimeterisolatie - PUR of PIR/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 2","Beam",null,"Oppervlakte middenas wand",null,1]
["17.","ONDERGRONDSE LEIDINGEN"]
["17.00.","ondergrondse leidingen - algemeen"]
["17.10.","rioolbuizen - algemeen"]
["17.11.","rioolbuizen - beton"]
["17.11.10.","rioolbuizen - beton ongewapend"]
["17.11.11.","rioolbuizen - beton/ongewapend - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.12.","rioolbuizen - beton/ongewapend - diam 250 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.13.","rioolbuizen - beton/ongewapend - diam 300 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.14.","rioolbuizen - beton/ongewapend - diam 400 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.15.","rioolbuizen - beton/ongewapend - diam 500 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.16.","rioolbuizen - beton/ongewapend - diam 600 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.20.","rioolbuizen - beton gewapend"]
["17.11.21.","rioolbuizen - beton/gewapend - diam 300 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,null,"m","TYPE 5","Object","MEP",null,null,1]
["17.11.22.","rioolbuizen - beton/gewapend - diam 400 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,null,"m","TYPE 5","Object","MEP",null,null,1]
["17.11.23.","rioolbuizen - beton/gewapend - diam 500 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.24.","rioolbuizen - beton/gewapend - diam 600 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.25.","rioolbuizen - beton/gewapend - diam 800 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.","rioolbuizen - kunststof"]
["17.12.10.","rioolbuizen - kunststof/PVC"]
["17.12.11.","rioolbuizen - kunststof/PVC - diam 110 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.12.","rioolbuizen - kunststof/PVC - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.13.","rioolbuizen - kunststof/PVC - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.14.","rioolbuizen - kunststof/PVC - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.15.","rioolbuizen - kunststof/PVC - diam 315 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.16.","rioolbuizen - kunststof/PVC - diam 400 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.20.","rioolbuizen - kunststof/PE"]
["17.12.21.","rioolbuizen - kunststof/PE - diam 110 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.22.","rioolbuizen - kunststof/PE - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.23.","rioolbuizen - kunststof/PE - diam 140 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.24.","rioolbuizen - kunststof/PE - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.25.","rioolbuizen - kunststof/PE - diam 180 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.26.","rioolbuizen - kunststof/PE - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.27.","rioolbuizen - kunststof/PE - diam 225 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.28.","rioolbuizen - kunststof/PE - diam 250 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.30.","rioolbuizen - kunststof/PP"]
["17.12.31.","rioolbuizen - kunststof/PP - diam 110 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.32.","rioolbuizen - kunststof/PP - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.33.","rioolbuizen - kunststof/PP - diam 140 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.34.","rioolbuizen - kunststof/PP - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.35.","rioolbuizen - kunststof/PP - diam 180 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.36.","rioolbuizen - kunststof/PP - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.37.","rioolbuizen - kunststof/PP - diam 225 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.38.","rioolbuizen - kunststof/PP - diam 250 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.20.","draineerbuizen - algemeen"]
["17.21.","draineerbuizen - poreus beton"]
["17.21.10.","draineerbuizen - poreus beton/diam 80 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.21.20.","draineerbuizen - poreus beton/diam 100 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.21.30.","draineerbuizen - poreus beton/diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.21.40.","draineerbuizen - poreus beton/diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.21.50.","draineerbuizen - poreus beton/diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.22.","draineerbuizen - vezelcement"]
["17.22.10.","draineerbuizen - poreus beton/diam 80 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.22.20.","draineerbuizen - poreus beton/diam 100 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.22.30.","draineerbuizen - poreus beton/diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.22.40.","draineerbuizen - poreus beton/diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.22.50.","draineerbuizen - poreus beton/diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.","draineerbuizen - kunststof"]
["17.23.10.","draineerbuizen - kunststof/PVC"]
["17.23.11.","draineerbuizen - kunststof/PVC - diam 50 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.12.","draineerbuizen - kunststof/PVC - diam 65 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.13.","draineerbuizen - kunststof/PVC - diam 80 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.14.","draineerbuizen - kunststof/PVC - diam 100 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.15.","draineerbuizen - kunststof/PVC - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.16.","draineerbuizen - kunststof/PVC - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.17.","draineerbuizen - kunststof/PVC - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.20.","draineerbuizen - kunststof/PE"]
["17.23.21.","draineerbuizen - kunststof/PE - diam 50 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.22.","draineerbuizen - kunststof/PE - diam 60 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.23.","draineerbuizen - kunststof/PE - diam 80 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.24.","draineerbuizen - kunststof/PE - diam 100 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.25.","draineerbuizen - kunststof/PE - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.26.","draineerbuizen - kunststof/PE - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.27.","draineerbuizen - kunststof/PE - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.30.","toezichtputten - algemeen"]
["17.31.","toezichtputten - metselwerk ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.32.","toezichtsputten - beton"]
["17.32.10.","toezichtsputten - beton/stortklaar ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.32.20.","toezichtsputten - beton/prefab ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.33.","toezichtputten - vezelcement ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.34.","toezichtsputten - kunststof"]
["17.34.10.","toezichtputten - kunststof/PVC ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.34.20.","toezichtputten - kunststof/PE ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.34.30.","toezichtputten - kunststof/polyester ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.40.","ontvangtoestellen - algemeen"]
["17.41.","ontvangtoestellen - buitenontvanger"]
["17.41.10.","ontvangtoestellen - buitenontvanger/met klok ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.41.20.","ontvangtoestellen - buitenontvanger/met korf ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.42.","ontvangtoestellen - geulen"]
["17.42.10.","ontvangtoestellen - geulen/beton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.42.20.","ontvangtoestellen - geulen/glasvezelbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.42.30.","ontvangtoestellen - geulen/polyesterbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.43.","ontvangtoestellen - straatkolken ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.44.","ontvangtoestellen - prefab pompputten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.50.","putdeksels en roosters - algemeen"]
["17.51.","putdeksels en roosters - enkel deksel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.52.","putdeksels en roosters - dubbel deksel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.53.","putdeksels en roosters - geulroosters ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["17.60.","afvalwaterbehandeling - algemeen"]
["17.61.","afvalwaterbehandeling - septische putten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.70.","regenwaterbehandeling - algemeen"]
["17.71.","regenwaterbehandeling - regenwaterputten"]
["17.71.10.","regenwaterbehandeling - regenwaterputten/beton ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.71.20.","regenwaterbehandeling - regenwaterputten/HDPE ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.71.30.","regenwaterbehandeling - regenwaterputten/polyester ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.71.40.","regenwaterbehandeling - regenwaterputten/metselwerk ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.72.","regenwaterbehandeling - hergebruik regenwater ","PM",null,"Geen",{"$nulls":4},1]
["17.73.","regenwaterbehandeling - voorfilters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.74.","regenwaterbehandeling - overloop en terugslagklep ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.75.","regenwaterbehandeling - infiltratievoorzieningen"]
["17.75.10.","regenwaterbehandeling - infiltratievoorzieningen/infiltratieputten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.75.20.","regenwaterbehandeling - infiltratievoorzieningen/infiltratieblokken ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.75.30.","regenwaterbehandeling - infiltratievoorzieningen/infiltratiebuizen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.80.","aansluitingen - algemeen"]
["17.81.","aansluitingen - openbare riolering ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.82.","aansluitingen - doorvoer- en wachtbuizen ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["17.83.","aansluitingen - wachtput ","FH","st","TYPE 5","Object",null,"Stuks",null,1]

{"sheet":"20 Bovenbouw","index":4,"n_rows":681,"n_cols":10,"rows_kept":681,"cut":false,"hidden":false,"merged":[]}
["Artikelnummer","Artikelomschrijving","AvO","Eenheid","Type","Element","Element specificatie","Wat rekent de Meetstaat Manager?","Aandachtspunten"]
["20.","METSELWERK"]
["20.00.","metselwerken - algemeen"]
["20.01.","metselwerken - ter plaatse gemetst"]
["20.02.","metselwerken - prefab"]
["20.10.","materialen - algemeen"]
["20.11.","materialen - metselmortel"]
["20.11.10.","materialen - metselmortel/voor algemene toepassing (G) ","PM",null,"Geen",{"$nulls":4},1]
["20.11.20.","materialen - metselmortel/lijmmortel (T) ","PM",null,"Geen",{"$nulls":4},1]
["20.11.30.","materialen - metselmortel/lichtgewicht metselmortel (L) ","PM",null,"Geen",{"$nulls":4},1]
["20.12.","materialen - hulpstukken"]
["20.12.10.","materialen - hulpstukken/spouwankers"]
["20.12.11.","materialen - hulpstukken/spouwankers - gewone spouwankers ","PM",null,"Geen",{"$nulls":4},1]
["20.12.12.","materialen - hulpstukken/spouwankers - slag- en schroefankers met isolatieplug ","PM",null,"Geen",{"$nulls":4},1]
["20.12.13.","materialen - hulpstukken/spouwankers - akoestisch spouwanker ","PM",null,"Geen",{"$nulls":4},1]
["20.12.20.","materialen - hulpstukken/lateien"]
["20.12.21.","materialen - hulpstukken/lateien - beton ","PM",null,"Geen",{"$nulls":4},1]
["20.12.22.","materialen - hulpstukken/lateien - staal ","PM",null,"Geen",{"$nulls":4},1]
["20.12.23.","materialen - hulpstukken/lateien - bekistingsmetselstenen ","PM",null,"Geen",{"$nulls":4},1]
["20.12.30.","materialen - hulpstukken/waterkering ","PM",null,"Geen",{"$nulls":4},1]
["20.12.40.","materialen - hulpstukken/wapening ","FH","m","TYPE 5","Object","Meetstaat Manager 27 KM","Vul de waarde Lengte (cm) in bij de Object settings",null,1]
["20.12.50.","materialen - hulpstukken/akoestische stroken ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 27 KM","Vul de waarde Lengte (cm) in bij de Object settings",null,1]
["20.13.","materialen - kimblokken"]
["20.13.10.","materialen - kimblokken/cellenbeton ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[{"$nulls":4},"TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
["20.13.20.","materialen - kimblokken/samengestelde blok ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[{"$nulls":4},"TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
["20.13.30.","materialen - kimblokken/thermisch verbeterde steen ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[{"$nulls":4},"TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
["20.13.40.","materialen - kimblokken/cellenglas ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[{"$nulls":4},"TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
["20.20.","binnenspouwblad - algemeen"]
["20.21.","binnenspouwblad - snelbouw"]
["20.21.10.","binnenspouwblad - snelbouw/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.21.20.","binnenspouwblad - snelbouw/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.22.","binnenspouwblad - kalkzandsteen"]
["20.22.10.","binnenspouwblad - kalkzandsteen/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.22.20.","binnenspouwblad - kalkzandsteen/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.22.30.","binnenspouwblad - kalkzandsteen/dikte 21,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.22.40.","binnenspouwblad - kalkzandsteen/dikte 30 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.23.","binnenspouwblad - betonsteen met gewone granulaten"]
["20.23.10.","binnenspouwblad - betonsteen met gewone granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.23.20.","binnenspouwblad - betonsteen met gewone granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.24.","binnenspouwblad - betonsteen met lichte granulaten"]
["20.24.10.","binnenspouwblad - betonsteen met lichte granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.24.20.","binnenspouwblad - betonsteen met lichte granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.","binnenspouwblad - cellenbeton"]
["20.25.10.","binnenspouwblad - cellenbeton/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.20.","binnenspouwblad - cellenbeton/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.30.","binnenspouwblad - cellenbeton/dikte 20 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.40.","binnenspouwblad - cellenbeton/dikte 24 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.50.","binnenspouwblad - cellenbeton/dikte 30 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.60.","binnenspouwblad - cellenbeton/dikte 36,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.70.","binnenspouwblad - cellenbeton/dikte 40 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.80.","binnenspouwblad - cellenbeton/dikte 50 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.30.","woningscheidende wand - algemeen"]
["20.31.","woningscheidende wand - snelbouw"]
["20.31.10.","woningscheidende wand - snelbouw/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.31.20.","woningscheidende wand - snelbouw/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.32.","woningscheidende wand - kalkzandsteen"]
["20.32.10.","woningscheidende wand - kalkzandsteen/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.32.20.","woningscheidende wand - kalkzandsteen/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.32.30.","woningscheidende wand - kalkzandsteen/dikte 21,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.32.40.","woningscheidende wand - kalkzandsteen/dikte 30 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.33.","woningscheidende wand - betonsteen met gewone granulaten"]
["20.33.10.","woningscheidende wand - betonsteen met gewone granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.33.20.","woningscheidende wand - betonsteen met gewone granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.34.","woningscheidende wand - betonsteen met lichte granulaten"]
["20.34.10.","woningscheidende wand - betonsteen met lichte granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.34.20.","woningscheidende wand - betonsteen met lichte granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.35.","woningscheidende wand - cellenbeton"]
["20.35.10.","woningscheidende wand - cellenbeton/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.35.20.","woningscheidende wand - cellenbeton/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.35.30.","woningscheidende wand - cellenbeton/dikte 20 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.35.40.","woningscheidende wand - cellenbeton/dikte 24 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.40.","dragende binnenmuur - algemeen"]
["20.41.","dragende binnenmuur - snelbouw"]
["20.41.10.","dragende binnenmuur - snelbouw/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.41.20.","dragende binnenmuur - snelbouw/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.42.","dragende binnenmuur - kalkzandsteen"]
["20.42.10.","dragende binnenmuur - kalkzandsteen/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.42.20.","dragende binnenmuur - kalkzandsteen/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.42.30.","dragende binnenmuur - kalkzandsteen/dikte 21,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.43.","dragende binnenmuur - betonsteen met gewone granulaten"]
["20.43.10.","dragende binnenmuur - betonsteen met gewone granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.43.20.","dragende binnenmuur - betonsteen met gewone granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.44.","dragende binnenmuur - betonsteen met lichte granulaten"]
["20.44.10.","dragende binnenmuur - betonsteen met lichte granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.44.20.","dragende binnenmuur - betonsteen met lichte granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.45.","dragende binnenmuur - cellenbeton"]
["20.45.10.","dragende binnenmuur - cellenbeton/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.45.20.","dragende binnenmuur - cellenbeton/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.45.30.","dragende binnenmuur - cellenbeton/dikte 20 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.45.40.","dragende binnenmuur - cellenbeton/dikte 24 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.50.","niet-dragende binnenmuur - algemeen"]
["20.51.","niet-dragende binnenmuur - snelbouw"]
["20.51.10.","niet-dragende binnenmuur - snelbouw/dikte 9 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.51.20.","niet-dragende binnenmuur - snelbouw/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.52.","niet-dragende binnenmuur - kalkzandsteen"]
["20.52.10.","niet-dragende binnenmuur - kalkzandsteen/dikte 10 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.52.20.","niet-dragende binnenmuur - kalkzandsteen/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.53.","niet-dragende binnenmuur - betonsteen met lichte granulaten"]
["20.53.10.","niet-dragende binnenmuur - betonsteen met lichte granulaten/dikte 9 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.53.20.","niet-dragende binnenmuur - betonsteen met lichte granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.54.","niet-dragende binnenmuur - cellenbeton"]
["20.54.10.","niet-dragende binnenmuur - cellenbeton/dikte 7 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.54.20.","niet-dragende binnenmuur - cellenbeton/dikte 10 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.54.30.","niet-dragende binnenmuur - cellenbeton/dikte 11,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.55.","niet-dragende binnenmuur - gipsblokken"]
["20.55.10.","niet-dragende binnenmuur - gipsblokken/dikte 6 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.55.20.","niet-dragende binnenmuur - gipsblokken/dikte 7 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.55.30.","niet-dragende binnenmuur - gipsblokken/dikte 8 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.55.40.","niet-dragende binnenmuur - gipsblokken/dikte 10 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.60.","renovatiewerken - algemeen"]
["20.61.","renovatiewerken - behandeling tegen opstijgend vocht"]
["20.61.10.","renovatiewerken - behandeling tegen opstijgend vocht/injecteren ","FH/VH","m","TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Lengte (cm) in bij de Object settings",null,1]
["20.61.20.","renovatiewerken - behandeling tegen opstijgend vocht/plaatsen dichtingsmembraan ","FH/VH","m","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Lengte (cm) in bij de Object settings",null,1]
[null,null,null,"m","TYPE 3","Wall",null,"Reference line length",null,1]
["21.","SPOUWMUURISOLATIE"]
["21.00.","spouwmuurisolatie - algemeen"]
["21.10.","spouwmuurisolatie buitenspouwblad - algemeen"]
["21.11.","spouwmuurisolatie buitenspouwblad - MW"]
["21.11.10.","spouwmuurisolatie buitenspouwblad - MW / 12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.11.20.","spouwmuurisolatie buitenspouwblad - MW / 14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.12.","spouwmuurisolatie buitenspouwblad - PUR of PIR"]
["21.12.10.","spouwmuurisolatie buitenspouwblad - PUR of PIR/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.12.20.","spouwmuurisolatie buitenspouwblad - PUR of PIR/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.13.","spouwmuurisolatie buitenspouwblad - PF"]
["21.13.10.","spouwmuurisolatie buitenspouwblad - PF/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.13.20.","spouwmuurisolatie buitenspouwblad - PF/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.14.","spouwmuurisolatie buitenspouwblad - XPS"]
["21.14.10.","spouwmuurisolatie buitenspouwblad - XPS/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.14.20.","spouwmuurisolatie buitenspouwblad - XPS/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.15.","spouwmuurisolatie buitenspouwblad - EPS"]
["21.15.10.","spouwmuurisolatie buitenspouwblad - EPS/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.15.20.","spouwmuurisolatie buitenspouwblad - EPS/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.20.","spouwmuurisolatie woningscheidende wand - algemeen"]
["21.21.","spouwmuurisolatie woningscheidende wand - MW"]
["21.21.10.","spouwmuurisolatie woningscheidende wand - MW/4 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.21.20.","spouwmuurisolatie woningscheidende wand - MW/5 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.22.","spouwmuurisolatie woningscheidende wand - XPS"]
["21.22.10.","spouwmuurisolatie woningscheidende wand - XPS/2 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.22.20.","spouwmuurisolatie woningscheidende wand - XPS/3 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.23.","spouwmuurisolatie woningscheidende wand - PUR of PIR"]
["21.23.10.","spouwmuurisolatie woningscheidende wand - PUR of PIR/3 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.23.20.","spouwmuurisolatie woningscheidende wand - PUR of PIR/4 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.30.","spouwmuurisolatie navulling - algemeen"]
["21.31.","spouwmuurisolatie navulling - MW ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["21.32.","spouwmuurisolatie navulling - PUR ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["21.33.","spouwmuurisolatie navulling - EPS ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["22.","GEVELMETSELWERK"]
["22.00.","gevelmetselwerken - algemeen"]
["22.01.","algemeen - ter plaatse gemetst gevelmetselwerk"]
["22.02.","algemeen - prefab gevelmetselwerk"]
["22.10.","materialen - algemeen"]
["22.11.","materialen - mortel"]
["22.11.10.","materialen - mortel/metselmortel"]
["22.11.11.","materialen - mortel/metselmortel - voor algemene toepassing ","PM",null,"Geen",{"$nulls":4},1]
["22.11.12.","materialen - mortel/metselmortel - dunbedmortel ","PM",null,"Geen",{"$nulls":4},1]
["22.11.13.","materialen - mortel/metselmortel - lijmmortel ","PM",null,"Geen",{"$nulls":4},1]
["22.11.20.","materialen - mortel/voegmortel"]
["22.12.","materialen - spouwankers ","PM",null,"Geen",{"$nulls":4},1]
["22.13.","materialen - waterkering ","PM",null,"Geen",{"$nulls":4},1]
["22.14.","materialen - wapening ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["22.20.","gevelstenen - algemeen"]
["22.21.","gevelstenen - baksteen"]
["22.21.10.","gevelstenen - baksteen/strengpersstenen ","FH","m2","TYPE 3","Wall",null,"Conditional surface area on the Inside Face\n\n",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
["22.21.20.","gevelstenen - bakstenen/handvorm- en vormbakstenen ","FH","m2","TYPE 3","Wall",null,"Conditional surface area on the Inside Face\n\n",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
["22.22.","gevelstenen - betonsteen ","FH","m2","TYPE 3","Wall",null,"Conditional surface area on the Inside Face\n\n",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
["22.30.","renovatiewerken - algemeen"]
["22.31.","renovatiewerken - herstelling en aanpassing bestaand gevelmetselwerk ","FH","m2","TYPE 3","Wall",null,"Conditional surface area on the Inside Face\n\n",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
["23.00.","dorpels, plinten en dekstenen - algemeen"]
["23.01.","algemeen - blauwe hardsteen"]
["23.02.","algemeen - beton"]
["23.03.","algemeen - vezelcement"]
["23.10.","raam- en deurdorpels - algemeen"]
["23.11.","raam- en deurdorpels - blauwe hardsteen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[null,null,null,"m2","TYPE 3","Beam",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","breedte dagkant * diepte dorpel",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Area",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","breedte dagkant * diepte dorpel * dikte dorpel",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Stuks",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Stuks",null,1]
["23.12.","raam- en deurdorpels - prefabbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","breedte dagkant * diepte dorpel * dikte dorpel",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Stuks",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Stuks",null,1]
["23.13.","raam- en deurdorpels - vezelcement ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
["23.14.","raam- en deurdorpels - gevelsteen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","breedte dagkant * diepte dorpel * dikte dorpel",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
["23.20.","garagepoortdorpels - algemeen"]
["23.21.","garagepoortdorpels - blauwe hardsteen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[null,null,null,"m2","TYPE 3","Beam",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","breedte dagkant * diepte dorpel",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","breedte dagkant * diepte dorpel * dikte dorpel",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","Stuks",null,1]
["23.22.","garagepoortdorpels - prefabbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","breedte dagkant * diepte dorpel * dikte dorpel",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","Stuks",null,1]
["23.30.","gevelplinten - algemeen"]
["23.31.","gevelplinten - blauwe hardsteen ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume ( heel element)",null,1]
["23.32.","gevelplinten - sierbeton ","FH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Projected Area",null,1]
["23.33.","gevelplinten - vezelcement ","FH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 3","Wall ",null,"Projected Area",null,1]
["23.40.","omkaderingselementen - algemeen"]
["23.41.","omkaderingselementen - blauwe steen ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["23.50.","muurdekstenen - algemeen"]
["23.51.","muurdekstenen - blauwe steen ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["23.52.","muurdekstenen - prefabbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Omtrek vloer zonder openingen",null,1]
["23.53.","muurdekstenen - vezelcement ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Omtrek vloer zonder openingen",null,1]
["23.60.","schoorsteendekplaten - algemeen"]
["23.61.","schoorsteendekplaten - blauwe steen ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Stuks",null,1]
["23.62.","schoorsteendekplaten - beton ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Stuks",null,1]
["23.63.","schoorsteendekplaten - vezelcement ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Stuks",null,1]
["24.","RUWBOUWKANALEN"]
["24.00.","ruwbouw kanalen - algemeen"]
["24.10.","modulaire ruwbouwkanalen - algemeen"]
["24.11.","modulaire ruwbouwkanalen - beton "]
["24.11.10.","modulaire ruwbouwkanalen - beton/rookgasafvoer ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["24.11.20.","modulaire ruwbouwkanalen - beton/ventilatie ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["24.12.","modulaire ruwbouwkanalen - keramische blokken"]
["24.12.10.","modulaire ruwbouwkanalen - keramische blokken/rookgasafvoer ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["24.12.20.","modulaire ruwbouwkanalen - keramische blokken/ventilatie ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["25.","STRUCTUURELEMENTEN HOUT"]
["25.00.","structuurelementen hout - algemeen"]
["25.01.","algemeen - stabiliteitsstudie ","PM",null,"Geen",{"$nulls":4},1]
["25.02.","algemeen - opleg- en bevestigingsmaterialen"]
["25.02.10.","algemeen - opleg- en bevestigingsmaterialen/metalen schoenen ","PM",null,"Geen",{"$nulls":4},1]
["25.02.20.","algemeen - opleg- en bevestigingsmaterialen/schroeven, nagels en nieten ","PM",null,"Geen",{"$nulls":4},1]
["25.02.30.","algemeen - opleg- en bevestigingsmaterialen/lijmen ","PM",null,"Geen",{"$nulls":4},1]
["25.02.40.","algemeen - opleg- en bevestigingsmaterialen/metalen hechtplaten ","PM",null,"Geen",{"$nulls":4},1]
["25.10.","balken - algemeen"]
["25.11.","balken - massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["25.12.","balken - LVL ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["25.13.","balken - lichte samengestelde liggers ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["25.14.","balken - gelijmd gelamineerd hout (GL) ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["25.20.","kolommen - algemeen"]
["25.21.","kolommen - massief hout ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
["25.22.","kolommen - LVL ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
["25.23.","kolommen - gelijmd gelamineerd hout"]
["25.30.","vloeren - algemeen"]
["25.31.","vloeren - roostering met beplating"]
["25.31.10.","vloeren - roostering met beplating/balken"]
["25.31.11.","vloeren - roostering met beplating/balken - massief hout ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["25.31.12.","vloeren - roostering met beplating/balken - LVL ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["25.31.13.","vloeren - roostering met beplating/balken - lichte samengestelde liggers ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["25.31.14.","vloeren - roostering met beplating/balken - gelijmd gelamineerd hout ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["25.31.20.","vloeren - roostering met beplating/beplating"]
["25.31.21.","vloeren - roostering met beplating/beplating - OSB ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["25.31.22.","vloeren - roostering met beplating/beplating - spaanplaat ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["25.31.23.","vloeren - roostering met beplating/beplating - LVL ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.","STRUCTUURELEMENTEN BETON"]
["26.00.","structuurelementen gewapend beton - algemeen"]
["26.01.","algemeen - stabiliteitsstudie ","PM",null,"Geen",{"$nulls":4},1]
["26.10.","materialen - algemeen"]
["26.11.","materialen - wapening"]
["26.11.10.","materialen - wapening/staven en netten"]
["26.11.11.","materialen - wapening/staven en netten - staven ","FH","kg","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Gewicht (kg) in bij Settings van het Object",null,1]
["26.11.12.","materialen - wapening/staven en netten - netten ","FH","kg","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Gewicht (kg) in bij Settings van het Object",null,1]
["26.11.20.","materialen - wapening/vezels"]
["26.11.21.","materialen - wapening/vezels - staalvezels ","VH of FH","kg","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Gewicht (kg) in bij Settings van het Object",null,1]
["26.11.30.","materialen - wapening/voorspanstaal ","PM",null,"Geen",{"$nulls":4},1]
["26.12.","materialen - beton"]
["26.12.10.","materialen - beton/stortklaar beton"]
["26.12.11.","materialen - beton/stortklaar beton - met staaf- en netwapening ","PM",null,"Geen",{"$nulls":4},1]
["26.12.12.","materialen - beton/stortklaar beton - met vezelwapening ","PM",null,"Geen",{"$nulls":4},1]
["26.12.13.","materialen - beton/stortklaar beton - zichtbeton ","FH","m2","TYPE 3","Column",null,"Core surface",null,1]
[{"$nulls":4},"TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW Zichtbeton  ","Net Area",null,1]
[{"$nulls":4},"TYPE 4","Slab","Gebruik ARCHICAD Property: VMSW Zichtbeton  ","Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 4","Wall","Gebruik ARCHICAD Property: VMSW Zichtbeton  ","ARCHICAD Property: Oppervlakte middenas wand",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["26.12.20.","materialen - beton/geprefabriceerd beton ","PM",null,"Geen",{"$nulls":4},1]
["26.12.30.","materialen - beton/architectonisch beton ","PM",null,"Geen",{"$nulls":4},1]
["26.13.","materialen - bekistingen ","PM",null,"Geen",{"$nulls":4},1]
["26.14.","materialen - nabehandeling"]
["26.15.","materialen - chemische verankering ","FH of VH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM ",null,"Geen",{"$nulls":4},1]
["26.16.","materialen - thermische onderbreking ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,"PM ",null,"Geen",{"$nulls":4},1]
["26.20.","ter plaatse gestorte elementen - algemeen"]
["26.21.","ter plaatse gestorte elementen - wanden"]
["26.21.10.","ter plaatse gestorte elementen - wanden/traditionele bekisting ","FH","m3","TYPE 3","Wall",null,"Net Volume",null,1]
["26.21.20.","ter plaatse gestorte elementen - wanden/holle wanden"]
["26.21.21.","ter plaatse gestorte elementen - wanden/holle wanden - prefab elementen ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["26.21.22.","ter plaatse gestorte elementen - wanden/holle wanden - vulbeton ","FH","m3","TYPE 3","Wall",null,"Net Volume",null,1]
["26.22.","ter plaatse gestorte elementen - kolommen ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
["26.23.","ter plaatse gestorte elementen - balken ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["26.24.","ter plaatse gestorte elementen - balken met afwijkend bekistingsprofiel ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["26.25.","ter plaatse gestorte elementen - trappen en bordessen ","FH","trede","TYPE 5","Stair",null,"Totaal aantal treden",null,1]
["26.26.","ter plaatse gestorte elementen - draagvloeren"]
["26.26.10.","ter plaatse gestorte elementen - draagvloeren/traditionele bekisting ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.26.20.","ter plaatse gestorte elementen - draagvloeren/verloren bekisting ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.26.30.","ter plaatse gestorte elementen - draagvloeren/breedplaatvloeren"]
["26.26.31.","ter plaatse gestorte elementen - draagvloeren/breedplaatvloeren - prefab breedplaten ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.26.32.","ter plaatse gestorte elementen - draagvloeren/breedplaatvloeren - opstort ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.27.","ter plaatse gestorte elementen - uitkragende elementen"]
["26.27.10.","ter plaatse gestorte elementen - uitkragende elementen/balkons ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.27.20.","ter plaatse gestorte elementen - uitkragende elementen/galerijen ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.27.30.","ter plaatse gestorte elementen - uitkragende elementen/luifels ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.27.40.","ter plaatse gestorte elementen - uitkragende elementen/kroonlijsten ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["26.30.","prefab elementen - algemeen"]
["26.31.","prefab elementen - wanden ","FH","m3","TYPE 3","Wall",null,"Net Volume",null,1]
["26.32.","prefab elementen - kolommen ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
["26.33.","prefab elementen - balken ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["26.34.","prefab elementen - deur- en raamlateien ","PM",null,"Geen",{"$nulls":4},1]
["26.35.","prefab elementen - trappen en bordessen ","FH","st","TYPE 5","Stair",null,"Stuks",null,1]
["26.36.","prefab elementen - draagvloeren"]
["26.36.10.","prefab elementen - draagvloeren/welfsels"]
["26.36.11.","prefab elementen - draagvloeren/welfsels - zonder druklaag ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.12.","prefab elementen - draagvloeren/welfsels - met druklaag ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.20.","prefab elementen - draagvloeren/voorgespannen welfsels"]
["26.36.21.","prefab elementen - draagvloeren/voorgespannen welfsels - zonder druklaag ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.22.","prefab elementen - draagvloeren/voorgespannen welfsels - met druklaag ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.30.","prefab elementen - draagvloeren/cellenbeton ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.40.","prefab elementen - draagvloeren/balken en vulblokken"]
["26.36.41.","prefab elementen - draagvloeren/balken en vulblokken - vulblokken beton ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.42.","prefab elementen - draagvloeren/balken en vulblokken - vulblokken gebakken klei  ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.43.","prefab elementen - draagvloeren/balken en vulblokken - vulblokken EPS ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.37.","prefab elementen - uitkragende elementen"]
["26.37.10.","prefab elementen - uitkragende elementen/balkons ","FH","st","TYPE 3","Slab",null,"Stuks",null,1]
["26.37.20.","prefab elementen - uitkragende elementen/galerijen ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.37.30.","prefab elementen - uitkragende elementen/luifels ","FH","st","TYPE 3","Slab",null,"Stuks",null,1]
[null,null,null,"m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.37.40.","prefab elementen - uitkragende elementen/kroonlijsten ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["26.40.","betonrenovatie - algemeen"]
["26.41.","betonrenovatie - passivatie van vrijgemaakte wapeningsstaven ","VH","m","TYPE 4","Object","Gebruik ARCHICAD Property: VMSW betonrenovatie  ","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,null,"m","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW betonrenovatie  ","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["26.42.","betonrenovatie - vervangen van wapening ","VH","kg","TYPE 3","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
["26.43.","betonrenovatie - handmatig te plaatsen mortel"]
["26.43.10.","betonrenovatie - handmatig te plaatsen mortel/ gemodificeerde hydraulische mortel  ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings",null,1]
["26.43.20.","betonrenovatie - handmatig te plaatsen mortel/ harsgebonden mortel ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings",null,1]
["26.44.","betonrenovatie - gietmortel"]
["26.44.10.","betonrenovatie - gietmortel/ gemodificeerde hydraulische mortel ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings",null,1]
[null,null,null,"dm3","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Volume (dm3) in bij Settings van het Object",null,1]
["26.44.20.","betonrenovatie - gietmortel/ beton ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings",null,1]
[null,null,null,"dm3","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Volume (dm3) in bij Settings van het Object",null,1]
["26.45.","betonrenovatie - spuitbeton ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings",null,1]
[null,null,null,"dm3","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Volume (dm3) in bij Settings van het Object",null,1]
["26.46.","betonrenovatie - injecteren van scheuren ","VH","m","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Lengte (cm) in bij de Object settings",null,1]
["26.47.","betonrenovatie - coating ","FH of VH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (m2) in bij de Object Settings",null,1]
["27.","STRUCTUURELEMENTEN STAAL"]
["27.00.","structuurelementen staal - algemeen"]
["27.01.","algemeen - verbindingen ","PM",null,"Geen",{"$nulls":4},1]
["27.02.","algemeen - stabiliteitsstudie ","PM",null,"Geen",{"$nulls":4},1]
["27.10.","balken - algemeen"]
["27.11.","balken - blank profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.12.","balken - gemetalliseerd profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.13.","balken - thermisch verzinkt profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.14.","balken - thermisch verzinkt profielstaal met coating ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.15.","balken - roestvast profielstaal (RVS) ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.20.","lateien - algemeen"]
["27.21.","lateien - blank profielstaal ","PM",null,"Geen",{"$nulls":4},1]
["27.22.","lateien - gemetalliseerd profielstaal ","PM",null,"Geen",{"$nulls":4},1]
["27.23.","lateien - thermisch verzinkt profielstaal ","PM",null,"Geen",{"$nulls":4},1]
["27.24.","lateien - thermisch verzinkt profielstaal met coating ","PM",null,"Geen",{"$nulls":4},1]
["27.25.","lateien - roestvast profielstaal (RVS) ","PM",null,"Geen",{"$nulls":4},1]
["27.26.","lateien - regelbare consoles"]
["27.26.10.","lateien - regelbare consoles/zichtbaar"]
["27.26.11.","lateien - regelbare consoles/zichtbaar - gemetalliseerd ","PM",null,"Geen",{"$nulls":4},1]
["27.26.12.","lateien - regelbare consoles/zichtbaar - thermisch verzinkt ","PM",null,"Geen",{"$nulls":4},1]
["27.26.13.","lateien - regelbare consoles/zichtbaar - thermisch verzinkt + coating ","PM",null,"Geen",{"$nulls":4},1]
["27.26.14.","lateien - regelbare consoles/zichtbaar - roestvast staal (RVS) ","PM",null,"Geen",{"$nulls":4},1]
["27.26.20.","lateien - regelbare consoles/niet-zichtbaar"]
["27.26.21.","lateien - regelbare consoles/niet-zichtbaar - gemetalliseerd ","PM",null,"Geen",{"$nulls":4},1]
["27.26.22.","lateien - regelbare consoles/niet-zichtbaar - thermisch verzinkt ","PM",null,"Geen",{"$nulls":4},1]
["27.26.23.","lateien - regelbare consoles/niet-zichtbaar - roestvast staal (RVS) ","PM",null,"Geen",{"$nulls":4},1]
["27.30.","kolommen - algemeen"]
["27.31.","kolommen - blank profielstaal ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.32.","kolommen - gemetalliseerd profielstaal ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.33.","kolommen - thermisch verzinkt profielstaal ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.34.","kolommen - thermisch verzinkt profielstaal met coating ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.35.","kolommen - roestvast profielstaal (RVS) ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.40.","vlakke spanten - algemeen","FH"]
["27.41.","vlakke spanten - blank profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 5","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["27.42.","vlakke spanten - gemetalliseerd profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 5","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["27.43.","vlakke spanten - thermisch verzinkt profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 5","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["27.44.","vlakke spanten - thermisch verzinkt profielstaal met coating ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 5","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["27.50.","hulpstukken - algemeen"]
["27.51.","hulpstukken - oplegstukken"]
["27.51.10.","hulpstukken - oplegstukken/thermisch verzinkt ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.51.20.","hulpstukken - oplegstukken/roestvast staal (RVS) ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.52.","hulpstukken - spankabels ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"SOG"]
["27.53.","hulpstukken - geveldragers"]
["27.53.10.","hulpstukken - geveldragers/gemetalliseerd ","PM",null,"Geen",{"$nulls":4},1]
["27.53.20.","hulpstukken - geveldragers/thermisch verzinkt ","PM",null,"Geen",{"$nulls":4},1]
["27.53.30.","hulpstukken - geveldragers/roestvast staal ","PM",null,"Geen",{"$nulls":4},1]
["27.54.","hulpstukken - verhandelingsysteem liften"]
["27.60.","corrosiebescherming - algemeen"]
["27.61.","corrosiebescherming - metallisatie"]
["27.61.10.","corrosiebescherming - metallisatie/zonder bijkomende afwerkingslaag ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.61.20.","corrosiebescherming - metallisatie/metallisatie + natlak ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.61.30.","corrosiebescherming - metallisatie/metallisatie + poederlak ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.62.","corrosiebescherming - thermisch verzinken ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.63.","corrosiebescherming - duplexsysteem ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.64.","corrosiebescherming - roestwerende verfsystemen ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.70.","brandbeveiliging - algemeen"]
["27.71.","brandbeveiliging - brandwerend verfsysteem ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.72.","brandbeveiliging - spuitmortel ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.80.","renovatie stalen constructie-elementen - algemeen"]
["27.81.","renovatie stalen constructie-elementen - ontroesten ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["28.","HOUTSKELETBOUW"]
["28.00.","houtskeletbouw - algemeen"]
["28.01.","algemeen - stabiliteitsstudie ","PM",null,"Geen",{"$nulls":4},1]
["28.02.","algemeen - prestaties ","PM",null,"Geen",{"$nulls":4},1]
["28.10.","materialen - algemeen"]
["28.11.","materialen - onderdelen regelwerk"]
["28.11.10.","materialen - onderdelen regelwerk/stijlen"]
["28.11.11.","materialen - onderdelen regelwerk /stijlen - massief hout ","PM",null,"Geen",{"$nulls":4},1]
["28.11.12.","materialen - onderdelen regelwerk /stijlen - I-vormige stijlen ","PM",null,"Geen",{"$nulls":4},1]
["28.11.20.","materialen - onderdelen regelwerk/regels"]
["28.11.21.","materialen - onderdelen regelwerk /regels - onder- en bovenregels ","PM",null,"Geen",{"$nulls":4},1]
["28.11.22.","materialen - onderdelen regelwerk /regels - grondregels ","PM",null,"Geen",{"$nulls":4},1]
["28.11.23.","materialen - onderdelen regelwerk /regels - stelregels ","PM",null,"Geen",{"$nulls":4},1]
["28.11.24.","materialen - onderdelen regelwerk /regels - koppelregels ","PM",null,"Geen",{"$nulls":4},1]
["28.11.30.","materialen - onderdelen regelwerk/lateien ","PM",null,"Geen",{"$nulls":4},1]
["28.12.","materialen - beplating"]
["28.12.10.","materialen - beplating/houtachtige platen"]
["28.12.11.","materialen - beplating/houtachtige platen - OSB ","PM",null,"Geen",{"$nulls":4},1]
["28.12.12.","materialen - beplating/houtachtige platen - spaanplaat ","PM",null,"Geen",{"$nulls":4},1]
["28.12.13.","materialen - beplating/houtachtige platen - multiplex ","PM",null,"Geen",{"$nulls":4},1]
["28.12.14.","materialen - beplating/houtachtige platen - MDF ","PM",null,"Geen",{"$nulls":4},1]
["28.12.15.","materialen - beplating/houtachtige platen - LVL ","PM",null,"Geen",{"$nulls":4},1]
["28.12.16.","materialen - beplating/houtachtige platen - houtvezelisolatieplaat ","PM",null,"Geen",{"$nulls":4},1]
["28.12.17.","materialen - beplating/houtachtige platen - houtvezelcementplaat ","PM",null,"Geen",{"$nulls":4},1]
["28.12.20.","materialen - beplating/gipsachtige platen"]
["28.12.21.","materialen - beplating/gipsachtige platen - gipskartonplaten ","PM",null,"Geen",{"$nulls":4},1]
["28.12.22.","materialen - beplating/gipsachtige platen - gipsvezelplaten ","PM",null,"Geen",{"$nulls":4},1]
["28.12.30.","materialen - beplating/vezelcementplaten ","PM",null,"Geen",{"$nulls":4},1]
["28.12.40.","materialen - beplating/calciumsilicaatplaten ","PM",null,"Geen",{"$nulls":4},1]
["28.13.","materialen - isolatie"]
["28.13.10.","materialen - isolatie/minerale wol ","PM",null,"Geen",{"$nulls":4},1]
["28.13.20.","materialen - isolatie/cellulosevlokken ","PM",null,"Geen",{"$nulls":4},1]
["28.13.30.","materialen - isolatie/houtwol ","PM",null,"Geen",{"$nulls":4},1]
["28.14.","materialen - folies"]
["28.14.10.","materialen - folies/buitenfolies"]
["28.14.11.","materialen - folies/buitenfolies - wanden ","PM",null,"Geen",{"$nulls":4},1]
["28.14.12.","materialen - folies/buitenfolies - hellende daken ","PM",null,"Geen",{"$nulls":4},1]
["28.14.20.","materialen - folies/binnenfolies"]
["28.14.21.","materialen - folies/binnenfolies - wanden ","PM",null,"Geen",{"$nulls":4},1]
["28.14.22.","materialen - folies/binnenfolies - hellende daken ","PM",null,"Geen",{"$nulls":4},1]
["28.14.23.","materialen - folies/binnenfolies - platte daken ","PM",null,"Geen",{"$nulls":4},1]
["28.15.","materialen - regelstructuur voor binnenafwerking"]
["28.15.10.","materialen - regelstructuur voor binnenafwerking/hout ","PM",null,"Geen",{"$nulls":4},1]
["28.15.20.","materialen - regelstructuur voor binnenafwerking/metaal ","PM",null,"Geen",{"$nulls":4},1]
["28.16.","materialen - opleg- en bevestigingsmaterialen"]
["28.16.10.","materialen - opleg- en bevestigingsmaterialen/metalen schoenen ","PM",null,"Geen",{"$nulls":4},1]
["28.16.20.","materialen - opleg- en bevestigingsmaterialen/tie-downs ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["28.16.30.","materialen - opleg- en bevestigingsmaterialen/schroeven ","PM",null,"Geen",{"$nulls":4},1]
["28.16.40.","materialen - opleg- en bevestigingsmaterialen/nagels ","PM",null,"Geen",{"$nulls":4},1]
["28.16.50.","materialen - opleg- en bevestigingsmaterialen/nieten ","PM",null,"Geen",{"$nulls":4},1]
["28.16.60.","materialen - opleg- en bevestigingsmaterialen/lijmen ","PM",null,"Geen",{"$nulls":4},1]
["28.16.70.","materialen - opleg- en bevestigingsmaterialen/metalen hechtplaten ","PM",null,"Geen",{"$nulls":4},1]
["28.20.","structuurelementen - algemeen"]
["28.21.","structuurelementen - vloerbalken"]
["28.21.10.","structuurelementen - vloerbalken/massief hout ","PM",null,"Geen",{"$nulls":4},1]
["28.21.20.","structuurelementen - vloerbalken/LVL ","PM",null,"Geen",{"$nulls":4},1]
["28.21.30.","structuurelementen - vloerbalken/lichte samengestelde liggers ","PM",null,"Geen",{"$nulls":4},1]
["28.21.40.","structuurelementen - vloerbalken/gelijmd gelamineerd hout (GL) ","PM",null,"Geen",{"$nulls":4},1]
["28.22.","structuurelementen - balken"]
["28.22.10.","structuurelementen - balken/massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.22.20.","structuurelementen - balken/LVL ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.22.30.","structuurelementen - balken/lichte samengestelde liggers ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.22.40.","structuurelementen - balken/gelijmd gelamineerd hout (GL) ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.22.50.","structuurelementen - balken/staal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.23.","structuurelementen - lateien"]
["28.23.10.","structuurelementen - lateien/massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.23.20.","structuurelementen - lateien/LVL ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.23.30.","structuurelementen - lateien/gelijmd gelamineerd hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.23.40.","structuurelementen - lateien/staal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.24.","structuurelementen - kolommen"]
["28.24.10.","structuurelementen - kolommen/massief hout ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
["28.24.20.","structuurelementen - kolommen/LVL ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
["28.24.30.","structuurelementen - kolommen/gelijmd gelamineerd hout (GL) ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
["28.24.40.","structuurelementen - kolommen/staal ","FH","kg","TYPE 3","Column",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
["28.25.","structuurelementen - onderdelen hellend dak"]
["28.25.10.","structuurelementen - onderdelen hellend dak/gordingen"]
["28.25.11.","structuurelementen - onderdelen hellend dak/gordingen - massief hout ","PM",null,"Geen",{"$nulls":4},1]
["28.25.12.","structuurelementen - onderdelen hellend dak/gordingen - gelamineerd hout ","PM",null,"Geen",{"$nulls":4},1]
["28.25.20.","structuurelementen - onderdelen hellend dak/keperwerk"]
["28.25.21.","structuurelementen - onderdelen hellend dak/keperwerk - massief hout ","PM",null,"Geen",{"$nulls":4},1]
["28.25.30.","structuurelementen - onderdelen hellend dak/spanten"]
["28.25.31.","structuurelementen - onderdelen hellend dak/spanten - massief hout"]
["28.25.40.","structuurelementen - onderdelen hellend dak/scharnierdak ","PM",null,"Geen",{"$nulls":4},1]
["28.25.50.","structuurelementen - onderdelen hellend dak/bakgootconstructies"]
["28.25.51.","structuurelementen - onderdelen hellend dak/bakgootconstructies - massief hout ","PM",null,"Geen",{"$nulls":4},1]
["28.25.60.","structuurelementen - onderdelen hellend dak/dakrandoversteken"]
["28.25.61.","structuurelementen - onderdelen hellend dak/dakrandoversteken - massief hout ","PM",null,"Geen",{"$nulls":4},1]
["28.25.70.","structuurelementen - onderdelen hellend dak/tengel- en panlatten ","PM",null,"Geen",{"$nulls":4},1]
["28.30.","wanden - algemeen"]
["28.31.","wanden - buitenwanden "]
["28.31.10.","wanden - buitenwanden/type I ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["28.31.20.","wanden - buitenwanden/type II ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["28.31.30.","wanden - buitenwanden/type III ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["28.32.","wanden - binnenwanden "]
["28.32.10.","wanden - binnenwanden/type I ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["28.32.20.","wanden - binnenwanden/type II ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["28.33.","wanden - woningscheidende wanden ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["28.34.","wanden - dakopstanden ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["28.40.","vloeren - algemeen"]
["28.41.","vloeren - roostering met beplating ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.42.","vloeren - geprefabriceerde houten vloeren"]
["28.42.10.","vloeren - geprefabriceerde houten vloeren/roostering met beplating ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.42.20.","vloeren - geprefabriceerde houten vloeren/kokervormige vloeren ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.42.30.","vloeren - geprefabriceerde houten vloeren/massieve houten vloeren ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.43.","vloeren - hout-betonvloeren ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.50.","hellende daken - algemeen"]
["28.51.","hellende daken - spanten ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Shell",null,null,null,1]
["28.52.","hellende daken - gordingen ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Shell",null,null,null,1]
["28.53.","hellende daken - scharnierdaken ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Shell",null,null,null,1]
["28.60.","platte daken - algemeen"]
["28.61.","platte daken - roostering met beplating ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.62.","platte daken - geprefabriceerde houten vloeren"]
["28.62.10.","platte daken - geprefabriceerde houten vloeren/roostering met beplating ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.62.20.","platte daken - geprefabriceerde houten vloeren/kokervormige vloeren ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.62.30.","platte daken - geprefabriceerde houten vloeren/massieve houten vloeren ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.63.","platte daken - hout-betonvloeren ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.64.","platte daken - randisolatie ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Roof",null,"Omtrek ",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Omtrek ",null,1]

{"sheet":"30 Dak","index":5,"n_rows":535,"n_cols":10,"rows_kept":535,"cut":false,"hidden":false,"merged":[]}
["Artikelnummer","Artikelomschrijving","AvO","Eenheid","Type","Element","Element specificatie","Wat rekent de Meetstaat Manager?","Aandachtspunten"]
["30.","DAKOPBOUW HELLEND DAK"]
["30.00.","dakopbouw hellend dak - algemeen"]
["30.01.","dakopbouw hellend dak - stabiliteitsstudie ","PM",null,"Geen",{"$nulls":4},1]
["30.10.","houten dakstructuur - algemeen ","FH","m3","TYPE 3","Roof",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Roof",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Stuks",null,1]
[null,null,"PM"]
["30.11.","houten dakstructuur - muurplaten ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["30.12.","houten dakstructuur - gordingen"]
["30.12.10.","houten dakstructuur - gordingen/massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["30.12.20.","houten dakstructuur - gordingen/gelamineerd hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["30.13.","houten dakstructuur - keperwerk ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["30.14.","houten dakstructuur - keperspanten ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["30.15.","houten dakstructuur - prefabspanten ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
[{"$nulls":5},"Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["30.16.","houten dakstructuur - bakgootconstructies ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["30.17.","houten dakstructuur - dakrandoversteken ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["30.18.","houten dakstructuur - boordplanken"]
["30.18.10.","houten dakstructuur - boordplanken/massief hout ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["30.18.20.","houten dakstructuur - boordplanken/multiplex ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["30.20.","onderdak - algemeen"]
["30.21.","onderdak - soepele membranen ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
["30.22.","onderdak - platen"]
["30.22.10.","onderdak - platen/vezelcement ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["30.22.20.","onderdak - platen/houtvezelplaten ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["30.30.","tengel- & panlatten - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["31.","THERMISCHE ISOLATIE HELLEND DAK"]
["31.00.","thermische isolatie hellend dak - algemeen"]
["31.10.","isolatieplaten tussen dakstructuur - algemeen"]
["31.11.","isolatieplaten tussen dakstructuur - MW"]
["31.11.10.","isolatieplaten tussen dakstructuur - MW/18 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.11.20.","isolatieplaten tussen dakstructuur - MW/20 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.12.","isolatieplaten tussen dakstructuur - houtwol (WW)"]
["31.12.10.","isolatieplaten tussen dakstructuur - houtwol (WW)/18 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.12.20.","isolatieplaten tussen dakstructuur - houtwol (WW)/20 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.13.","isolatieplaten tussen dakstructuur - cellulose"]
["31.13.10.","isolatieplaten tussen dakstructuur - cellulose/18 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.13.20.","isolatieplaten tussen dakstructuur - cellulose/20 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.20.","isolatieplaten op dakstructuur (sarking) - algemeen"]
["31.21.","isolatieplaten op dakstructuur (sarking) - PUR of PIR"]
["31.21.10.","isolatieplaten op dakstructuur (sarking) - PUR of PIR/14 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.21.20.","isolatieplaten op dakstructuur (sarking) - PUR of PIR/16 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.22.","isolatieplaten op dakstructuur (sarking) - PF"]
["31.22.10.","isolatieplaten op dakstructuur (sarking) - PF/14 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.22.20.","isolatieplaten op dakstructuur (sarking) - PF/16 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.23.","isolatieplaten op dakstructuur (sarking) - XPS"]
["31.23.10.","isolatieplaten op dakstructuur (sarking) - XPS/14 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.23.20.","isolatieplaten op dakstructuur (sarking) - XPS/16 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.30.","ingeblazen isolatie - algemeen"]
["31.31.","ingeblazen isolatie - cellulose"]
["31.31.10.","ingeblazen isolatie - cellulose/18 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.31.20.","ingeblazen isolatie - cellulose/23 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.40.","binnenfolie - algemeen"]
["31.41.","binnenfolie - damprem ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["31.42.","binnenfolie - dampscherm ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["31.50.","isolerende dakelementen - algemeen"]
["31.51.","isolerende dakelementen - tweeschalig ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["32.","DAKBEDEKKING HELLEND DAK"]
["32.00.","dakbedekking hellend dak - algemeen"]
["32.01.","dakbedekking hellend dak - prestaties"]
["32.10.","pannen - algemeen"]
["32.11.","pannen - gebakken aarde ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["32.11.10.","pannen - gebakken aarde/dakvlak ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["32.11.20.","pannen - gebakken aarde/vormstukken ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[]
["32.11.30.","pannen - gebakken aarde/toebehoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["32.12.","pannen - beton ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["32.12.10.","pannen - beton/dakvlak ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["32.12.20.","pannen - beton/vormstukken ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["32.12.30.","pannen - beton/toebehoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["32.13.","pannen - metaal ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
["32.13.10.","pannen - gecoat staal/dakvlak ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["32.13.20.","pannen - gecoat staal/vormstukken ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["32.13.30.","pannen - gecoat staal/toebehoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["32.20.","leien - algemeen"]
["32.21.","leien - vezelcement ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["32.22.","leien - natuurleien ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["32.30.","golfplaten - algemeen"]
["32.31.","golfplaten - vezelcement ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
["32.31.10.","golfplaten - vezelcement/dakvlakken ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
["32.31.20.","golfplaten - vezelcement/vormstukken ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["32.31.30.","golfplaten - vezelcement/toebehoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["32.40.","geprofileerde metaalplaten - algemeen"]
["32.41.","geprofileerde metaalplaten - gecoat staal ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["32.42.","geprofileerde metaalplaten - aluminium ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["32.43.","geprofileerde metaalplaten - RVS ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["32.50.","toebehoren hellend dak - algemeen"]
["32.51.","toebehoren hellend dak - dakdoorvoeren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["32.52.","toebehoren hellend dak - verankeringssystemen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["32.53.","toebehoren hellend dak - valbeveiliging"]
["32.53.10.","toebehoren hellend dak - valbeveiliging / ankerpunten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["32.53.20.","toebehoren hellend dak - valbeveiliging / lijnsysteem ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["32.54.","toebehoren hellend dak - ladderhaken ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["33.","DAKVLOER PLAT DAK"]
["33.00.","dakvloer plat dak - algemeen"]
["33.01.","algemeen - stabiliteitsstudie"]
["33.10.","houten roostering - algemeen"]
["33.11.","houten roostering - muurplaten ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
["33.12.","houten roostering - balken"]
["33.12.10.","houten roostering - balken/massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
["33.12.20.",null,"FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,0,"FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"m3","TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["33.12.30.","houten roostering - balken/lichte samengestelde liggers ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["33.20.","beplating op houten roostering - algemeen",null,null,"TYPE 5",{"$nulls":4},1]
["33.21.","beplating op houten roostering - multiplex ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.22.","beplating op houten roostering - OSB ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.23.","beplating op houten roostering - spaanplaat ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.24.","beplating op houten roostering - cementgebonden spaanplaat ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.30.","zelfdragende elementen - algemeen"]
["33.31.","zelfdragende elementen - profielplaten staal"]
["33.31.10.","zelfdragende elementen - profielplaten staal/enkelvoudig ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.32.","zelfdragende elementen - sandwichplaten hout ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.40.","hellingsbeton - algemeen"]
["33.41.","hellingsbeton - niet isolerend"]
["33.41.10.","hellingsbeton - niet isolerend/mager beton ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.41.20.","hellingsbeton - niet isolerend/zandcement dekvloer ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.52.","hellingsbeton - licht isolerend"]
["33.52.10.","hellingsbeton - licht isolerend/granulaten ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.52.20.","hellingsbeton - licht isolerend/schuimbeton ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.","THERMISCHE ISOLATIE PLAT DAK"]
["34.00.","thermische isolatie plat dak - algemeen"]
["34.10.","isolatieplaten plat dak - algemeen"]
["34.11.","isolatieplaten plat dak - MW"]
["34.11.10.","isolatieplaten plat dak - MW/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.11.20.","isolatieplaten plat dak - MW/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.12.","isolatieplaten plat dak - PUR of PIR"]
["34.12.10.","isolatieplaten plat dak - PUR of PIR/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.12.20.","isolatieplaten plat dak - PUR of PIR/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.13.","isolatieplaten plat dak - EPS"]
["34.13.10.","isolatieplaten plat dak - EPS/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.13.20.","isolatieplaten plat dak - EPS/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.14.","isolatieplaten plat dak - CG"]
["34.14.10.","isolatieplaten plat dak - CG/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.14.20.","isolatieplaten plat dak - CG/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.15.","isolatieplaten omkeerdak - XPS"]
["34.15.10.","isolatieplaten omkeerdak - XPS/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.15.20.","isolatieplaten omkeerdak - XPS/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.20.","dampscherm - algemeen"]
["34.21.","dampscherm - gewapend bitumen ","PM",null,"Geen",{"$nulls":4},1]
["35.","AFDICHTING & AFWERKING PLAT DAK"]
["35.00.","afdichting & afwerking plat dak - algemeen"]
["35.01.","afdichting & afwerking plat dak - waterdichtheidsproeven ","PM",null,"Geen",{"$nulls":4},1]
["35.02.","afdichting & afwerking plat dak - waarborgen & attesten ","PM",null,"Geen",{"$nulls":4},1]
["35.03.","afdichting & afwerking plat dak - renovatie bestaande daken ","PM",null,"Geen",{"$nulls":4},1]
["35.10.","bitumineuze dakafdichting - algemeen"]
["35.11.","bitumineuze dakafdichting - SBS"]
["35.11.10.","bitumineuze dakafdichting - SBS/losliggend (L) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.11.20.","bitumineuze dakafdichting - SBS/deelgekleefd (P) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.11.30.","bitumineuze dakafdichting - SBS/volgekleefd (T) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.11.40.","bitumineuze dakafdichting - SBS/mechanisch (M) ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.12.","bitumineuze dakafdichting - APP","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
["35.12.10.","bitumineuze dakafdichting - APP/losliggend (L) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.12.20.","bitumineuze dakafdichting - APP/deelgekleefd (P) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.12.30.","bitumineuze dakafdichting - APP/volgekleefd (T) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.12.40.","bitumineuze dakafdichting - APP/mechanisch (M) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.13.","bitumineuze dakafdichting - PBE"]
["35.20.","kunststof dakafdichting - algemeen"]
["35.21.","kunststof dakafdichting - EPDM"]
["35.21.10.","kunststof dakafdichting - EPDM/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.21.20.","kunststof dakafdichting - EPDM/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.21.30.","kunststof dakafdichting - EPDM/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.22.","kunststof dakafdichting - TPO"]
["35.22.10.","kunststof dakafdichting - TPO/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.22.20.","kunststof dakafdichting - TPO/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.22.30.","kunststof dakafdichting - TPO/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.23.","kunststof dakafdichting - PVC"]
["35.23.10.","kunststof dakafdichting - PVC/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.23.20.","kunststof dakafdichting - PVC/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.23.30.","kunststof dakafdichting - PVC/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.24.","kunststof dakafdichting - CPE"]
["35.24.10.","kunststof dakafdichting - CPE/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.24.20.","kunststof dakafdichting - CPE/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.24.30.","kunststof dakafdichting - CPE/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.25.","kunststof dakafdichting - PIB"]
["35.25.10.","kunststof dakafdichting - PIB/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.25.20.","kunststof dakafdichting - PIB/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.25.30.","kunststof dakafdichting - PIB/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.26.","kunststof dakafdichting - ECB"]
["35.26.10.","kunststof dakafdichting - ECB/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.26.20.","kunststof dakafdichting - ECB/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.26.30.","kunststof dakafdichting - ECB/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.30.","ballastlaag - algemeen"]
["35.31.","ballastlaag - grind ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.32.","ballastlaag - tegels ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.33.","ballastlaag - geotextiel ","PM",null,"Geen",{"$nulls":4},1]
["35.40.","groendak - algemeen"]
["35.41.","groendak - extensief ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.42.","groendak - intensief ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.50.","toebehoren plat dak - algemeen"]
["35.51.","toebehoren plat dak - dakdoorvoeren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["35.52.","toebehoren plat dak - verankeringssystemen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["35.53.","toebehoren plat dak - valbeveiliging"]
["35.53.10.","toebehoren plat dak - valbeveiliging/doodgewicht ankers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["35.53.20.","toebehoren plat dak - valbeveiliging/vaste ankerpunten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["35.53.30.","toebehoren plat dak - valbeveiliging/lijnsysteem ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,null,"m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["36.","DAKLICHTOPENINGEN"]
["36.00.","daklichtopeningen - algemeen"]
["36.10.","dakvlakramen - algemeen"]
["36.11.","dakvlakramen - hout"]
["36.11.10.","dakvlakramen - hout/wentel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.11.20.","dakvlakramen - hout/uitzet en wentel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.11.30.","dakvlakramen - hout/uitzet ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.11.40.","dakvlakramen - hout/rook- & warmteafvoer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.12.","dakvlakramen - kunststof"]
["36.12.10.","dakvlakramen - kunststof/wentel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.12.20.","dakvlakramen - kunststof/uitzet-wentel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.12.30.","dakvlakramen - kunststof/uitzet ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.12.40.","dakvlakramen - kunststof/rook- en warmteafvoer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.13.","dakvlakramen - zolderraam ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.20.","platdakramen - algemeen"]
["36.21.","platdakramen - kunststof"]
["36.21.10.","platdakramen - kunststof/vast ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.21.20.","platdakramen - kunststof/opengaand ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.21.30.","platdakramen - kunststof/rook- en warmteafvoer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.30.","koepels - algemeen"]
["36.31.","koepels - kunststof acrylaat (PMMA)"]
["36.31.10.","koepels - kunststof acrylaat (PMMA)/vast ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.31.20.","koepels - kunststof acrylaat (PMMA)/opengaand ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.31.30.","koepels - kunststof acrylaat (PMMA)/rook en warmteafvoer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.32.","koepels - kunststof polycarbonaat (PC) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.40.","daglichtreflectiebuizen - algemeen"]
["36.41.","daglichtreflectiebuizen - plat dak ","FH","m2","TYPE 5","Object",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Net Area",null,1]
["36.42.","daglichtreflectiebuizen - hellend dak ","FH","m2","TYPE 5","Object",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Net Area",null,1]
["36.50.","lichtstraten - algemeen"]
["36.51.","lichtstraten - profielen hout"]
["36.51.10.","lichtstraten - profielen hout/met beglazing ","FH","m2","TYPE 3","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Area",null,1]
[{"$nulls":5},"Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Skylight",null,"Net Area",null,1]
["36.52.","lichtstraten - profielen aluminium"]
["36.52.10.","lichtstraten - profielen aluminium met beglazing ","FH","m2","TYPE 3","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Area",null,1]
[{"$nulls":5},"Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Skylight",null,"Net Area",null,1]
["36.60.","dakkapellen - algemeen"]
["36.61.","dakkapellen - traditioneel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["37.","DAKRANDEN EN KROONLIJSTEN"]
["37.00.","dakranden en kroonlijsten - algemeen"]
["37.10.","slabben, loketten en aansluitbanden - algemeen"]
["37.11.","slabben, loketten en aansluitbanden - metaal"]
["37.11.10.","slabben, loketten en aansluitbanden - metaal/lood ","FH of VH","kg","TYPE 3","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,null,"kg","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Gewicht (kg) in bij Settings van het Object",null,1]
["37.11.20.","slabben, loketten en aansluitbanden - metaal/aluminium ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.11.30.","slabben, loketten en aansluitbanden - metaal/zink ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.11.40.","slabben, loketten en aansluitbanden - metaal/koper ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.12.","slabben, loketten en aansluitbanden - membranen"]
["37.12.10.","slabben, loketten en aansluitbanden - membraan/EPDM ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.12.20.","slabben, loketten en aansluitbanden - membraan/PIB ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.12.30.","slabben, loketten en aansluitbanden - membraan/bitumen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.20.","dakrandprofielen - algemeen"]
["37.21.","dakrandprofielen - metaal"]
["37.21.10.","dakrandprofielen - metaal/zink ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.21.20.","dakrandprofielen - metaal/aluminium ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.21.30.","dakrandprofielen - metaal/metaalfolieplaten ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.22.","dakrandprofielen - kunststof"]
["37.22.10.","dakrandprofielen - kunststof/polyester ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.30.","muurkappen - algemeen","FH","m","TYPE 3","Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
["37.31.","muurkappen - metaal"]
["37.31.10.","muurkappen - metaal/zink ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
["37.31.20.","muurkappen - metaal/aluminium ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
["37.32.","muurkappen - kunststof ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
["37.40.","uitbekleding kroonlijsten en luifels - algemeen"]
["37.41.","uitbekleding kroonlijsten en luifels - planchetten"]
["37.41.10.","uitbekleding kroonlijsten en luifels - planchetten/massief hout ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["37.41.20.","uitbekleding kroonlijsten en luifels - planchetten/kunststof ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.41.30.","uitbekleding kroonlijsten en luifels - planchetten/vezelcement ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.42.","uitbekleding kroonlijsten en luifels - platen"]
["37.42.10.","uitbekleding kroonlijsten en luifels - platen/multiplex ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.42.20.","uitbekleding kroonlijsten en luifels - platen/kunststof ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.42.30.","uitbekleding kroonlijsten en luifels - platen/vezelcement ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.42.40.","uitbekleding kroonlijsten en luifels - platen/kunsthars ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.42.50.","uitbekleding kroonlijsten en luifels - platen/minerale vezels ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.43.","uitbekleding kroonlijsten en luifels - leien"]
["37.43.10.","uitbekleding kroonlijsten en luifels - leien/vezelcement ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.43.20.","uitbekleding kroonlijsten en luifels - leien hout ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.50.","toebehoren dakranden - algemeen"]
["37.51.","toebehoren dakranden - valbeveiliging"]
["37.51.10.","toebehoren dakranden - valbeveiliging/lijn- of railsysteem ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["37.51.20.","toebehoren dakranden - valbeveiliging/permanente leuning ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["37.52.","toebehoren dakranden - gevelonderhoudsinstallaties"]
["37.52.10.","toebehoren dakranden - gevelonderhoud/railsysteem ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["37.53.","toebehoren dakranden - verhuisbalk ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
["38.","DAKWATERAFVOER"]
["38.00.","dakwaterafvoer - algemeen"]
["38.10.","bakgootdichtingen - algemeen"]
["38.11.","bakgootdichtingen - metaalbladen"]
["38.11.10.","bakgootdichtingen - metaalbladen/zink ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.11.20.","bakgootdichtingen - metaalbladen/koper ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.12.","bakgootdichtingen - bitumen"]
["38.12.10.","bakgootdichtingen - bitumen/SBS ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.12.20.","bakgootdichtingen - bitumen/APP ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.13.","bakgootdichtingen - hoog polymeermembranen"]
["38.13.10.","bakgootdichtingen - hoog polymeermembranen/EPDM ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.13.20.","bakgootdichtingen - hoog polymeermembranen/TPO ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.13.30.","bakgootdichtingen - hoog polymeermembranen/PVC ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.20.","hanggoten - algemeen"]
["38.21.","hanggoten - kunststof"]
["38.21.10.","hanggoten - kunststof/PVC ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.21.20.","hanggoten - kunststof/polyesterhars ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.22.","hanggoten - metaal"]
["38.22.10.","hanggoten - metaal/zink ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.22.20.","hanggoten - metaal/aluminium ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.22.30.","hanggoten - metaal/koper ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.22.40.","hanggoten - metaal/gecoat staal ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.22.50.","hanggoten - metaal/roestvast staal ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.30.","afvoerpijpen - algemeen"]
["38.31.","afvoerpijpen - kunststof"]
["38.31.10.","afvoerpijpen - kunststof/PVC ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.31.20.","afvoerpijpen - kunststof/HDPE ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.32.","afvoerpijpen - metaal","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.32.10.","afvoerpijpen - metaal/zink ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.32.20.","afvoerpijpen - metaal/koper ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.32.30.","afvoerpijpen - metaal/aluminium ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.32.40.","afvoerpijpen - metaal/gecoat staal ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.32.50.","afvoerpijpen - metaal/roestvast staal ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.40.","eindstukken - algemeen","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.41.","eindstukken - slagvast kunststof ","FH","st","TYPE 5","Object",null,"Stuks",null,2]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["38.42.","eindstukken - behandeld gietijzer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["38.43.","eindstukken - gegoten aluminium ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["38.50.","toebehoren - algemeen",null,null,"Geen",{"$nulls":4},1]
["38.51.","toebehoren - dakkolken en tapbuizen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["38.52.","toebehoren - draad- en bolroosters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["38.53.","toebehoren - balkonafvoerputjes ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["38.54.","toebehoren - noodspuwers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]

{"sheet":"40 Gevelsluiting","index":6,"n_rows":231,"n_cols":10,"rows_kept":231,"cut":false,"hidden":false,"merged":[]}
["Artikelnummer","Artikelomschrijving","AvO","Eenheid","Type","Element","Element specificatie","Wat rekent de Meetstaat Manager?","Aandachtspunten"]
["40.","BUITENSCHRIJNWERK"]
["40.00.","buitenschrijnwerk - algemeen"]
["40.01.","buitenschrijnwerk - prestaties"]
["40.02.","buitenschrijnwerk - proeven"]
["40.02.10.","buitenschrijnwerk - proeven/op kosten ongelijk ","PM",null,"Geen",{"$nulls":4},1]
["40.02.20.","buitenschrijnwerk - proeven/op kosten aannemer ","VH","st","TYPE 5","Object",null,"Stuks",null,1]
["40.03.","buitenschrijnwerk - montage"]
["40.03.10.","buitenschrijnwerk - montage/spouwconstructie en dorpel ","PM",null,"Geen",{"$nulls":4},1]
["40.03.20.","buitenschrijnwerk - montage/buitengevelisolatiesysteem ","PM",null,"Geen",{"$nulls":4},1]
["40.03.30.","buitenschrijnwerk - montage/gevelbekledingsysteem ","PM",null,"Geen",{"$nulls":4},1]
["40.03.40.","buitenschrijnwerk - montage/houtskeletbouw ","PM",null,"Geen",{"$nulls":4},1]
["40.03.50.","buitenschrijnwerk - montage/vervanging schrijnwerk ","PM",null,"Geen",{"$nulls":4},1]
["40.04.","buitenschrijnwerk - borderel"]
["40.10.","profielsystemen - algemeen"]
["40.11.","profielsysteem - hout"]
["40.11.10.","profielsysteem - hout/vaste ramen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.11.20.","profielsysteem - hout/draairamen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.11.30.","profielsysteem - hout/schuiframen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,null,"m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
["40.11.40.","profielsysteem - hout/buitendeuren ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.12.","profielsysteem - aluminium"]
["40.12.10.","profielsysteem - aluminium/vaste ramen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.12.20.","profielsysteem - aluminium/draairamen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.12.30.","profielsysteem - aluminium/schuiframen ","FH of PM","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,null,"m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
["40.12.40.","profielsysteem - aluminium/buitendeuren ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
["40.13.","profielsysteem - pvc"]
["40.13.10.","profielsysteem - pvc/vaste ramen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.13.20.","profielsysteem - pvc/draairamen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,null,"m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
["40.13.30.","profielsysteem - pvc/schuiframen ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.13.40.","profielsysteem - pvc/buitendeuren ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
["40.14.","profielsysteem - staal"]
["40.14.10.","profielsysteem - staal/vaste ramen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.14.20.","profielsysteem - staal/buitendeuren ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
[]
["40.20.","hang- en sluitwerk - algemeen"]
["40.21.","hang- en sluitwerk - standaard beslag ","PM",null,"Geen",{"$nulls":4},1]
["40.22.","hang- en sluitwerk - scharnieren en paumellen ","PM",null,"Geen",{"$nulls":4},1]
["40.23.","hang- en sluitwerk - sloten ","PM",null,"Geen",{"$nulls":4},1]
["40.23.10.","hang- en sluitwerk - sloten/manueel ","PM",null,"Geen",{"$nulls":4},1]
["40.23.20.","hang- en sluitwerk - sloten/elektromagnetisch ","PM",null,"Geen",{"$nulls":4},1]
["40.23.30.","hang- en sluitwerk - sloten/schuifdeurslot ","PM",null,"Geen",{"$nulls":4},1]
["40.23.40.","hang- en sluitwerk - sloten/glasdeurslot ","PM",null,"Geen",{"$nulls":4},1]
["40.23.50.","hang- en sluitwerk - sloten/sleutelplan ","PM",null,"Geen",{"$nulls":4},1]
["40.24.","hang- en sluitwerk - deurdrangers ","PM",null,"Geen",{"$nulls":4},1]
["40.24.10.","hang- en sluitwerk - deurdrangers/manueel ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurdranger","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.24.20.","hang- en sluitwerk - deurdrangers/gemotoriseerd ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurdranger","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.25.","hang- en sluitwerk - panieksluitingen ","PM",null,"Geen",{"$nulls":4},1]
["40.26.","hang- en sluitwerk - raamkrukken ","PM",null,"Geen",{"$nulls":4},1]
["40.27.","hang- en sluitwerk - deurkrukken ","PM",null,"Geen",{"$nulls":4},1]
["40.28.","hang- en sluitwerk - vaste handgrepen ","PM",null,"Geen",{"$nulls":4},1]
["40.29.","hang- en sluitwerk - toebehoren"]
["40.30.","ventilatieroosters - algemeen"]
["40.31.","ventilatieroosters - op glas"]
["40.31.10.","ventilatieroosters - op glas/kleprooster ","PM",null,"Geen",{"$nulls":4},1]
["40.32.","ventilatieroosters - op profiel"]
["40.32.10.","ventilatieroosters - op profiel/kleprooster ","PM",null,"Geen",{"$nulls":4},1]
["40.40","beglazing - algemeen"]
["40.40.10.","beglazing - prestaties"]
["40.41.","beglazing - enkel glas"]
["40.41.10.","beglazing - enkel glas/type 1 ","PM",null,"Geen",{"$nulls":4},1]
["40.42.","beglazing - dubbele beglazing"]
["40.42.10.","beglazing - dubbele beglazing/type 1 ","PM",null,"Geen",{"$nulls":4},1]
["40.42.20.","beglazing - dubbele beglazing/type 2 ","PM",null,"Geen",{"$nulls":4},1]
["40.43.","beglazing - drievoudige beglazing"]
["40.43.10.","beglazing - drievoudige beglazing/type 1 ","PM",null,"Geen",{"$nulls":4},1]
["40.43.20.","beglazing - driedubbele beglazing/type 2 ","PM",null,"Geen",{"$nulls":4},1]
["40.44.","beglazing - bijzondere beglazing"]
["40.44.10.","beglazing - bijzondere beglazing/dun monumentenglas ","PM",null,"Geen",{"$nulls":4},1]
["40.50.","vulelementen - algemeen"]
["40.51.","vulelementen - kunststof ","PM",null,"Geen",{"$nulls":4},1]
["40.52.","vulelementen - aluminium ","PM",null,"Geen",{"$nulls":4},1]
["40.53.","vulelementen - kunsthars ","PM",null,"Geen",{"$nulls":4},1]
["40.54.","vulelementen - vezelcement ","PM",null,"Geen",{"$nulls":4},1]
["40.55.","vulelementen - multiplexplaten  ","PM",null,"Geen",{"$nulls":4},1]
["40.56.","vulelementen - massief houten beplanking ","PM",null,"Geen",{"$nulls":4},1]
["40.60.","raamdorpels - algemeen"]
["40.70.","omkaderingselementen - algemeen"]
["40.71.","omkaderingselementen - hout ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten","Lengte omkaderingselement",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.72.","omkaderingselementen - aluminium ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten","omtrek dagkant uitgezonderd lengte dorpel",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten","Lengte omkaderingselement",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.80.","toebehoren - algemeen"]
["40.81.","toebehoren - brievenkleppen ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.82.","toebehoren - deurspionnen ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.83.","toebehoren - beschermplaten ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.84.","toebehoren - deurstoppen ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.85.","toebehoren - huisnummers ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.86.","toebehoren - deur- en naambordjes ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.87.","toebehoren - doorvalbeveiliging"]
["40.87.10.","toebehoren - doorvalbeveiliging/kokerprofiel ","FH","m ","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.87.20.","toebehoren - doorvalbeveiliging/glasplaat ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["41.","POORTEN & EXTERNE ZONWERING"]
["41.00.","poorten & externe zonwering - algemeen"]
["41.10.","kantelpoorten - algemeen"]
["41.11.","kantelpoorten - poortblad staal"]
["41.11.10.","kantelpoorten - poortblad staal/manueel ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.11.20.","kantelpoorten - poortblad staal/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.12.","kantelpoorten - poortblad hout"]
["41.12.10.","kantelpoorten - poortblad hout/manueel ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.12.20.","kantelpoorten - poortblad hout/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.13.","kantelpoorten - poortblad kunststof"]
["41.13.10.","kantelpoorten - poortblad kunststof/manueel ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.13.20.","kantelpoorten - poortblad kunststof/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.20.","sectionaalpoorten - algemeen"]
["41.21.","sectionaalpoorten - staal"]
["41.21.10.","sectionaalpoorten - staal/manueel ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.21.20.","sectionaalpoorten - staal/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.22.","sectionaalpoorten - aluminium"]
["41.22.10.","sectionaalpoorten - aluminium/manueel ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.22.20.","sectionaalpoorten - aluminium/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.30.","Externe zonnewering - algemeen",{"$nulls":6},"Uitbreiding op de basis VMSW artikellijst"]
["41.31.","Externe zonnewering - rolluiken","FH","m2","TYPE 4","Window","ARCHICAD property: VMSW zonnewering","W/D Opening Surface on the Reveal Side","Uitbreiding op de basis VMSW artikellijst",1]
["41.32.","Externe zonnewering - screens","FH","m2","TYPE 4","Window","ARCHICAD property: VMSW zonnewering","W/D Opening Surface on the Reveal Side","Uitbreiding op de basis VMSW artikellijst",1]
["42.","GEVELBEKLEDINGEN"]
["42.00.","gevelbekledingen - algemeen"]
["42.10.","regelstructuur - algemeen"]
["42.11.","regelstructuur - hout ","PM",null,"Geen",{"$nulls":4},1]
["42.12.","regelstructuur - aluminium ","PM",null,"Geen",{"$nulls":4},1]
["42.20.","thermische isolatie voorhanggevel - algemeen"]
["42.21.","thermische isolatie voorhanggevel - MW"]
["42.21.10.","thermische isolatie voorhanggevel - MW/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.21.20.","thermische isolatie voorhanggevel - MW/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.22.","thermische isolatie voorhanggevel - PUR of PIR"]
["42.22.10.","thermische isolatie voorhanggevel - PUR of PIR/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.22.20.","thermische isolatie voorhanggevel - PUR of PIR/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.23.","thermische isolatie voorhanggevel - PF"]
["42.23.10.","thermische isolatie voorhanggevel - PF/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.23.20.","thermische isolatie voorhanggevel - PF/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.24.","thermische isolatie voorhanggevel - EPS"]
["42.24.10.","thermische isolatie voorhanggevel - EPS/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.24.20.","thermische isolatie voorhanggevel - EPS/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.25.","thermische isolatie voorhanggevel - XPS"]
["42.25.10.","thermische isolatie voorhanggevel - XPS/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.25.20.","thermische isolatie voorhanggevel - XPS/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.30.","buitenfolie - algemeen"]
["42.31.","buitenfolie - gevelfolie ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["42.40.","bekledingspanelen - algemeen"]
["42.41.","bekledingspanelen - HPL ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["42.42.","bekledingspanelen - vezelcement ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["42.43.","bekledingspanelen - minerale vezels ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["42.50.","bekledingsplanchetten - algemeen"]
["42.51.","bekledingsplanchetten - massief hout ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["42.52.","bekledingsplanchetten - kunststof ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["42.53.","bekledingsplanchetten - vezelcement ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["42.60.","gevelleien - algemeen"]
["42.61.","gevelleien - vezelcementleien ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["42.70.","geprofileerde metaalplaten - algemeen"]
["42.71.","geprofileerde metaalplaten - gecoat staal ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["42.72.","geprofileerde metaalplaten - aluminium ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["43.","BUITENBEPLEISTERING"]
["43.00.","buitenbepleistering - algemeen"]
["43.10.","sierpleisters op metselwerk - algemeen"]
["43.11.","sierpleisters op metselwerk - minerale pleister ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["43.20.","buitengevelisolatiesystemen met pleister - algemeen"]
["43.21.","buitengevelisolatiesystemen met pleister - EPS"]
["43.21.10.","buitengevelisolatiesystemen met pleister - EPS/isolatie"]
["43.21.11.","buitengevelisolatiesystemen met pleister - EPS/isolatie - 14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["43.21.12.","buitengevelisolatiesystemen met pleister - EPS/isolatie - 16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["43.21.20.","buitengevelisolatiesystemen met pleister - EPS/pleister ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["43.22.","buitengevelisolatiesystemen met pleister - MW"]
["43.22.10.","buitengevelisolatiesystemen met pleister - MW/isolatie"]
["43.22.11.","buitengevelisolatiesystemen met pleister - MW/isolatie - 14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["43.22.12.","buitengevelisolatiesystemen met pleister - MW/isolatie - 16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["43.22.20.","buitengevelisolatiesystemen met pleister - MW/pleister ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["44.","BUITENTRAPPEN & BORSTWERINGEN"]
["44.00.","buitentrappen en borstweringen - algemeen"]
["44.10.","trappen - algemeen"]
["44.11.","trappen - staal ","FH","st","TYPE 5","Stair",null,"Stuks",null,1]
[null,null,"SOG"]
["44.20.","borstweringen - algemeen"]
["44.21.","borstweringen - staal ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
[null,null,null,"st","TYPE 5","Railing",null,"Stuks",null,1]
["44.22.","borstweringen - roestvast staal (RVS) ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["44.23.","borstweringen - aluminium ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["44.24.","borstweringen - veiligheidsglas ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["44.30.","trapleuningen - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["44.40.","vulpanelen en -roosters - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["44.50.","handgrepen - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["44.60.","brandladders - algemeen"]
["44.61.","brandladders - verzinkt staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Stair",null,"Stuks",null,1]
["44.62.","brandladders - aluminium ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Stair",null,"Stuks",null,1]

{"sheet":"50 Afwerking (bi)","index":7,"n_rows":566,"n_cols":10,"rows_kept":566,"cut":false,"hidden":false,"merged":[]}
["Artikelnummer","Artikelomschrijving","AvO","Eenheid","Type","Element","Element specificatie","Wat rekent de Meetstaat Manager?","Aandachtspunten"]
["50.","BINNENPLEISTERWERKEN"]
["50.00.","binnenpleisterwerken - algemeen"]
["50.10.","wandbepleistering - algemeen"]
["50.11.","wandbepleistering - gipspleisters"]
["50.11.10.","wandbepleistering - gipspleisters/dikpleister op metselwerk"]
["50.11.11.","wandbepleistering - gipspleisters/dikpleisters op metselwerk - wandvlakken ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,null,"m2","TYPE 5","Object","Interieurafwerking ","Hoeveelheid onder negge/dagkant",null,1]
["50.11.12.","wandbepleistering - gipspleisters/dikpleisters op metselwerk - dagkanten ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m","TYPE 4","Object","Interieurafwerking - Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","Hoeveelheid onder negge/dagkant",null,1]
["50.11.20.","wandbepleistering - gipspleisters/dunpleister op lijmblokken"]
["50.11.21.","wandbepleistering - gipspleisters/dunpleister op lijmblokken - wandvlakken ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,null,"m2","TYPE 5","Object","Interieurafwerking ","Hoeveelheid onder negge/dagkant",null,1]
["50.11.22.","wandbepleistering - gipspleisters/dunpleister op lijmblokken - dagkanten ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m","TYPE 4","Object","Interieurafwerking - Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","Hoeveelheid onder negge/dagkant",null,1]
["50.11.30.","wandbepleistering - gipspleisters/pleister op beplating"]
["50.11.31.","wandbepleistering - gipspleisters/pleister op beplating - wandvlakken ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,null,"m2","TYPE 5","Object","Interieurafwerking ","Hoeveelheid onder negge/dagkant",null,1]
["50.11.32.","wandbepleistering - gipspleisters/pleister op beplating - dagkanten ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m","TYPE 4","Object","Interieurafwerking - Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","Hoeveelheid onder negge/dagkant",null,1]
["50.11.40.","wandbepleistering - gipspleisters/pleister op gaas"]
["50.11.41.","wandbepleistering - gipspleisters/pleister op gaas - wandvlakken ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,null,"m2","TYPE 5","Object","Interieurafwerking ","Hoeveelheid onder negge/dagkant",null,1]
["50.11.42.","wandbepleistering - gipspleisters/pleister op gaas - dagkanten ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m","TYPE 4","Object","Interieurafwerking - Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","Hoeveelheid onder negge/dagkant",null,1]
["50.12.","wandbepleistering - cementpleisters"]
["50.12.10.","wandbepleistering - cementpleisters/te betegelen ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,null,"m2","TYPE 5","Object","Interieurafwerking ","Hoeveelheid onder negge/dagkant",null,1]
["50.12.20.","wandbepleistering - cementpleisters/afwerksysteem ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,null,"m2","TYPE 5","Object","Interieurafwerking ","Hoeveelheid onder negge/dagkant",null,1]
["50.20.","plafondbepleistering - algemeen"]
["50.21.","plafondbepleistering - gipspleisters"]
["50.21.10.","plafondbepleistering - gipspleisters/dikpleister op welfsels"]
["50.21.11.","plafondbepleistering - gipspleisters/dikpleister op welfsels - plafondoppervlakte ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
[null,null,null,"m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m2","TYPE 5","Object","Plafondafwerking object","Hoeveelheden uit project",null,1]
[null,null,null,"m2","TYPE 4","Object","Plafondafwerking object bestaande uit meerdere schildelen (2 en 3)","Hoeveelheden uit project",null,1]
[null,null,null,"m3","TYPE 5","Object","Plafondafwerking object - enkel schil 1 ","Hoeveelheden uit project",null,1]
["50.21.12.","plafondbepleistering - gipspleisters/dikpleister op welfsels - zijkanten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[null,null,null,"m","TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["50.21.20.","plafondbepleistering - gipspleisters/dunpleister op breedplaatvloeren "]
["50.21.21.","plafondbepleistering - gipspleisters/dunpleister op breedplaatvloeren - plafondoppervlakte ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
[null,null,null,"m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m2","TYPE 5","Object","Plafondafwerking object","Hoeveelheden uit project",null,1]
[null,null,null,"m2","TYPE 4","Object","Plafondafwerking object bestaande uit meerdere schildelen (2 en 3)","Hoeveelheden uit project",null,1]
[null,null,null,"m3","TYPE 5","Object","Plafondafwerking object - enkel schil 1 ","Hoeveelheden uit project",null,1]
["50.21.22.","plafondbepleistering - gipspleisters/dunpleister op breedplaatvloeren - zijkanten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[null,null,null,"m","TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["50.21.30.","plafondbepleistering - gipspleisters/pleister op beplating "]
["50.21.31.","plafondbepleistering - gipspleisters/pleister op beplating - plafondoppervlakte ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
[null,null,null,"m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m2","TYPE 5","Object","Plafondafwerking object","Hoeveelheden uit project",null,1]
[null,null,null,"m2","TYPE 4","Object","Plafondafwerking object bestaande uit meerdere schildelen (2 en 3)","Hoeveelheden uit project",null,1]
[null,null,null,"m3","TYPE 5","Object","Plafondafwerking object - enkel schil 1 wordt in m3 berekend","Hoeveelheden uit project",null,1]
["50.21.32.","plafondbepleistering - gipspleisters/pleister op beplating - zijkanten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[null,null,null,"m","TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["50.21.40.","plafondbepleistering - gipspleisters/pleister op pleisterdrager "]
["50.21.41.","plafondbepleistering - gipspleisters/pleister op pleisterdrager - plafondoppervlakte ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
[null,null,null,"m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m2","TYPE 5","Object","Plafondafwerking object","Hoeveelheden uit project",null,1]
[null,null,null,"m2","TYPE 4","Object","Plafondafwerking object bestaande uit meerdere schildelen (2 en 3)","Hoeveelheden uit project",null,1]
[null,null,null,"m3","TYPE 5","Object","Plafondafwerking object - enkel schil 1 ","Hoeveelheden uit project",null,1]
["50.21.42.","plafondbepleistering - gipspleisters/pleister op pleisterdrager - zijkanten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["50.30.","renovatie pleisterwerk - algemeen ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
[null,null,null,"m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["51.","BINNENPLAATAFWERKINGEN"]
["51.00.","binnenplaatafwerkingen - algemeen"]
["51.10.","lichte scheidingswanden - algemeen"]
["51.11.","lichte scheidingswanden - gipskartonplaten ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.12.","lichte scheidingswanden - gipsvezelplaten ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.13.","lichte scheidingswanden - calciumsilicaatplaten ","FH","m2","TYPE 2","Wall",null,null,null,1]
[null,"lichte scheidingswanden - vezelcementplaten ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.14.","lichte scheidingswanden - calciumsilicaatplaten ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.15.","lichte scheidingswanden - multiplexplaten ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.16.","lichte scheidingswanden - OSB-platen ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.17.","lichte scheidingswanden - MDF-platen","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.20.","voorzetwanden - algemeen"]
["51.21.","voorzetwanden - gipskartonplaten"]
["51.21.10.","voorzetwanden - gipskartonplaten/op regelstructuur ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.21.20.","voorzetwanden - gipskartonplaten/gekleefd ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.22.","voorzetwanden - gipsvezelplaten"]
["51.22.10.","voorzetwanden - gipsvezelplaten/op regelstructuur ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.22.20.","voorzetwanden - gipsvezelplaten/gekleefd ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.23.","voorzetwanden - vezelcementplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.24.","voorzetwanden - calciumsilicaatplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.25.","voorzetwanden - multiplex ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.26.","voorzetwanden - OSB-platen ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.27.","voorzetwanden - MDF-platen","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.30.","schachtwanden - algemeen"]
["51.31.","schachtwanden - gipskartonplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.32.","schachtwanden - gipsvezelplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.33.","schachtwanden - vezelcementplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.34.","schachtwanden - calciumsilicaatplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.35.","schachtwanden - multiplexplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.36.","schachtwanden - OSB-platen ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.37.","schachtwanden - MDF-platen","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.38.","schachtwanden - kunstharsplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.40.","toegangsluiken - algemeen"]
["51.41.","toegangsluiken - hout ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Window",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["51.42.","toegangsluiken - kunsthars ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Window",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["51.43.","toegangsluiken - vezelcement ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Window",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["51.44.","toegangsluiken - metalen kader ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Window",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["51.50.","plafondafwerking - algemeen"]
["51.51.","plafondafwerking - uitbekleding plafond"]
["51.51.10.","plafondafwerking - uitbekleding plafond/gipskartonplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,2]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,2]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",2]
[{"$nulls":4},"TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,2]
["51.51.20.","plafondafwerking - uitbekleding plafond/gipsvezelplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.51.30.","plafondafwerking - uitbekleding plafond/vezelcementplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.51.40.","plafondafwerking - uitbekleding plafond/calciumsilicaatplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.51.50.","plafondafwerking - uitbekleding plafond/OSB","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.52.","plafondafwerking - uitbekleding daklichtopeningen ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 4","Object","gebruik ARCHICAD property: VMSW uitbekleding daglichtopeningen ",null,null,1]
[{"$nulls":4},"TYPE 4","Skylight","gebruik ARCHICAD property: VMSW uitbekleding daglichtopeningen ",null,null,1]
[null,null,null,"m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Object","gebruik ARCHICAD property: VMSW uitbekleding daglichtopeningen ",null,null,1]
[{"$nulls":4},"TYPE 4","Skylight","gebruik ARCHICAD property: VMSW uitbekleding daglichtopeningen ","Oppervlakte volgens openingshoogte daklicht en dikte dak",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["51.53.","plafondafwerking - verlaagd plafond"]
["51.53.10.","plafondafwerking - verlaagd plafond/gipskartonplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.53.20.","plafondafwerking - verlaagd plafond/gipsvezelplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.53.30.","plafondafwerking - verlaagd plafond/vezelcementplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.53.40.","plafondafwerking - verlaagd plafond/calciumsilicaatplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.60.","uitbekleding buitenramen en -deuren - algemeen"]
["51.61.","uitbekleding buitenramen en -deuren - isolatieplaten voor bepleistering ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["51.62.","uitbekleding buitenramen en -deuren - multiplex ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["51.63.","uitbekleding buitenramen en -deuren - MDF ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["51.64.","uitbekleding buitenramen en -deuren - massief hout ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["51.65.","uitbekleding buitenramen en -deuren - PVC ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["51.66.","uitbekleding buitenramen en -deuren - gipskarton ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["51.70.","uitbekleding sanitaire toestellen - algemeen"]
["51.71.","uitbekleding sanitaire toestellen - te betegelen plaat"]
["51.72.","uitbekleding sanitaire toestellen - plaat als eindafwerking"]
["52.","DEK- EN BEDRIJFSVLOEREN"]
["52.00.","dek- en bedrijfsvloeren - algemeen"]
["52.10.","isolerende uitvullagen - algemeen"]
["52.11.","isolerende uitvullagen - cementgebonden ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface"]
["52.12.","isolerende uitvullagen - schuimbeton ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface"]
["52.13.","isolerende uitvullagen - gespoten polyurethaan ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface"]
["52.14.","isolerende uitvullagen - droge granulaten ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface"]
["52.20.","vochtwerende lagen - algemeen"]
["52.21.","vochtwerende lagen - PE-folie ","PM",null,"Geen",{"$nulls":4},1]
["52.30.","thermische isolatie vloer - algemeen"]
["52.31.","thermische isolatie vloer - MW"]
["52.31.10.","thermische isolatie vloer - MW/8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.31.20.","thermische isolatie vloer - MW/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.32.","thermische isolatie vloer - PUR of PIR"]
["52.32.10.","thermische isolatie vloer - PUR of PIR 8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.32.20.","thermische isolatie vloer - PUR of PIR/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.33.","thermische isolatie vloer - PF"]
["52.33.10.","thermische isolatie vloer - PF/8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.33.20.","thermische isolatie vloer - PF/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.34.","thermische isolatie vloer - XPS"]
["52.34.10.","thermische isolatie vloer - XPS/8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.34.20.","thermische isolatie vloer - XPS/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.35.","thermische isolatie vloer - EPS"]
["52.35.10.","thermische isolatie vloer - EPS/8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.35.20.","thermische isolatie vloer - EPS/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.40.","akoestische isolatie vloer - algemeen"]
["52.41.","akoestische isolatie vloer - kunststofschuim ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.42.","akoestische isolatie vloer - kokosvezels ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.50.","cementgebonden dekvloeren - algemeen"]
["52.51.","cementgebonden dekvloeren - hechtend ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.52.","cementgebonden dekvloeren - niet hechtend ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.53.","cementgebonden dekvloeren - zwevend ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.54.","cementgebonden dekvloeren - zwevend en gepolierd ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.60.","calciumsulfaatgebonden dekvloeren - algemeen"]
["52.61.","calciumsulfaatgebonden dekvloeren - niet hechtend ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.62.","calciumsulfaatgebonden dekvloeren - zwevend ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.70.","bedrijfsvloeren - algemeen"]
["52.71.","bedrijfsvloeren - gepolierd beton ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.72.","bedrijfsvloeren - epoxymortel ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.","BINNENVLOERAFWERKINGEN"]
["53.00.","binnenvloerafwerkingen - algemeen"]
["53.10.","tegelvloeren - algemeen"]
["53.11.","tegelvloeren - keramisch"]
["53.11.10.","tegelvloeren - keramisch/getrokken tegels ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.11.20.","tegelvloeren - keramisch/geperste tegels ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.12.","tegelvloeren - marmermozaiek ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.13.","tegelvloeren - natuursteen"]
["53.13.10.","tegelvloeren - natuursteen/blauwe hardsteen ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.13.20.","tegelvloeren - natuursteen/travertijn ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.13.30.","tegelvloeren - natuursteen/jura ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.14.","tegelvloeren - betontegels ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.20.","soepele vloerbekledingen - algemeen"]
["53.21.","soepele vloerbekledingen - linoleum ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.22.","soepele vloerbekledingen - vinyl (PVC) ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.23.","soepele vloerbekledingen - rubber ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.24.","soepele vloerbekledingen - douchecellen ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.30.","houten vloerbekledingen - algemeen"]
["53.31.","houten vloerbekledingen - laminaat ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.32.","houten vloerbekledingen - opschuren bij renovatie ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.40.","plinten - algemeen"]
["53.41.","plinten - steen"]
["53.41.10.","plinten - steen/keramisch ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object ","Object interieurafwerking - enkel plint actief","Lengte","Let op! Enkel Horizontale lengte wordt gemeten ",1]
[{"$nulls":4},"TYPE 4","Object ","Object interieurafwerking - in dit object zijn andere opties (wandafwerking/lambrisering) actief > plint als type 4","Lengte","Let op! Enkel Horizontale lengte wordt gemeten ",1]
["53.41.20.","plinten - steen/marmermozaiek ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object","Object interieurafwerking - enkel plint actief","Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"TYPE 4","Object ","Object interieurafwerking - in dit object zijn andere opties (wandafwerking/lambrisering) actief > plint als type 4","Lengte","Let op! Enkel Horizontale lengte wordt gemeten ",1]
["53.41.30.","plinten - steen/natuursteen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object","Object interieurafwerking - enkel plint actief","Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"TYPE 4","Object ","Object interieurafwerking - in dit object zijn andere opties (wandafwerking/lambrisering) actief > plint als type 4","Lengte","Let op! Enkel Horizontale lengte wordt gemeten ",1]
["53.42.","plinten - hout"]
["53.42.10.","plinten - hout/massief hout ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object","Object interieurafwerking - enkel plint actief","Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"TYPE 4","Object ","Object interieurafwerking - in dit object zijn andere opties (wandafwerking/lambrisering) actief > plint als type 4","Lengte","Let op! Enkel Horizontale lengte wordt gemeten ",1]
["53.42.20.","plinten - hout/MDF ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object","Object interieurafwerking - enkel plint actief","Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"TYPE 4","Object ","Object interieurafwerking - in dit object zijn andere opties (wandafwerking/lambrisering) actief > plint als type 4","Lengte","Let op! Enkel Horizontale lengte wordt gemeten ",1]
["53.43.","plinten - soepel"]
["53.43.10.","plinten - soepel/linoleum ","FH\n","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object","Object interieurafwerking - enkel plint actief","Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"TYPE 4","Object ","Object interieurafwerking - in dit object zijn andere opties (wandafwerking/lambrisering) actief > plint als type 4","Lengte","Let op! Enkel Horizontale lengte wordt gemeten ",1]
["53.43.20.","plinten - soepel/PVC ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object","Object interieurafwerking - enkel plint actief","Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"TYPE 4","Object ","Object interieurafwerking - in dit object zijn andere opties (wandafwerking/lambrisering) actief > plint als type 4","Lengte","Let op! Enkel Horizontale lengte wordt gemeten ",1]
["53.43.30.","plinten - soepel/rubber ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object","Object interieurafwerking - enkel plint actief","Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"TYPE 4","Object ","Object interieurafwerking - in dit object zijn andere opties (wandafwerking/lambrisering) actief > plint als type 4","Lengte","Let op! Enkel Horizontale lengte wordt gemeten ",1]
["53.50.","tussendorpels - algemeen"]
["53.51.","tussendorpels - steen"]
["53.51.10.","tussendorpels - steen/natuursteen ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW tussendorpel binnendeur","breedte deuropening * muurdikte",null,1]
["53.51.20.","tussendorpels - steen/marmermozaiek ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW tussendorpel binnendeur","breedte deuropening * muurdikte",null,1]
["53.51.30.","tussendorpels - steen/composiet ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW tussendorpel binnendeur","breedte deuropening * muurdikte",null,1]
["53.60.","trapbekledingen - algemeen"]
["53.61.","trapbekledingen - steen"]
["53.61.10.","trapbekledingen - steen/keramisch ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks",null,1]
["53.61.20.","trapbekledingen - steen/marmermozaiek ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks",null,1]
["53.61.30.","trapbekledingen - steen/natuursteen ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks",null,1]
["53.62.","trapbekledingen - hout"]
["53.62.10.","trapbekledingen - hout/massief ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks",null,1]
["53.62.20.","trapbekledingen - hout/gelamineerd ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks",null,1]
["53.63.","trapbekledingen - soepel"]
["53.63.10.","trapbekledingen - soepel/rubber ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks",null,1]
["53.70.","toebehoren - algemeen"]
["53.71.","toebehoren - scheidingsprofielen ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["53.72.","toebehoren - vloermatkaders ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"Stuks",null,1]
["53.73.","toebehoren - vloermatten ","FH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"st","TYPE 3","Slab",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["53.74.","toebehoren - vloerdeksels "]
["53.74.10.","toebehoren - vloerdeksels/metaal","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["53.74.20.","toebehoren - vloerdeksels/betegelbaar","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["53.75.","toebehoren - vloerroosters ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"Stuks",null,1]
["53.76.","toebehoren - zettingsprofielen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["54.","BINNENDEUREN en -RAMEN"]
["54.00.","binnendeuren en -ramen - algemeen"]
["54.01.","binnendeuren en -ramen - prestaties"]
["54.02.","binnendeuren en -ramen - keuring en proeven"]
["54.03.","binnendeuren en -ramen - proefopstelling"]
["54.10.","deurkozijnen - algemeen"]
["54.11.","deurkozijnen - hout"]
["54.11.10.","deurkozijnen - hout/massief ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks",null,1]
["54.11.20.","deurkozijnen - hout/multiplex ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks",null,1]
["54.11.30.","deurkozijnen - hout/MDF ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks",null,1]
["54.12.","deurkozijnen - staal"]
["54.12.10.","deurkozijnen - staal/montagekozijn ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks",null,1]
["54.12.20.","deurkozijnen - staal/inbouwkozijn ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks",null,1]
["54.20.","deurbladen - algemeen"]
["54.21.","deurbladen - hout met holle kern"]
["54.21.10.","deurbladen - hout met holle kern/celrooster ","FH","st","TYPE 4","Door ","Gebruik ARCHICAD property: VMSW deurblad","Stuks",null,1]
["54.21.20.","deurbladen - hout met holle kern/tubespaan ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurblad","Stuks",null,1]
["54.22.","deurbladen - hout met volle kern"]
["54.22.10.","deurbladen - hout met volle kern/spaan ","FH","st","TYPE 4","Door ","Gebruik ARCHICAD property: VMSW deurblad","Stuks",null,1]
["54.22.20.","deurbladen - hout met volle kern/multiplex ","FH","st","TYPE 4","Door ","Gebruik ARCHICAD property: VMSW deurblad","Stuks",null,1]
["54.30.","deurgehelen - algemeen"]
["54.31.","deurgehelen - kozijnen hout"]
["54.31.10.","deurgehelen - kozijnen hout/brandwerend ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.31.20.","deurgehelen - kozijnen hout/inbraakwerend ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.31.30.","deurgehelen - kozijnen hout/passiefdeur ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.32.","deurgehelen - kozijnen staal"]
["54.32.10.","deurgehelen - kozijnen staal/brandwerend ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.32.20.","deurgehelen - kozijnen staal/inbraakwerend ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.40.","schuif- en vouwdeuren - algemeen"]
["54.41.","schuif- en vouwdeuren - schuifsystemen"]
["54.41.10.","schuif- en vouwdeuren - schuifsystemen/voorbouw ","FH","st","TYPE 5","Door ",null,"Stuks",null,1]
[{"$nulls":5},"Window ",null,"Stuks",null,1]
["54.41.20.","schuif- en vouwdeuren - schuifsystemen/inbouwmodule ","FH","st","TYPE 5","Door ",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Window ",null,"Stuks",null,1]
["54.42.","schuif- en vouwdeuren - vouwsystemen"]
["54.42.10.","schuif- en vouwdeuren - vouwsystemen/kunststof ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Window",null,"Stuks",null,1]
["54.50.","glazen deuren - algemeen"]
["54.51.","glazen deuren - opendraaiend ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.52.","glazen deuren - openschuivend ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.60.","hang- en sluitwerk - algemeen"]
["54.61.","hang- en sluitwerk - scharnieren en paumellen"]
["54.61.10.","hang- en sluitwerk - scharnieren en paumellen/aluminium ","PM",null,"Geen",{"$nulls":4},1]
["54.61.20.","hang- en sluitwerk - scharnieren en paumellen/vernikkeld staal ","PM",null,"Geen",{"$nulls":4},1]
["54.61.30.","hang- en sluitwerk - scharnieren en paumellen/roestvast staal ","PM",null,"Geen",{"$nulls":4},1]
["54.62.","hang- en sluitwerk - deursloten"]
["54.62.10.","hang- en sluitwerk - deursloten/klaviersloten ","PM",null,"Geen",{"$nulls":4},1]
["54.62.20.","hang- en sluitwerk - deursloten/veiligheidssloten ","PM",null,"Geen",{"$nulls":4},1]
["54.62.30.","hang- en sluitwerk - deursloten/elektromagnetisch ","PM",null,"Geen",{"$nulls":4},1]
["54.62.40.","hang- en sluitwerk - deursloten/kantschuiven ","PM",null,"Geen",{"$nulls":4},1]
["54.62.50.","hang- en sluitwerk - deursloten/panieksluitingen ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW panieksluiting","Stuks",null,1]
["54.63.","hang- en sluitwerk - deurkrukken"]
["54.63.10.","hang- en sluitwerk - deurkrukken/aluminium ","PM",null,"Geen",{"$nulls":4},1]
["54.63.20.","hang- en sluitwerk - deurkrukken/RVS ","PM",null,"Geen",{"$nulls":4},1]
["54.63.30.","hang- en sluitwerk - deurkrukken/kunststof ","PM",null,"Geen",{"$nulls":4},1]
["54.64.","hang- en sluitwerk - vaste handgrepen ","PM",null,"Geen",{"$nulls":4},1]
["54.65.","hang- en sluitwerk - deurdrangers ","PM",null,"Geen",{"$nulls":4},1]
["54.70.","vaste binnenramen - algemeen"]
["54.71.","vaste binnenramen - hout ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
["54.80.","toebehoren - algemeen"]
["54.81.","toebehoren - deurroosters"]
["54.82.","toebehoren - beschermplaten"]
["54.82.10.","toebehoren - beschermplaten/aluminium ","PM",null,"Geen",{"$nulls":4},1]
["55.","BINNENTRAPPEN EN LEUNINGEN"]
["55.00.","binnentrappen en leuningen - algemeen"]
["55.10.","trappen - algemeen"]
["55.11.","trappen - hout"]
["55.11.10.","trappen - hout/rechte treden ","FH","st","TYPE 5","Stair",null,"Stuks",null,1]
["55.11.20.","trappen - hout/verdreven treden ","FH","st","TYPE 5","Stair",null,"Stuks",null,1]
["55.12.","trappen - staal"]
["55.12.10.","trappen - staal/rechte treden ","FH","st","TYPE 5","Stair",null,"Stuks",null,1]
["55.12.20.","trappen - staal/verdreven treden ","FH","st","TYPE 5","Stair",null,"Stuks",null,1]
["55.20.","borstweringen - algemeen"]
["55.21.","borstweringen - hout ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["55.22.","borstweringen - staal ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["55.23.","borstweringen - roestvast staal ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["55.24.","borstweringen - aluminium ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["55.25.","borstweringen - veiligheidsglas ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["55.30.","handgrepen - algemeen"]
["55.31.","handgrepen - hout ","PM",null,"Geen",{"$nulls":4},1]
["55.32.","handgrepen - staal ","PM",null,"Geen",{"$nulls":4},1]
["55.33.","handgrepen - roestvast staal ","PM",null,"Geen",{"$nulls":4},1]
["55.34.","handgrepen - aluminium ","PM",null,"Geen",{"$nulls":4},1]
["55.40.","zoldertrappen en -luiken - algemeen"]
["55.41.","zoldertrappen en -luiken - hout ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["55.42.","zoldertrappen en -luiken - aluminium ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.","VAST BINNENMEUBILAIR",{"$nulls":5},"wat met samengestelde onderdelen?"]
["56.00.","vast binnenmeubilair - algemeen"]
["56.10.","keukenmeubelen - algemeen"]
["56.11.","keukenmeubelen - onderdelen"]
["56.11.10.","keukenmeubelen - onderdelen/stelpoten en plintplaat ","PM",null,"Geen",{"$nulls":4},1]
["56.11.20.","keukenmeubelen - onderdelen/corpus en leggers ","PM",null,"Geen",{"$nulls":4},1]
["56.11.30.","keukenmeubelen - onderdelen/fronten en zichtwanden ","PM",null,"Geen",{"$nulls":4},1]
["56.11.40.","keukenmeubelen - onderdelen/werkbladen ","PM",null,"Geen",{"$nulls":4},1]
["56.11.50.","keukenmeubelen - onderdelen/beslag en handgrepen ","PM",null,"Geen",{"$nulls":4},1]
["56.11.60.","keukenmeubelen - onderdelen/toebehoren ","PM",null,"Geen",{"$nulls":4},1]
["56.12.","keukenmeubelen - type 1 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.13.","keukenmeubelen - type 2 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.14.","keukenmeubelen - type 3 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.20.","badkamermeubelen - algemeen"]
["56.21.","badkamermeubelen - onderdelen"]
["56.21.10.","badkamermeubelen - onderdelen/stelpoten en plintplaat ","PM",null,"Geen",{"$nulls":4},1]
["56.21.20.","badkamermeubelen - onderdelen/corpus en leggers ","PM",null,"Geen",{"$nulls":4},1]
["56.21.30.","badkamermeubelen - onderdelen/fronten en zichtwanden ","PM",null,"Geen",{"$nulls":4},1]
["56.21.40.","badkamermeubelen - onderdelen/wastafeltabletten ","PM",null,"Geen",{"$nulls":4},1]
["56.21.50.","badkamermeubelen - onderdelen/beslag en handgrepen ","PM",null,"Geen",{"$nulls":4},1]
["56.21.60.","badkamermeubelen - onderdelen/toebehoren ","PM",null,"Geen",{"$nulls":4},1]
["56.22.","badkamermeubelen - type 1 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.23.","badkamermeubelen - type 2 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.24.","badkamermeubelen - type 3 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.30.","inbouwkasten - algemeen"]
["56.31.","inbouwkasten - onderdelen"]
["56.31.10.","inbouwkasten - onderdelen/stelpoten en plintplaat ","PM",null,"Geen",{"$nulls":4},1]
["56.31.20.","inbouwkasten - onderdelen/corpus en leggers ","PM",null,"Geen",{"$nulls":4},1]
["56.31.30.","inbouwkasten - onderdelen/fronten en zichtwanden ","PM",null,"Geen",{"$nulls":4},1]
["56.31.40.","inbouwkasten - onderdelen/tabletten en bureelbladen ","PM",null,"Geen",{"$nulls":4},1]
["56.31.50.","inbouwkasten - onderdelen/beslag en handgrepen ","PM",null,"Geen",{"$nulls":4},1]
["56.31.60.","inbouwkasten - onderdelen/toebehoren ","PM",null,"Geen",{"$nulls":4},1]
["56.32.","inbouwkasten - kastgeheel type 1 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.33.","inbouwkasten - kastgeheel type 2 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.34.","inbouwkasten - kastgeheel type 3 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.40.","parlofoonconsoles - algemeen"]
["56.41.","parlofoonconsoles - multiplexplaat ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["56.42.","parlofoonconsoles - kunstharsplaat ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["56.43.","parlofoonconsoles - metaalplaat"]
["56.43.10.","parlofoonconsoles - metaalplaat/gemoffeld staal ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["56.43.20.","parlofoonconsoles - metaalplaat/roestvast staal (RVS) ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["56.43.30.","parlofoonconsoles - metaalplaat/aluminium ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["56.50.","brievenbusgehelen - algemeen"]
["56.51.","brievenbusgehelen - multiplexplaat ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
["56.52.","brievenbusgehelen - kunstharsplaat ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
["56.53.","brievenbusgehelen - metaalplaat"]
["56.53.10.","brievenbusgehelen - metaalplaat/gemoffeld staal ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
["56.53.20.","brievenbusgehelen - metaalplaat/roestvast staal (RVS) ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
["56.53.30.","brievenbusgehelen - metaalplaat/gemoffeld aluminium ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
["56.60.","gordijnkasten - algemeen"]
["56.61.","gordijnkasten - hout"]
["56.61.10.","gordijnkasten - hout/massief ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
["56.61.20.","gordijnkasten - hout/houtspaanplaat ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
["56.61.30.","gordijnkasten - hout/multiplex ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
["56.61.40.","gordijnkasten - hout/MDF ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
["56.62.","gordijnkasten - kunststof ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[]
["57.","TABLET- EN WANDBEKLEDINGEN"]
["57.00.","tablet- en wandbekledingen - algemeen"]
["57.10.","venstertabletten - algemeen"]
["57.11.","venstertabletten - natuursteen"]
["57.11.10.","venstertabletten - natuursteen/marmer ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.11.20.","venstertabletten - natuursteen/blauwe hardsteen ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.11.30.","venstertabletten - natuursteen/leisteen ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.11.40.","venstertabletten - natuursteen/volgens prestaties ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.12.","venstertabletten - kunststeen"]
["57.12.10.","venstertabletten - kunststeen/marmermozaïek ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.12.20.","venstertabletten - kunststeen/vezelcement ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.12.30.","venstertabletten - kunststeen/composiet ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.13.","venstertabletten - hout"]
["57.13.10.","venstertabletten - hout/massief ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.13.20.","venstertabletten - hout/laminaat ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.14.","venstertabletten - kunststof"]
["57.14.10.","venstertabletten - kunststof/PVC ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.20.","wandbekledingen - algemeen"]
["57.21.","wandbekledingen - betegeling ","FH","m2","TYPE 3","Wall",null,"Netto oppervlakte binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["57.21.10.","wandbekledingen - betegeling/keramisch ","FH","m2","TYPE 3","Wall",null,"Netto oppervlakte binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]

{"sheet":"60 Installaties ","index":8,"n_rows":478,"n_cols":10,"rows_kept":478,"cut":false,"hidden":false,"merged":[]}
["Artikelnummer","Artikelomschrijving","AvO","Eenheid","Type","Element","Element specificatie","Wat rekent de Meetstaat Manager?","Aandachtspunten"]
["60.","SANITAIR LEIDINGNET"]
["60.00.","sanitair leidingnet - algemeen"]
["60.10.","afvoerbuizen - algemeen"]
["60.11.","afvoerbuizen - PVC ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["60.12.","afvoerbuizen - PE ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["60.13.","afvoerbuizen - PP ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["60.20.","verluchtingsbuizen - algemeen"]
["60.21.","verluchtingsbuizen - PVC ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.22.","verluchtingsbuizen - PE ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.23.","verluchtingsbuizen - beluchtingsventielen ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.30.","klokroosters - intern - algemeen"]
["60.31.","klokroosters - gietijzer ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.32.","klokroosters - aluminium ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.33.","klokroosters - roestvast staal (RVS) ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.34.","klokroosters - kunststof ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.40.","putdeksels - algemeen"]
["60.41.","putdeksels - gietijzer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.42.","putdeksels - aluminium ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.43.","putdeksels - roestvast staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.44.","putdeksels - kunststof ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.50.","sanitaire drukleidingen - algemeen"]
["60.51.","sanitaire drukleidingen - buizen"]
["60.51.10.","sanitaire drukleidingen - buizen/verzinkt staal ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.51.20.","sanitaire drukleidingen - buizen/koper ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.51.30.","sanitaire drukleidingen - buizen/kunststof ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.52.","sanitaire drukleidingen - collectoren ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.53.","sanitaire drukleidingen - leidingisolatie ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.54.","sanitaire drukleidingen - brandwerende doorvoeren ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.55.","sanitaire drukleidingen - verwarmingslint ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["60.56.","sanitaire drukleidingen - flexibele leidingen ","PM",null,"Geen",{"$nulls":4},1]
["60.60.","aansluiting leidingnet - algemeen"]
["60.61.","aansluiting leidingnet - reglementaire meterstraat ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["60.62.","aansluiting leidingnet - voedingsleidingen & tellers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["60.63.","aansluiting leidingnet - waterfilters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["60.70.","waterbehandeling - algemeen"]
["60.71.","waterbehandeling - ontharders ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["60.72.","waterbehandeling - filters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.","SANITAIRE TOESTELLEN & TOEBEHOREN"]
["61.00.","sanitaire toestellen en toebehoren - algemeen"]
["61.10.","toiletpotten en toebehoren - algemeen"]
["61.11.","toiletpotten en toebehoren - staand ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.12.","toiletpotten en toebehoren - hangend ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.20.","handwastafels en toebehoren - algemeen"]
["61.21.","handwastafels & toebehoren - wandmodel"]
["61.21.10.","handwastafels & toebehoren - wandmodel/porselein ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.22.","handwastafels en toebehoren - inbouwmodel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.30.","wastafels en toebehoren - algemeen"]
["61.31.","wastafels en toebehoren - wandmodel"]
["61.31.10.","wastafels en toebehoren - wandmodel/porselein ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.32.","wastafels en toebehoren - inbouwmodel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.40.","baden - algemeen"]
["61.41.","baden - geëmailleerd staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.42.","baden - acrylaat ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.50.","douches - algemeen"]
["61.51.","douches - geëmailleerd staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.52.","douches - acrylaat ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.53.","douches - tegeldouche ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.60.","speciale toebehoren - algemeen"]
["61.61.","speciale toebehoren - rail en douchegordijn ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.62.","speciale toebehoren - douchedeuren en -wanden ","FH","st","TYPE 3","Wall",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Door",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Window",null,"Stuks",null,1]
["61.63.","speciale toebehoren - muurhandgrepen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.64.","speciale toebehoren - douchezitjes ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.70.","afwastafels - algemeen"]
["61.71.","afwastafels - opbouwmodel"]
["61.71.10.","afwastafels - opbouwmodel/roestvast staal (RVS) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.72.","afwastafels - inbouwmodel"]
["61.72.10.","afwastafels - inbouwmodel/roestvast staal (RVS) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.80.","uitgietbakken - algemeen"]
["61.81.","uitgietbakken - sanitair porselein ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.","SANITAIRE KRANEN & KLEPPEN"]
["62.00.","sanitaire kranen - kleppen - algemeen"]
["62.10.","terugslagkleppen - algemeen"]
["62.11.","terugslagkleppen - messing ","PM",null,"Geen",{"$nulls":4},1]
["62.20.","installatieafsluitkranen - algemeen"]
["62.21.","installatieafsluitkranen - messing"]
["62.21.10.","installatieafsluitkranen - messing/zonder aftapkraan ","PM",null,"Geen",{"$nulls":4},1]
["62.21.20.","installatieafsluitkranen - messing/met aftapkraan ","PM",null,"Geen",{"$nulls":4},1]
["62.22.","installatieafsluitkranen - kunststof"]
["62.22.10.","installatieafsluitkranen - kunststof/zonder aftapkraan ","PM",null,"Geen",{"$nulls":4},1]
["62.30.","wandafsluitkranen - algemeen"]
["62.31.","wandafsluitkranen - enkelvoudige stopkraan ","PM",null,"Geen",{"$nulls":4},1]
["62.32.","wandafsluitkranen - stopkraan met dienstkraan ","PM",null,"Geen",{"$nulls":4},1]
["62.40.","dienstkranen - algemeen"]
["62.41.","dienstkranen - enkele dienstkraan"]
["62.41.10.","dienstkranen - enkele dienstkraan/vaste uitloop ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.41.20.","dienstkranen - enkele dienstkraan/draaibare uitloop ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.42.","dienstkranen - dubbele dienstkraan"]
["62.42.10.","dienstkranen - dubbele dienstkraan/binnen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.42.20.","dienstkranen - dubbele dienstkraan/buiten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.50.","ééngatskranen - algemeen"]
["62.51.","ééngatskranen - handwastafelkraan ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.52.","ééngatskranen - lavabomengkraan ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.53.","ééngatskranen - afwastafelmengkraan ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.60.","muurmengkranen - algemeen"]
["62.61.","muurmengkranen - badmengkraan & armatuur ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.62.","muurmengkranen - douchemengkraan/armatuur ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.63.","muurmengkranen - afwastafelmengkraan ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.70.","regenwaterpompen - algemeen"]
["62.71.","regenwaterpompen - zelfaanzuigende hydrofoorgroep ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.72.","regenwaterpompen - dompelpomp ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.73.","regenwaterpompen - handpomp ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.","SANITAIR WARM WATER"]
["63.00.","sanitair warm water - algemeen"]
["63.10.","doorstroomwaterverwarmers op gas - algemeen"]
["63.11.","doorstroomwaterverwarmers op gas - badgeisers"]
["63.11.10.","doorstroomwaterverwarmers op gas - badgeisers/type B11BS ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.11.20.","doorstroomwaterverwarmers op gas - badgeisers/type C13-C33 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.12.","doorstroomwaterverwarmers op gas - keukengeisers"]
["63.12.10.","doorstroomwaterverwarmers op gas - keukengeisers/type AAS ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.20.","voorraadtoestellen op gas ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.30.","elektroboilers - algemeen"]
["63.31.","elektroboilers - kokend water toestellen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.32.","elektroboilers - inbouwmodel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.33.","elektroboilers - spaarboilers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.40.","voorraadboilers indirecte opwarming - algemeen"]
["63.41.","voorraadboilers indirecte opwarming - enkelvoudige warmtewisselaar ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.42.","voorraadboilers indirecte opwarming - dubbelvoudige warmtewisselaar ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.50.","zonneboilers - algemeen"]
["63.51.","zonneboilers - collectoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.52.","zonneboilers - opslagvat ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.53.","zonneboilers - leidingsysteem en toebehoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.54.","zonneboilers - circulatoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.55.","zonneboilers - expansiesysteem ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.56.","zonneboilers - regelsystemen en beveiliging"]
["63.56.10.","zonneboilers - regelsystemen en beveiliging/aflaat- en vulkranen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["63.56.20.","zonneboilers - regelsystemen en beveiliging/regelkranen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["63.56.30.","zonneboilers - regelsystemen en beveiliging/ontluchters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["63.56.40.","zonneboilers - regelsystemen en beveiliging/veiligheidskleppen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["63.56.50.","zonneboilers - regelsystemen en beveiliging/keerkleppen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["63.56.60.","zonneboilers - regelsystemen en beveiliging/mengventielen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["63.60.","warmtepompboilers - algemeen"]
["63.70.","satellietsystemen - algemeen "]
["63.71.","satellietsystemen - voorraadboilers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.72.","satellietsystemen - platenwisselaars ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["64.","GASINSTALLATIES"]
["64.00.","gasinstallaties - algemeen"]
["64.10.","gasleidingen - algemeen"]
["64.11.","gasleidingen - staal ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["64.12.","gasleidingen - koper ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["64.13.","gasleidingen - PE ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["64.14.","gasleidingen - PLT-buissysteem ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["64.20.","gaskranen - algemeen"]
["64.21.","gaskranen - gasfilter ","PM",null,"Geen",{"$nulls":4},1]
["64.22.","gaskranen - afsluitkranen ","PM",null,"Geen",{"$nulls":4},1]
["64.30.","gasaansluiting ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["64.40.","gastoestellen - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["65.","VERWARMING INDIVIDUELE INSTALLATIES"]
["65.00.","verwarming individuele installaties - algemeen"]
["65.01.","verwarming individuele installaties - proefopstelling ","PM",null,"Geen",{"$nulls":4},1]
["65.02.","verwarming individuele installaties - grenzen van de aanneming ","PM",null,"Geen",{"$nulls":4},1]
["65.10.","gasvloerketels - algemeen"]
["65.11.","gasvloerketels - open"]
["65.11.10.","gasvloerketels - open/enkel CV ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.11.20.","gasvloerketels - open/CV & SWW (voorraad) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.12.","gasvloerketels - gesloten"]
["65.12.10.","gasvloerketels - gesloten/enkel CV ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.12.20.","gasvloerketels - gesloten/CV & SWW (voorraad) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.20.","gaswandketels - algemeen"]
["65.21.","gaswandketels - gesloten"]
["65.21.10.","gaswandketels - gesloten/enkel CV ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.21.20.","gaswandketels - gesloten/CV & SWW (doorstroom) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.21.30.","gaswandketels - gesloten/CV & SWW (voorraad) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.30.","leidingnet & toebehoren - algemeen"]
["65.31.","leidingnet & toebehoren - buizen"]
["65.31.10.","leidingnet & toebehoren - buizen/staal ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["65.31.20.","leidingnet & toebehoren - buizen/koper ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["65.31.30.","leidingnet & toebehoren - buizen/kunststof ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["65.31.40.","leidingnet & toebehoren - buizen/dunwandige verzinkte buis ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["65.32.","leidingnet & toebehoren - collectoren ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["65.33.","leidingnet & toebehoren - leidingisolatie ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["65.34.","leidingnet & toebehoren - brandwerende doorvoeren ","PM",null,"Geen",{"$nulls":4},1]
["65.35.","leidingnet & toebehoren - verwarmingslint ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["65.40.","installatieonderdelen - algemeen"]
["65.41.","installatieonderdelen - aflaatkranen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.42.","installatieonderdelen - regel- en afsluitkranen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.43.","installatieonderdelen - drukregelaars ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.44.","installatieonderdelen - circulatoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["65.45.","installatieonderdelen - expansiesysteem ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.46.","installatieonderdelen - vlotterontluchters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.47.","installatieonderdelen - microbellenafscheider ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.50.","verwarmingselementen & toebehoren - algemeen"]
["65.51.","verwarmingselementen & toebehoren - plaatradiatoren ","FH","kW","TYPE 5","Object",null,"vul het vermogen in bij ARCHICAD property: Vermogen verwarmingselement",null,1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["65.52.","verwarmingselementen & toebehoren - wandconvectoren ","FH","kW","TYPE 5","Object",null,"vul het vermogen in bij ARCHICAD property: Vermogen verwarmingselement",null,1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["65.53.","verwarmingselementen & toebehoren - vloerverwarming","FH","m2","TYPE 5","Object",null,null,null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["65.60.","warmteregeling & toebehoren - algemeen"]
["65.61.","warmteregeling & toebehoren - radiatorkranen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.62.","warmteregeling & toebehoren - thermostaatkoppen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.63.","warmteregeling & toebehoren - kamerthermostaten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.64.","warmteregeling & toebehoren - weersafhankelijke regeling","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.65.","warmteregeling & toebehoren - manometer","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.66.","warmteregeling & toebehoren - thermometer","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[]
["66.","BIJZONDERE INSTALLATIES"]
["66.00.","bijzondere installaties - algemeen"]
["66.10.","warmtepompen - algemeen"]
["66.11.","warmtepompen - grond-water ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["66.12.","warmtepompen - water-water ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["66.13.","warmtepompen - lucht-water monoblok ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["66.14.","warmtepompen - lucht-water met binnen- en buitenunit (split-systeem) ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["66.15.","warmtepompen - gasabsorptiewarmtepompen"]
["66.16.","warmtepompen - verticale aardsondes ","SOG",null,"Geen",{"$nulls":4},1]
["66.16.10.","warmtepompen - verticale aardsondes/warmtewisselaar ","FH","SOG","Geen",{"$nulls":4},1]
["66.16.20.","warmtepompen - verticale aardsondes/collector ","PM",null,"Geen",{"$nulls":4},1]
["67.","BRANDBESTRIJDING"]
["67.00.","brandbestrijding - algemeen"]
["67.10.","brandblusapparaten - algemeen"]
["67.11.","brandblusapparaten - poedersnelblussers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.12.","brandblusapparaten - CO2-snelblussers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.13.","brandblusapparaten - schuimsnelblussers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.14.","brandblusapparaten - vast opgestelde poederblussers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.20.","externe bluswatervoorziening - algemeen ","SOG",null,"Geen",{"$nulls":4},1]
["67.21.","externe bluswatervoorziening - leidingen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["67.22.","externe bluswatervoorziening - buitenhydranten"]
["67.22.10.","externe bluswatervoorziening - buitenhydranten/bovengronds ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.22.20.","externe bluswatervoorziening - buitenhydranten/ondergronds ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.30.","interne bluswatervoorziening - algemeen ","SOG",null,"Geen",{"$nulls":4},1]
["67.31.","interne bluswatervoorziening - leidingen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["67.32.","interne bluswatervoorziening - brandkranen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.33.","interne bluswatervoorziening - muurhaspels zonder kast ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.34.","interne bluswatervoorziening - kasten voor slanghaspels ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.35.","interne bluswatervoorziening - manometers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.36.","interne bluswatervoorziening - pictogrammen ","PM",null,"Geen",{"$nulls":4},1]
["67.40.","sprinklerinstallatie - algemeen ","SOG",null,"Geen",{"$nulls":4},1]
["67.50.","brandwerende bescherming - algemeen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["68.","VENTILATIE"]
["68.00.","ventilatie - algemeen"]
["68.01.","ventilatie - proefopstelling ","PM",null,"Geen",{"$nulls":4},1]
["68.02.","ventilatie - proeven"]
["68.02.10.","ventilatie - proeven/debietmeting ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["68.02.20.","ventilatie - proeven/meting kanaaldichtheid ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["68.02.30.","ventilatie - proeven/dichtheid collectieve kanalen ","SOG",null,"Geen",{"$nulls":4},1]
["68.10.","ventilatiekanalen - algemeen"]
["68.11.","ventilatiekanalen - metaal"]
["68.11.10.","ventilatiekanalen - metaal/rond ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["68.11.20.","ventilatiekanalen - metaal/rechthoekig ","FH of SOG","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom","Let op! Geef in de classificatie de breedte van het kanaal op.",1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"Geen",{"$nulls":4},1]
["68.12.","ventilatiekanalen - kunststof"]
["68.12.10.","ventilatiekanalen - kunststof/rond ","FH of SOG","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"Geen",{"$nulls":4},1]
["68.12.20.","ventilatiekanalen - kunststof/rechthoekig of ovaal ","FH of SOG","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"Geen",{"$nulls":4},1]
["68.13.","ventilatiekanalen - flexibele kanalen ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["68.14.","ventilatiekanalen - thermische isolatie ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom","Let op! Geef in de classificatie de breedte van het kanaal op.",1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["68.15.","ventilatiekanalen - ophanging en bevestiging ","PM",null,"Geen",{"$nulls":4},1]
["68.20.","toebehoren ventilatiekanalen - algemeen"]
["68.30.","woonhuisventilatoren - algemeen"]
["68.31.","woonhuisventilatoren - systeem C ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.32.","woonhuisventilatoren - systeem D ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.40.","ventilatoren - algemeen"]
["68.41.","ventilatoren - dakventilatoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.42.","ventilatoren - kanaalventilatoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.43.","ventilatoren - sanitaire ventilatoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.50.","dampkappen - algemeen"]
["68.51.","dampkappen - inbouwmotor ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.52.","dampkappen - motorloos ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.60.","ventilatieventielen en -roosters - algemeen"]
["68.61.","ventilatiemonden - ventiel met regelbare conus ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.62.","ventilatiemonden - zelfregelend ventiel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.63.","ventilatiemonden - gevelroosters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.64.","ventilatiemonden - dakventielen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["69.","OPBOUWKANALEN ROOKGAS EN VENTILATIE"]
["69.00.","opbouwkanalen rookgas en ventilatie - algemeen"]
["69.10.","schoorstenen - algemeen"]
["69.11.","schoorstenen - roestvast staal"]
["69.11.10.","schoorstenen - roestvast staal/CLV ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.11.20.","schoorstenen - roestvast staal/enkelvoudig kanaal ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.11.30.","schoorstenen - roestvast staal/buigzame kanaalvoering ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.12.","schoorstenen - aluminium"]
["69.12.10.","schoorstenen - aluminium/CLV ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.12.20.","schoorstenen - aluminium/enkelvoudig ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.12.30.","schoorstenen - aluminium/buigzame kanaalvoering ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.13.","schoorstenen - kunststof "]
["69.13.10.","schoorstenen - kunststof/CLV ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.13.20.","schoorstenen - kunststof/enkelvoudig ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.13.30.","schoorstenen - kunststof/buigzame kanaalvoering ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.20.","dakdoorgang - algemeen"]
["69.21.","dakdoorgang - enkelvoudig ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["69.22.","dakdoorgang - multifunctioneel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]

{"sheet":"70 Electriciteit","index":9,"n_rows":185,"n_cols":10,"rows_kept":185,"cut":false,"hidden":false,"merged":[]}
["Artikelnummer","Artikelomschrijving","AvO","Eenheid","Type","Element","Element specificatie","Wat rekent de Meetstaat Manager?","Aandachtspunten"]
["70.","ELEKTRICITEIT BINNENNET"]
["70.00.","elektriciteit binnennet - algemeen"]
["70.10.","aansluitingen - algemeen"]
["70.11.","aansluitingen - ondergrondse aansluiting ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["70.12.","aansluitingen - aansluitbocht ","PM",null,"Geen",{"$nulls":4},1]
["70.13.","aansluitingen - aansluitplaat ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["70.14.","aansluitingen - tellerkasten ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["70.15.","aansluitingen - verbindingskabels ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["70.20.","verdeelkasten - algemeen"]
["70.21.","verdeelkasten - hoofdverdeelborden ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["70.30.","stroombeveiliging - algemeen"]
["70.31.","stroombeveiliging - hoofdschakelaars ","PM",null,"Geen",{"$nulls":4},1]
["70.32.","stroombeveiliging - differentieelschakelaars ","PM",null,"Geen",{"$nulls":4},1]
["70.33.","stroombeveiliging - automatische schakelaars ","PM",null,"Geen",{"$nulls":4},1]
["70.40.","aarding - algemeen"]
["70.41.","aarding - aardingslus ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"v","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["70.42.","aarding - afzonderlijke aardverbindingen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["70.43.","aarding - aardingsonderbrekers ","PM",null,"Geen",{"$nulls":4},1]
["70.44.","aarding - hoofdbeschermingsgeleiders ","PM",null,"Geen",{"$nulls":4},1]
["70.45.","aarding - hoofdequipotentiaalverbindingen ","PM",null,"Geen",{"$nulls":4},1]
["70.46.","aarding - bijkomende equipotentiaalverbindingen ","PM",null,"Geen",{"$nulls":4},1]
["70.47.","aarding - bliksemafleidersinstalatie ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Bliksemafleiderinstallatie","Stuks",null,1]
["70.50.","leidingen - algemeen"]
["70.53.","leidingen - inbouw kabelbuizen ","PM",null,"Geen",{"$nulls":4},1]
["70.54.","leidingen - opbouw kabelbuizen ","PM",null,"Geen",{"$nulls":4},1]
["70.55.","leidingen - plint- & wandkanalen ","PM",null,"Geen",{"$nulls":4},1]
["70.56.","leidingen - kabelgoten en -ladders ","PM",null,"Geen",{"$nulls":4},1]
["70.57.","leidingen - wachtbuizen ","PM",null,"Geen",{"$nulls":4},1]
["70.60.","trek- en verbindingsdozen - algemeen"]
["70.61.","trek- en verbindingsdozen - inbouw metselwerk ","PM",null,"Geen",{"$nulls":4},1]
["70.62.","trek- en verbindingsdozen - inbouw holle wanden ","PM",null,"Geen",{"$nulls":4},1]
["70.63.","trek- en verbindingsdozen - inbouw verlaagde plafonds ","PM",null,"Geen",{"$nulls":4},1]
["70.64.","trek- en verbindingsdozen - inbouw vloeren ","PM",null,"Geen",{"$nulls":4},1]
["70.65.","trek- en verbindingsdozen - opbouw ","PM",null,"Geen",{"$nulls":4},1]
["70.70.","bijzondere voorzieningen - algemeen"]
["70.71.","bijzondere voorzieningen - voeding liften ","PM",null,"Geen",{"$nulls":4},1]
["71.","ELEKTRICITEIT SCHAKELAARS & CONTACTDOZEN"]
["71.00.","elektriciteit schakelaars & contactdozen - algemeen"]
["71.10.","stopcontacten - algemeen"]
["71.11.","stopcontacten - 10/16A ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.12.","stopcontacten - 20/32A ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.20.","aansluitdozen - algemeen"]
["71.21.","aansluitdozen - voeding elektrisch fornuis ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.22.","aansluitdozen - voeding was- & vaatwasmachine ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.23.","aansluitdozen - voeding HVAC en andere ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.30.","schakelaars - algemeen"]
["71.31.","schakelaars - enkelpolig ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.32.","schakelaars - dubbelpolig ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.33.","schakelaars - wissel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.34.","schakelaars - kruis ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.35.","schakelaars - timerschakelaars ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.36.","schakelaars - teleruptoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.37.","schakelaars - dimmers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.40.","speciale toebehoren - algemeen"]
["71.41.","speciale toebehoren - bewegingsdetectoren ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Schakelaar Toebehoren ","Stuks",null,1]
["71.42.","speciale toebehoren - foto-elektrisch schakelaar ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Schakelaar Toebehoren ","Stuks",null,1]
["71.43.","speciale toebehoren - schemerschakelaar ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Schakelaar Toebehoren ","Stuks",null,1]
["72.","ELEKTRICITEIT LICHTARMATUREN"]
["72.00.","elektriciteit lichtarmaturen - algemeen"]
["72.10.","binnenarmaturen E27 - algemeen ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.11.","binnenarmaturen E27 - met lenskap ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.12.","binnenarmaturen E27 - andere ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.20.","binnenarmaturen TL - algemeen"]
["72.21.","binnenarmaturen TL - opbouwarmatuur plafond"]
["72.21.10.","binnenarmaturen TL - opbouwarmatuur plafond - T8 ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.21.20.","binnenarmaturen TL - opbouwarmatuur plafond - T5 ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.22.","binnenarmaturen TL - lichtstrip keukenaanrecht ",{"$nulls":7},1]
["72.22.10.","binnenarmaturen TL - lichtstrip keukenaanrecht/T8 ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.22.20.","binnenarmaturen TL - lichtstrip keukenaanrecht/T5 ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.40.","binnenarmaturen halogeen - algemeen"]
["72.41.","binnenarmaturen halogeen - transfo ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.42.","binnenarmaturen halogeen - inbouwspots ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.43.","binnenarmaturen halogeen - opbouwspots ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.50.","veiligheidsverlichting - algemeen"]
["72.51.","veiligheidsverlichting - autonoom niet-permanent ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.52.","veiligheidsverlichting - autonoom permanent ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.53.","veiligheidsverlichting - centrale noodvoeding ","SOG",null,"Geen",{"$nulls":4},1]
["72.54.","veiligheidsverlichting - armaturen ","SOG",null,"Geen",{"$nulls":4},1]
["72.55.","veiligheidsverlichting - signalisatie & pictogrammen ","PM",null,"Geen",{"$nulls":4},1]
["72.60.","buitenarmaturen - algemeen"]
["72.70.","armaturen geleverd door het bestuur - algemeen"]
["73.","ELEKTRICITEIT BEL & PARLOFOON"]
["73.00.","elektriciteit bel & parlofoon - algemeen"]
["73.10.","individuele belinstallaties - algemeen"]
["73.11.","individuele belinstallaties - huisbel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["73.12.","individuele belinstallaties - beldrukknop ","PM",null,"Geen",{"$nulls":4},1]
["73.13.","individuele belinstallaties - beltransfo ","PM",null,"Geen",{"$nulls":4},1]
["73.14.","individuele belinstallaties - bedrading ","PM",null,"Geen",{"$nulls":4},1]
["73.20.","parlofooninstallatie - algemeen"]
["73.21.","parlofooninstallatie - binnenposten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["73.22.","parlofooninstallatie - deurstation ","PM",null,"Geen",{"$nulls":4},1]
["73.23.","parlofooninstallatie - beltransfo ","PM",null,"Geen",{"$nulls":4},1]
["73.24.","parlofooninstallatie - verdeeldozen ","PM",null,"Geen",{"$nulls":4},1]
["73.25.","parlofooninstallatie - bedrading ","PM",null,"Geen",{"$nulls":4},1]
["73.26.","parlofooninstallatie - elektrisch deurslot ","PM",null,"Geen",{"$nulls":4},1]
["73.30.","toegangscontrolesysteem - algemeen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["74.","ELEKTRICITEIT TELECOM & DOMOTICA"]
["74.00.","elektriciteit telecom & domotica - algemeen"]
["74.10.","telefoon - algemeen"]
["74.11.","telefoon - buitenbekabeling ","SOG",null,"Geen",{"$nulls":4},1]
["74.12.","telefoon - basis aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.13.","telefoon - extra aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.14.","telefoon - binnenbekabeling ","PM",null,"Geen",{"$nulls":4},1]
["74.20.","kabeldistributie - algemeen"]
["74.21.","kabeldistributie - buitenbekabeling ","SOG",null,"Geen",{"$nulls":4},1]
["74.22.","kabeldistributie - basis aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.23.","kabeldistributie - extra aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.24.","kabeldistributie - binnenbekabeling ","PM",null,"Geen",{"$nulls":4},1]
["74.30.","netwerkbekabeling - algemeen"]
["74.31.","netwerkbekabeling - buitenbekabeling ","SOG",null,"Geen",{"$nulls":4},1]
["74.32.","netwerkbekabeling - basis aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.33.","netwerkbekabeling - extra aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.34.","netwerkbekabeling - binnenbekabeling ","PM",null,"Geen",{"$nulls":4},1]
["74.40.","satelietontvangstsysteem - algemeen"]
["74.41.","satelietontvangstsysteem - centrale schotelantenne ","SOG",null,"Geen",{"$nulls":4},1]
["74.42.","satelietontvangstsysteem - buitenbekabeling ","SOG",null,"Geen",{"$nulls":4},1]
["74.43.","satelietontvangstsysteem - basis aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.44.","satelietontvangstsysteem - extra aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.45.","satelietontvangstsysteem - binnenbekabeling ","PM",null,"Geen",{"$nulls":4},1]
["74.50.","alarmkabel - algemeen"]
["74.60.","luidsprekerkabel - algemeen"]
["74.70.","oproepsystemen ADL - algemeen"]
["74.80.","multimediakast","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["75.","ELEKTRICITEIT VERWARMING"]
["75.00.","elektriciteit verwarming - algemeen"]
["75.10.","direct systeem - algemeen"]
["75.11.","direct systeem - gedecentraliseerd"]
["75.11.10.","direct systeem - gedecentraliseerd/wandconvectoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["75.11.20.","direct systeem - gedecentraliseerd/plintconvectoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["75.11.30.","direct systeem - gedecentraliseerd/stralingselementen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["75.20.","accumulatiesysteem - algemeen"]
["75.21.","accumulatiesysteem - gedecentraliseerd"]
["75.21.10.","accumulatiesysteem - gedecentraliseerd/dynamisch gemengd ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["75.30.","meet- & regeltoestellen - algemeen"]
["75.31.","meet- & regeltoestellen - klokthermostaten "]
["75.31.10.","meet- & regeltoestellen - klokthermostaten/direct systeem ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["75.31.20.","meet- & regeltoestellen - klokthermostaten/accumulatie systeem ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["76.","ELEKTROMECHANICA LIFTEN"]
["76.00.","elektromechanica liften - algemeen"]
["76.01.","algemeen - grenzen van de aanneming ","PM",null,"Geen",{"$nulls":4},1]
["76.02.","algemeen - controle op afmetingen ","PM",null,"Geen",{"$nulls":4},1]
["76.03.","algemeen - documentatie en studie ","PM",null,"Geen",{"$nulls":4},1]
["76.04.","algemeen - werfinstallatie en -organisatie ","PM",null,"Geen",{"$nulls":4},1]
["76.05.","algemeen - onderhoud tijdens waarborgperiode ","PM",null,"Geen",{"$nulls":4},1]
["76.10.","bestaande installaties - algemeen"]
["76.11.","bestaande installaties - afbraak ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Lift Bestaande installaties","Stuks",null,1]
["76.12.","bestaande installaties - renovatie ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Lift Bestaande installaties","Stuks",null,1]
["76.20.","elektrische liften - algemeen"]
["76.21.","elektrische liften - met machinekamer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["76.22.","elektrische liften - zonder machinekamer (gearless) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["76.30.","kooiuitrusting - algemeen"]
["76.31.","kooiuitrusting - personenlift ","PM",null,"Geen",{"$nulls":4},1]
["76.32.","kooiuitrusting - goederenlift ","PM",null,"Geen",{"$nulls":4},1]
["76.33.","kooiuitrusting - vandalismewerend ","PM",null,"Geen",{"$nulls":4},1]
["76.40.","deuren & fronten - algemeen"]
["76.41.","deuren & fronten - personenlift ","PM",null,"Geen",{"$nulls":4},1]
["76.50.","bedienings- & signalisatiepanelen - algemeen"]
["76.51.","bedienings- & signalisatiepanelen - personenlift ","PM",null,"Geen",{"$nulls":4},1]
["77.","BRANDDETECTIE & ALARMSYSTEMEN"]
["77.00.","branddetectie & alarmsystemen - algemeen"]
["77.10.","centrale eenheid - algemeen ","SOG",null,"Geen",{"$nulls":4},1]
["77.20.","energievoorziening - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["77.30.","bekabeling - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["77.40.","brandmelding - algemeen"]
["77.41.","brandmelding - branddetectoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["77.42.","brandmelding - handmelders ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["77.43.","brandmelding - gasdetectoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["77.44.","brandmelding - autonome rookmelders ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["77.50.","alarmsirenes - algemeen"]
["77.51.","alarmsirenes - signal fast sweep ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["77.60.","evacuatietoebehoren - algemeen"]
["77.61.","evacuatietoebehoren - deurpomp met magneethouder ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurpomp","Stuks",null,1]
["77.62.","evacuatietoebehoren - pictogrammen ","PM",null,"Geen",{"$nulls":4},1]
["77.63.","evacuatietoebehoren - brandweersleutelkluis","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]

{"sheet":"80 Binnenschilderw","index":10,"n_rows":505,"n_cols":10,"rows_kept":505,"cut":false,"hidden":false,"merged":[]}
["Artikelnummer","Artikelomschrijving","AvO","Eenheid","Type","Element","Element specificatie","Wat rekent de Meetstaat Manager?","Aandachtspunten"]
["80.","BINNENSCHILDERWERKEN"]
["80.00.","schilderwerken - algemeen"]
["80.10.","binnenschilderwerken op pleisterwerk - algemeen"]
["80.11.","binnenschilderwerken op pleisterwerk - acrylaathars ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.12.","binnenschilderwerken op pleisterwerk - acrylaatdispersie ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.13.","binnenschilderwerken op pleisterwerk - vinyllatex ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.14.","binnenschilderwerken op pleisterwerk - kwartshoudende structuurverf ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.15.","binnenschilderwerken op pleisterwerk - meerkleurige effectverf ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.20.","binnenschilderwerken op gipskartonplaten - algemeen"]
["80.21.","binnenschilderwerken op gipskartonplaten - acrylaathars ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.22.","binnenschilderwerken op gipskartonplaten - acrylaatdispersie ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.23.","binnenschilderwerken op gipskartonplaten - vinyllatex ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.24.","binnenschilderwerken op gipskartonplaten - kwartshoudende structuurverf ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.25.","binnenschilderwerken op gipskartonplaten - meerkleurige effectverf ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.30.","binnenschilderwerken op beton - algemeen"]
["80.31.","binnenschilderwerken op beton - acrylaathars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.32.","binnenschilderwerken op beton - acrylaatdispersie ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.33.","binnenschilderwerken op beton - vinyllatex ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.34.","binnenschilderwerken op beton - kwartshoudende structuurverf ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.35.","binnenschilderwerken op beton - meerkleurig effectverf ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.36.","binnenschilderwerken op beton - epoxyverf ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.40.","binnenschilderwerken op metselwerk - algemeen"]
["80.41.","binnenschilderwerken op metselwerk - acrylaathars ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.42.","binnenschilderwerken op metselwerk - acrylaatdispersie ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.43.","binnenschilderwerken op metselwerkwerk - vinyllatex ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.44.","binnenschilderwerken op metselwerk - kwartshoudende structuurverf ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.45.","binnenschilderwerken op metselwerk - meerkleurige effectverf ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.50.","binnenschilderwerken op hout en houtachtige platen - algemeen"]
["80.51.","binnenschilderwerken op hout en houtachtige platen - lak"]
["80.51.10.","op hout en houtachtige platen - lak/acryllaatdispersie ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.51.20.","op hout en houtachtige platen - lak/polyurethaan acrylaathars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.51.30.","op hout en houtachtige platen - lak/alkyd-urethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.51.40.","op hout en houtachtige platen - lak/alkydhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.52.","binnenschilderwerken op hout en houtachtige platen - vernis"]
["80.52.10.","op hout en houtachtige platen - vernis / acrylurethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.52.20.","op hout en houtachtige platen - vernis/polyurethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.52.30.","op hout en houtachtige platen - vernis/alkydurethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.53.","binnenschilderwerken op hout en houtachtige platen - beits ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.60.","binnenschilderwerken op metaal - algemeen"]
["81.","BEHANGWERKEN"]
["81.00.","behangwerken - algemeen"]
["81.10.","verwijderen van behangpapier - algemeen ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["81.20.","behangen met glasvezeldoek - algemeen"]
["81.21.","behangen met glasvezeldoek - op nieuw pleisterwerk ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["81.22.","behangen met glasvezeldoek - op oud pleisterwerk ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["81.23.","behangen met glasvezeldoek - op gipskartonplaten ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.","BUITENSCHILDERWERKEN"]
["82.00.","buitenschilderwerken - algemeen"]
["82.10.","buitenschilderwerken op buitenbepleistering - algemeen"]
["82.11.","buitenschilderwerken op buitenbepleisteringen - acrylaatdispersie ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.12.","buitenschilderwerken op buitenbepleisteringen - siloxaan ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.13.","buitenschilderwerken op buitenbepleisteringen - silicaat ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.20.","buitenschilderwerken op beton - algemeen"]
["82.21.","buitenschilderwerken op beton - acrylaatdispersie ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.22.","buitenschilderwerken op beton - siloxaan ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.23.","buitenschilderwerken op beton - silicaat ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.24.","buitenschilderwerken op beton - kwartshoudende structuurverf ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.30.","buitenschilderwerken op gevelmetselwerk - algemeen"]
["82.31.","buitenschilderwerken op gevelmetselwerk - acrylaatdispersie ","FH","m2","TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.32.","buitenschilderwerken op gevelmetselwerk - siloxaan ","FH","m2","TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.33.","buitenschilderwerken op gevelmetselwerk - silicaat ","FH","m2","TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.34.","buitenschilderwerken op gevelmetselwerk - kwartshoudende structuurverf ","FH","m2","TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.40.","buitenschilderwerken op hout en houtachtige platen - algemeen"]
["82.41.","buitenschilderwerken op hout en houtachtige platen - lak"]
["82.41.10.","op hout en houtachtige platen - lak/acryllaatdispersie watergedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.41.20.","op hout en houtachtige platen - lak/alkyd-urethaan watergedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.41.30.","op hout en houtachtige platen - lak/alkydhars solventgedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.41.40.","op hout en houtachtige platen - lak/urethaan-alkyd solventgedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.42.","buitenschilderwerken op hout en houtachtige platen - vernis"]
["82.42.10.","op hout en houtachtige platen - vernis/alkyd-urethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.43.","buitenschilderwerken op hout en houtachtige platen - beits"]
["82.43.10.","op hout en houtachtige platen - beits/alkydhars watergedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.43.20.","op hout en houtachtige platen - beits/alkydhars solventgedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.50.","nabehandelingen op metselwerk - algemeen"]
["82.51.","nabehandelingen op metselwerk - hydrofobering ","FH","m2","TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.52.","nabehandelingen op metselwerk - antigraffiti ","FH","m2","TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.60.","buitenschilderwerken op metaal - algemeen"]

{"sheet":"90 Buitenverhardingen","index":11,"n_rows":186,"n_cols":10,"rows_kept":186,"cut":false,"hidden":false,"merged":[]}
["Artikelnummer","Artikelomschrijving","AvO","Eenheid","Type","Element","Element specificatie","Wat rekent de Meetstaat Manager?","Aandachtspunten"]
["90.","BUITENVERHARDINGEN"]
["90.00.","buitenverhardingen - algemeen"]
["90.10.","funderingen - algemeen"]
["90.11.","funderingen - steenslag"]
["90.11.10.","funderingen - steenslag/niet-continue korrelverdeling ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.11.20.","funderingen - steenslag/continue korrelverdeling zonder toevoegsels ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.11.30.","funderingen - steenslag/continue korrelverdeling met toevoegsels ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.12.","funderingen - ternair mengsel ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.13.","funderingen - zandcement ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.14.","funderingen - schraal beton"]
["90.14.10.","funderingen - schraal beton/ongewapend ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.14.20.","funderingen - schraal beton/gewapend ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.20.","verhardingen - algemeen"]
["90.21.","verhardingen - in rijen te leggen kasseien ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.22.","verhardingen - mozaïekkeien ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.23.","verhardingen - betonstraatstenen"]
["90.23.10.","verhardingen - betonstraatstenen/kleurvast ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.23.20.","verhardingen - betonstraatstenen/waterdoorlatend ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.24.","verhardingen - gebakken straatstenen ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.25.","verhardingen - betontegels"]
["90.25.10.","verhardingen - betontegels/kleurvast ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.25.20.","verhardingen - betontegels/waterdoorlatend ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.25.30.","verhardingen - betontegels/grasbetontegels ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.25.40.","verhardingen - betontegels/silexbetontegels ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.26.","verhardingen - tegels in natuursteen ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.27.","verhardingen - dolomiet ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.28.","verhardingen - gepolierd beton ","FH of VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["90.29.","verhardingen - tactiele oppervlakken ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.30.","lijnvormige elementen - algemeen"]
["90.31.","lijnvormige elementen - boordstenen"]
["90.31.10.","lijnvormige elementen - boordstenen/beton"]
["90.31.11.","lijnvormige elementen - boordstenen/beton - prefab ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["90.31.12.","lijnvormige elementen - boordstenen/beton - ter plaatse gestort ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["90.31.20.","lijnvormige elementen - boordstenen/palissaden ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["90.31.30.","lijnvormige elementen - boordstenen/metaal ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["90.32.","lijnvormige elementen - watergreppels"]
["90.32.10.","lijnvormige elementen - watergreppels/beton"]
["90.32.11.","lijnvormige elementen - watergreppels/beton - prefab ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["91.","BUITENCONSTRUCTIES EN AFSLUITINGEN"]
["91.00.","buitenconstructies en afsluitingen - algemeen"]
["91.10.","tuinafsluitingspalen - algemeen"]
["91.11.","tuinafsluitingspalen - staal ","PM",null,"Geen",{"$nulls":4},1]
["91.12.","tuinafsluitingspalen - hout ","PM",null,"Geen",{"$nulls":4},1]
["91.13.","tuinafsluitingspalen - beton ","PM",null,"Geen",{"$nulls":4},1]
["91.20.","draadafsluitingen - algemeen"]
["91.21.","draadafsluitingen - gladde draad ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["91.22.","draadafsluitingen - draadgaas ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["91.30.","tuinschermen - algemeen"]
["91.31.","tuinschermen - schapenhek ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["91.32.","tuinschermen - houtschermen ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["91.33.","tuinschermen - betonplaten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["91.40.","tuinhekken - algemeen"]
["91.41.","tuinhekken - staal ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["91.42.","tuinhekken - hout ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["91.50.","terrassen tuinhout - algemeen"]
["91.51.","terrassen tuinhout - tegels ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["91.52.","terrassen tuinhout - beplanking ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["91.60.","constructies tuinhout - algemeen"]
["92.","BUITENMEUBILAIR EN UITRUSTINGSELEMENTEN"]
["92.00.","buitenmeubilair en uitrustingselementen - algemeen"]
["92.10.","brievenbussen - algemeen"]
["92.11.","brievenbussen - geleverd door het bestuur ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.12.","brievenbussen - prefab beton ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.13.","brievenbussen - staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.14.","brievenbussen - aluminium ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.20.","vuilnisbakken - algemeen"]
["92.21.","vuilnisbakken - geleverd door het bestuur ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.22.","vuilnisbakken - staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.23.","vuilnisbakken - kunststof ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.30.","fietsrekken - algemeen"]
["92.31.","fietsrekken - blokken beton ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.32.","fietsrekken - modules staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.33.","fietsrekken - aanleunbeugels staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.34.","fietsrekken - ophangelementen staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.35.","fietsrekken - klemmen staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.40.","parkingelementen - algemeen"]
["92.41.","parkingelementen - parkeerpalen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.42.","parkingelementen - parkeerbeugels ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.50.","zitbanken - algemeen"]
["92.51.","zitbanken - geleverd door het bestuur ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.52.","zitbanken - zonder rugleuning ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.53.","zitbanken - met rugleuning ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.60.","boomomrandingen - algemeen"]
["92.61.","boomomrandingen - roosters beton ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.62.","boomomrandingen - roosters gietijzer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.63.","boomomrandingen - roosters kunststof ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.64.","boomomrandingen - roosters staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.70.","plantbescherming - algemeen"]
["92.71.","plantbescherming - boombeugels staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.73.","plantbescherming - boomkorven staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.74.","plantbescherming - plantkorven staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["93.","GROENAANLEG EN -ONDERHOUD"]
["93.00.","groenaanleg en -onderhoud - algemeen"]
["93.10.","grondbewerkingen - algemeen"]
["93.11.","grondbewerkingen - diepspitten ","PM",null,"Geen",{"$nulls":4},1]
["93.12.","grondbewerkingen - egaliseren ","PM",null,"Geen",{"$nulls":4},1]
["93.13.","grondbewerkingen - frezen ","PM",null,"Geen",{"$nulls":4},1]
["93.20.","verwerking teelaarde - algemeen"]
["93.21.","verwerking teelaarde - afkomstig van afgraving ","FH/VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["93.22.","verwerking teelaarde - te leveren door de aannemer ","FH/VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["93.30.","verwerken van bodemverbeteringsmiddelen - algemeen ","FH/VH","kg","TYPE 4","Slab","vul de ARCHICAD property 'Soortelijk gewicht' in","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Mesh","vul de ARCHICAD property 'Soortelijk gewicht' in","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Morph","vul de ARCHICAD property 'Soortelijk gewicht' in","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["93.40.","aanleg grasmatten - algemeen"]
["93.41.","aanleg grasmatten - door bezaaiing ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["93.42.","aanleg grasmatten - door bezoding ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["93.50.","aanplanting houtachtige vegetaties - algemeen"]
["93.51.","aanplanting houtachtige vegetaties - bomen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["93.52.","aanplanting houtachtige gewassen - hagen ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"Stuks",null,1]
["93.53.","aanplanting houtachtige gewassen - heesters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["93.60.","hulpmiddelen groenaanleg - algemeen"]
["93.61.","hulpmiddelen groenaanleg - boompaalconstructies ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW hulpmiddelen groenaanleg","Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["93.62.","hulpmiddelen groenaanleg - boomroosters ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW hulpmiddelen groenaanleg","Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["93.63.","hulpmiddelen groenaanleg - ondergrondse verankering van bomen ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW hulpmiddelen groenaanleg","Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["93.64.","hulpmiddelen groenaanleg - groeiplaatsverbetering van bomen (irrigatie) ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW hulpmiddelen groenaanleg","Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["93.65.","hulpmiddelen groenaanleg - haagsteun ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["93.70.","groenonderhoud - algemeen"]
["93.71.","groenonderhoud - maaien van grasmatten ","FH","m2","TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["93.72.","groenonderhoud - bomen snoeien ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW bomen snoeien","Stuks",null,1]
["93.73.","groenonderhoud - scheren van hagen en beplantingsmassieven ","FH","m2","TYPE 4","Morph","Gebruik ARCHICAD Property: VMSW_scheren van hagen en beplantingsmassieven","Surface Area",null,1]
[{"$nulls":4},"TYPE 4","Wall","Gebruik ARCHICAD Property: VMSW_scheren van hagen en beplantingsmassieven","Top Surface",null,1]
["93.74.","groenonderhoud - snoeien van heesters ","FH","st","TYPE 5",null,null,"Stuks",null,1]

{"sheet":"Volledige artikellijst","index":12,"n_rows":4227,"n_cols":10,"rows_kept":4227,"cut":false,"hidden":false,"merged":[]}
["Artikelnummer","Artikelomschrijving","AvO","Eenheid","Type","Element","Element specificatie","Wat rekent de Meetstaat Manager?","Aandachtspunten","Column1"]
[{"$nulls":9},"Totaal"]
["00.","ALGEMENE BEPALINGEN"]
["00.10.","projectgegevens"]
["00.20.","ontwerpteam"]
["00.21.","ontwerpteam - architecturaal ontwerp",null,null,"Geen",{"$nulls":4},1]
["00.22.","ontwerpteam - studie stabiliteit",null,null,"Geen",{"$nulls":4},1]
["00.23.","ontwerpteam - studie technieken",null,null,"Geen",{"$nulls":4},1]
["00.24.","ontwerpteam - veiligheidscoördinatie",null,null,"Geen",{"$nulls":4},1]
["00.25.","ontwerpteam - EPB verslaggeving",null,null,"Geen",{"$nulls":4},1]
["00.30.","documenten"]
["00.31.","documenten - architectuur",null,null,"Geen",{"$nulls":4},1]
["00.32.","documenten - stabiliteit",null,null,"Geen",{"$nulls":4},1]
["00.33.","documenten - technieken",null,null,"Geen",{"$nulls":4},1]
["00.34.","documenten - veiligheidscoördinatie",null,null,"Geen",{"$nulls":4},1]
["00.35.","documenten - EPB verslaggeving",null,null,"Geen",{"$nulls":4},1]
["00.36.","documenten - diepsonderingsverslag",null,null,"Geen",{"$nulls":4},1]
["00.37.","documenten - verslag milieutechnisch bodemonderzoek",null,null,"Geen",{"$nulls":4},1]
["01.","AANNEMINGSMODALITEITEN"]
["01.00.","aannemingsmodaliteiten - algemeen"]
["01.01.","aannemingsmodaliteiten - bestek ","PM",null,"Geen",{"$nulls":4},1]
["01.02.","aannemingsmodaliteiten - voorafgaand plaatsbezoek ","PM",null,"Geen",{"$nulls":4},1]
["01.03.","aannemingsmodaliteiten - burgerlijke aansprakelijkheid ","PM",null,"Geen",{"$nulls":4},1]
["01.04.","aannemingsmodaliteiten - volledigheid van inschrijving ","PM",null,"Geen",{"$nulls":4},1]
["01.05.","aannemingsmodaliteiten - onderaanneming ","PM",null,"Geen",{"$nulls":4},1]
["01.06.","aannemingsmodaliteiten - verrekeningen ","PM",null,"Geen",{"$nulls":4},1]
["01.07.","aannemingsmodaliteiten - keuringsattesten ","PM",null,"Geen",{"$nulls":4},1]
["01.08.","aannemingsmodaliteiten - materialenlijst ","PM",null,"Geen",{"$nulls":4},1]
["01.10.","plaatsbeschrijvingen - algemeen"]
["01.11.","plaatsbeschrijvingen - aangrenzende constructies"]
["01.11.10.","plaatsbeschrijvingen – aangrenzende constructies/bij aanvang van de werken","PM",null,"Geen",{"$nulls":4},1]
["01.11.20.","plaatsbeschrijvingen – aangrenzende constructies/staat van vergelijking","PM",null,"Geen",{"$nulls":4},1]
["01.12.","plaatsbeschrijvingen - te renoveren constructies",null,null,"Geen",{"$nulls":4},1]
["01.12.10.","plaatsbeschrijvingen – te renoveren constructies/bij aanvang van de werken","PM",null,"Geen",{"$nulls":4},1]
["01.12.20.","plaatsbeschrijvingen – te renoveren constructies/staat van vergelijking","PM",null,"Geen",{"$nulls":4},1]
["01.13.","plaatsbeschrijvingen - inboedel bij blijvende bewoning"]
["01.13.10.","plaatsbeschrijvingen – inboedel bij blijvende bewoning/bij aanvang van de werken","PM",null,"Geen",{"$nulls":4},1]
["01.13.20.","plaatsbeschrijvingen – inboedel bij blijvende bewoning/staat van vergelijking","PM",null,"Geen",{"$nulls":4},1]
["01.14.","plaatsbeschrijvingen - wegenis en voetpaden"]
["01.14.10.","plaatsbeschrijvingen – wegenis en voetpaden bij aanvang van de werken","PM",null,"Geen",{"$nulls":4},1]
["01.14.20.","plaatsbeschrijvingen – wegenis en voetpaden/staat van vergelijking","PM",null,"Geen",{"$nulls":4},1]
["01.15.","plaatsbeschrijvingen - beplanting"]
["01.15.10.","plaatsbeschrijvingen – beplanting/bij aanvang van de werken","PM",null,"Geen",{"$nulls":4},1]
["01.15.20.","plaatsbeschrijvingen – beplanting/staat van vergelijking","PM",null,"Geen",{"$nulls":4},1]
["01.20.","werfcoördinatie - algemeen"]
["01.21.","werfcoördinatie - planning van de werken ","PM",null,"Geen",{"$nulls":4},1]
["01.22.","werfcoördinatie - werfleiding en controle ","PM",null,"Geen",{"$nulls":4},1]
["01.23.","werfcoördinatie - werfvergaderingen ","PM",null,"Geen",{"$nulls":4},1]
["01.24.","werfcoördinatie - uitzetten bouwwerken ","PM",null,"Geen",{"$nulls":4},1]
["01.25.","werfcoördinatie - as-builtdossier ","PM",null,"Geen",{"$nulls":4},1]
["01.26.","werfcoördinatie - renovaties met blijvende bewoning ","PM",null,"Geen",{"$nulls":4},1]
["01.30.","werfcondities - algemeen"]
["01.31.","werfcondities - orde en netheid ","PM",null,"Geen",{"$nulls":4},1]
["01.32.","werfcondities - geluids- en stofhinder ","PM",null,"Geen",{"$nulls":4},1]
["01.33.","werfcondities - nazorg ","PM",null,"Geen",{"$nulls":4},1]
["01.40.","veiligheidsvoorschriften - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["02.","BOUWPLAATSVOORZIENINGEN"]
["02.00.","bouwplaatsvoorzieningen - algemeen"]
["02.10.","beschermingswerken - algemeen"]
["02.11.","beschermingwerken - openbare weg ","PM",null,"Geen",{"$nulls":4},1]
["02.12.","beschermingswerken - beplantingen"]
["02.12.10.","beschermingswerken – beplantingen/bomen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["02.12.20.","beschermingswerken – beplantingen/struiken en hagen","PM"]
["02.20.","opruiming beplantingen - algemeen"]
["02.21.","opruiming beplantingen - bomen ","PM ",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["02.22.","opruiming beplantingen - struiken en hagen ","PM",null,"Geen",{"$nulls":4},1]
["02.30.","toegangswegen - algemeen"]
["02.31.","toegangswegen - voorlopige verharding voor voetgangers ","PM",null,"Geen",{"$nulls":4},1]
["02.32.","toegangswegen - voorlopige verharding voor zware lasten ","PM",null,"Geen",{"$nulls":4},1]
["02.33.","toegangswegen - parkeerruimte voor laden en lossen ","PM",null,"Geen",{"$nulls":4},1]
["02.40.","voorlopige omheining - algemeen"]
["02.50.","aankondiging werf - algemeen"]
["02.51.","aankondiging werf - werfbord ","PM",null,"Geen",{"$nulls":4},1]
["02.52.","aankondiging werf - werfdoek ","PM",null,"Geen",{"$nulls":4},1]
["02.60.","werflokalen - algemeen"]
["02.61.","werflokalen - berging van materieel en bouwmaterialen ","PM",null,"Geen",{"$nulls":4},1]
["02.62.","werflokalen - kantoorruimte ","PM",null,"Geen",{"$nulls":4},1]
["02.63.","werflokalen - personeelslokaal ","PM",null,"Geen",{"$nulls":4},1]
["02.64.","werflokalen - sanitaire voorzieningen ","PM",null,"Geen",{"$nulls":4},1]
["02.70.","voorlopige aansluitingen - algemeen"]
["02.71.","voorlopige aansluitingen - stroomvoorziening ","PM",null,"Geen",{"$nulls":4},1]
["02.72.","voorlopige aansluitingen - watervoorziening ","PM",null,"Geen",{"$nulls":4},1]
["02.73.","voorlopige aansluitingen - waterafvoer ","PM",null,"Geen",{"$nulls":4},1]
["02.80.","arbeidsmiddelen - algemeen"]
["02.81.","arbeidsmiddelen - werken op hoogte"]
["02.81.10","arbeidsmiddelen - werken op hoogte/ladders","PM",null,"Geen",{"$nulls":4},1]
["02.81.20","arbeidsmiddelen - werken op hoogte/steigers","PM",null,"Geen",{"$nulls":4},1]
["02.82.","arbeidsmiddelen - hijsen en heffen van lasten ","PM",null,"Geen",{"$nulls":4},1]
["03.","AFBRAAKWERKEN"]
["03.00.","afbraakwerken - algemeen"]
["03.01.","afbraakwerken - asbestverwijdering"]
["03.02.","afbraakwerken - schoring"]
["03.03.","afbraakwerken - in bewoonde gebouwen"]
["03.10.","afbraak volledige constructie - algemeen"]
["03.11.","afbraak volledige constructie - vrijstaand"]
["03.11.10.","afbraak volledige constructie - vrijstaand/asbestverwijdering"]
["03.11.11.","afbraak volledige constructie – vrijstaand/asbestverwijdering - dakbedekking","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["03.11.12.","afbraak volledige constructie – vrijstaand/asbestverwijdering - onderdak","FH","m2","TYPE 3","Roof",null,"Top Surface",null,2]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["03.11.13.","afbraak volledige constructie – vrijstaand/asbestverwijdering - asbestcementbuizen","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["03.11.14.","afbraak volledige constructie – vrijstaand/asbestverwijdering - vloerafwerking","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.11.15.","afbraak volledige constructie – vrijstaand/asbestverwijdering - plaatmateriaal","FH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["03.11.16.","afbraak volledige constructie – vrijstaand/asbestverwijdering - buisisolatie","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.11.17.","afbraak volledige constructie – vrijstaand/asbestverwijdering - asbestkoord","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.11.18.","afbraak volledige constructie – vrijstaand/asbestverwijdering - raam- en deurkitten","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.11.20.","afbraak volledige constructie - vrijstaand/slopen gebouw","FH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.11.30.","afbraak volledige constructie - vrijstaand/ondergrondse massieven","VH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["03.11.40.","afbraak volledige constructie - vrijstaand/te behouden gevels","PM",null,"Geen",{"$nulls":4},1]
["03.12.","afbraak volledige constructie - grenzend aan andere gebouwen"]
["03.12.10.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering"]
["03.12.11.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - dakbedekking","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.12.12.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - onderdak","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.12.13.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - asbestcementbuizen","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["03.12.14.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - vloerafwerking","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.12.15.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - plaatmateriaal","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["03.12.16.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - buisisolatie","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.12.17.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - asbestkoord","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.12.18.","afbraak volledige constructie – grenzend aan andere gebouwen/asbestverwijdering - raam- en deurkitten","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.12.20.","afbraak volledige constructie – grenzend aan andere gebouwen/slopen gebouw","FH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.12.30.","afbraak volledige constructie – grenzend aan andere gebouwen/ondergrondse massieven","VH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["03.12.40.","afbraak volledige constructie – grenzend aan andere gebouwen/te behouden gevels","PM",null,"Geen",{"$nulls":4},1]
["03.20.","afbraak ruwbouwelementen - algemeen"]
["03.21.","afbraak ruwbouwelementen - muren"]
["03.21.10.","afbraak ruwbouwelementen – muren/metselwerk","FH of VH","m3","TYPE 3","Wall",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"Net Volume"]
[{"$nulls":4},"TYPE 5","Opening"]
["03.21.20.","afbraak ruwbouwelementen – muren/beton","FH of VH","m3","TYPE 3","Wall",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"Net Volume"]
[{"$nulls":4},"TYPE 5","Opening"]
["03.21.30.","afbraak ruwbouwelementen – muren/houtskelet","FH of VH","m3","TYPE 3","Wall",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"Net Volume"]
[{"$nulls":4},"TYPE 5","Opening"]
["03.22.","afbraak ruwbouwelementen - vloeren"]
["03.22.10.","afbraak ruwbouwelementen – vloeren/potten en balken","FH of VH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m3","TYPE 3","Roof",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Roof",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Shell",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Slab",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Opening"]
["03.22.20.","afbraak ruwbouwelementen – vloeren/beton"]
["03.22.21.","afbraak ruwbouwelementen – vloeren/beton - verdiepingsvloer","FH of VH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m3","TYPE 3","Roof",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Roof",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Shell",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Slab",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Opening"]
["03.22.22.","afbraak ruwbouwelementen – vloeren/beton - vloer op volle grond","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m3","TYPE 3","Slab",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Slab",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Opening"]
["03.22.30.","afbraak ruwbouwelementen – vloeren/houten roostering","FH of VH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m3","TYPE 3","Roof",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Roof",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Shell",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Slab",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 5","Opening"]
["03.30.","afbraak dakelementen - algemeen"]
["03.31.","afbraak dakelementen - hellend dak"]
["03.31.10.","afbraak dakelementen – hellend dak/asbestverwijdering"]
["03.31.11.","afbraak dakelementen – hellend dak/asbestverwijdering - dakbedekking","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["03.31.12.","afbraak dakelementen – hellend dak/asbestverwijdering - onderdak","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["03.31.13.","afbraak dakelementen – hellend dak/asbestverwijdering - asbestcement","FH","st","TYPE 3","Roof",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Stuks",null,1]
["03.31.20.","afbraak dakelementen – hellend dak/volledige dakopbouw","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.31.30.","afbraak dakelementen – hellend dak/dakbedekking","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["03.31.40.","afbraak dakelementen – hellend dak/dakisolatie","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.31.50.","afbraak dakelementen – hellend dak/daklichtelementen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.31.60.","afbraak dakelementen – hellend dak/dakdoorvoeren en schouwen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.32.","afbraak dakelementen - plat dak"]
["03.32.10.","afbraak dakelementen – plat dak/asbestverwijdering"]
["03.32.11.","afbraak dakelementen – plat dak/asbestverwijdering - asbestcement","FH","st","TYPE 3","Roof",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Stuks",null,1]
["03.32.20.","afbraak dakelementen – plat dak/volledige dakopbouw","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"SOG",{"$nulls":6},1]
["03.32.30.","afbraak dakelementen – plat dak/dakdichting","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.32.40.","afbraak dakelementen – plat dak/dakisolatie","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.32.50.","afbraak dakelementen – plat dak/daklichtelementen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.32.60.","afbraak dakelementen – plat dak/dakdoorvoeren","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["03.40.","afbraak gevelelementen - algemeen"]
["03.41.","afbraak gevelelementen - gevelmetselwerk ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["03.42.","afbraak gevelelementen - leien"]
["03.42.10.","afbraak gevelelementen – leien/asbesthoudend","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["03.42.20.","afbraak gevelelementen – leien/niet-asbesthoudend","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["03.43.","afbraak gevelelementen - beplating ","FH","m2","TYPE 3","Wall",null,"Projected Area on the side opposite to the reference line",null,1]
["03.44.","afbraak gevelelementen - buitenschrijnwerk"]
["03.44.10.","afbraak gevelelementen – buitenschrijnwerk/asbestverwijdering"]
["03.44.11.","afbraak gevelelementen – buitenschrijnwerk/asbestverwijdering - kitten","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["03.44.20.","afbraak gevelelementen – buitenschrijnwerk/ramen, deuren en poorten","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
[{"$nulls":4},"TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.45.","afbraak gevelelementen - buitentrappen ","FH","m2","TYPE 5","Stair ","Tread total area","Net Area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.46.","afbraak gevelelementen - balustraden ","FH","st","TYPE 5","Railing",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.50.","afbraak binnenafwerking - algemeen"]
["03.51.","afbraak binnenafwerking - volledige ontmanteling ","SOG",null,"Geen",{"$nulls":4},1]
["03.52.","afbraak binnenafwerking - afkappen pleisterwerk ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["03.53.","afbraak binnenafwerking - plaatafwerking"]
["03.53.10.","afbraak binnenafwerking – plaatafwerking/asbestverwijdering","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["03.53.20.","afbraak binnenafwerking – plaatafwerking/lichte scheidingswanden","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.53.30.","afbraak binnenafwerking – plaatafwerking/plafondafwerking","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.53.40.","afbraak binnenafwerking – plaatafwerking/uitbekleding wanden","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.54.","afbraak binnenafwerking - dekvloer",{"$nulls":5},"Property: Oppervlakte middenas wand"]
["03.54.10.","afbraak binnenafwerking – dekvloer/asbestverwijdering","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.54.20.","afbraak binnenafwerking – dekvloer/tot op draagstructuur","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.55.","afbraak binnenafwerking - vloerafwerking"]
["03.55.10.","afbraak binnenafwerking – vloerafwerking/asbestverwijdering","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["03.55.20.","afbraak binnenafwerking – vloerafwerking/linoleum","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.55.30.","afbraak binnenafwerking – vloerafwerking/tegels"]
["03.55.31.","afbraak binnenafwerking – vloerafwerking/tegels - op dekvloer","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.55.32.","afbraak binnenafwerking – vloerafwerking/tegels - op zandbed","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.55.40.","afbraak binnenafwerking – vloerafwerking/houten vloer","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.56.","afbraak binnenafwerking - binnendeuren ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.57.","afbraak binnenafwerking - trappen en leuningen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Railing",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Stair",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.58.","afbraak binnenafwerking - vast meubilair"]
["03.58.10.","afbraak binnenafwerking – vast meubilair/keukenmeubilair","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.58.20.","afbraak binnenafwerking – vast meubilair/badkamermeubilair","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["03.60.","afbraak technieken fluïda - algemeen"]
["03.61.","afbraak technieken fluïda - leidingen"]
["03.61.10.","afbraak technieken fluïda – leidingen/asbestverwijdering"]
["03.61.11.","afbraak technieken fluïda – leidingen/asbestverwijdering - asbestcement","FH of VH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["03.61.12.","afbraak technieken fluïda – leidingen/asbestverwijdering - leidingisolatie","FH of VH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["03.61.20.","afbraak technieken fluïda – leidingen/toevoer en afvoerleidingen","PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.62.","afbraak technieken fluïda - sanitaire toestellen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.63.","afbraak technieken fluïda - radiatoren & toebehoren","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.64.","afbraak technieken fluïda - gasleidingen & toebehoren","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.65.","afbraak technieken fluïda - CV-ketel & toebehoren","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["03.70.","afbraak technieken elektro - algemeen"]
["03.71.","afbraak technieken elektro - leidingnet ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["04.","GEBOUWPRESTATIES"]
["04.00.","gebouwprestaties - algemeen"]
["04.10.","energieprestatie en binnenklimaat (EPB) - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["04.20.","luchtdichtheid - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["04.30.","akoestiek - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["04.40.","brandveiligheid - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["05.","PROEVEN"]
["05.00.","proeven - algemeen"]
["05.10.","proeven - luchtdichtheidsmeting"]
["05.11.","proeven - luchtdichtheidsmeting / wooneenheid ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks",null,1]
["05.12.","proeven - luchtdichtheidsmeting / gebouw ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks",null,1]
["05.20.","proeven - akoestiek"]
["05.21.","proeven - akoestiek / luchtgeluidiolatie ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks",null,1]
["05.22.","proeven - akoestiek / contactgeluidiolatie ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks",null,1]
["05.23.","proeven - akoestiek / geluidisolatie van de gevel ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks",null,1]
["05.24.","proeven - akoestiek / geluid van technische installaties ","FH","st","TYPE 5","Object","Meetstaat Manager 22 KM","Stuks",null,1]
[]
["10.","GRONDWERKEN"]
["10.00.","grondwerken - algemeen"]
["10.10.","voorafgaande afgraving van het terrein - algemeen"]
["10.11.","voorafgaande afgraving terrein - ontzoden ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Projected Area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["10.12.","voorafgaande afgraving terrein - afgraven teelaarde ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Projected Area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["10.13.","voorafgaande afgraving terrein - machinale nivellering ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Projected Area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["10.20.","uitgraving bouwputten - algemeen"]
["10.21.","uitgraving bouwputten - gewone bouwputten ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
["10.22.","uitgraving bouwputten - prefabkelders ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["10.23.","uitgraving bouwputten - rioleringselementen ","PM",null,"Geen",{"$nulls":4},1]
["10.30.","uitgraving sleuven - algemeen"]
["10.31.","uitgraving sleuven - funderingssleuven ","FH/VH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
["10.32.","uitgraving sleuven - funderingsbalken ","FH/VH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
["10.33.","uitgraving sleuven - ondergrondse leidingen ","FH/VH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["10.40.","grondverzet - algemeen"]
["10.41.","grondverzet - projectopvolging ","SOG",null,"Geen",{"$nulls":4},1]
["10.42.","grondverzet - hergebruik uitgegraven grond op werf ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.43.","grondverzet - afvoer uitgegraven bodem"]
["10.43.10.","grondverzet - afvoer uitgegraven bodem/naar bestemming voor gebruik"]
["10.43.11.","grondverzet - afvoer uitgegraven bodem/naar bestemming voor gebruik - kwaliteit vrij gebruik ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.43.12.","grondverzet - afvoer uitgegraven bodem/naar bestemming voor gebruik - kwaliteit bouwkundig bodemgebruik ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.43.20.","grondverzet - afvoer uitgegraven bodem/naar tussentijdse opslagplaats (TOP) ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.43.30.","grondverzet - afvoer uitgegraven bodem/naar grondreinigingscentrum (GRC) ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.43.40.","grondverzet - afvoer uitgegraven bodem/naar erkende stortplaats"]
["10.43.41.","grondverzet - afvoer uitgegraven bodem/naar erkende stortplaats - klasse I ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.43.42.","grondverzet - afvoer uitgegraven bodem/naar erkende stortplaats - klasse II ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.43.43.","grondverzet - afvoer uitgegraven bodem/naar erkende stortplaats - klasse III ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.44.","grondverzet - fysische scheiding"]
["10.44.10.","grondverzet - fysische scheiding/uitzeving ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.44.20.","grondverzet - fysische scheiding/afvoer steenachtige materialen ","VH","ton","TYPE 3","Slab","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":4},"TYPE 5","Mesh","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":4},"TYPE 5","Morph","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":6},"ARCHICAD property koppelen aan object KM","ARCHICAD Property: Grondverzet",null,1]
["10.44.30.","grondverzet - fysische scheiding/afvoer bodemvreemde materialen ","VH","ton","TYPE 3","Slab","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":4},"TYPE 5","Mesh","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":4},"TYPE 5","Morph","Vul ARCHICAD property 'Soortelijk Gewicht' in","ARCHICAD Property: Grondverzet",null,1]
[{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM of ARCHICAD property koppelen aan object KM","ARCHICAD Property: Grondverzet",null,1]
["10.50.","verwijdering massieven - algemeen ","VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.60.","bronbemaling - algemeen ","SOG",null,"Geen",{"$nulls":4},1]
["10.70.","aanvullingen - algemeen"]
["10.71.","aanvullingen - wederaanvullingen"]
["10.71.10.","aanvullingen - wederaanvullingen/grond van uitgravingen ","PM",null,"Geen",{"$nulls":4},1]
["10.71.20.","aanvullingen - wederaanvullingen/aangevoerde grond ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.71.30.","aanvullingen - wederaanvullingen/gestabiliseerd zand ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.71.40.","aanvullingen - wederaanvullingen/kunststeenslag ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.71.50.","aanvullingen - wederaanvullingen/natuursteenslag ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.72.","aanvullingen - ophoging terrein"]
["10.72.10.","aanvullingen - ophoging terrein/grond van afgravingen ","PM",null,"Geen",{"$nulls":4},1]
["10.72.20","aanvullingen - ophoging terrein/aangevoerde grond ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.72.30.","aanvullingen - ophoging terrein/gestabiliseerd zand ","FH/VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.80.","grondbehandeling - algemeen"]
["10.81.","grondbehandeling - kalk ","VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["10.82.","grondbehandeling - cement ","VH","m3","TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["11.","STUT- & ONDERVANGINGSWERKEN"]
["11.00.","stut- & ondervangingswerken - algemeen"]
["11.10.","beschoeiing bouwputten - algemeen"]
["11.11.","beschoeiing bouwputten - damplanken"]
["11.11.10.","beschoeiing bouwputten - damplanken/aanvoer & installatie machine ","SOG",null,"Geen",{"$nulls":4},1]
["11.11.20.","beschoeiing bouwputten - damplanken/materialen & verwerking ","FH/VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (m2) in bij de Object Settings",null,1]
["11.12.","beschoeiing bouwputten - berlinerwand"]
["11.12.10.","beschoeiing bouwputten - berlinerwand/ aanvoer & installatie machine ","SOG",null,"Geen",{"$nulls":4},1]
["11.12.20.","beschoeiing bouwputten - berlinerwand/materialen & verwerking ","FH/VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (m2) in bij de Object Settings",null,1]
["11.13.","beschoeiing bouwputten - secanspalenwand"]
["11.13.10.","beschoeiing bouwputten - secanspalenwand/installatie palenmachine ","SOG",null,"Geen",{"$nulls":4},1]
["11.13.20.","beschoeiing bouwputten - secanspalenwand/realisatie palenwand ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["11.13.30.","beschoeiing bouwputten - secanspalenwand/verbindingsbalk ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["11.13.50.","beschoeiing bouwputten - secanspalenwand/horizontale verankering ","FH/VH","st","TYPE 5","Object",null,"Stuks",null,1]
["11.13.60.","beschoeiing bouwputten - secanspalenwand/sonische integriteitstesten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["11.13.70.","beschoeiing bouwputten - secanspalenwand/afwerking als kelderwand ","FH","m3","TYPE 3","Wall",null,"Net Volume (heel element)",null,1]
["11.20.","onderschoeiingen - algemeen"]
["11.21.","onderschoeiingen - stortklaar beton ","VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume (heel element)",null,1]
["11.22.","onderschoeiingen - metselwerk ","VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume",null,1]
["11.23.","onderschoeiingen - groutkolommen",{"$nulls":7},1]
["11.23.10.","onderschoeiingen - groutkolommen/aanvoer en installatie van de machine ","SOG",null,"Geen",{"$nulls":4},1]
["11.23.20.","onderschoeiingen - groutkolommen/materialen en verwerking ","VH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["11.30.","keermuren - algemeen"]
["11.31.","keermuren - stortklaar beton ","VH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Projected Area",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume ",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume (heel element)",null,1]
["12.","FUNDERINGEN OP STAAL"]
["12.00.","funderingen op staal - algemeen"]
["12.10.","funderingszolen en -stroken - algemeen"]
["12.11.","funderingszolen en -stroken - ongewapend beton ","VH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume (heel element)",null,1]
["12.12.","funderingszolen en -stroken - gewapend beton ","VH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume (heel element)",null,1]
["12.20.","ondergronds metselwerk - algemeen"]
["12.21.","ondergronds metselwerk - betonblokken"]
["12.21.10.","ondergronds metselwerk - betonblokken/muurdikte 35 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["12.21.20.","ondergronds metselwerk - betonblokken/muurdikte 40 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["12.21.30.","ondergronds metselwerk - betonblokken/muurdikte 45 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["12.22.","ondergronds metselwerk - snelbouw"]
["12.22.10.","ondergronds metselwerk - snelbouw/muurdikte 35 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["12.22.20.","ondergronds metselwerk - snelbouw/muurdikte 40 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["12.22.30.","ondergronds metselwerk - snelbouw/muurdikte 45 cm ","VH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["12.30.","doorbrekingen ondergronds metselwerk - algemeen"]
["12.31.","doorbrekingen ondergronds metselwerk - aansluitbocht ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["12.40.","aardingslus - algemeen","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"FH","st","TYPE 5","Object",null,"Stuks",null,1]
["13.","SPECIALE FUNDERINGEN"]
["13.00.","speciale funderingen - algemeen"]
["13.01.","algemeen - diepsonderingsverslag"]
["13.10.","paalfundering - algemeen"]
["13.11.","paalfundering - schroefpalen"]
["13.11.10.","paalfundering - schroefpalen/enkele grondverdringing"]
["13.11.11.","paalfundering - schroefpalen/enkele grondverdringing - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.11.12.","paalfundering - schroefpalen/enkele grondverdringing - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.11.20.","paalfundering - schroefpalen/dubbele grondverdringing"]
["13.11.21.","paalfundering - schroefpalen/dubbele grondverdringing - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.11.22.","paalfundering - schroefpalen/dubbele grondverdringing - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.12.","paalfundering - boorpalen"]
["13.12.10.","paalfundering - boorpalen/verbuisd"]
["13.12.11.","paalfundering - boorpalen/verbuisd - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.12.12.","paalfundering - boorpalen/verbuisd - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.12.20.","paalfundering - boorpalen/steunvloeistof"]
["13.12.21.","paalfundering - boorpalen/steunvloeistof - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.12.22.","paalfundering - boorpalen/steunvloeistof - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.13.","paalfundering - kokerpalen"]
["13.13.10.","paalfundering - kokerpalen/geschroefd"]
["13.13.11.","paalfundering - kokerpalen/geschroefd - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.13.12.","paalfundering - kokerpalen/geschroefd - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.13.20.","paalfundering - kokerpalen geheid"]
["13.13.21.","paalfundering - kokerpalen geheid - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.13.22.","paalfundering - kokerpalen/geheid - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.14.","paalfundering - heipalen"]
["13.14.10.","paalfundering - heipalen/in de grond gevormd"]
["13.14.11.","paalfundering - heipalen/in de grond gevormd - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.14.12.","paalfundering - heipalen/in de grond gevormd - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.14.20.","paalfundering - heipalen/prefab beton"]
["13.14.21.","paalfundering - heipalen/prefab beton - werfinstallatie ","SOG",null,"Geen",{"$nulls":4},1]
["13.14.22.","paalfundering - heipalen/prefab beton - realisatie palen ","FH","st","TYPE 3","Column",null,"Stuks",null,1]
["13.20.","fundering op valse putten - algemeen"]
["13.21.","fundering op valse putten - ongewapend stortklaar beton ","FH/VH","m","TYPE 2","Column",null,"diepte / hoogte kolom",null,1]
[null,null,"FH/VH","m","TYPE 3","Slab",null,null,null,1]
[null,null,"FH/VH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"FH/VH","m","TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,"FH/VH","m2","TYPE 2","Column",null,"Top Surface <> rekent momenteel core uit",null,1]
[null,null,"FH/VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"FH/VH","m2","TYPE 3","Column",null,"Net Area",null,1]
[null,null,"FH/VH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,"FH/VH","m3","TYPE 2","Column",null,"Net Volume",null,1]
[null,null,"FH/VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"FH/VH","m3","TYPE 3","Column",null,"Net Volume",null,1]
[null,null,"FH/VH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
["13.22.","fundering op valse putten - gewapend stortklaar beton ","FH/VH","m","TYPE 2","Column",null,"diepte / hoogte kolom",null,1]
[null,null,"FH/VH","m","TYPE 3","Slab",null,null,null,1]
[null,null,"FH/VH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"FH/VH","m","TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,"FH/VH","m2","TYPE 2","Column",null,"Top Surface <> rekent momenteel core uit",null,1]
[null,null,"FH/VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"FH/VH","m2","TYPE 3","Column",null,"Net Area",null,1]
[null,null,"FH/VH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,"FH/VH","m3","TYPE 2","Column",null,"Net Volume",null,1]
[null,null,"FH/VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"FH/VH","m3","TYPE 3","Column",null,"Net Volume",null,1]
[null,null,"FH/VH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
["13.23.","fundering op valse putten - gestabiliseerd zand ","FH/VH","m","TYPE 2","Column",null,"diepte / hoogte kolom",null,1]
[null,null,"FH/VH","m","TYPE 3","Slab",null,null,null,1]
[null,null,"FH/VH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"FH/VH","m","TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,"FH/VH","m2","TYPE 2","Column",null,"Top Surface <> rekent momenteel core uit",null,1]
[null,null,"FH/VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"FH/VH","m2","TYPE 3","Column",null,"Net Area",null,1]
[null,null,"FH/VH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,"FH/VH","m3","TYPE 2","Column",null,"Net Volume",null,1]
[null,null,"FH/VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"FH/VH","m3","TYPE 3","Column",null,"Net Volume",null,1]
[null,null,"FH/VH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
["13.24.","fundering op valse putten - steenslag ","FH/VH","m","TYPE 2","Column",null,"diepte / hoogte kolom",null,1]
[null,null,"FH/VH","m","TYPE 3","Slab",null,null,null,1]
[null,null,"FH/VH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"FH/VH","m","TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,"FH/VH","m2","TYPE 2","Column",null,"Top Surface <> rekent momenteel core uit",null,1]
[null,null,"FH/VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"FH/VH","m2","TYPE 3","Column",null,"Net Area",null,1]
[null,null,"FH/VH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,"FH/VH","m3","TYPE 2","Column",null,"Net Volume",null,1]
[null,null,"FH/VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"FH/VH","m3","TYPE 3","Column",null,"Net Volume",null,1]
[null,null,"FH/VH","m3","TYPE 5","Morph",null,"Net Volume",null,1]
["13.30.","funderingsbalken - algemeen"]
["13.31.","funderingsbalken - stortklaar beton ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume",null,1]
["13.40.","plaat op putten - algemeen"]
["13.41.","plaat op putten - gewapend stortklaar beton ","FH","m3","TYPE 3","Beam ",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume",null,1]
["13.42.","plaat op putten - gewapend & gepolierd stortklaar beton ","FH","m3","TYPE 3","Beam ",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume",null,1]
["13.50.","plaatfunderingen - algemeen"]
["13.51.","plaatfunderingen - gewapend stortklaar beton ","FH","m3","TYPE 3","Beam ",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume",null,1]
["13.52.","plaatfunderingen - gewapend en gepolierd stortklaar beton ","FH","m3","TYPE 3","Beam ",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume",null,1]
["13.60.","liftputten - algemeen"]
["13.61.","liftputten - stortklaar beton ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["13.70.","doorbrekingen speciale funderingen - algemeen"]
["13.71.","doorbrekingen speciale funderingen - aansluitbocht ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["13.72.","doorbrekingen speciale funderingen - doorvoermoffen voor buizen en kabels ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["14.","ONDERGRONDSE WANDEN"]
["14.00.","ondergrondse wanden - algemeen"]
["14.10.","funderingswanden - algemeen"]
["14.11.","funderingswanden - beton"]
["14.11.10.","funderingswanden - beton/ter plaatse gestort"]
["14.11.11.","funderingswanden - beton/ter plaatse gestort - dikte 20 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.11.12.","funderingswanden - beton/ter plaatse gestort - dikte 25 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.11.13.","funderingswanden - beton/ter plaatse gestort - dikte 30 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.11.14.","funderingswanden - beton/ter plaatse gestort - dikte 35 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.11.20.","funderingswanden - beton/holle wanden"]
["14.11.21.","funderingswanden - beton/holle wanden - prefabelementen ","FH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Projected Area",null,1]
["14.11.22.","funderingswanden - beton/holle wanden - vulbeton ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume",null,1]
["14.11.30.","funderingswanden - beton/injectie van onvermijdelijke scheuren ","VH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["14.12.","funderingswanden - metselwerk"]
["14.12.01.","funderingswanden - metselwerk/mortel ","PM",null,"Geen",{"$nulls":4},1]
["14.12.02.","funderingswanden - metselwerk/wapening ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["14.12.10.","funderingswanden - metselwerk/betonblokken"]
["14.12.11.","funderingswanden - metselwerk/betonblokken - muurdikte 29 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.12.12.","funderingswanden - metselwerk/betonblokken - muurdikte 35 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.12.13.","funderingswanden - metselwerk/betonblokken - muurdikte 39 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.12.14.","funderingswanden - metselwerk/betonblokken - muurdikte 40 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.20.","dragende kelderwanden - algemeen"]
["14.21.","dragende kelderwanden - beton"]
["14.21.10.","dragende kelderwanden - beton/ter plaatse gestort"]
["14.21.11.","dragende kelderwanden - beton/ter plaatse gestort - dikte 20 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.21.12.","dragende kelderwanden - beton/ter plaatse gestort - dikte 25 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.21.13.","dragende kelderwanden - beton/ter plaatse gestort - dikte 30 cm ","FH","m3","TYPE 2","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Net Volume",null,1]
["14.21.20.","dragende kelderwanden - beton/holle wanden"]
["14.21.21.","dragende kelderwanden - beton/holle wanden - prefabelementen ","FH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Projected Area",null,1]
["14.21.22.","dragende kelderwanden - beton/holle wanden - vulbeton ","FH","m3","TYPE 3","Wall",null,"Net Volume",null,1]
["14.21.30.","dragende kelderwanden - beton/injectie van onvermijdelijke scheuren ","VH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["14.22.","dragende kelderwanden - metselwerk"]
["14.22.01.","dragende kelderwanden - metselwerk/mortel ","PM",null,"Geen",{"$nulls":4},1]
["14.22.02.","dragende kelderwanden - metselwerk/wapening ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["14.22.03.","dragende kelderwanden - metselwerk/lateien ","PM",null,"Geen",{"$nulls":4},1]
["14.22.10.","dragende kelderwanden - metselwerk/betonblokken"]
["14.22.11.","dragende kelderwanden - metselwerk/betonblokken - muurdikte 14 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.12.","dragende kelderwanden - metselwerk/betonblokken - muurdikte 19 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.13.","dragende kelderwanden - metselwerk/betonblokken - muurdikte 29 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.20.","dragende kelderwanden - metselwerk/baksteen"]
["14.22.21.","dragende kelderwanden - metselwerk/baksteen - muurdikte 14 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.22.","dragende kelderwanden - metselwerk/baksteen - muurdikte 19 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.30.","dragende kelderwanden - metselwerk/kalkzandsteen"]
["14.22.31.","dragende kelderwanden - metselwerk/kalkzandsteen - muurdikte 15 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.32.","dragende kelderwanden - metselwerk/kalkzandsteen - muurdikte 17,5 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.22.33.","dragende kelderwanden - metselwerk/kalkzandsteen - muurdikte 21,5 cm ","FH","m3","TYPE 2","Wall",null,"Net Volume",null,1]
["14.30.","geprefabriceerde kelders - algemeen"]
["14.31.","geprefabriceerde kelders - gedeeltelijke onderkeldering ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":5},"Wall",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Slab",null,"Stuks",null,1]
["14.40.","waterdichting ondergrondse wanden - algemeen"]
["14.41.","waterdichting ondergrondse wanden - mineraliserende mortel ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["14.42.","waterdichting ondergrondse wanden - gemodificeerde cementmortel ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["14.43.","waterdichting ondergrondse wanden - bitumenemulsie ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["14.44.","waterdichting ondergrondse wanden - noppenbanen ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["14.50.","doorbrekingen ondergrondse wanden - algemeen"]
["14.51.","doorbrekingen ondergrondse wanden - aansluitbocht ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["14.52.","doorbrekingen ondergrondse wanden - doorvoermoffen buizen en kabels ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["14.60.","verluchtingselementen ondergrondse wanden - algemeen"]
["14.61.","verluchtingselementen ondergrondse wanden - telescopische kokers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["15.","VLOERLAGEN ONDERBOUW"]
["15.00.","vloerlagen onderbouw - algemeen"]
["15.10.","zuiverheidslagen - algemeen"]
["15.11.","zuiverheidslagen - stortklaar beton ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m3","TYPE 2","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["15.20.","draagvloeren op volle grond - algemeen"]
["15.21.","draagvloeren op volle grond - stortklaar gewapend beton ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["15.30.","vochtwerende lagen - algemeen"]
["15.31.","vochtwerende lagen - folies"]
["15.31.10.","vochtwerende lagen - folies/PE ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["15.31.20.","vochtwerende lagen - folies/PVC ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["15.31.30.","vochtwerende lagen - folies/PIB ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["15.32.","vochtwerende lagen - banen"]
["15.32.10.","vochtwerende lagen - banen/HDPE ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["15.33.","vochtwerende lagen - bitumenglasvlies ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["16.","THERMISCHE ISOLATIE ONDERBOUW"]
["16.00.","thermische isolatie onderbouw - algemeen"]
["16.10.","isolatieplaten op volle grond - algemeen"]
["16.11.","isolatieplaten op volle grond - XPS"]
["16.11.10.","isolatieplaten op volle grond - XPS/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["16.11.20.","isolatieplaten op volle grond - XPS/12 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["16.12.","isolatieplaten op volle grond - PUR of PIR"]
["16.12.10.","isolatieplaten op volle grond - PUR of PIR/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["16.12.20.","isolatieplaten op volle grond - PUR of PIR/12 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["16.13.","isolatieplaten op volle grond - EPS"]
["16.13.10.","isolatieplaten op volle grond - EPS/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["16.13.20.","isolatieplaten op volle grond - EPS/12 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["16.20.","perimeterisolatie - algemeen"]
["16.21.","perimeterisolatie - XPS"]
["16.21.10.","perimeterisolatie - XPS/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 2","Beam",null,"Oppervlakte middenas wand",null,1]
["16.21.20.","perimeterisolatie - XPS/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 2","Beam",null,"Oppervlakte middenas wand",null,1]
["16.22.","perimeterisolatie - PUR of PIR"]
["16.22.10.","perimeterisolatie - PUR of PIR/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 2","Beam",null,"Oppervlakte middenas wand",null,1]
["16.22.20.","perimeterisolatie - PUR of PIR/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 2","Beam",null,"Oppervlakte middenas wand",null,1]
["17.","ONDERGRONDSE LEIDINGEN"]
["17.00.","ondergrondse leidingen - algemeen"]
["17.10.","rioolbuizen - algemeen"]
["17.11.","rioolbuizen - beton"]
["17.11.10.","rioolbuizen - beton ongewapend"]
["17.11.11.","rioolbuizen - beton/ongewapend - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.12.","rioolbuizen - beton/ongewapend - diam 250 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.13.","rioolbuizen - beton/ongewapend - diam 300 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.14.","rioolbuizen - beton/ongewapend - diam 400 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.15.","rioolbuizen - beton/ongewapend - diam 500 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.16.","rioolbuizen - beton/ongewapend - diam 600 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.20.","rioolbuizen - beton gewapend"]
["17.11.21.","rioolbuizen - beton/gewapend - diam 300 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,null,"m","TYPE 5","Object","MEP",null,null,1]
["17.11.22.","rioolbuizen - beton/gewapend - diam 400 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,null,"m","TYPE 5","Object","MEP",null,null,1]
["17.11.23.","rioolbuizen - beton/gewapend - diam 500 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.24.","rioolbuizen - beton/gewapend - diam 600 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.11.25.","rioolbuizen - beton/gewapend - diam 800 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.","rioolbuizen - kunststof"]
["17.12.10.","rioolbuizen - kunststof/PVC"]
["17.12.11.","rioolbuizen - kunststof/PVC - diam 110 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.12.","rioolbuizen - kunststof/PVC - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.13.","rioolbuizen - kunststof/PVC - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.14.","rioolbuizen - kunststof/PVC - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.15.","rioolbuizen - kunststof/PVC - diam 315 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.16.","rioolbuizen - kunststof/PVC - diam 400 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.20.","rioolbuizen - kunststof/PE"]
["17.12.21.","rioolbuizen - kunststof/PE - diam 110 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.22.","rioolbuizen - kunststof/PE - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.23.","rioolbuizen - kunststof/PE - diam 140 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.24.","rioolbuizen - kunststof/PE - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.25.","rioolbuizen - kunststof/PE - diam 180 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.26.","rioolbuizen - kunststof/PE - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.27.","rioolbuizen - kunststof/PE - diam 225 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.28.","rioolbuizen - kunststof/PE - diam 250 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.30.","rioolbuizen - kunststof/PP"]
["17.12.31.","rioolbuizen - kunststof/PP - diam 110 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.32.","rioolbuizen - kunststof/PP - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.33.","rioolbuizen - kunststof/PP - diam 140 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.34.","rioolbuizen - kunststof/PP - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.35.","rioolbuizen - kunststof/PP - diam 180 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.36.","rioolbuizen - kunststof/PP - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.37.","rioolbuizen - kunststof/PP - diam 225 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.12.38.","rioolbuizen - kunststof/PP - diam 250 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP",null,null,1]
["17.20.","draineerbuizen - algemeen"]
["17.21.","draineerbuizen - poreus beton"]
["17.21.10.","draineerbuizen - poreus beton/diam 80 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.21.20.","draineerbuizen - poreus beton/diam 100 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.21.30.","draineerbuizen - poreus beton/diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.21.40.","draineerbuizen - poreus beton/diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.21.50.","draineerbuizen - poreus beton/diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.22.","draineerbuizen - vezelcement"]
["17.22.10.","draineerbuizen - poreus beton/diam 80 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.22.20.","draineerbuizen - poreus beton/diam 100 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.22.30.","draineerbuizen - poreus beton/diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.22.40.","draineerbuizen - poreus beton/diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.22.50.","draineerbuizen - poreus beton/diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.","draineerbuizen - kunststof"]
["17.23.10.","draineerbuizen - kunststof/PVC"]
["17.23.11.","draineerbuizen - kunststof/PVC - diam 50 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.12.","draineerbuizen - kunststof/PVC - diam 65 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.13.","draineerbuizen - kunststof/PVC - diam 80 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.14.","draineerbuizen - kunststof/PVC - diam 100 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.15.","draineerbuizen - kunststof/PVC - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.16.","draineerbuizen - kunststof/PVC - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.17.","draineerbuizen - kunststof/PVC - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.20.","draineerbuizen - kunststof/PE"]
["17.23.21.","draineerbuizen - kunststof/PE - diam 50 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.22.","draineerbuizen - kunststof/PE - diam 60 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.23.","draineerbuizen - kunststof/PE - diam 80 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.24.","draineerbuizen - kunststof/PE - diam 100 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.25.","draineerbuizen - kunststof/PE - diam 125 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.26.","draineerbuizen - kunststof/PE - diam 160 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.23.27.","draineerbuizen - kunststof/PE - diam 200 ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.30.","toezichtputten - algemeen"]
["17.31.","toezichtputten - metselwerk ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.32.","toezichtsputten - beton"]
["17.32.10.","toezichtsputten - beton/stortklaar ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.32.20.","toezichtsputten - beton/prefab ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.33.","toezichtputten - vezelcement ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.34.","toezichtsputten - kunststof"]
["17.34.10.","toezichtputten - kunststof/PVC ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.34.20.","toezichtputten - kunststof/PE ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.34.30.","toezichtputten - kunststof/polyester ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.40.","ontvangtoestellen - algemeen"]
["17.41.","ontvangtoestellen - buitenontvanger"]
["17.41.10.","ontvangtoestellen - buitenontvanger/met klok ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.41.20.","ontvangtoestellen - buitenontvanger/met korf ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.42.","ontvangtoestellen - geulen"]
["17.42.10.","ontvangtoestellen - geulen/beton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.42.20.","ontvangtoestellen - geulen/glasvezelbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.42.30.","ontvangtoestellen - geulen/polyesterbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["17.43.","ontvangtoestellen - straatkolken ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.44.","ontvangtoestellen - prefab pompputten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.50.","putdeksels en roosters - algemeen"]
["17.51.","putdeksels en roosters - enkel deksel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.52.","putdeksels en roosters - dubbel deksel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.53.","putdeksels en roosters - geulroosters ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["17.60.","afvalwaterbehandeling - algemeen"]
["17.61.","afvalwaterbehandeling - septische putten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.70.","regenwaterbehandeling - algemeen"]
["17.71.","regenwaterbehandeling - regenwaterputten"]
["17.71.10.","regenwaterbehandeling - regenwaterputten/beton ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.71.20.","regenwaterbehandeling - regenwaterputten/HDPE ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.71.30.","regenwaterbehandeling - regenwaterputten/polyester ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.71.40.","regenwaterbehandeling - regenwaterputten/metselwerk ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.72.","regenwaterbehandeling - hergebruik regenwater ","PM",null,"Geen",{"$nulls":4},1]
["17.73.","regenwaterbehandeling - voorfilters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.74.","regenwaterbehandeling - overloop en terugslagklep ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.75.","regenwaterbehandeling - infiltratievoorzieningen"]
["17.75.10.","regenwaterbehandeling - infiltratievoorzieningen/infiltratieputten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.75.20.","regenwaterbehandeling - infiltratievoorzieningen/infiltratieblokken ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.75.30.","regenwaterbehandeling - infiltratievoorzieningen/infiltratiebuizen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.80.","aansluitingen - algemeen"]
["17.81.","aansluitingen - openbare riolering ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["17.82.","aansluitingen - doorvoer- en wachtbuizen ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["17.83.","aansluitingen - wachtput ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[]
["20.","METSELWERK"]
["20.00.","metselwerken - algemeen"]
["20.01.","metselwerken - ter plaatse gemetst"]
["20.02.","metselwerken - prefab"]
["20.10.","materialen - algemeen"]
["20.11.","materialen - metselmortel"]
["20.11.10.","materialen - metselmortel/voor algemene toepassing (G) ","PM",null,"Geen",{"$nulls":4},1]
["20.11.20.","materialen - metselmortel/lijmmortel (T) ","PM",null,"Geen",{"$nulls":4},1]
["20.11.30.","materialen - metselmortel/lichtgewicht metselmortel (L) ","PM",null,"Geen",{"$nulls":4},1]
["20.12.","materialen - hulpstukken"]
["20.12.10.","materialen - hulpstukken/spouwankers"]
["20.12.11.","materialen - hulpstukken/spouwankers - gewone spouwankers ","PM",null,"Geen",{"$nulls":4},1]
["20.12.12.","materialen - hulpstukken/spouwankers - slag- en schroefankers met isolatieplug ","PM",null,"Geen",{"$nulls":4},1]
["20.12.13.","materialen - hulpstukken/spouwankers - akoestisch spouwanker ","PM",null,"Geen",{"$nulls":4},1]
["20.12.20.","materialen - hulpstukken/lateien"]
["20.12.21.","materialen - hulpstukken/lateien - beton ","PM",null,"Geen",{"$nulls":4},1]
["20.12.22.","materialen - hulpstukken/lateien - staal ","PM",null,"Geen",{"$nulls":4},1]
["20.12.23.","materialen - hulpstukken/lateien - bekistingsmetselstenen ","PM",null,"Geen",{"$nulls":4},1]
["20.12.30.","materialen - hulpstukken/waterkering ","PM",null,"Geen",{"$nulls":4},1]
["20.12.40.","materialen - hulpstukken/wapening ","FH","m","TYPE 5","Object","Meetstaat Manager 27 KM","Vul de waarde Lengte (cm) in bij de Object settings",null,1]
["20.12.50.","materialen - hulpstukken/akoestische stroken ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 27 KM","Vul de waarde Lengte (cm) in bij de Object settings",null,1]
["20.13.","materialen - kimblokken"]
["20.13.10.","materialen - kimblokken/cellenbeton ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[{"$nulls":4},"TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
["20.13.20.","materialen - kimblokken/samengestelde blok ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[{"$nulls":4},"TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
["20.13.30.","materialen - kimblokken/thermisch verbeterde steen ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[{"$nulls":4},"TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
["20.13.40.","materialen - kimblokken/cellenglas ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 2","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom"]
[{"$nulls":4},"TYPE 3","Wall",null,"Lengte volgens eigen middenas"]
["20.20.","binnenspouwblad - algemeen"]
["20.21.","binnenspouwblad - snelbouw"]
["20.21.10.","binnenspouwblad - snelbouw/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.21.20.","binnenspouwblad - snelbouw/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.22.","binnenspouwblad - kalkzandsteen"]
["20.22.10.","binnenspouwblad - kalkzandsteen/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.22.20.","binnenspouwblad - kalkzandsteen/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.22.30.","binnenspouwblad - kalkzandsteen/dikte 21,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.22.40.","binnenspouwblad - kalkzandsteen/dikte 30 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.23.","binnenspouwblad - betonsteen met gewone granulaten"]
["20.23.10.","binnenspouwblad - betonsteen met gewone granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.23.20.","binnenspouwblad - betonsteen met gewone granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.24.","binnenspouwblad - betonsteen met lichte granulaten"]
["20.24.10.","binnenspouwblad - betonsteen met lichte granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.24.20.","binnenspouwblad - betonsteen met lichte granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.","binnenspouwblad - cellenbeton"]
["20.25.10.","binnenspouwblad - cellenbeton/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.20.","binnenspouwblad - cellenbeton/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.30.","binnenspouwblad - cellenbeton/dikte 20 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.40.","binnenspouwblad - cellenbeton/dikte 24 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.50.","binnenspouwblad - cellenbeton/dikte 30 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.60.","binnenspouwblad - cellenbeton/dikte 36,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.70.","binnenspouwblad - cellenbeton/dikte 40 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.25.80.","binnenspouwblad - cellenbeton/dikte 50 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.30.","woningscheidende wand - algemeen"]
["20.31.","woningscheidende wand - snelbouw"]
["20.31.10.","woningscheidende wand - snelbouw/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.31.20.","woningscheidende wand - snelbouw/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.32.","woningscheidende wand - kalkzandsteen"]
["20.32.10.","woningscheidende wand - kalkzandsteen/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.32.20.","woningscheidende wand - kalkzandsteen/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.32.30.","woningscheidende wand - kalkzandsteen/dikte 21,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.32.40.","woningscheidende wand - kalkzandsteen/dikte 30 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.33.","woningscheidende wand - betonsteen met gewone granulaten"]
["20.33.10.","woningscheidende wand - betonsteen met gewone granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.33.20.","woningscheidende wand - betonsteen met gewone granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.34.","woningscheidende wand - betonsteen met lichte granulaten"]
["20.34.10.","woningscheidende wand - betonsteen met lichte granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.34.20.","woningscheidende wand - betonsteen met lichte granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.35.","woningscheidende wand - cellenbeton"]
["20.35.10.","woningscheidende wand - cellenbeton/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.35.20.","woningscheidende wand - cellenbeton/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.35.30.","woningscheidende wand - cellenbeton/dikte 20 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.35.40.","woningscheidende wand - cellenbeton/dikte 24 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.40.","dragende binnenmuur - algemeen"]
["20.41.","dragende binnenmuur - snelbouw"]
["20.41.10.","dragende binnenmuur - snelbouw/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.41.20.","dragende binnenmuur - snelbouw/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.42.","dragende binnenmuur - kalkzandsteen"]
["20.42.10.","dragende binnenmuur - kalkzandsteen/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.42.20.","dragende binnenmuur - kalkzandsteen/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.42.30.","dragende binnenmuur - kalkzandsteen/dikte 21,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.43.","dragende binnenmuur - betonsteen met gewone granulaten"]
["20.43.10.","dragende binnenmuur - betonsteen met gewone granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.43.20.","dragende binnenmuur - betonsteen met gewone granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.44.","dragende binnenmuur - betonsteen met lichte granulaten"]
["20.44.10.","dragende binnenmuur - betonsteen met lichte granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.44.20.","dragende binnenmuur - betonsteen met lichte granulaten/dikte 19 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.45.","dragende binnenmuur - cellenbeton"]
["20.45.10.","dragende binnenmuur - cellenbeton/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.45.20.","dragende binnenmuur - cellenbeton/dikte 17,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.45.30.","dragende binnenmuur - cellenbeton/dikte 20 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.45.40.","dragende binnenmuur - cellenbeton/dikte 24 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.50.","niet-dragende binnenmuur - algemeen"]
["20.51.","niet-dragende binnenmuur - snelbouw"]
["20.51.10.","niet-dragende binnenmuur - snelbouw/dikte 9 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.51.20.","niet-dragende binnenmuur - snelbouw/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.52.","niet-dragende binnenmuur - kalkzandsteen"]
["20.52.10.","niet-dragende binnenmuur - kalkzandsteen/dikte 10 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.52.20.","niet-dragende binnenmuur - kalkzandsteen/dikte 15 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.53.","niet-dragende binnenmuur - betonsteen met lichte granulaten"]
["20.53.10.","niet-dragende binnenmuur - betonsteen met lichte granulaten/dikte 9 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.53.20.","niet-dragende binnenmuur - betonsteen met lichte granulaten/dikte 14 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.54.","niet-dragende binnenmuur - cellenbeton"]
["20.54.10.","niet-dragende binnenmuur - cellenbeton/dikte 7 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.54.20.","niet-dragende binnenmuur - cellenbeton/dikte 10 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.54.30.","niet-dragende binnenmuur - cellenbeton/dikte 11,5 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.55.","niet-dragende binnenmuur - gipsblokken"]
["20.55.10.","niet-dragende binnenmuur - gipsblokken/dikte 6 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.55.20.","niet-dragende binnenmuur - gipsblokken/dikte 7 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.55.30.","niet-dragende binnenmuur - gipsblokken/dikte 8 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.55.40.","niet-dragende binnenmuur - gipsblokken/dikte 10 cm ","FH","m3","TYPE 1","Wall",null,"Net Volume",null,1]
["20.60.","renovatiewerken - algemeen"]
["20.61.","renovatiewerken - behandeling tegen opstijgend vocht"]
["20.61.10.","renovatiewerken - behandeling tegen opstijgend vocht/injecteren ","FH/VH","m","TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Lengte (cm) in bij de Object settings",null,1]
["20.61.20.","renovatiewerken - behandeling tegen opstijgend vocht/plaatsen dichtingsmembraan ","FH/VH","m","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Lengte (cm) in bij de Object settings",null,1]
[null,null,null,"m","TYPE 3","Wall",null,"Reference line length",null,1]
["21.","SPOUWMUURISOLATIE"]
["21.00.","spouwmuurisolatie - algemeen"]
["21.10.","spouwmuurisolatie buitenspouwblad - algemeen"]
["21.11.","spouwmuurisolatie buitenspouwblad - MW"]
["21.11.10.","spouwmuurisolatie buitenspouwblad - MW / 12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.11.20.","spouwmuurisolatie buitenspouwblad - MW / 14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.12.","spouwmuurisolatie buitenspouwblad - PUR of PIR"]
["21.12.10.","spouwmuurisolatie buitenspouwblad - PUR of PIR/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.12.20.","spouwmuurisolatie buitenspouwblad - PUR of PIR/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.13.","spouwmuurisolatie buitenspouwblad - PF"]
["21.13.10.","spouwmuurisolatie buitenspouwblad - PF/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.13.20.","spouwmuurisolatie buitenspouwblad - PF/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.14.","spouwmuurisolatie buitenspouwblad - XPS"]
["21.14.10.","spouwmuurisolatie buitenspouwblad - XPS/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.14.20.","spouwmuurisolatie buitenspouwblad - XPS/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.15.","spouwmuurisolatie buitenspouwblad - EPS"]
["21.15.10.","spouwmuurisolatie buitenspouwblad - EPS/10 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.15.20.","spouwmuurisolatie buitenspouwblad - EPS/12 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.20.","spouwmuurisolatie woningscheidende wand - algemeen"]
["21.21.","spouwmuurisolatie woningscheidende wand - MW"]
["21.21.10.","spouwmuurisolatie woningscheidende wand - MW/4 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.21.20.","spouwmuurisolatie woningscheidende wand - MW/5 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.22.","spouwmuurisolatie woningscheidende wand - XPS"]
["21.22.10.","spouwmuurisolatie woningscheidende wand - XPS/2 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.22.20.","spouwmuurisolatie woningscheidende wand - XPS/3 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.23.","spouwmuurisolatie woningscheidende wand - PUR of PIR"]
["21.23.10.","spouwmuurisolatie woningscheidende wand - PUR of PIR/3 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.23.20.","spouwmuurisolatie woningscheidende wand - PUR of PIR/4 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["21.30.","spouwmuurisolatie navulling - algemeen"]
["21.31.","spouwmuurisolatie navulling - MW ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["21.32.","spouwmuurisolatie navulling - PUR ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["21.33.","spouwmuurisolatie navulling - EPS ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["22.","GEVELMETSELWERK"]
["22.00.","gevelmetselwerken - algemeen"]
["22.01.","algemeen - ter plaatse gemetst gevelmetselwerk"]
["22.02.","algemeen - prefab gevelmetselwerk"]
["22.10.","materialen - algemeen"]
["22.11.","materialen - mortel"]
["22.11.10.","materialen - mortel/metselmortel"]
["22.11.11.","materialen - mortel/metselmortel - voor algemene toepassing ","PM",null,"Geen",{"$nulls":4},1]
["22.11.12.","materialen - mortel/metselmortel - dunbedmortel ","PM",null,"Geen",{"$nulls":4},1]
["22.11.13.","materialen - mortel/metselmortel - lijmmortel ","PM",null,"Geen",{"$nulls":4},1]
["22.11.20.","materialen - mortel/voegmortel"]
["22.12.","materialen - spouwankers ","PM",null,"Geen",{"$nulls":4},1]
["22.13.","materialen - waterkering ","PM",null,"Geen",{"$nulls":4},1]
["22.14.","materialen - wapening ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["22.20.","gevelstenen - algemeen"]
["22.21.","gevelstenen - baksteen"]
["22.21.10.","gevelstenen - baksteen/strengpersstenen ","FH","m2","TYPE 3","Wall",null,"Conditional surface area on the Inside Face\n\n",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
["22.21.20.","gevelstenen - bakstenen/handvorm- en vormbakstenen ","FH","m2","TYPE 3","Wall",null,"Conditional surface area on the Inside Face\n\n",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
["22.22.","gevelstenen - betonsteen ","FH","m2","TYPE 3","Wall",null,"Conditional surface area on the Inside Face\n\n",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
["22.30.","renovatiewerken - algemeen"]
["22.31.","renovatiewerken - herstelling en aanpassing bestaand gevelmetselwerk ","FH","m2","TYPE 3","Wall",null,"Conditional surface area on the Inside Face\n\n",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
["23.00.","dorpels, plinten en dekstenen - algemeen"]
["23.01.","algemeen - blauwe hardsteen"]
["23.02.","algemeen - beton"]
["23.03.","algemeen - vezelcement"]
["23.10.","raam- en deurdorpels - algemeen"]
["23.11.","raam- en deurdorpels - blauwe hardsteen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[null,null,null,"m2","TYPE 3","Beam",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","breedte dagkant * diepte dorpel",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Area",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","breedte dagkant * diepte dorpel * dikte dorpel",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Stuks",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Stuks",null,1]
["23.12.","raam- en deurdorpels - prefabbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","breedte dagkant * diepte dorpel * dikte dorpel",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Stuks",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Stuks",null,1]
["23.13.","raam- en deurdorpels - vezelcement ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
["23.14.","raam- en deurdorpels - gevelsteen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","breedte dagkant * diepte dorpel * dikte dorpel",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","Net Volume",null,1]
["23.20.","garagepoortdorpels - algemeen"]
["23.21.","garagepoortdorpels - blauwe hardsteen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[null,null,null,"m2","TYPE 3","Beam",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","breedte dagkant * diepte dorpel",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","breedte dagkant * diepte dorpel * dikte dorpel",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","Stuks",null,1]
["23.22.","garagepoortdorpels - prefabbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW raam-en deurdorpels","ARCHICAD property: Lengte dorpel",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","breedte dagkant * diepte dorpel * dikte dorpel",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW garagepoortdorpels","Stuks",null,1]
["23.30.","gevelplinten - algemeen"]
["23.31.","gevelplinten - blauwe hardsteen ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Volume ( heel element)",null,1]
["23.32.","gevelplinten - sierbeton ","FH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Projected Area",null,1]
["23.33.","gevelplinten - vezelcement ","FH","m2","TYPE 3","Beam",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 3","Wall ",null,"Projected Area",null,1]
["23.40.","omkaderingselementen - algemeen"]
["23.41.","omkaderingselementen - blauwe steen ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["23.50.","muurdekstenen - algemeen"]
["23.51.","muurdekstenen - blauwe steen ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["23.52.","muurdekstenen - prefabbeton ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Omtrek vloer zonder openingen",null,1]
["23.53.","muurdekstenen - vezelcement ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Omtrek vloer zonder openingen",null,1]
["23.60.","schoorsteendekplaten - algemeen"]
["23.61.","schoorsteendekplaten - blauwe steen ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Stuks",null,1]
["23.62.","schoorsteendekplaten - beton ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Stuks",null,1]
["23.63.","schoorsteendekplaten - vezelcement ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Stuks",null,1]
["24.","RUWBOUWKANALEN"]
["24.00.","ruwbouw kanalen - algemeen"]
["24.10.","modulaire ruwbouwkanalen - algemeen"]
["24.11.","modulaire ruwbouwkanalen - beton "]
["24.11.10.","modulaire ruwbouwkanalen - beton/rookgasafvoer ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["24.11.20.","modulaire ruwbouwkanalen - beton/ventilatie ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["24.12.","modulaire ruwbouwkanalen - keramische blokken"]
["24.12.10.","modulaire ruwbouwkanalen - keramische blokken/rookgasafvoer ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["24.12.20.","modulaire ruwbouwkanalen - keramische blokken/ventilatie ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["25.","STRUCTUURELEMENTEN HOUT"]
["25.00.","structuurelementen hout - algemeen"]
["25.01.","algemeen - stabiliteitsstudie ","PM",null,"Geen",{"$nulls":4},1]
["25.02.","algemeen - opleg- en bevestigingsmaterialen"]
["25.02.10.","algemeen - opleg- en bevestigingsmaterialen/metalen schoenen ","PM",null,"Geen",{"$nulls":4},1]
["25.02.20.","algemeen - opleg- en bevestigingsmaterialen/schroeven, nagels en nieten ","PM",null,"Geen",{"$nulls":4},1]
["25.02.30.","algemeen - opleg- en bevestigingsmaterialen/lijmen ","PM",null,"Geen",{"$nulls":4},1]
["25.02.40.","algemeen - opleg- en bevestigingsmaterialen/metalen hechtplaten ","PM",null,"Geen",{"$nulls":4},1]
["25.10.","balken - algemeen"]
["25.11.","balken - massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["25.12.","balken - LVL ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["25.13.","balken - lichte samengestelde liggers ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["25.14.","balken - gelijmd gelamineerd hout (GL) ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["25.20.","kolommen - algemeen"]
["25.21.","kolommen - massief hout ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
["25.22.","kolommen - LVL ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
["25.23.","kolommen - gelijmd gelamineerd hout"]
["25.30.","vloeren - algemeen"]
["25.31.","vloeren - roostering met beplating"]
["25.31.10.","vloeren - roostering met beplating/balken"]
["25.31.11.","vloeren - roostering met beplating/balken - massief hout ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["25.31.12.","vloeren - roostering met beplating/balken - LVL ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["25.31.13.","vloeren - roostering met beplating/balken - lichte samengestelde liggers ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["25.31.14.","vloeren - roostering met beplating/balken - gelijmd gelamineerd hout ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["25.31.20.","vloeren - roostering met beplating/beplating"]
["25.31.21.","vloeren - roostering met beplating/beplating - OSB ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["25.31.22.","vloeren - roostering met beplating/beplating - spaanplaat ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["25.31.23.","vloeren - roostering met beplating/beplating - LVL ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.","STRUCTUURELEMENTEN BETON"]
["26.00.","structuurelementen gewapend beton - algemeen"]
["26.01.","algemeen - stabiliteitsstudie ","PM",null,"Geen",{"$nulls":4},1]
["26.10.","materialen - algemeen"]
["26.11.","materialen - wapening"]
["26.11.10.","materialen - wapening/staven en netten"]
["26.11.11.","materialen - wapening/staven en netten - staven ","FH","kg","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Gewicht (kg) in bij Settings van het Object",null,1]
["26.11.12.","materialen - wapening/staven en netten - netten ","FH","kg","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Gewicht (kg) in bij Settings van het Object",null,1]
["26.11.20.","materialen - wapening/vezels"]
["26.11.21.","materialen - wapening/vezels - staalvezels ","VH of FH","kg","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Gewicht (kg) in bij Settings van het Object",null,1]
["26.11.30.","materialen - wapening/voorspanstaal ","PM",null,"Geen",{"$nulls":4},1]
["26.12.","materialen - beton"]
["26.12.10.","materialen - beton/stortklaar beton"]
["26.12.11.","materialen - beton/stortklaar beton - met staaf- en netwapening ","PM",null,"Geen",{"$nulls":4},1]
["26.12.12.","materialen - beton/stortklaar beton - met vezelwapening ","PM",null,"Geen",{"$nulls":4},1]
["26.12.13.","materialen - beton/stortklaar beton - zichtbeton ","FH","m2","TYPE 3","Column",null,"Core surface",null,1]
[{"$nulls":4},"TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW Zichtbeton  ","Net Area",null,1]
[{"$nulls":4},"TYPE 4","Slab","Gebruik ARCHICAD Property: VMSW Zichtbeton  ","Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 4","Wall","Gebruik ARCHICAD Property: VMSW Zichtbeton  ","ARCHICAD Property: Oppervlakte middenas wand",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["26.12.20.","materialen - beton/geprefabriceerd beton ","PM",null,"Geen",{"$nulls":4},1]
["26.12.30.","materialen - beton/architectonisch beton ","PM",null,"Geen",{"$nulls":4},1]
["26.13.","materialen - bekistingen ","PM",null,"Geen",{"$nulls":4},1]
["26.14.","materialen - nabehandeling"]
["26.15.","materialen - chemische verankering ","FH of VH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM ",null,"Geen",{"$nulls":4},1]
["26.16.","materialen - thermische onderbreking ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,"PM ",null,"Geen",{"$nulls":4},1]
["26.20.","ter plaatse gestorte elementen - algemeen"]
["26.21.","ter plaatse gestorte elementen - wanden"]
["26.21.10.","ter plaatse gestorte elementen - wanden/traditionele bekisting ","FH","m3","TYPE 3","Wall",null,"Net Volume",null,1]
["26.21.20.","ter plaatse gestorte elementen - wanden/holle wanden"]
["26.21.21.","ter plaatse gestorte elementen - wanden/holle wanden - prefab elementen ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["26.21.22.","ter plaatse gestorte elementen - wanden/holle wanden - vulbeton ","FH","m3","TYPE 3","Wall",null,"Net Volume",null,1]
["26.22.","ter plaatse gestorte elementen - kolommen ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
["26.23.","ter plaatse gestorte elementen - balken ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["26.24.","ter plaatse gestorte elementen - balken met afwijkend bekistingsprofiel ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["26.25.","ter plaatse gestorte elementen - trappen en bordessen ","FH","trede","TYPE 5","Stair",null,"Totaal aantal treden",null,1]
["26.26.","ter plaatse gestorte elementen - draagvloeren"]
["26.26.10.","ter plaatse gestorte elementen - draagvloeren/traditionele bekisting ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.26.20.","ter plaatse gestorte elementen - draagvloeren/verloren bekisting ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.26.30.","ter plaatse gestorte elementen - draagvloeren/breedplaatvloeren"]
["26.26.31.","ter plaatse gestorte elementen - draagvloeren/breedplaatvloeren - prefab breedplaten ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.26.32.","ter plaatse gestorte elementen - draagvloeren/breedplaatvloeren - opstort ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.27.","ter plaatse gestorte elementen - uitkragende elementen"]
["26.27.10.","ter plaatse gestorte elementen - uitkragende elementen/balkons ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.27.20.","ter plaatse gestorte elementen - uitkragende elementen/galerijen ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.27.30.","ter plaatse gestorte elementen - uitkragende elementen/luifels ","FH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.27.40.","ter plaatse gestorte elementen - uitkragende elementen/kroonlijsten ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["26.30.","prefab elementen - algemeen"]
["26.31.","prefab elementen - wanden ","FH","m3","TYPE 3","Wall",null,"Net Volume",null,1]
["26.32.","prefab elementen - kolommen ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
["26.33.","prefab elementen - balken ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
["26.34.","prefab elementen - deur- en raamlateien ","PM",null,"Geen",{"$nulls":4},1]
["26.35.","prefab elementen - trappen en bordessen ","FH","st","TYPE 5","Stair",null,"Stuks",null,1]
["26.36.","prefab elementen - draagvloeren"]
["26.36.10.","prefab elementen - draagvloeren/welfsels"]
["26.36.11.","prefab elementen - draagvloeren/welfsels - zonder druklaag ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.12.","prefab elementen - draagvloeren/welfsels - met druklaag ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.20.","prefab elementen - draagvloeren/voorgespannen welfsels"]
["26.36.21.","prefab elementen - draagvloeren/voorgespannen welfsels - zonder druklaag ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.22.","prefab elementen - draagvloeren/voorgespannen welfsels - met druklaag ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.30.","prefab elementen - draagvloeren/cellenbeton ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.40.","prefab elementen - draagvloeren/balken en vulblokken"]
["26.36.41.","prefab elementen - draagvloeren/balken en vulblokken - vulblokken beton ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.42.","prefab elementen - draagvloeren/balken en vulblokken - vulblokken gebakken klei  ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.36.43.","prefab elementen - draagvloeren/balken en vulblokken - vulblokken EPS ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.37.","prefab elementen - uitkragende elementen"]
["26.37.10.","prefab elementen - uitkragende elementen/balkons ","FH","st","TYPE 3","Slab",null,"Stuks",null,1]
["26.37.20.","prefab elementen - uitkragende elementen/galerijen ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.37.30.","prefab elementen - uitkragende elementen/luifels ","FH","st","TYPE 3","Slab",null,"Stuks",null,1]
[null,null,null,"m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["26.37.40.","prefab elementen - uitkragende elementen/kroonlijsten ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["26.40.","betonrenovatie - algemeen"]
["26.41.","betonrenovatie - passivatie van vrijgemaakte wapeningsstaven ","VH","m","TYPE 4","Object","Gebruik ARCHICAD Property: VMSW betonrenovatie  ","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,null,"m","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW betonrenovatie  ","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["26.42.","betonrenovatie - vervangen van wapening ","VH","kg","TYPE 3","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
["26.43.","betonrenovatie - handmatig te plaatsen mortel"]
["26.43.10.","betonrenovatie - handmatig te plaatsen mortel/ gemodificeerde hydraulische mortel  ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings",null,1]
["26.43.20.","betonrenovatie - handmatig te plaatsen mortel/ harsgebonden mortel ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings",null,1]
["26.44.","betonrenovatie - gietmortel"]
["26.44.10.","betonrenovatie - gietmortel/ gemodificeerde hydraulische mortel ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings",null,1]
[null,null,null,"dm3","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Volume (dm3) in bij Settings van het Object",null,1]
["26.44.20.","betonrenovatie - gietmortel/ beton ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings",null,1]
[null,null,null,"dm3","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Volume (dm3) in bij Settings van het Object",null,1]
["26.45.","betonrenovatie - spuitbeton ","VH","dm2","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (dm2) in bij de Object Settings",null,1]
[null,null,null,"dm3","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Volume (dm3) in bij Settings van het Object",null,1]
["26.46.","betonrenovatie - injecteren van scheuren ","VH","m","TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Lengte (cm) in bij de Object settings",null,1]
["26.47.","betonrenovatie - coating ","FH of VH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[{"$nulls":4},"TYPE 5","Object","Meetstaat Manager 22 KM","Vul de waarde Oppervlakte (m2) in bij de Object Settings",null,1]
["27.","STRUCTUURELEMENTEN STAAL"]
["27.00.","structuurelementen staal - algemeen"]
["27.01.","algemeen - verbindingen ","PM",null,"Geen",{"$nulls":4},1]
["27.02.","algemeen - stabiliteitsstudie ","PM",null,"Geen",{"$nulls":4},1]
["27.10.","balken - algemeen"]
["27.11.","balken - blank profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.12.","balken - gemetalliseerd profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.13.","balken - thermisch verzinkt profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.14.","balken - thermisch verzinkt profielstaal met coating ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.15.","balken - roestvast profielstaal (RVS) ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.20.","lateien - algemeen"]
["27.21.","lateien - blank profielstaal ","PM",null,"Geen",{"$nulls":4},1]
["27.22.","lateien - gemetalliseerd profielstaal ","PM",null,"Geen",{"$nulls":4},1]
["27.23.","lateien - thermisch verzinkt profielstaal ","PM",null,"Geen",{"$nulls":4},1]
["27.24.","lateien - thermisch verzinkt profielstaal met coating ","PM",null,"Geen",{"$nulls":4},1]
["27.25.","lateien - roestvast profielstaal (RVS) ","PM",null,"Geen",{"$nulls":4},1]
["27.26.","lateien - regelbare consoles"]
["27.26.10.","lateien - regelbare consoles/zichtbaar"]
["27.26.11.","lateien - regelbare consoles/zichtbaar - gemetalliseerd ","PM",null,"Geen",{"$nulls":4},1]
["27.26.12.","lateien - regelbare consoles/zichtbaar - thermisch verzinkt ","PM",null,"Geen",{"$nulls":4},1]
["27.26.13.","lateien - regelbare consoles/zichtbaar - thermisch verzinkt + coating ","PM",null,"Geen",{"$nulls":4},1]
["27.26.14.","lateien - regelbare consoles/zichtbaar - roestvast staal (RVS) ","PM",null,"Geen",{"$nulls":4},1]
["27.26.20.","lateien - regelbare consoles/niet-zichtbaar"]
["27.26.21.","lateien - regelbare consoles/niet-zichtbaar - gemetalliseerd ","PM",null,"Geen",{"$nulls":4},1]
["27.26.22.","lateien - regelbare consoles/niet-zichtbaar - thermisch verzinkt ","PM",null,"Geen",{"$nulls":4},1]
["27.26.23.","lateien - regelbare consoles/niet-zichtbaar - roestvast staal (RVS) ","PM",null,"Geen",{"$nulls":4},1]
["27.30.","kolommen - algemeen"]
["27.31.","kolommen - blank profielstaal ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.32.","kolommen - gemetalliseerd profielstaal ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.33.","kolommen - thermisch verzinkt profielstaal ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.34.","kolommen - thermisch verzinkt profielstaal met coating ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.35.","kolommen - roestvast profielstaal (RVS) ","FH","kg","TYPE 5","Column",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
["27.40.","vlakke spanten - algemeen","FH"]
["27.41.","vlakke spanten - blank profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 5","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["27.42.","vlakke spanten - gemetalliseerd profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 5","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["27.43.","vlakke spanten - thermisch verzinkt profielstaal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 5","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["27.44.","vlakke spanten - thermisch verzinkt profielstaal met coating ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 5","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["27.50.","hulpstukken - algemeen"]
["27.51.","hulpstukken - oplegstukken"]
["27.51.10.","hulpstukken - oplegstukken/thermisch verzinkt ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.51.20.","hulpstukken - oplegstukken/roestvast staal (RVS) ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.52.","hulpstukken - spankabels ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"SOG"]
["27.53.","hulpstukken - geveldragers"]
["27.53.10.","hulpstukken - geveldragers/gemetalliseerd ","PM",null,"Geen",{"$nulls":4},1]
["27.53.20.","hulpstukken - geveldragers/thermisch verzinkt ","PM",null,"Geen",{"$nulls":4},1]
["27.53.30.","hulpstukken - geveldragers/roestvast staal ","PM",null,"Geen",{"$nulls":4},1]
["27.54.","hulpstukken - verhandelingsysteem liften"]
["27.60.","corrosiebescherming - algemeen"]
["27.61.","corrosiebescherming - metallisatie"]
["27.61.10.","corrosiebescherming - metallisatie/zonder bijkomende afwerkingslaag ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.61.20.","corrosiebescherming - metallisatie/metallisatie + natlak ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.61.30.","corrosiebescherming - metallisatie/metallisatie + poederlak ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.62.","corrosiebescherming - thermisch verzinken ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.63.","corrosiebescherming - duplexsysteem ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.64.","corrosiebescherming - roestwerende verfsystemen ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.70.","brandbeveiliging - algemeen"]
["27.71.","brandbeveiliging - brandwerend verfsysteem ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.72.","brandbeveiliging - spuitmortel ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["27.80.","renovatie stalen constructie-elementen - algemeen"]
["27.81.","renovatie stalen constructie-elementen - ontroesten ","FH","kg","TYPE 4","Beam","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Column","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 4","Object","Gebruik ARCHICAD Property: VMSW corrosiebescherming ","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["28.","HOUTSKELETBOUW"]
["28.00.","houtskeletbouw - algemeen"]
["28.01.","algemeen - stabiliteitsstudie ","PM",null,"Geen",{"$nulls":4},1]
["28.02.","algemeen - prestaties ","PM",null,"Geen",{"$nulls":4},1]
["28.10.","materialen - algemeen"]
["28.11.","materialen - onderdelen regelwerk"]
["28.11.10.","materialen - onderdelen regelwerk/stijlen"]
["28.11.11.","materialen - onderdelen regelwerk /stijlen - massief hout ","PM",null,"Geen",{"$nulls":4},1]
["28.11.12.","materialen - onderdelen regelwerk /stijlen - I-vormige stijlen ","PM",null,"Geen",{"$nulls":4},1]
["28.11.20.","materialen - onderdelen regelwerk/regels"]
["28.11.21.","materialen - onderdelen regelwerk /regels - onder- en bovenregels ","PM",null,"Geen",{"$nulls":4},1]
["28.11.22.","materialen - onderdelen regelwerk /regels - grondregels ","PM",null,"Geen",{"$nulls":4},1]
["28.11.23.","materialen - onderdelen regelwerk /regels - stelregels ","PM",null,"Geen",{"$nulls":4},1]
["28.11.24.","materialen - onderdelen regelwerk /regels - koppelregels ","PM",null,"Geen",{"$nulls":4},1]
["28.11.30.","materialen - onderdelen regelwerk/lateien ","PM",null,"Geen",{"$nulls":4},1]
["28.12.","materialen - beplating"]
["28.12.10.","materialen - beplating/houtachtige platen"]
["28.12.11.","materialen - beplating/houtachtige platen - OSB ","PM",null,"Geen",{"$nulls":4},1]
["28.12.12.","materialen - beplating/houtachtige platen - spaanplaat ","PM",null,"Geen",{"$nulls":4},1]
["28.12.13.","materialen - beplating/houtachtige platen - multiplex ","PM",null,"Geen",{"$nulls":4},1]
["28.12.14.","materialen - beplating/houtachtige platen - MDF ","PM",null,"Geen",{"$nulls":4},1]
["28.12.15.","materialen - beplating/houtachtige platen - LVL ","PM",null,"Geen",{"$nulls":4},1]
["28.12.16.","materialen - beplating/houtachtige platen - houtvezelisolatieplaat ","PM",null,"Geen",{"$nulls":4},1]
["28.12.17.","materialen - beplating/houtachtige platen - houtvezelcementplaat ","PM",null,"Geen",{"$nulls":4},1]
["28.12.20.","materialen - beplating/gipsachtige platen"]
["28.12.21.","materialen - beplating/gipsachtige platen - gipskartonplaten ","PM",null,"Geen",{"$nulls":4},1]
["28.12.22.","materialen - beplating/gipsachtige platen - gipsvezelplaten ","PM",null,"Geen",{"$nulls":4},1]
["28.12.30.","materialen - beplating/vezelcementplaten ","PM",null,"Geen",{"$nulls":4},1]
["28.12.40.","materialen - beplating/calciumsilicaatplaten ","PM",null,"Geen",{"$nulls":4},1]
["28.13.","materialen - isolatie"]
["28.13.10.","materialen - isolatie/minerale wol ","PM",null,"Geen",{"$nulls":4},1]
["28.13.20.","materialen - isolatie/cellulosevlokken ","PM",null,"Geen",{"$nulls":4},1]
["28.13.30.","materialen - isolatie/houtwol ","PM",null,"Geen",{"$nulls":4},1]
["28.14.","materialen - folies"]
["28.14.10.","materialen - folies/buitenfolies"]
["28.14.11.","materialen - folies/buitenfolies - wanden ","PM",null,"Geen",{"$nulls":4},1]
["28.14.12.","materialen - folies/buitenfolies - hellende daken ","PM",null,"Geen",{"$nulls":4},1]
["28.14.20.","materialen - folies/binnenfolies"]
["28.14.21.","materialen - folies/binnenfolies - wanden ","PM",null,"Geen",{"$nulls":4},1]
["28.14.22.","materialen - folies/binnenfolies - hellende daken ","PM",null,"Geen",{"$nulls":4},1]
["28.14.23.","materialen - folies/binnenfolies - platte daken ","PM",null,"Geen",{"$nulls":4},1]
["28.15.","materialen - regelstructuur voor binnenafwerking"]
["28.15.10.","materialen - regelstructuur voor binnenafwerking/hout ","PM",null,"Geen",{"$nulls":4},1]
["28.15.20.","materialen - regelstructuur voor binnenafwerking/metaal ","PM",null,"Geen",{"$nulls":4},1]
["28.16.","materialen - opleg- en bevestigingsmaterialen"]
["28.16.10.","materialen - opleg- en bevestigingsmaterialen/metalen schoenen ","PM",null,"Geen",{"$nulls":4},1]
["28.16.20.","materialen - opleg- en bevestigingsmaterialen/tie-downs ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["28.16.30.","materialen - opleg- en bevestigingsmaterialen/schroeven ","PM",null,"Geen",{"$nulls":4},1]
["28.16.40.","materialen - opleg- en bevestigingsmaterialen/nagels ","PM",null,"Geen",{"$nulls":4},1]
["28.16.50.","materialen - opleg- en bevestigingsmaterialen/nieten ","PM",null,"Geen",{"$nulls":4},1]
["28.16.60.","materialen - opleg- en bevestigingsmaterialen/lijmen ","PM",null,"Geen",{"$nulls":4},1]
["28.16.70.","materialen - opleg- en bevestigingsmaterialen/metalen hechtplaten ","PM",null,"Geen",{"$nulls":4},1]
["28.20.","structuurelementen - algemeen"]
["28.21.","structuurelementen - vloerbalken"]
["28.21.10.","structuurelementen - vloerbalken/massief hout ","PM",null,"Geen",{"$nulls":4},1]
["28.21.20.","structuurelementen - vloerbalken/LVL ","PM",null,"Geen",{"$nulls":4},1]
["28.21.30.","structuurelementen - vloerbalken/lichte samengestelde liggers ","PM",null,"Geen",{"$nulls":4},1]
["28.21.40.","structuurelementen - vloerbalken/gelijmd gelamineerd hout (GL) ","PM",null,"Geen",{"$nulls":4},1]
["28.22.","structuurelementen - balken"]
["28.22.10.","structuurelementen - balken/massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.22.20.","structuurelementen - balken/LVL ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.22.30.","structuurelementen - balken/lichte samengestelde liggers ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.22.40.","structuurelementen - balken/gelijmd gelamineerd hout (GL) ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.22.50.","structuurelementen - balken/staal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.23.","structuurelementen - lateien"]
["28.23.10.","structuurelementen - lateien/massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.23.20.","structuurelementen - lateien/LVL ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.23.30.","structuurelementen - lateien/gelijmd gelamineerd hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.23.40.","structuurelementen - lateien/staal ","FH","kg","TYPE 5","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
["28.24.","structuurelementen - kolommen"]
["28.24.10.","structuurelementen - kolommen/massief hout ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
["28.24.20.","structuurelementen - kolommen/LVL ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
["28.24.30.","structuurelementen - kolommen/gelijmd gelamineerd hout (GL) ","FH","m3","TYPE 3","Column",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
["28.24.40.","structuurelementen - kolommen/staal ","FH","kg","TYPE 3","Column",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
["28.25.","structuurelementen - onderdelen hellend dak"]
["28.25.10.","structuurelementen - onderdelen hellend dak/gordingen"]
["28.25.11.","structuurelementen - onderdelen hellend dak/gordingen - massief hout ","PM",null,"Geen",{"$nulls":4},1]
["28.25.12.","structuurelementen - onderdelen hellend dak/gordingen - gelamineerd hout ","PM",null,"Geen",{"$nulls":4},1]
["28.25.20.","structuurelementen - onderdelen hellend dak/keperwerk"]
["28.25.21.","structuurelementen - onderdelen hellend dak/keperwerk - massief hout ","PM",null,"Geen",{"$nulls":4},1]
["28.25.30.","structuurelementen - onderdelen hellend dak/spanten"]
["28.25.31.","structuurelementen - onderdelen hellend dak/spanten - massief hout"]
["28.25.40.","structuurelementen - onderdelen hellend dak/scharnierdak ","PM",null,"Geen",{"$nulls":4},1]
["28.25.50.","structuurelementen - onderdelen hellend dak/bakgootconstructies"]
["28.25.51.","structuurelementen - onderdelen hellend dak/bakgootconstructies - massief hout ","PM",null,"Geen",{"$nulls":4},1]
["28.25.60.","structuurelementen - onderdelen hellend dak/dakrandoversteken"]
["28.25.61.","structuurelementen - onderdelen hellend dak/dakrandoversteken - massief hout ","PM",null,"Geen",{"$nulls":4},1]
["28.25.70.","structuurelementen - onderdelen hellend dak/tengel- en panlatten ","PM",null,"Geen",{"$nulls":4},1]
["28.30.","wanden - algemeen"]
["28.31.","wanden - buitenwanden "]
["28.31.10.","wanden - buitenwanden/type I ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["28.31.20.","wanden - buitenwanden/type II ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["28.31.30.","wanden - buitenwanden/type III ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["28.32.","wanden - binnenwanden "]
["28.32.10.","wanden - binnenwanden/type I ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["28.32.20.","wanden - binnenwanden/type II ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["28.33.","wanden - woningscheidende wanden ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["28.34.","wanden - dakopstanden ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["28.40.","vloeren - algemeen"]
["28.41.","vloeren - roostering met beplating ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.42.","vloeren - geprefabriceerde houten vloeren"]
["28.42.10.","vloeren - geprefabriceerde houten vloeren/roostering met beplating ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.42.20.","vloeren - geprefabriceerde houten vloeren/kokervormige vloeren ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.42.30.","vloeren - geprefabriceerde houten vloeren/massieve houten vloeren ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.43.","vloeren - hout-betonvloeren ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.50.","hellende daken - algemeen"]
["28.51.","hellende daken - spanten ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Shell",null,null,null,1]
["28.52.","hellende daken - gordingen ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Shell",null,null,null,1]
["28.53.","hellende daken - scharnierdaken ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Shell",null,null,null,1]
["28.60.","platte daken - algemeen"]
["28.61.","platte daken - roostering met beplating ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.62.","platte daken - geprefabriceerde houten vloeren"]
["28.62.10.","platte daken - geprefabriceerde houten vloeren/roostering met beplating ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.62.20.","platte daken - geprefabriceerde houten vloeren/kokervormige vloeren ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.62.30.","platte daken - geprefabriceerde houten vloeren/massieve houten vloeren ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.63.","platte daken - hout-betonvloeren ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Slab",null,null,null,1]
["28.64.","platte daken - randisolatie ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Roof",null,"Omtrek ",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Omtrek ",null,1]
[]
[]
["30.","DAKOPBOUW HELLEND DAK"]
["30.00.","dakopbouw hellend dak - algemeen"]
["30.01.","dakopbouw hellend dak - stabiliteitsstudie ","PM",null,"Geen",{"$nulls":4},1]
["30.10.","houten dakstructuur - algemeen ","FH","m3","TYPE 3","Roof",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Net Volume",null,1]
[null,null,null,"st","TYPE 3","Roof",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Stuks",null,1]
[null,null,"PM"]
["30.11.","houten dakstructuur - muurplaten ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["30.12.","houten dakstructuur - gordingen"]
["30.12.10.","houten dakstructuur - gordingen/massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["30.12.20.","houten dakstructuur - gordingen/gelamineerd hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["30.13.","houten dakstructuur - keperwerk ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["30.14.","houten dakstructuur - keperspanten ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["30.15.","houten dakstructuur - prefabspanten ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
[{"$nulls":5},"Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["30.16.","houten dakstructuur - bakgootconstructies ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["30.17.","houten dakstructuur - dakrandoversteken ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["30.18.","houten dakstructuur - boordplanken"]
["30.18.10.","houten dakstructuur - boordplanken/massief hout ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["30.18.20.","houten dakstructuur - boordplanken/multiplex ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["30.20.","onderdak - algemeen"]
["30.21.","onderdak - soepele membranen ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
["30.22.","onderdak - platen"]
["30.22.10.","onderdak - platen/vezelcement ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["30.22.20.","onderdak - platen/houtvezelplaten ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["30.30.","tengel- & panlatten - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["31.","THERMISCHE ISOLATIE HELLEND DAK"]
["31.00.","thermische isolatie hellend dak - algemeen"]
["31.10.","isolatieplaten tussen dakstructuur - algemeen"]
["31.11.","isolatieplaten tussen dakstructuur - MW"]
["31.11.10.","isolatieplaten tussen dakstructuur - MW/18 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.11.20.","isolatieplaten tussen dakstructuur - MW/20 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.12.","isolatieplaten tussen dakstructuur - houtwol (WW)"]
["31.12.10.","isolatieplaten tussen dakstructuur - houtwol (WW)/18 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.12.20.","isolatieplaten tussen dakstructuur - houtwol (WW)/20 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.13.","isolatieplaten tussen dakstructuur - cellulose"]
["31.13.10.","isolatieplaten tussen dakstructuur - cellulose/18 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.13.20.","isolatieplaten tussen dakstructuur - cellulose/20 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.20.","isolatieplaten op dakstructuur (sarking) - algemeen"]
["31.21.","isolatieplaten op dakstructuur (sarking) - PUR of PIR"]
["31.21.10.","isolatieplaten op dakstructuur (sarking) - PUR of PIR/14 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.21.20.","isolatieplaten op dakstructuur (sarking) - PUR of PIR/16 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.22.","isolatieplaten op dakstructuur (sarking) - PF"]
["31.22.10.","isolatieplaten op dakstructuur (sarking) - PF/14 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.22.20.","isolatieplaten op dakstructuur (sarking) - PF/16 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.23.","isolatieplaten op dakstructuur (sarking) - XPS"]
["31.23.10.","isolatieplaten op dakstructuur (sarking) - XPS/14 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.23.20.","isolatieplaten op dakstructuur (sarking) - XPS/16 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.30.","ingeblazen isolatie - algemeen"]
["31.31.","ingeblazen isolatie - cellulose"]
["31.31.10.","ingeblazen isolatie - cellulose/18 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.31.20.","ingeblazen isolatie - cellulose/23 cm ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Shell",null,"Top Surface",null,1]
["31.40.","binnenfolie - algemeen"]
["31.41.","binnenfolie - damprem ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["31.42.","binnenfolie - dampscherm ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["31.50.","isolerende dakelementen - algemeen"]
["31.51.","isolerende dakelementen - tweeschalig ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["32.","DAKBEDEKKING HELLEND DAK"]
["32.00.","dakbedekking hellend dak - algemeen"]
["32.01.","dakbedekking hellend dak - prestaties"]
["32.10.","pannen - algemeen"]
["32.11.","pannen - gebakken aarde ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["32.11.10.","pannen - gebakken aarde/dakvlak ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["32.11.20.","pannen - gebakken aarde/vormstukken ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[]
["32.11.30.","pannen - gebakken aarde/toebehoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["32.12.","pannen - beton ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["32.12.10.","pannen - beton/dakvlak ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["32.12.20.","pannen - beton/vormstukken ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["32.12.30.","pannen - beton/toebehoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["32.13.","pannen - metaal ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
["32.13.10.","pannen - gecoat staal/dakvlak ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Shell",null,"Top Surface",null,1]
["32.13.20.","pannen - gecoat staal/vormstukken ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["32.13.30.","pannen - gecoat staal/toebehoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["32.20.","leien - algemeen"]
["32.21.","leien - vezelcement ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["32.22.","leien - natuurleien ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["32.30.","golfplaten - algemeen"]
["32.31.","golfplaten - vezelcement ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
["32.31.10.","golfplaten - vezelcement/dakvlakken ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
["32.31.20.","golfplaten - vezelcement/vormstukken ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["32.31.30.","golfplaten - vezelcement/toebehoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["32.40.","geprofileerde metaalplaten - algemeen"]
["32.41.","geprofileerde metaalplaten - gecoat staal ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["32.42.","geprofileerde metaalplaten - aluminium ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["32.43.","geprofileerde metaalplaten - RVS ","FH","m2","TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
["32.50.","toebehoren hellend dak - algemeen"]
["32.51.","toebehoren hellend dak - dakdoorvoeren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["32.52.","toebehoren hellend dak - verankeringssystemen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["32.53.","toebehoren hellend dak - valbeveiliging"]
["32.53.10.","toebehoren hellend dak - valbeveiliging / ankerpunten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["32.53.20.","toebehoren hellend dak - valbeveiliging / lijnsysteem ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["32.54.","toebehoren hellend dak - ladderhaken ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["33.","DAKVLOER PLAT DAK"]
["33.00.","dakvloer plat dak - algemeen"]
["33.01.","algemeen - stabiliteitsstudie"]
["33.10.","houten roostering - algemeen"]
["33.11.","houten roostering - muurplaten ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
["33.12.","houten roostering - balken"]
["33.12.10.","houten roostering - balken/massief hout ","FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
["33.12.20.",null,"FH","m3","TYPE 3","Beam",null,"Net Volume",null,1]
[null,0,"FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"m3","TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["33.12.30.","houten roostering - balken/lichte samengestelde liggers ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"m3","TYPE 3","Beam",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Volume","Enkel mogelijk bij horizontale of verticale plaatsing",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["33.20.","beplating op houten roostering - algemeen",null,null,"TYPE 5",{"$nulls":4},1]
["33.21.","beplating op houten roostering - multiplex ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.22.","beplating op houten roostering - OSB ","FH","m2","TYPE 2","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Roof",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.23.","beplating op houten roostering - spaanplaat ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.24.","beplating op houten roostering - cementgebonden spaanplaat ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.30.","zelfdragende elementen - algemeen"]
["33.31.","zelfdragende elementen - profielplaten staal"]
["33.31.10.","zelfdragende elementen - profielplaten staal/enkelvoudig ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.32.","zelfdragende elementen - sandwichplaten hout ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.40.","hellingsbeton - algemeen"]
["33.41.","hellingsbeton - niet isolerend"]
["33.41.10.","hellingsbeton - niet isolerend/mager beton ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.41.20.","hellingsbeton - niet isolerend/zandcement dekvloer ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.52.","hellingsbeton - licht isolerend"]
["33.52.10.","hellingsbeton - licht isolerend/granulaten ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["33.52.20.","hellingsbeton - licht isolerend/schuimbeton ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.","THERMISCHE ISOLATIE PLAT DAK"]
["34.00.","thermische isolatie plat dak - algemeen"]
["34.10.","isolatieplaten plat dak - algemeen"]
["34.11.","isolatieplaten plat dak - MW"]
["34.11.10.","isolatieplaten plat dak - MW/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.11.20.","isolatieplaten plat dak - MW/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.12.","isolatieplaten plat dak - PUR of PIR"]
["34.12.10.","isolatieplaten plat dak - PUR of PIR/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.12.20.","isolatieplaten plat dak - PUR of PIR/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.13.","isolatieplaten plat dak - EPS"]
["34.13.10.","isolatieplaten plat dak - EPS/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.13.20.","isolatieplaten plat dak - EPS/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.14.","isolatieplaten plat dak - CG"]
["34.14.10.","isolatieplaten plat dak - CG/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.14.20.","isolatieplaten plat dak - CG/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.15.","isolatieplaten omkeerdak - XPS"]
["34.15.10.","isolatieplaten omkeerdak - XPS/14 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.15.20.","isolatieplaten omkeerdak - XPS/16 cm ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["34.20.","dampscherm - algemeen"]
["34.21.","dampscherm - gewapend bitumen ","PM",null,"Geen",{"$nulls":4},1]
["35.","AFDICHTING & AFWERKING PLAT DAK"]
["35.00.","afdichting & afwerking plat dak - algemeen"]
["35.01.","afdichting & afwerking plat dak - waterdichtheidsproeven ","PM",null,"Geen",{"$nulls":4},1]
["35.02.","afdichting & afwerking plat dak - waarborgen & attesten ","PM",null,"Geen",{"$nulls":4},1]
["35.03.","afdichting & afwerking plat dak - renovatie bestaande daken ","PM",null,"Geen",{"$nulls":4},1]
["35.10.","bitumineuze dakafdichting - algemeen"]
["35.11.","bitumineuze dakafdichting - SBS"]
["35.11.10.","bitumineuze dakafdichting - SBS/losliggend (L) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.11.20.","bitumineuze dakafdichting - SBS/deelgekleefd (P) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.11.30.","bitumineuze dakafdichting - SBS/volgekleefd (T) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.11.40.","bitumineuze dakafdichting - SBS/mechanisch (M) ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.12.","bitumineuze dakafdichting - APP","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
["35.12.10.","bitumineuze dakafdichting - APP/losliggend (L) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.12.20.","bitumineuze dakafdichting - APP/deelgekleefd (P) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.12.30.","bitumineuze dakafdichting - APP/volgekleefd (T) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.12.40.","bitumineuze dakafdichting - APP/mechanisch (M) ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.13.","bitumineuze dakafdichting - PBE"]
["35.20.","kunststof dakafdichting - algemeen"]
["35.21.","kunststof dakafdichting - EPDM"]
["35.21.10.","kunststof dakafdichting - EPDM/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.21.20.","kunststof dakafdichting - EPDM/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.21.30.","kunststof dakafdichting - EPDM/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.22.","kunststof dakafdichting - TPO"]
["35.22.10.","kunststof dakafdichting - TPO/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.22.20.","kunststof dakafdichting - TPO/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.22.30.","kunststof dakafdichting - TPO/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.23.","kunststof dakafdichting - PVC"]
["35.23.10.","kunststof dakafdichting - PVC/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.23.20.","kunststof dakafdichting - PVC/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.23.30.","kunststof dakafdichting - PVC/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.24.","kunststof dakafdichting - CPE"]
["35.24.10.","kunststof dakafdichting - CPE/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.24.20.","kunststof dakafdichting - CPE/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.24.30.","kunststof dakafdichting - CPE/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.25.","kunststof dakafdichting - PIB"]
["35.25.10.","kunststof dakafdichting - PIB/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.25.20.","kunststof dakafdichting - PIB/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.25.30.","kunststof dakafdichting - PIB/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.26.","kunststof dakafdichting - ECB"]
["35.26.10.","kunststof dakafdichting - ECB/losliggend ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.26.20.","kunststof dakafdichting - ECB/gekleefd ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.26.30.","kunststof dakafdichting - ECB/mechanisch ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.30.","ballastlaag - algemeen"]
["35.31.","ballastlaag - grind ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.32.","ballastlaag - tegels ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.33.","ballastlaag - geotextiel ","PM",null,"Geen",{"$nulls":4},1]
["35.40.","groendak - algemeen"]
["35.41.","groendak - extensief ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.42.","groendak - intensief ","FH","m2","TYPE 2","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["35.50.","toebehoren plat dak - algemeen"]
["35.51.","toebehoren plat dak - dakdoorvoeren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["35.52.","toebehoren plat dak - verankeringssystemen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["35.53.","toebehoren plat dak - valbeveiliging"]
["35.53.10.","toebehoren plat dak - valbeveiliging/doodgewicht ankers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["35.53.20.","toebehoren plat dak - valbeveiliging/vaste ankerpunten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["35.53.30.","toebehoren plat dak - valbeveiliging/lijnsysteem ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,null,"m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["36.","DAKLICHTOPENINGEN"]
["36.00.","daklichtopeningen - algemeen"]
["36.10.","dakvlakramen - algemeen"]
["36.11.","dakvlakramen - hout"]
["36.11.10.","dakvlakramen - hout/wentel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.11.20.","dakvlakramen - hout/uitzet en wentel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.11.30.","dakvlakramen - hout/uitzet ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.11.40.","dakvlakramen - hout/rook- & warmteafvoer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.12.","dakvlakramen - kunststof"]
["36.12.10.","dakvlakramen - kunststof/wentel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.12.20.","dakvlakramen - kunststof/uitzet-wentel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.12.30.","dakvlakramen - kunststof/uitzet ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.12.40.","dakvlakramen - kunststof/rook- en warmteafvoer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.13.","dakvlakramen - zolderraam ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.20.","platdakramen - algemeen"]
["36.21.","platdakramen - kunststof"]
["36.21.10.","platdakramen - kunststof/vast ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.21.20.","platdakramen - kunststof/opengaand ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.21.30.","platdakramen - kunststof/rook- en warmteafvoer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.30.","koepels - algemeen"]
["36.31.","koepels - kunststof acrylaat (PMMA)"]
["36.31.10.","koepels - kunststof acrylaat (PMMA)/vast ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.31.20.","koepels - kunststof acrylaat (PMMA)/opengaand ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.31.30.","koepels - kunststof acrylaat (PMMA)/rook en warmteafvoer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.32.","koepels - kunststof polycarbonaat (PC) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Stuks",null,1]
["36.40.","daglichtreflectiebuizen - algemeen"]
["36.41.","daglichtreflectiebuizen - plat dak ","FH","m2","TYPE 5","Object",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Net Area",null,1]
["36.42.","daglichtreflectiebuizen - hellend dak ","FH","m2","TYPE 5","Object",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Skylight",null,"Net Area",null,1]
["36.50.","lichtstraten - algemeen"]
["36.51.","lichtstraten - profielen hout"]
["36.51.10.","lichtstraten - profielen hout/met beglazing ","FH","m2","TYPE 3","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Area",null,1]
[{"$nulls":5},"Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Skylight",null,"Net Area",null,1]
["36.52.","lichtstraten - profielen aluminium"]
["36.52.10.","lichtstraten - profielen aluminium met beglazing ","FH","m2","TYPE 3","Roof",null,null,null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Area",null,1]
[{"$nulls":5},"Roof",null,"Top Surface",null,1]
[{"$nulls":5},"Skylight",null,"Net Area",null,1]
["36.60.","dakkapellen - algemeen"]
["36.61.","dakkapellen - traditioneel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["37.","DAKRANDEN EN KROONLIJSTEN"]
["37.00.","dakranden en kroonlijsten - algemeen"]
["37.10.","slabben, loketten en aansluitbanden - algemeen"]
["37.11.","slabben, loketten en aansluitbanden - metaal"]
["37.11.10.","slabben, loketten en aansluitbanden - metaal/lood ","FH of VH","kg","TYPE 3","Beam",null,"ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,null,"kg","TYPE 5","Object","Meetstaat Manager 22 KM","Vul Gewicht (kg) in bij Settings van het Object",null,1]
["37.11.20.","slabben, loketten en aansluitbanden - metaal/aluminium ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.11.30.","slabben, loketten en aansluitbanden - metaal/zink ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.11.40.","slabben, loketten en aansluitbanden - metaal/koper ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.12.","slabben, loketten en aansluitbanden - membranen"]
["37.12.10.","slabben, loketten en aansluitbanden - membraan/EPDM ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.12.20.","slabben, loketten en aansluitbanden - membraan/PIB ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.12.30.","slabben, loketten en aansluitbanden - membraan/bitumen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.20.","dakrandprofielen - algemeen"]
["37.21.","dakrandprofielen - metaal"]
["37.21.10.","dakrandprofielen - metaal/zink ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.21.20.","dakrandprofielen - metaal/aluminium ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.21.30.","dakrandprofielen - metaal/metaalfolieplaten ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.22.","dakrandprofielen - kunststof"]
["37.22.10.","dakrandprofielen - kunststof/polyester ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["37.30.","muurkappen - algemeen","FH","m","TYPE 3","Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
["37.31.","muurkappen - metaal"]
["37.31.10.","muurkappen - metaal/zink ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
["37.31.20.","muurkappen - metaal/aluminium ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
["37.32.","muurkappen - kunststof ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"ARCHICAD Property: Omtrek vloer zonder openingen",null,1]
["37.40.","uitbekleding kroonlijsten en luifels - algemeen"]
["37.41.","uitbekleding kroonlijsten en luifels - planchetten"]
["37.41.10.","uitbekleding kroonlijsten en luifels - planchetten/massief hout ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["37.41.20.","uitbekleding kroonlijsten en luifels - planchetten/kunststof ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.41.30.","uitbekleding kroonlijsten en luifels - planchetten/vezelcement ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.42.","uitbekleding kroonlijsten en luifels - platen"]
["37.42.10.","uitbekleding kroonlijsten en luifels - platen/multiplex ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.42.20.","uitbekleding kroonlijsten en luifels - platen/kunststof ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.42.30.","uitbekleding kroonlijsten en luifels - platen/vezelcement ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.42.40.","uitbekleding kroonlijsten en luifels - platen/kunsthars ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.42.50.","uitbekleding kroonlijsten en luifels - platen/minerale vezels ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.43.","uitbekleding kroonlijsten en luifels - leien"]
["37.43.10.","uitbekleding kroonlijsten en luifels - leien/vezelcement ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.43.20.","uitbekleding kroonlijsten en luifels - leien hout ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["37.50.","toebehoren dakranden - algemeen"]
["37.51.","toebehoren dakranden - valbeveiliging"]
["37.51.10.","toebehoren dakranden - valbeveiliging/lijn- of railsysteem ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["37.51.20.","toebehoren dakranden - valbeveiliging/permanente leuning ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["37.52.","toebehoren dakranden - gevelonderhoudsinstallaties"]
["37.52.10.","toebehoren dakranden - gevelonderhoud/railsysteem ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["37.53.","toebehoren dakranden - verhuisbalk ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
["38.","DAKWATERAFVOER"]
["38.00.","dakwaterafvoer - algemeen"]
["38.10.","bakgootdichtingen - algemeen"]
["38.11.","bakgootdichtingen - metaalbladen"]
["38.11.10.","bakgootdichtingen - metaalbladen/zink ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.11.20.","bakgootdichtingen - metaalbladen/koper ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.12.","bakgootdichtingen - bitumen"]
["38.12.10.","bakgootdichtingen - bitumen/SBS ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.12.20.","bakgootdichtingen - bitumen/APP ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.13.","bakgootdichtingen - hoog polymeermembranen"]
["38.13.10.","bakgootdichtingen - hoog polymeermembranen/EPDM ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.13.20.","bakgootdichtingen - hoog polymeermembranen/TPO ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.13.30.","bakgootdichtingen - hoog polymeermembranen/PVC ","FH","m2","TYPE 3","Beam","complex profile","Component Area",null,1]
["38.20.","hanggoten - algemeen"]
["38.21.","hanggoten - kunststof"]
["38.21.10.","hanggoten - kunststof/PVC ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.21.20.","hanggoten - kunststof/polyesterhars ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.22.","hanggoten - metaal"]
["38.22.10.","hanggoten - metaal/zink ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.22.20.","hanggoten - metaal/aluminium ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.22.30.","hanggoten - metaal/koper ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.22.40.","hanggoten - metaal/gecoat staal ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.22.50.","hanggoten - metaal/roestvast staal ","FH","m","TYPE 3","Beam","complex profile","ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.30.","afvoerpijpen - algemeen"]
["38.31.","afvoerpijpen - kunststof"]
["38.31.10.","afvoerpijpen - kunststof/PVC ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.31.20.","afvoerpijpen - kunststof/HDPE ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.32.","afvoerpijpen - metaal","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.32.10.","afvoerpijpen - metaal/zink ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.32.20.","afvoerpijpen - metaal/koper ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.32.30.","afvoerpijpen - metaal/aluminium ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.32.40.","afvoerpijpen - metaal/gecoat staal ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.32.50.","afvoerpijpen - metaal/roestvast staal ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["38.40.","eindstukken - algemeen","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["38.41.","eindstukken - slagvast kunststof ","FH","st","TYPE 5","Object",null,"Stuks",null,2]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["38.42.","eindstukken - behandeld gietijzer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["38.43.","eindstukken - gegoten aluminium ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["38.50.","toebehoren - algemeen",null,null,"Geen",{"$nulls":4},1]
["38.51.","toebehoren - dakkolken en tapbuizen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["38.52.","toebehoren - draad- en bolroosters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["38.53.","toebehoren - balkonafvoerputjes ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["38.54.","toebehoren - noodspuwers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[]
["40.","BUITENSCHRIJNWERK"]
["40.00.","buitenschrijnwerk - algemeen"]
["40.01.","buitenschrijnwerk - prestaties"]
["40.02.","buitenschrijnwerk - proeven"]
["40.02.10.","buitenschrijnwerk - proeven/op kosten ongelijk ","PM",null,"Geen",{"$nulls":4},1]
["40.02.20.","buitenschrijnwerk - proeven/op kosten aannemer ","VH","st","TYPE 5","Object",null,"Stuks",null,1]
["40.03.","buitenschrijnwerk - montage"]
["40.03.10.","buitenschrijnwerk - montage/spouwconstructie en dorpel ","PM",null,"Geen",{"$nulls":4},1]
["40.03.20.","buitenschrijnwerk - montage/buitengevelisolatiesysteem ","PM",null,"Geen",{"$nulls":4},1]
["40.03.30.","buitenschrijnwerk - montage/gevelbekledingsysteem ","PM",null,"Geen",{"$nulls":4},1]
["40.03.40.","buitenschrijnwerk - montage/houtskeletbouw ","PM",null,"Geen",{"$nulls":4},1]
["40.03.50.","buitenschrijnwerk - montage/vervanging schrijnwerk ","PM",null,"Geen",{"$nulls":4},1]
["40.04.","buitenschrijnwerk - borderel"]
["40.10.","profielsystemen - algemeen"]
["40.11.","profielsysteem - hout"]
["40.11.10.","profielsysteem - hout/vaste ramen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.11.20.","profielsysteem - hout/draairamen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.11.30.","profielsysteem - hout/schuiframen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,null,"m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
["40.11.40.","profielsysteem - hout/buitendeuren ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.12.","profielsysteem - aluminium"]
["40.12.10.","profielsysteem - aluminium/vaste ramen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.12.20.","profielsysteem - aluminium/draairamen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.12.30.","profielsysteem - aluminium/schuiframen ","FH of PM","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,null,"m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
["40.12.40.","profielsysteem - aluminium/buitendeuren ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
["40.13.","profielsysteem - pvc"]
["40.13.10.","profielsysteem - pvc/vaste ramen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.13.20.","profielsysteem - pvc/draairamen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
[null,null,null,"m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
["40.13.30.","profielsysteem - pvc/schuiframen ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.13.40.","profielsysteem - pvc/buitendeuren ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
["40.14.","profielsysteem - staal"]
["40.14.10.","profielsysteem - staal/vaste ramen ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.14.20.","profielsysteem - staal/buitendeuren ","FH","m2","TYPE 5","Door",null,"W/D opening nominal surface area",null,1]
[]
["40.20.","hang- en sluitwerk - algemeen"]
["40.21.","hang- en sluitwerk - standaard beslag ","PM",null,"Geen",{"$nulls":4},1]
["40.22.","hang- en sluitwerk - scharnieren en paumellen ","PM",null,"Geen",{"$nulls":4},1]
["40.23.","hang- en sluitwerk - sloten ","PM",null,"Geen",{"$nulls":4},1]
["40.23.10.","hang- en sluitwerk - sloten/manueel ","PM",null,"Geen",{"$nulls":4},1]
["40.23.20.","hang- en sluitwerk - sloten/elektromagnetisch ","PM",null,"Geen",{"$nulls":4},1]
["40.23.30.","hang- en sluitwerk - sloten/schuifdeurslot ","PM",null,"Geen",{"$nulls":4},1]
["40.23.40.","hang- en sluitwerk - sloten/glasdeurslot ","PM",null,"Geen",{"$nulls":4},1]
["40.23.50.","hang- en sluitwerk - sloten/sleutelplan ","PM",null,"Geen",{"$nulls":4},1]
["40.24.","hang- en sluitwerk - deurdrangers ","PM",null,"Geen",{"$nulls":4},1]
["40.24.10.","hang- en sluitwerk - deurdrangers/manueel ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurdranger","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.24.20.","hang- en sluitwerk - deurdrangers/gemotoriseerd ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurdranger","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.25.","hang- en sluitwerk - panieksluitingen ","PM",null,"Geen",{"$nulls":4},1]
["40.26.","hang- en sluitwerk - raamkrukken ","PM",null,"Geen",{"$nulls":4},1]
["40.27.","hang- en sluitwerk - deurkrukken ","PM",null,"Geen",{"$nulls":4},1]
["40.28.","hang- en sluitwerk - vaste handgrepen ","PM",null,"Geen",{"$nulls":4},1]
["40.29.","hang- en sluitwerk - toebehoren"]
["40.30.","ventilatieroosters - algemeen"]
["40.31.","ventilatieroosters - op glas"]
["40.31.10.","ventilatieroosters - op glas/kleprooster ","PM",null,"Geen",{"$nulls":4},1]
["40.32.","ventilatieroosters - op profiel"]
["40.32.10.","ventilatieroosters - op profiel/kleprooster ","PM",null,"Geen",{"$nulls":4},1]
["40.40","beglazing - algemeen"]
["40.40.10.","beglazing - prestaties"]
["40.41.","beglazing - enkel glas"]
["40.41.10.","beglazing - enkel glas/type 1 ","PM",null,"Geen",{"$nulls":4},1]
["40.42.","beglazing - dubbele beglazing"]
["40.42.10.","beglazing - dubbele beglazing/type 1 ","PM",null,"Geen",{"$nulls":4},1]
["40.42.20.","beglazing - dubbele beglazing/type 2 ","PM",null,"Geen",{"$nulls":4},1]
["40.43.","beglazing - drievoudige beglazing"]
["40.43.10.","beglazing - drievoudige beglazing/type 1 ","PM",null,"Geen",{"$nulls":4},1]
["40.43.20.","beglazing - driedubbele beglazing/type 2 ","PM",null,"Geen",{"$nulls":4},1]
["40.44.","beglazing - bijzondere beglazing"]
["40.44.10.","beglazing - bijzondere beglazing/dun monumentenglas ","PM",null,"Geen",{"$nulls":4},1]
["40.50.","vulelementen - algemeen"]
["40.51.","vulelementen - kunststof ","PM",null,"Geen",{"$nulls":4},1]
["40.52.","vulelementen - aluminium ","PM",null,"Geen",{"$nulls":4},1]
["40.53.","vulelementen - kunsthars ","PM",null,"Geen",{"$nulls":4},1]
["40.54.","vulelementen - vezelcement ","PM",null,"Geen",{"$nulls":4},1]
["40.55.","vulelementen - multiplexplaten  ","PM",null,"Geen",{"$nulls":4},1]
["40.56.","vulelementen - massief houten beplanking ","PM",null,"Geen",{"$nulls":4},1]
["40.60.","raamdorpels - algemeen"]
["40.70.","omkaderingselementen - algemeen"]
["40.71.","omkaderingselementen - hout ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten","Lengte omkaderingselement",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.72.","omkaderingselementen - aluminium ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten","omtrek dagkant uitgezonderd lengte dorpel",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten","Lengte omkaderingselement",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.80.","toebehoren - algemeen"]
["40.81.","toebehoren - brievenkleppen ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.82.","toebehoren - deurspionnen ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.83.","toebehoren - beschermplaten ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.84.","toebehoren - deurstoppen ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.85.","toebehoren - huisnummers ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.86.","toebehoren - deur- en naambordjes ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW toebehoren buitenschrijnwerk","Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.87.","toebehoren - doorvalbeveiliging"]
["40.87.10.","toebehoren - doorvalbeveiliging/kokerprofiel ","FH","m ","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["40.87.20.","toebehoren - doorvalbeveiliging/glasplaat ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["41.","POORTEN & EXTERNE ZONWERING"]
["41.00.","poorten & externe zonwering - algemeen"]
["41.10.","kantelpoorten - algemeen"]
["41.11.","kantelpoorten - poortblad staal"]
["41.11.10.","kantelpoorten - poortblad staal/manueel ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.11.20.","kantelpoorten - poortblad staal/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.12.","kantelpoorten - poortblad hout"]
["41.12.10.","kantelpoorten - poortblad hout/manueel ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.12.20.","kantelpoorten - poortblad hout/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.13.","kantelpoorten - poortblad kunststof"]
["41.13.10.","kantelpoorten - poortblad kunststof/manueel ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.13.20.","kantelpoorten - poortblad kunststof/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.20.","sectionaalpoorten - algemeen"]
["41.21.","sectionaalpoorten - staal"]
["41.21.10.","sectionaalpoorten - staal/manueel ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.21.20.","sectionaalpoorten - staal/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.22.","sectionaalpoorten - aluminium"]
["41.22.10.","sectionaalpoorten - aluminium/manueel ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.22.20.","sectionaalpoorten - aluminium/aangedreven ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["41.30.","Externe zonnewering - algemeen",{"$nulls":6},"Uitbreiding op de basis VMSW artikellijst"]
["41.31.","Externe zonnewering - rolluiken","FH","m2","TYPE 4","Window","ARCHICAD property: VMSW zonnewering","W/D Opening Surface on the Reveal Side","Uitbreiding op de basis VMSW artikellijst",1]
["41.32.","Externe zonnewering - screens","FH","m2","TYPE 4","Window","ARCHICAD property: VMSW zonnewering","W/D Opening Surface on the Reveal Side","Uitbreiding op de basis VMSW artikellijst",1]
["42.","GEVELBEKLEDINGEN"]
["42.00.","gevelbekledingen - algemeen"]
["42.10.","regelstructuur - algemeen"]
["42.11.","regelstructuur - hout ","PM",null,"Geen",{"$nulls":4},1]
["42.12.","regelstructuur - aluminium ","PM",null,"Geen",{"$nulls":4},1]
["42.20.","thermische isolatie voorhanggevel - algemeen"]
["42.21.","thermische isolatie voorhanggevel - MW"]
["42.21.10.","thermische isolatie voorhanggevel - MW/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.21.20.","thermische isolatie voorhanggevel - MW/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.22.","thermische isolatie voorhanggevel - PUR of PIR"]
["42.22.10.","thermische isolatie voorhanggevel - PUR of PIR/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.22.20.","thermische isolatie voorhanggevel - PUR of PIR/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.23.","thermische isolatie voorhanggevel - PF"]
["42.23.10.","thermische isolatie voorhanggevel - PF/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.23.20.","thermische isolatie voorhanggevel - PF/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.24.","thermische isolatie voorhanggevel - EPS"]
["42.24.10.","thermische isolatie voorhanggevel - EPS/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.24.20.","thermische isolatie voorhanggevel - EPS/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.25.","thermische isolatie voorhanggevel - XPS"]
["42.25.10.","thermische isolatie voorhanggevel - XPS/14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.25.20.","thermische isolatie voorhanggevel - XPS/16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["42.30.","buitenfolie - algemeen"]
["42.31.","buitenfolie - gevelfolie ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["42.40.","bekledingspanelen - algemeen"]
["42.41.","bekledingspanelen - HPL ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["42.42.","bekledingspanelen - vezelcement ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["42.43.","bekledingspanelen - minerale vezels ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["42.50.","bekledingsplanchetten - algemeen"]
["42.51.","bekledingsplanchetten - massief hout ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["42.52.","bekledingsplanchetten - kunststof ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["42.53.","bekledingsplanchetten - vezelcement ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["42.60.","gevelleien - algemeen"]
["42.61.","gevelleien - vezelcementleien ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["42.70.","geprofileerde metaalplaten - algemeen"]
["42.71.","geprofileerde metaalplaten - gecoat staal ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["42.72.","geprofileerde metaalplaten - aluminium ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["43.","BUITENBEPLEISTERING"]
["43.00.","buitenbepleistering - algemeen"]
["43.10.","sierpleisters op metselwerk - algemeen"]
["43.11.","sierpleisters op metselwerk - minerale pleister ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
["43.20.","buitengevelisolatiesystemen met pleister - algemeen"]
["43.21.","buitengevelisolatiesystemen met pleister - EPS"]
["43.21.10.","buitengevelisolatiesystemen met pleister - EPS/isolatie"]
["43.21.11.","buitengevelisolatiesystemen met pleister - EPS/isolatie - 14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["43.21.12.","buitengevelisolatiesystemen met pleister - EPS/isolatie - 16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["43.21.20.","buitengevelisolatiesystemen met pleister - EPS/pleister ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["43.22.","buitengevelisolatiesystemen met pleister - MW"]
["43.22.10.","buitengevelisolatiesystemen met pleister - MW/isolatie"]
["43.22.11.","buitengevelisolatiesystemen met pleister - MW/isolatie - 14 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["43.22.12.","buitengevelisolatiesystemen met pleister - MW/isolatie - 16 cm ","FH","m2","TYPE 2","Wall",null,"Projected Area",null,1]
["43.22.20.","buitengevelisolatiesystemen met pleister - MW/pleister ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD Property: VMSW gevelbekleding dagkant ramen/deuren","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["44.","BUITENTRAPPEN & BORSTWERINGEN"]
["44.00.","buitentrappen en borstweringen - algemeen"]
["44.10.","trappen - algemeen"]
["44.11.","trappen - staal ","FH","st","TYPE 5","Stair",null,"Stuks",null,1]
[null,null,"SOG"]
["44.20.","borstweringen - algemeen"]
["44.21.","borstweringen - staal ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
[null,null,null,"st","TYPE 5","Railing",null,"Stuks",null,1]
["44.22.","borstweringen - roestvast staal (RVS) ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["44.23.","borstweringen - aluminium ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["44.24.","borstweringen - veiligheidsglas ","FH","m","TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["44.30.","trapleuningen - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["44.40.","vulpanelen en -roosters - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["44.50.","handgrepen - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["44.60.","brandladders - algemeen"]
["44.61.","brandladders - verzinkt staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Stair",null,"Stuks",null,1]
["44.62.","brandladders - aluminium ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Stair",null,"Stuks",null,1]
[]
["50.","BINNENPLEISTERWERKEN"]
["50.00.","binnenpleisterwerken - algemeen"]
["50.10.","wandbepleistering - algemeen"]
["50.11.","wandbepleistering - gipspleisters"]
["50.11.10.","wandbepleistering - gipspleisters/dikpleister op metselwerk"]
["50.11.11.","wandbepleistering - gipspleisters/dikpleisters op metselwerk - wandvlakken ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,null,"m2","TYPE 5","Object","Interieurafwerking ","Hoeveelheid onder negge/dagkant",null,1]
["50.11.12.","wandbepleistering - gipspleisters/dikpleisters op metselwerk - dagkanten ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m","TYPE 4","Object","Interieurafwerking - Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","Hoeveelheid onder negge/dagkant",null,1]
["50.11.20.","wandbepleistering - gipspleisters/dunpleister op lijmblokken"]
["50.11.21.","wandbepleistering - gipspleisters/dunpleister op lijmblokken - wandvlakken ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,null,"m2","TYPE 5","Object","Interieurafwerking ","Hoeveelheid onder negge/dagkant",null,1]
["50.11.22.","wandbepleistering - gipspleisters/dunpleister op lijmblokken - dagkanten ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m","TYPE 4","Object","Interieurafwerking - Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","Hoeveelheid onder negge/dagkant",null,1]
["50.11.30.","wandbepleistering - gipspleisters/pleister op beplating"]
["50.11.31.","wandbepleistering - gipspleisters/pleister op beplating - wandvlakken ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,null,"m2","TYPE 5","Object","Interieurafwerking ","Hoeveelheid onder negge/dagkant",null,1]
["50.11.32.","wandbepleistering - gipspleisters/pleister op beplating - dagkanten ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m","TYPE 4","Object","Interieurafwerking - Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","Hoeveelheid onder negge/dagkant",null,1]
["50.11.40.","wandbepleistering - gipspleisters/pleister op gaas"]
["50.11.41.","wandbepleistering - gipspleisters/pleister op gaas - wandvlakken ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,null,"m2","TYPE 5","Object","Interieurafwerking ","Hoeveelheid onder negge/dagkant",null,1]
["50.11.42.","wandbepleistering - gipspleisters/pleister op gaas - dagkanten ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m","TYPE 4","Object","Interieurafwerking - Gebruik ARCHICAD property: VMSW wandbepleistering dagkanten","Hoeveelheid onder negge/dagkant",null,1]
["50.12.","wandbepleistering - cementpleisters"]
["50.12.10.","wandbepleistering - cementpleisters/te betegelen ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,null,"m2","TYPE 5","Object","Interieurafwerking ","Hoeveelheid onder negge/dagkant",null,1]
["50.12.20.","wandbepleistering - cementpleisters/afwerksysteem ","FH","m2","TYPE 3","Wall",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[null,null,null,"m2","TYPE 5","Object","Interieurafwerking ","Hoeveelheid onder negge/dagkant",null,1]
["50.20.","plafondbepleistering - algemeen"]
["50.21.","plafondbepleistering - gipspleisters"]
["50.21.10.","plafondbepleistering - gipspleisters/dikpleister op welfsels"]
["50.21.11.","plafondbepleistering - gipspleisters/dikpleister op welfsels - plafondoppervlakte ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
[null,null,null,"m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m2","TYPE 5","Object","Plafondafwerking object","Hoeveelheden uit project",null,1]
[null,null,null,"m2","TYPE 4","Object","Plafondafwerking object bestaande uit meerdere schildelen (2 en 3)","Hoeveelheden uit project",null,1]
[null,null,null,"m3","TYPE 5","Object","Plafondafwerking object - enkel schil 1 ","Hoeveelheden uit project",null,1]
["50.21.12.","plafondbepleistering - gipspleisters/dikpleister op welfsels - zijkanten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[null,null,null,"m","TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["50.21.20.","plafondbepleistering - gipspleisters/dunpleister op breedplaatvloeren "]
["50.21.21.","plafondbepleistering - gipspleisters/dunpleister op breedplaatvloeren - plafondoppervlakte ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
[null,null,null,"m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m2","TYPE 5","Object","Plafondafwerking object","Hoeveelheden uit project",null,1]
[null,null,null,"m2","TYPE 4","Object","Plafondafwerking object bestaande uit meerdere schildelen (2 en 3)","Hoeveelheden uit project",null,1]
[null,null,null,"m3","TYPE 5","Object","Plafondafwerking object - enkel schil 1 ","Hoeveelheden uit project",null,1]
["50.21.22.","plafondbepleistering - gipspleisters/dunpleister op breedplaatvloeren - zijkanten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[null,null,null,"m","TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["50.21.30.","plafondbepleistering - gipspleisters/pleister op beplating "]
["50.21.31.","plafondbepleistering - gipspleisters/pleister op beplating - plafondoppervlakte ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
[null,null,null,"m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m2","TYPE 5","Object","Plafondafwerking object","Hoeveelheden uit project",null,1]
[null,null,null,"m2","TYPE 4","Object","Plafondafwerking object bestaande uit meerdere schildelen (2 en 3)","Hoeveelheden uit project",null,1]
[null,null,null,"m3","TYPE 5","Object","Plafondafwerking object - enkel schil 1 wordt in m3 berekend","Hoeveelheden uit project",null,1]
["50.21.32.","plafondbepleistering - gipspleisters/pleister op beplating - zijkanten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[null,null,null,"m","TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["50.21.40.","plafondbepleistering - gipspleisters/pleister op pleisterdrager "]
["50.21.41.","plafondbepleistering - gipspleisters/pleister op pleisterdrager - plafondoppervlakte ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
[null,null,null,"m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m2","TYPE 5","Object","Plafondafwerking object","Hoeveelheden uit project",null,1]
[null,null,null,"m2","TYPE 4","Object","Plafondafwerking object bestaande uit meerdere schildelen (2 en 3)","Hoeveelheden uit project",null,1]
[null,null,null,"m3","TYPE 5","Object","Plafondafwerking object - enkel schil 1 ","Hoeveelheden uit project",null,1]
["50.21.42.","plafondbepleistering - gipspleisters/pleister op pleisterdrager - zijkanten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["50.30.","renovatie pleisterwerk - algemeen ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[null,null,null,"m2","TYPE 3","Shell",null,"Top Surface",null,1]
[null,null,null,"m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["51.","BINNENPLAATAFWERKINGEN"]
["51.00.","binnenplaatafwerkingen - algemeen"]
["51.10.","lichte scheidingswanden - algemeen"]
["51.11.","lichte scheidingswanden - gipskartonplaten ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.12.","lichte scheidingswanden - gipsvezelplaten ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.13.","lichte scheidingswanden - calciumsilicaatplaten ","FH","m2","TYPE 2","Wall",null,null,null,1]
[null,"lichte scheidingswanden - vezelcementplaten ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.14.","lichte scheidingswanden - calciumsilicaatplaten ","FH","m2","TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.15.","lichte scheidingswanden - multiplexplaten ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.16.","lichte scheidingswanden - OSB-platen ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.17.","lichte scheidingswanden - MDF-platen","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"ARCHICAD Property: Oppervlakte middenas wand",null,1]
["51.20.","voorzetwanden - algemeen"]
["51.21.","voorzetwanden - gipskartonplaten"]
["51.21.10.","voorzetwanden - gipskartonplaten/op regelstructuur ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.21.20.","voorzetwanden - gipskartonplaten/gekleefd ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.22.","voorzetwanden - gipsvezelplaten"]
["51.22.10.","voorzetwanden - gipsvezelplaten/op regelstructuur ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.22.20.","voorzetwanden - gipsvezelplaten/gekleefd ","FH","m2","TYPE 2","Wall",null,null,null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.23.","voorzetwanden - vezelcementplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.24.","voorzetwanden - calciumsilicaatplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.25.","voorzetwanden - multiplex ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.26.","voorzetwanden - OSB-platen ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.27.","voorzetwanden - MDF-platen","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,null,null,1]
["51.30.","schachtwanden - algemeen"]
["51.31.","schachtwanden - gipskartonplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.32.","schachtwanden - gipsvezelplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.33.","schachtwanden - vezelcementplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.34.","schachtwanden - calciumsilicaatplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.35.","schachtwanden - multiplexplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.36.","schachtwanden - OSB-platen ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.37.","schachtwanden - MDF-platen","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.38.","schachtwanden - kunstharsplaten ","FH","m2","TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,1]
["51.40.","toegangsluiken - algemeen"]
["51.41.","toegangsluiken - hout ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Window",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["51.42.","toegangsluiken - kunsthars ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Window",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["51.43.","toegangsluiken - vezelcement ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Window",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["51.44.","toegangsluiken - metalen kader ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Window",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["51.50.","plafondafwerking - algemeen"]
["51.51.","plafondafwerking - uitbekleding plafond"]
["51.51.10.","plafondafwerking - uitbekleding plafond/gipskartonplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,2]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,2]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",2]
[{"$nulls":4},"TYPE 3","Wall",null,"Netto oppervlak binnenkant wand",null,2]
["51.51.20.","plafondafwerking - uitbekleding plafond/gipsvezelplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.51.30.","plafondafwerking - uitbekleding plafond/vezelcementplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.51.40.","plafondafwerking - uitbekleding plafond/calciumsilicaatplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.51.50.","plafondafwerking - uitbekleding plafond/OSB","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.52.","plafondafwerking - uitbekleding daklichtopeningen ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 4","Object","gebruik ARCHICAD property: VMSW uitbekleding daglichtopeningen ",null,null,1]
[{"$nulls":4},"TYPE 4","Skylight","gebruik ARCHICAD property: VMSW uitbekleding daglichtopeningen ",null,null,1]
[null,null,null,"m2","TYPE 3","Wall",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 4","Object","gebruik ARCHICAD property: VMSW uitbekleding daglichtopeningen ",null,null,1]
[{"$nulls":4},"TYPE 4","Skylight","gebruik ARCHICAD property: VMSW uitbekleding daglichtopeningen ","Oppervlakte volgens openingshoogte daklicht en dikte dak",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["51.53.","plafondafwerking - verlaagd plafond"]
["51.53.10.","plafondafwerking - verlaagd plafond/gipskartonplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.53.20.","plafondafwerking - verlaagd plafond/gipsvezelplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.53.30.","plafondafwerking - verlaagd plafond/vezelcementplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.53.40.","plafondafwerking - verlaagd plafond/calciumsilicaatplaten ","FH","m2","TYPE 3","Roof",null,"Projected Area",null,1]
[{"$nulls":4},"TYPE 3","Shell",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["51.60.","uitbekleding buitenramen en -deuren - algemeen"]
["51.61.","uitbekleding buitenramen en -deuren - isolatieplaten voor bepleistering ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["51.62.","uitbekleding buitenramen en -deuren - multiplex ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["51.63.","uitbekleding buitenramen en -deuren - MDF ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["51.64.","uitbekleding buitenramen en -deuren - massief hout ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["51.65.","uitbekleding buitenramen en -deuren - PVC ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["51.66.","uitbekleding buitenramen en -deuren - gipskarton ","FH","m","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","ARCHICAD property: Uitbekleding binnenkant buitenschrijnwerk",null,1]
[null,null,null,"m2","TYPE 4","Door","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW uitbekleding dagkanten ","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
["51.70.","uitbekleding sanitaire toestellen - algemeen"]
["51.71.","uitbekleding sanitaire toestellen - te betegelen plaat"]
["51.72.","uitbekleding sanitaire toestellen - plaat als eindafwerking"]
["52.","DEK- EN BEDRIJFSVLOEREN"]
["52.00.","dek- en bedrijfsvloeren - algemeen"]
["52.10.","isolerende uitvullagen - algemeen"]
["52.11.","isolerende uitvullagen - cementgebonden ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface"]
["52.12.","isolerende uitvullagen - schuimbeton ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface"]
["52.13.","isolerende uitvullagen - gespoten polyurethaan ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface"]
["52.14.","isolerende uitvullagen - droge granulaten ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface"]
["52.20.","vochtwerende lagen - algemeen"]
["52.21.","vochtwerende lagen - PE-folie ","PM",null,"Geen",{"$nulls":4},1]
["52.30.","thermische isolatie vloer - algemeen"]
["52.31.","thermische isolatie vloer - MW"]
["52.31.10.","thermische isolatie vloer - MW/8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.31.20.","thermische isolatie vloer - MW/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.32.","thermische isolatie vloer - PUR of PIR"]
["52.32.10.","thermische isolatie vloer - PUR of PIR 8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.32.20.","thermische isolatie vloer - PUR of PIR/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.33.","thermische isolatie vloer - PF"]
["52.33.10.","thermische isolatie vloer - PF/8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.33.20.","thermische isolatie vloer - PF/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.34.","thermische isolatie vloer - XPS"]
["52.34.10.","thermische isolatie vloer - XPS/8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.34.20.","thermische isolatie vloer - XPS/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.35.","thermische isolatie vloer - EPS"]
["52.35.10.","thermische isolatie vloer - EPS/8 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.35.20.","thermische isolatie vloer - EPS/10 cm ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.40.","akoestische isolatie vloer - algemeen"]
["52.41.","akoestische isolatie vloer - kunststofschuim ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.42.","akoestische isolatie vloer - kokosvezels ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.50.","cementgebonden dekvloeren - algemeen"]
["52.51.","cementgebonden dekvloeren - hechtend ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.52.","cementgebonden dekvloeren - niet hechtend ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.53.","cementgebonden dekvloeren - zwevend ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.54.","cementgebonden dekvloeren - zwevend en gepolierd ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.60.","calciumsulfaatgebonden dekvloeren - algemeen"]
["52.61.","calciumsulfaatgebonden dekvloeren - niet hechtend ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.62.","calciumsulfaatgebonden dekvloeren - zwevend ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.70.","bedrijfsvloeren - algemeen"]
["52.71.","bedrijfsvloeren - gepolierd beton ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["52.72.","bedrijfsvloeren - epoxymortel ","FH","m2","TYPE 2","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.","BINNENVLOERAFWERKINGEN"]
["53.00.","binnenvloerafwerkingen - algemeen"]
["53.10.","tegelvloeren - algemeen"]
["53.11.","tegelvloeren - keramisch"]
["53.11.10.","tegelvloeren - keramisch/getrokken tegels ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.11.20.","tegelvloeren - keramisch/geperste tegels ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.12.","tegelvloeren - marmermozaiek ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.13.","tegelvloeren - natuursteen"]
["53.13.10.","tegelvloeren - natuursteen/blauwe hardsteen ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.13.20.","tegelvloeren - natuursteen/travertijn ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.13.30.","tegelvloeren - natuursteen/jura ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.14.","tegelvloeren - betontegels ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.20.","soepele vloerbekledingen - algemeen"]
["53.21.","soepele vloerbekledingen - linoleum ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.22.","soepele vloerbekledingen - vinyl (PVC) ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.23.","soepele vloerbekledingen - rubber ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.24.","soepele vloerbekledingen - douchecellen ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.30.","houten vloerbekledingen - algemeen"]
["53.31.","houten vloerbekledingen - laminaat ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.32.","houten vloerbekledingen - opschuren bij renovatie ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
["53.40.","plinten - algemeen"]
["53.41.","plinten - steen"]
["53.41.10.","plinten - steen/keramisch ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object ","Object interieurafwerking - enkel plint actief","Lengte","Let op! Enkel Horizontale lengte wordt gemeten ",1]
[{"$nulls":4},"TYPE 4","Object ","Object interieurafwerking - in dit object zijn andere opties (wandafwerking/lambrisering) actief > plint als type 4","Lengte","Let op! Enkel Horizontale lengte wordt gemeten ",1]
["53.41.20.","plinten - steen/marmermozaiek ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object","Object interieurafwerking - enkel plint actief","Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"TYPE 4","Object ","Object interieurafwerking - in dit object zijn andere opties (wandafwerking/lambrisering) actief > plint als type 4","Lengte","Let op! Enkel Horizontale lengte wordt gemeten ",1]
["53.41.30.","plinten - steen/natuursteen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object","Object interieurafwerking - enkel plint actief","Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"TYPE 4","Object ","Object interieurafwerking - in dit object zijn andere opties (wandafwerking/lambrisering) actief > plint als type 4","Lengte","Let op! Enkel Horizontale lengte wordt gemeten ",1]
["53.42.","plinten - hout"]
["53.42.10.","plinten - hout/massief hout ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object","Object interieurafwerking - enkel plint actief","Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"TYPE 4","Object ","Object interieurafwerking - in dit object zijn andere opties (wandafwerking/lambrisering) actief > plint als type 4","Lengte","Let op! Enkel Horizontale lengte wordt gemeten ",1]
["53.42.20.","plinten - hout/MDF ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object","Object interieurafwerking - enkel plint actief","Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"TYPE 4","Object ","Object interieurafwerking - in dit object zijn andere opties (wandafwerking/lambrisering) actief > plint als type 4","Lengte","Let op! Enkel Horizontale lengte wordt gemeten ",1]
["53.43.","plinten - soepel"]
["53.43.10.","plinten - soepel/linoleum ","FH\n","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object","Object interieurafwerking - enkel plint actief","Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"TYPE 4","Object ","Object interieurafwerking - in dit object zijn andere opties (wandafwerking/lambrisering) actief > plint als type 4","Lengte","Let op! Enkel Horizontale lengte wordt gemeten ",1]
["53.43.20.","plinten - soepel/PVC ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object","Object interieurafwerking - enkel plint actief","Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"TYPE 4","Object ","Object interieurafwerking - in dit object zijn andere opties (wandafwerking/lambrisering) actief > plint als type 4","Lengte","Let op! Enkel Horizontale lengte wordt gemeten ",1]
["53.43.30.","plinten - soepel/rubber ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Object","Object interieurafwerking - enkel plint actief","Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"TYPE 4","Object ","Object interieurafwerking - in dit object zijn andere opties (wandafwerking/lambrisering) actief > plint als type 4","Lengte","Let op! Enkel Horizontale lengte wordt gemeten ",1]
["53.50.","tussendorpels - algemeen"]
["53.51.","tussendorpels - steen"]
["53.51.10.","tussendorpels - steen/natuursteen ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW tussendorpel binnendeur","breedte deuropening * muurdikte",null,1]
["53.51.20.","tussendorpels - steen/marmermozaiek ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW tussendorpel binnendeur","breedte deuropening * muurdikte",null,1]
["53.51.30.","tussendorpels - steen/composiet ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW tussendorpel binnendeur","breedte deuropening * muurdikte",null,1]
["53.60.","trapbekledingen - algemeen"]
["53.61.","trapbekledingen - steen"]
["53.61.10.","trapbekledingen - steen/keramisch ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks",null,1]
["53.61.20.","trapbekledingen - steen/marmermozaiek ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks",null,1]
["53.61.30.","trapbekledingen - steen/natuursteen ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks",null,1]
["53.62.","trapbekledingen - hout"]
["53.62.10.","trapbekledingen - hout/massief ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks",null,1]
["53.62.20.","trapbekledingen - hout/gelamineerd ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks",null,1]
["53.63.","trapbekledingen - soepel"]
["53.63.10.","trapbekledingen - soepel/rubber ","FH","st","TYPE 5","Stair","Dit classificeren op het niveau van de trede( Flight - Tread) )","Stuks",null,1]
["53.70.","toebehoren - algemeen"]
["53.71.","toebehoren - scheidingsprofielen ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["53.72.","toebehoren - vloermatkaders ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"Stuks",null,1]
["53.73.","toebehoren - vloermatten ","FH","m2","TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[null,null,null,"st","TYPE 3","Slab",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["53.74.","toebehoren - vloerdeksels "]
["53.74.10.","toebehoren - vloerdeksels/metaal","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["53.74.20.","toebehoren - vloerdeksels/betegelbaar","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["53.75.","toebehoren - vloerroosters ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"Stuks",null,1]
["53.76.","toebehoren - zettingsprofielen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
["54.","BINNENDEUREN en -RAMEN"]
["54.00.","binnendeuren en -ramen - algemeen"]
["54.01.","binnendeuren en -ramen - prestaties"]
["54.02.","binnendeuren en -ramen - keuring en proeven"]
["54.03.","binnendeuren en -ramen - proefopstelling"]
["54.10.","deurkozijnen - algemeen"]
["54.11.","deurkozijnen - hout"]
["54.11.10.","deurkozijnen - hout/massief ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks",null,1]
["54.11.20.","deurkozijnen - hout/multiplex ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks",null,1]
["54.11.30.","deurkozijnen - hout/MDF ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks",null,1]
["54.12.","deurkozijnen - staal"]
["54.12.10.","deurkozijnen - staal/montagekozijn ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks",null,1]
["54.12.20.","deurkozijnen - staal/inbouwkozijn ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurkozijnen","Stuks",null,1]
["54.20.","deurbladen - algemeen"]
["54.21.","deurbladen - hout met holle kern"]
["54.21.10.","deurbladen - hout met holle kern/celrooster ","FH","st","TYPE 4","Door ","Gebruik ARCHICAD property: VMSW deurblad","Stuks",null,1]
["54.21.20.","deurbladen - hout met holle kern/tubespaan ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurblad","Stuks",null,1]
["54.22.","deurbladen - hout met volle kern"]
["54.22.10.","deurbladen - hout met volle kern/spaan ","FH","st","TYPE 4","Door ","Gebruik ARCHICAD property: VMSW deurblad","Stuks",null,1]
["54.22.20.","deurbladen - hout met volle kern/multiplex ","FH","st","TYPE 4","Door ","Gebruik ARCHICAD property: VMSW deurblad","Stuks",null,1]
["54.30.","deurgehelen - algemeen"]
["54.31.","deurgehelen - kozijnen hout"]
["54.31.10.","deurgehelen - kozijnen hout/brandwerend ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.31.20.","deurgehelen - kozijnen hout/inbraakwerend ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.31.30.","deurgehelen - kozijnen hout/passiefdeur ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.32.","deurgehelen - kozijnen staal"]
["54.32.10.","deurgehelen - kozijnen staal/brandwerend ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.32.20.","deurgehelen - kozijnen staal/inbraakwerend ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.40.","schuif- en vouwdeuren - algemeen"]
["54.41.","schuif- en vouwdeuren - schuifsystemen"]
["54.41.10.","schuif- en vouwdeuren - schuifsystemen/voorbouw ","FH","st","TYPE 5","Door ",null,"Stuks",null,1]
[{"$nulls":5},"Window ",null,"Stuks",null,1]
["54.41.20.","schuif- en vouwdeuren - schuifsystemen/inbouwmodule ","FH","st","TYPE 5","Door ",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Window ",null,"Stuks",null,1]
["54.42.","schuif- en vouwdeuren - vouwsystemen"]
["54.42.10.","schuif- en vouwdeuren - vouwsystemen/kunststof ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Window",null,"Stuks",null,1]
["54.50.","glazen deuren - algemeen"]
["54.51.","glazen deuren - opendraaiend ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.52.","glazen deuren - openschuivend ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["54.60.","hang- en sluitwerk - algemeen"]
["54.61.","hang- en sluitwerk - scharnieren en paumellen"]
["54.61.10.","hang- en sluitwerk - scharnieren en paumellen/aluminium ","PM",null,"Geen",{"$nulls":4},1]
["54.61.20.","hang- en sluitwerk - scharnieren en paumellen/vernikkeld staal ","PM",null,"Geen",{"$nulls":4},1]
["54.61.30.","hang- en sluitwerk - scharnieren en paumellen/roestvast staal ","PM",null,"Geen",{"$nulls":4},1]
["54.62.","hang- en sluitwerk - deursloten"]
["54.62.10.","hang- en sluitwerk - deursloten/klaviersloten ","PM",null,"Geen",{"$nulls":4},1]
["54.62.20.","hang- en sluitwerk - deursloten/veiligheidssloten ","PM",null,"Geen",{"$nulls":4},1]
["54.62.30.","hang- en sluitwerk - deursloten/elektromagnetisch ","PM",null,"Geen",{"$nulls":4},1]
["54.62.40.","hang- en sluitwerk - deursloten/kantschuiven ","PM",null,"Geen",{"$nulls":4},1]
["54.62.50.","hang- en sluitwerk - deursloten/panieksluitingen ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW panieksluiting","Stuks",null,1]
["54.63.","hang- en sluitwerk - deurkrukken"]
["54.63.10.","hang- en sluitwerk - deurkrukken/aluminium ","PM",null,"Geen",{"$nulls":4},1]
["54.63.20.","hang- en sluitwerk - deurkrukken/RVS ","PM",null,"Geen",{"$nulls":4},1]
["54.63.30.","hang- en sluitwerk - deurkrukken/kunststof ","PM",null,"Geen",{"$nulls":4},1]
["54.64.","hang- en sluitwerk - vaste handgrepen ","PM",null,"Geen",{"$nulls":4},1]
["54.65.","hang- en sluitwerk - deurdrangers ","PM",null,"Geen",{"$nulls":4},1]
["54.70.","vaste binnenramen - algemeen"]
["54.71.","vaste binnenramen - hout ","FH","m2","TYPE 5","Window",null,"W/D Opening Surface on the Reveal Side",null,1]
["54.80.","toebehoren - algemeen"]
["54.81.","toebehoren - deurroosters"]
["54.82.","toebehoren - beschermplaten"]
["54.82.10.","toebehoren - beschermplaten/aluminium ","PM",null,"Geen",{"$nulls":4},1]
["55.","BINNENTRAPPEN EN LEUNINGEN"]
["55.00.","binnentrappen en leuningen - algemeen"]
["55.10.","trappen - algemeen"]
["55.11.","trappen - hout"]
["55.11.10.","trappen - hout/rechte treden ","FH","st","TYPE 5","Stair",null,"Stuks",null,1]
["55.11.20.","trappen - hout/verdreven treden ","FH","st","TYPE 5","Stair",null,"Stuks",null,1]
["55.12.","trappen - staal"]
["55.12.10.","trappen - staal/rechte treden ","FH","st","TYPE 5","Stair",null,"Stuks",null,1]
["55.12.20.","trappen - staal/verdreven treden ","FH","st","TYPE 5","Stair",null,"Stuks",null,1]
["55.20.","borstweringen - algemeen"]
["55.21.","borstweringen - hout ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["55.22.","borstweringen - staal ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["55.23.","borstweringen - roestvast staal ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["55.24.","borstweringen - aluminium ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["55.25.","borstweringen - veiligheidsglas ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
[{"$nulls":4},"TYPE 5","Railing",null,"Lengte railing horizontale projectie",null,1]
["55.30.","handgrepen - algemeen"]
["55.31.","handgrepen - hout ","PM",null,"Geen",{"$nulls":4},1]
["55.32.","handgrepen - staal ","PM",null,"Geen",{"$nulls":4},1]
["55.33.","handgrepen - roestvast staal ","PM",null,"Geen",{"$nulls":4},1]
["55.34.","handgrepen - aluminium ","PM",null,"Geen",{"$nulls":4},1]
["55.40.","zoldertrappen en -luiken - algemeen"]
["55.41.","zoldertrappen en -luiken - hout ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["55.42.","zoldertrappen en -luiken - aluminium ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.","VAST BINNENMEUBILAIR",{"$nulls":5},"wat met samengestelde onderdelen?"]
["56.00.","vast binnenmeubilair - algemeen"]
["56.10.","keukenmeubelen - algemeen"]
["56.11.","keukenmeubelen - onderdelen"]
["56.11.10.","keukenmeubelen - onderdelen/stelpoten en plintplaat ","PM",null,"Geen",{"$nulls":4},1]
["56.11.20.","keukenmeubelen - onderdelen/corpus en leggers ","PM",null,"Geen",{"$nulls":4},1]
["56.11.30.","keukenmeubelen - onderdelen/fronten en zichtwanden ","PM",null,"Geen",{"$nulls":4},1]
["56.11.40.","keukenmeubelen - onderdelen/werkbladen ","PM",null,"Geen",{"$nulls":4},1]
["56.11.50.","keukenmeubelen - onderdelen/beslag en handgrepen ","PM",null,"Geen",{"$nulls":4},1]
["56.11.60.","keukenmeubelen - onderdelen/toebehoren ","PM",null,"Geen",{"$nulls":4},1]
["56.12.","keukenmeubelen - type 1 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.13.","keukenmeubelen - type 2 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.14.","keukenmeubelen - type 3 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.20.","badkamermeubelen - algemeen"]
["56.21.","badkamermeubelen - onderdelen"]
["56.21.10.","badkamermeubelen - onderdelen/stelpoten en plintplaat ","PM",null,"Geen",{"$nulls":4},1]
["56.21.20.","badkamermeubelen - onderdelen/corpus en leggers ","PM",null,"Geen",{"$nulls":4},1]
["56.21.30.","badkamermeubelen - onderdelen/fronten en zichtwanden ","PM",null,"Geen",{"$nulls":4},1]
["56.21.40.","badkamermeubelen - onderdelen/wastafeltabletten ","PM",null,"Geen",{"$nulls":4},1]
["56.21.50.","badkamermeubelen - onderdelen/beslag en handgrepen ","PM",null,"Geen",{"$nulls":4},1]
["56.21.60.","badkamermeubelen - onderdelen/toebehoren ","PM",null,"Geen",{"$nulls":4},1]
["56.22.","badkamermeubelen - type 1 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.23.","badkamermeubelen - type 2 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.24.","badkamermeubelen - type 3 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.30.","inbouwkasten - algemeen"]
["56.31.","inbouwkasten - onderdelen"]
["56.31.10.","inbouwkasten - onderdelen/stelpoten en plintplaat ","PM",null,"Geen",{"$nulls":4},1]
["56.31.20.","inbouwkasten - onderdelen/corpus en leggers ","PM",null,"Geen",{"$nulls":4},1]
["56.31.30.","inbouwkasten - onderdelen/fronten en zichtwanden ","PM",null,"Geen",{"$nulls":4},1]
["56.31.40.","inbouwkasten - onderdelen/tabletten en bureelbladen ","PM",null,"Geen",{"$nulls":4},1]
["56.31.50.","inbouwkasten - onderdelen/beslag en handgrepen ","PM",null,"Geen",{"$nulls":4},1]
["56.31.60.","inbouwkasten - onderdelen/toebehoren ","PM",null,"Geen",{"$nulls":4},1]
["56.32.","inbouwkasten - kastgeheel type 1 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.33.","inbouwkasten - kastgeheel type 2 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.34.","inbouwkasten - kastgeheel type 3 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["56.40.","parlofoonconsoles - algemeen"]
["56.41.","parlofoonconsoles - multiplexplaat ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["56.42.","parlofoonconsoles - kunstharsplaat ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["56.43.","parlofoonconsoles - metaalplaat"]
["56.43.10.","parlofoonconsoles - metaalplaat/gemoffeld staal ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["56.43.20.","parlofoonconsoles - metaalplaat/roestvast staal (RVS) ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["56.43.30.","parlofoonconsoles - metaalplaat/aluminium ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["56.50.","brievenbusgehelen - algemeen"]
["56.51.","brievenbusgehelen - multiplexplaat ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
["56.52.","brievenbusgehelen - kunstharsplaat ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
["56.53.","brievenbusgehelen - metaalplaat"]
["56.53.10.","brievenbusgehelen - metaalplaat/gemoffeld staal ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
["56.53.20.","brievenbusgehelen - metaalplaat/roestvast staal (RVS) ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
["56.53.30.","brievenbusgehelen - metaalplaat/gemoffeld aluminium ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
["56.60.","gordijnkasten - algemeen"]
["56.61.","gordijnkasten - hout"]
["56.61.10.","gordijnkasten - hout/massief ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
["56.61.20.","gordijnkasten - hout/houtspaanplaat ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
["56.61.30.","gordijnkasten - hout/multiplex ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
["56.61.40.","gordijnkasten - hout/MDF ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Reference line length",null,1]
["56.62.","gordijnkasten - kunststof ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[]
["57.","TABLET- EN WANDBEKLEDINGEN"]
["57.00.","tablet- en wandbekledingen - algemeen"]
["57.10.","venstertabletten - algemeen"]
["57.11.","venstertabletten - natuursteen"]
["57.11.10.","venstertabletten - natuursteen/marmer ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.11.20.","venstertabletten - natuursteen/blauwe hardsteen ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.11.30.","venstertabletten - natuursteen/leisteen ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.11.40.","venstertabletten - natuursteen/volgens prestaties ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.12.","venstertabletten - kunststeen"]
["57.12.10.","venstertabletten - kunststeen/marmermozaïek ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.12.20.","venstertabletten - kunststeen/vezelcement ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.12.30.","venstertabletten - kunststeen/composiet ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.13.","venstertabletten - hout"]
["57.13.10.","venstertabletten - hout/massief ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.13.20.","venstertabletten - hout/laminaat ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.14.","venstertabletten - kunststof"]
["57.14.10.","venstertabletten - kunststof/PVC ","FH","m","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","breedte binnendagkant",null,1]
[null,null,null,"m2","TYPE 4","Window","Gebruik ARCHICAD property: VMSW venstertabletten","Oppervlakte (breedte opening x diepte tablet)",null,1]
["57.20.","wandbekledingen - algemeen"]
["57.21.","wandbekledingen - betegeling ","FH","m2","TYPE 3","Wall",null,"Netto oppervlakte binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["57.21.10.","wandbekledingen - betegeling/keramisch ","FH","m2","TYPE 3","Wall",null,"Netto oppervlakte binnenkant wand",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
[]
["60.","SANITAIR LEIDINGNET"]
["60.00.","sanitair leidingnet - algemeen"]
["60.10.","afvoerbuizen - algemeen"]
["60.11.","afvoerbuizen - PVC ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["60.12.","afvoerbuizen - PE ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["60.13.","afvoerbuizen - PP ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["60.20.","verluchtingsbuizen - algemeen"]
["60.21.","verluchtingsbuizen - PVC ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.22.","verluchtingsbuizen - PE ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.23.","verluchtingsbuizen - beluchtingsventielen ","FH","m","TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.30.","klokroosters - intern - algemeen"]
["60.31.","klokroosters - gietijzer ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.32.","klokroosters - aluminium ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.33.","klokroosters - roestvast staal (RVS) ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.34.","klokroosters - kunststof ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.40.","putdeksels - algemeen"]
["60.41.","putdeksels - gietijzer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.42.","putdeksels - aluminium ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.43.","putdeksels - roestvast staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.44.","putdeksels - kunststof ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.50.","sanitaire drukleidingen - algemeen"]
["60.51.","sanitaire drukleidingen - buizen"]
["60.51.10.","sanitaire drukleidingen - buizen/verzinkt staal ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.51.20.","sanitaire drukleidingen - buizen/koper ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.51.30.","sanitaire drukleidingen - buizen/kunststof ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["60.52.","sanitaire drukleidingen - collectoren ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.53.","sanitaire drukleidingen - leidingisolatie ","FH","st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.54.","sanitaire drukleidingen - brandwerende doorvoeren ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["60.55.","sanitaire drukleidingen - verwarmingslint ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["60.56.","sanitaire drukleidingen - flexibele leidingen ","PM",null,"Geen",{"$nulls":4},1]
["60.60.","aansluiting leidingnet - algemeen"]
["60.61.","aansluiting leidingnet - reglementaire meterstraat ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["60.62.","aansluiting leidingnet - voedingsleidingen & tellers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["60.63.","aansluiting leidingnet - waterfilters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["60.70.","waterbehandeling - algemeen"]
["60.71.","waterbehandeling - ontharders ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["60.72.","waterbehandeling - filters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.","SANITAIRE TOESTELLEN & TOEBEHOREN"]
["61.00.","sanitaire toestellen en toebehoren - algemeen"]
["61.10.","toiletpotten en toebehoren - algemeen"]
["61.11.","toiletpotten en toebehoren - staand ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.12.","toiletpotten en toebehoren - hangend ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.20.","handwastafels en toebehoren - algemeen"]
["61.21.","handwastafels & toebehoren - wandmodel"]
["61.21.10.","handwastafels & toebehoren - wandmodel/porselein ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.22.","handwastafels en toebehoren - inbouwmodel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.30.","wastafels en toebehoren - algemeen"]
["61.31.","wastafels en toebehoren - wandmodel"]
["61.31.10.","wastafels en toebehoren - wandmodel/porselein ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.32.","wastafels en toebehoren - inbouwmodel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.40.","baden - algemeen"]
["61.41.","baden - geëmailleerd staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.42.","baden - acrylaat ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.50.","douches - algemeen"]
["61.51.","douches - geëmailleerd staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.52.","douches - acrylaat ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.53.","douches - tegeldouche ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.60.","speciale toebehoren - algemeen"]
["61.61.","speciale toebehoren - rail en douchegordijn ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.62.","speciale toebehoren - douchedeuren en -wanden ","FH","st","TYPE 3","Wall",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Door",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Window",null,"Stuks",null,1]
["61.63.","speciale toebehoren - muurhandgrepen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.64.","speciale toebehoren - douchezitjes ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.70.","afwastafels - algemeen"]
["61.71.","afwastafels - opbouwmodel"]
["61.71.10.","afwastafels - opbouwmodel/roestvast staal (RVS) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.72.","afwastafels - inbouwmodel"]
["61.72.10.","afwastafels - inbouwmodel/roestvast staal (RVS) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["61.80.","uitgietbakken - algemeen"]
["61.81.","uitgietbakken - sanitair porselein ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.","SANITAIRE KRANEN & KLEPPEN"]
["62.00.","sanitaire kranen - kleppen - algemeen"]
["62.10.","terugslagkleppen - algemeen"]
["62.11.","terugslagkleppen - messing ","PM",null,"Geen",{"$nulls":4},1]
["62.20.","installatieafsluitkranen - algemeen"]
["62.21.","installatieafsluitkranen - messing"]
["62.21.10.","installatieafsluitkranen - messing/zonder aftapkraan ","PM",null,"Geen",{"$nulls":4},1]
["62.21.20.","installatieafsluitkranen - messing/met aftapkraan ","PM",null,"Geen",{"$nulls":4},1]
["62.22.","installatieafsluitkranen - kunststof"]
["62.22.10.","installatieafsluitkranen - kunststof/zonder aftapkraan ","PM",null,"Geen",{"$nulls":4},1]
["62.30.","wandafsluitkranen - algemeen"]
["62.31.","wandafsluitkranen - enkelvoudige stopkraan ","PM",null,"Geen",{"$nulls":4},1]
["62.32.","wandafsluitkranen - stopkraan met dienstkraan ","PM",null,"Geen",{"$nulls":4},1]
["62.40.","dienstkranen - algemeen"]
["62.41.","dienstkranen - enkele dienstkraan"]
["62.41.10.","dienstkranen - enkele dienstkraan/vaste uitloop ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.41.20.","dienstkranen - enkele dienstkraan/draaibare uitloop ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.42.","dienstkranen - dubbele dienstkraan"]
["62.42.10.","dienstkranen - dubbele dienstkraan/binnen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.42.20.","dienstkranen - dubbele dienstkraan/buiten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.50.","ééngatskranen - algemeen"]
["62.51.","ééngatskranen - handwastafelkraan ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.52.","ééngatskranen - lavabomengkraan ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.53.","ééngatskranen - afwastafelmengkraan ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.60.","muurmengkranen - algemeen"]
["62.61.","muurmengkranen - badmengkraan & armatuur ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.62.","muurmengkranen - douchemengkraan/armatuur ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.63.","muurmengkranen - afwastafelmengkraan ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.70.","regenwaterpompen - algemeen"]
["62.71.","regenwaterpompen - zelfaanzuigende hydrofoorgroep ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.72.","regenwaterpompen - dompelpomp ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["62.73.","regenwaterpompen - handpomp ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.","SANITAIR WARM WATER"]
["63.00.","sanitair warm water - algemeen"]
["63.10.","doorstroomwaterverwarmers op gas - algemeen"]
["63.11.","doorstroomwaterverwarmers op gas - badgeisers"]
["63.11.10.","doorstroomwaterverwarmers op gas - badgeisers/type B11BS ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.11.20.","doorstroomwaterverwarmers op gas - badgeisers/type C13-C33 ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.12.","doorstroomwaterverwarmers op gas - keukengeisers"]
["63.12.10.","doorstroomwaterverwarmers op gas - keukengeisers/type AAS ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.20.","voorraadtoestellen op gas ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.30.","elektroboilers - algemeen"]
["63.31.","elektroboilers - kokend water toestellen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.32.","elektroboilers - inbouwmodel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.33.","elektroboilers - spaarboilers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.40.","voorraadboilers indirecte opwarming - algemeen"]
["63.41.","voorraadboilers indirecte opwarming - enkelvoudige warmtewisselaar ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.42.","voorraadboilers indirecte opwarming - dubbelvoudige warmtewisselaar ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.50.","zonneboilers - algemeen"]
["63.51.","zonneboilers - collectoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.52.","zonneboilers - opslagvat ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.53.","zonneboilers - leidingsysteem en toebehoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.54.","zonneboilers - circulatoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.55.","zonneboilers - expansiesysteem ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.56.","zonneboilers - regelsystemen en beveiliging"]
["63.56.10.","zonneboilers - regelsystemen en beveiliging/aflaat- en vulkranen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["63.56.20.","zonneboilers - regelsystemen en beveiliging/regelkranen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["63.56.30.","zonneboilers - regelsystemen en beveiliging/ontluchters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["63.56.40.","zonneboilers - regelsystemen en beveiliging/veiligheidskleppen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["63.56.50.","zonneboilers - regelsystemen en beveiliging/keerkleppen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["63.56.60.","zonneboilers - regelsystemen en beveiliging/mengventielen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["63.60.","warmtepompboilers - algemeen"]
["63.70.","satellietsystemen - algemeen "]
["63.71.","satellietsystemen - voorraadboilers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["63.72.","satellietsystemen - platenwisselaars ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["64.","GASINSTALLATIES"]
["64.00.","gasinstallaties - algemeen"]
["64.10.","gasleidingen - algemeen"]
["64.11.","gasleidingen - staal ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["64.12.","gasleidingen - koper ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["64.13.","gasleidingen - PE ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["64.14.","gasleidingen - PLT-buissysteem ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["64.20.","gaskranen - algemeen"]
["64.21.","gaskranen - gasfilter ","PM",null,"Geen",{"$nulls":4},1]
["64.22.","gaskranen - afsluitkranen ","PM",null,"Geen",{"$nulls":4},1]
["64.30.","gasaansluiting ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["64.40.","gastoestellen - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["65.","VERWARMING INDIVIDUELE INSTALLATIES"]
["65.00.","verwarming individuele installaties - algemeen"]
["65.01.","verwarming individuele installaties - proefopstelling ","PM",null,"Geen",{"$nulls":4},1]
["65.02.","verwarming individuele installaties - grenzen van de aanneming ","PM",null,"Geen",{"$nulls":4},1]
["65.10.","gasvloerketels - algemeen"]
["65.11.","gasvloerketels - open"]
["65.11.10.","gasvloerketels - open/enkel CV ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.11.20.","gasvloerketels - open/CV & SWW (voorraad) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.12.","gasvloerketels - gesloten"]
["65.12.10.","gasvloerketels - gesloten/enkel CV ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.12.20.","gasvloerketels - gesloten/CV & SWW (voorraad) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.20.","gaswandketels - algemeen"]
["65.21.","gaswandketels - gesloten"]
["65.21.10.","gaswandketels - gesloten/enkel CV ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.21.20.","gaswandketels - gesloten/CV & SWW (doorstroom) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.21.30.","gaswandketels - gesloten/CV & SWW (voorraad) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.30.","leidingnet & toebehoren - algemeen"]
["65.31.","leidingnet & toebehoren - buizen"]
["65.31.10.","leidingnet & toebehoren - buizen/staal ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["65.31.20.","leidingnet & toebehoren - buizen/koper ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["65.31.30.","leidingnet & toebehoren - buizen/kunststof ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["65.31.40.","leidingnet & toebehoren - buizen/dunwandige verzinkte buis ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
["65.32.","leidingnet & toebehoren - collectoren ","FH","st","TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["65.33.","leidingnet & toebehoren - leidingisolatie ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 3","Beam",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Stuks",null,1]
[{"$nulls":7},"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["65.34.","leidingnet & toebehoren - brandwerende doorvoeren ","PM",null,"Geen",{"$nulls":4},1]
["65.35.","leidingnet & toebehoren - verwarmingslint ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["65.40.","installatieonderdelen - algemeen"]
["65.41.","installatieonderdelen - aflaatkranen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.42.","installatieonderdelen - regel- en afsluitkranen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.43.","installatieonderdelen - drukregelaars ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.44.","installatieonderdelen - circulatoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["65.45.","installatieonderdelen - expansiesysteem ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.46.","installatieonderdelen - vlotterontluchters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.47.","installatieonderdelen - microbellenafscheider ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.50.","verwarmingselementen & toebehoren - algemeen"]
["65.51.","verwarmingselementen & toebehoren - plaatradiatoren ","FH","kW","TYPE 5","Object",null,"vul het vermogen in bij ARCHICAD property: Vermogen verwarmingselement",null,1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["65.52.","verwarmingselementen & toebehoren - wandconvectoren ","FH","kW","TYPE 5","Object",null,"vul het vermogen in bij ARCHICAD property: Vermogen verwarmingselement",null,1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["65.53.","verwarmingselementen & toebehoren - vloerverwarming","FH","m2","TYPE 5","Object",null,null,null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["65.60.","warmteregeling & toebehoren - algemeen"]
["65.61.","warmteregeling & toebehoren - radiatorkranen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.62.","warmteregeling & toebehoren - thermostaatkoppen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.63.","warmteregeling & toebehoren - kamerthermostaten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.64.","warmteregeling & toebehoren - weersafhankelijke regeling","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.65.","warmteregeling & toebehoren - manometer","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["65.66.","warmteregeling & toebehoren - thermometer","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[]
["66.","BIJZONDERE INSTALLATIES"]
["66.00.","bijzondere installaties - algemeen"]
["66.10.","warmtepompen - algemeen"]
["66.11.","warmtepompen - grond-water ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["66.12.","warmtepompen - water-water ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["66.13.","warmtepompen - lucht-water monoblok ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["66.14.","warmtepompen - lucht-water met binnen- en buitenunit (split-systeem) ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["66.15.","warmtepompen - gasabsorptiewarmtepompen"]
["66.16.","warmtepompen - verticale aardsondes ","SOG",null,"Geen",{"$nulls":4},1]
["66.16.10.","warmtepompen - verticale aardsondes/warmtewisselaar ","FH","SOG","Geen",{"$nulls":4},1]
["66.16.20.","warmtepompen - verticale aardsondes/collector ","PM",null,"Geen",{"$nulls":4},1]
["67.","BRANDBESTRIJDING"]
["67.00.","brandbestrijding - algemeen"]
["67.10.","brandblusapparaten - algemeen"]
["67.11.","brandblusapparaten - poedersnelblussers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.12.","brandblusapparaten - CO2-snelblussers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.13.","brandblusapparaten - schuimsnelblussers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.14.","brandblusapparaten - vast opgestelde poederblussers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.20.","externe bluswatervoorziening - algemeen ","SOG",null,"Geen",{"$nulls":4},1]
["67.21.","externe bluswatervoorziening - leidingen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["67.22.","externe bluswatervoorziening - buitenhydranten"]
["67.22.10.","externe bluswatervoorziening - buitenhydranten/bovengronds ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.22.20.","externe bluswatervoorziening - buitenhydranten/ondergronds ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.30.","interne bluswatervoorziening - algemeen ","SOG",null,"Geen",{"$nulls":4},1]
["67.31.","interne bluswatervoorziening - leidingen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["67.32.","interne bluswatervoorziening - brandkranen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.33.","interne bluswatervoorziening - muurhaspels zonder kast ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.34.","interne bluswatervoorziening - kasten voor slanghaspels ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.35.","interne bluswatervoorziening - manometers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["67.36.","interne bluswatervoorziening - pictogrammen ","PM",null,"Geen",{"$nulls":4},1]
["67.40.","sprinklerinstallatie - algemeen ","SOG",null,"Geen",{"$nulls":4},1]
["67.50.","brandwerende bescherming - algemeen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["68.","VENTILATIE"]
["68.00.","ventilatie - algemeen"]
["68.01.","ventilatie - proefopstelling ","PM",null,"Geen",{"$nulls":4},1]
["68.02.","ventilatie - proeven"]
["68.02.10.","ventilatie - proeven/debietmeting ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["68.02.20.","ventilatie - proeven/meting kanaaldichtheid ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["68.02.30.","ventilatie - proeven/dichtheid collectieve kanalen ","SOG",null,"Geen",{"$nulls":4},1]
["68.10.","ventilatiekanalen - algemeen"]
["68.11.","ventilatiekanalen - metaal"]
["68.11.10.","ventilatiekanalen - metaal/rond ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["68.11.20.","ventilatiekanalen - metaal/rechthoekig ","FH of SOG","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom","Let op! Geef in de classificatie de breedte van het kanaal op.",1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"Geen",{"$nulls":4},1]
["68.12.","ventilatiekanalen - kunststof"]
["68.12.10.","ventilatiekanalen - kunststof/rond ","FH of SOG","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"Geen",{"$nulls":4},1]
["68.12.20.","ventilatiekanalen - kunststof/rechthoekig of ovaal ","FH of SOG","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[{"$nulls":4},"Geen",{"$nulls":4},1]
["68.13.","ventilatiekanalen - flexibele kanalen ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":5},"Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["68.14.","ventilatiekanalen - thermische isolatie ","FH","m","TYPE 2","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom","Let op! Geef in de classificatie de breedte van het kanaal op.",1]
[{"$nulls":4},"TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 5","Object","MEP","Lengte",null,1]
[{"$nulls":7},"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["68.15.","ventilatiekanalen - ophanging en bevestiging ","PM",null,"Geen",{"$nulls":4},1]
["68.20.","toebehoren ventilatiekanalen - algemeen"]
["68.30.","woonhuisventilatoren - algemeen"]
["68.31.","woonhuisventilatoren - systeem C ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.32.","woonhuisventilatoren - systeem D ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.40.","ventilatoren - algemeen"]
["68.41.","ventilatoren - dakventilatoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.42.","ventilatoren - kanaalventilatoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.43.","ventilatoren - sanitaire ventilatoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.50.","dampkappen - algemeen"]
["68.51.","dampkappen - inbouwmotor ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.52.","dampkappen - motorloos ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.60.","ventilatieventielen en -roosters - algemeen"]
["68.61.","ventilatiemonden - ventiel met regelbare conus ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.62.","ventilatiemonden - zelfregelend ventiel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.63.","ventilatiemonden - gevelroosters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["68.64.","ventilatiemonden - dakventielen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["69.","OPBOUWKANALEN ROOKGAS EN VENTILATIE"]
["69.00.","opbouwkanalen rookgas en ventilatie - algemeen"]
["69.10.","schoorstenen - algemeen"]
["69.11.","schoorstenen - roestvast staal"]
["69.11.10.","schoorstenen - roestvast staal/CLV ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.11.20.","schoorstenen - roestvast staal/enkelvoudig kanaal ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.11.30.","schoorstenen - roestvast staal/buigzame kanaalvoering ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.12.","schoorstenen - aluminium"]
["69.12.10.","schoorstenen - aluminium/CLV ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.12.20.","schoorstenen - aluminium/enkelvoudig ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.12.30.","schoorstenen - aluminium/buigzame kanaalvoering ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.13.","schoorstenen - kunststof "]
["69.13.10.","schoorstenen - kunststof/CLV ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.13.20.","schoorstenen - kunststof/enkelvoudig ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.13.30.","schoorstenen - kunststof/buigzame kanaalvoering ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"st","TYPE 5","Object",null,"Stuks",null,1]
["69.20.","dakdoorgang - algemeen"]
["69.21.","dakdoorgang - enkelvoudig ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["69.22.","dakdoorgang - multifunctioneel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[]
["70.","ELEKTRICITEIT BINNENNET"]
["70.00.","elektriciteit binnennet - algemeen"]
["70.10.","aansluitingen - algemeen"]
["70.11.","aansluitingen - ondergrondse aansluiting ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["70.12.","aansluitingen - aansluitbocht ","PM",null,"Geen",{"$nulls":4},1]
["70.13.","aansluitingen - aansluitplaat ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["70.14.","aansluitingen - tellerkasten ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["70.15.","aansluitingen - verbindingskabels ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["70.20.","verdeelkasten - algemeen"]
["70.21.","verdeelkasten - hoofdverdeelborden ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["70.30.","stroombeveiliging - algemeen"]
["70.31.","stroombeveiliging - hoofdschakelaars ","PM",null,"Geen",{"$nulls":4},1]
["70.32.","stroombeveiliging - differentieelschakelaars ","PM",null,"Geen",{"$nulls":4},1]
["70.33.","stroombeveiliging - automatische schakelaars ","PM",null,"Geen",{"$nulls":4},1]
["70.40.","aarding - algemeen"]
["70.41.","aarding - aardingslus ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"v","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["70.42.","aarding - afzonderlijke aardverbindingen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["70.43.","aarding - aardingsonderbrekers ","PM",null,"Geen",{"$nulls":4},1]
["70.44.","aarding - hoofdbeschermingsgeleiders ","PM",null,"Geen",{"$nulls":4},1]
["70.45.","aarding - hoofdequipotentiaalverbindingen ","PM",null,"Geen",{"$nulls":4},1]
["70.46.","aarding - bijkomende equipotentiaalverbindingen ","PM",null,"Geen",{"$nulls":4},1]
["70.47.","aarding - bliksemafleidersinstalatie ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Bliksemafleiderinstallatie","Stuks",null,1]
["70.50.","leidingen - algemeen"]
["70.53.","leidingen - inbouw kabelbuizen ","PM",null,"Geen",{"$nulls":4},1]
["70.54.","leidingen - opbouw kabelbuizen ","PM",null,"Geen",{"$nulls":4},1]
["70.55.","leidingen - plint- & wandkanalen ","PM",null,"Geen",{"$nulls":4},1]
["70.56.","leidingen - kabelgoten en -ladders ","PM",null,"Geen",{"$nulls":4},1]
["70.57.","leidingen - wachtbuizen ","PM",null,"Geen",{"$nulls":4},1]
["70.60.","trek- en verbindingsdozen - algemeen"]
["70.61.","trek- en verbindingsdozen - inbouw metselwerk ","PM",null,"Geen",{"$nulls":4},1]
["70.62.","trek- en verbindingsdozen - inbouw holle wanden ","PM",null,"Geen",{"$nulls":4},1]
["70.63.","trek- en verbindingsdozen - inbouw verlaagde plafonds ","PM",null,"Geen",{"$nulls":4},1]
["70.64.","trek- en verbindingsdozen - inbouw vloeren ","PM",null,"Geen",{"$nulls":4},1]
["70.65.","trek- en verbindingsdozen - opbouw ","PM",null,"Geen",{"$nulls":4},1]
["70.70.","bijzondere voorzieningen - algemeen"]
["70.71.","bijzondere voorzieningen - voeding liften ","PM",null,"Geen",{"$nulls":4},1]
["71.","ELEKTRICITEIT SCHAKELAARS & CONTACTDOZEN"]
["71.00.","elektriciteit schakelaars & contactdozen - algemeen"]
["71.10.","stopcontacten - algemeen"]
["71.11.","stopcontacten - 10/16A ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.12.","stopcontacten - 20/32A ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.20.","aansluitdozen - algemeen"]
["71.21.","aansluitdozen - voeding elektrisch fornuis ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.22.","aansluitdozen - voeding was- & vaatwasmachine ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.23.","aansluitdozen - voeding HVAC en andere ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.30.","schakelaars - algemeen"]
["71.31.","schakelaars - enkelpolig ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.32.","schakelaars - dubbelpolig ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.33.","schakelaars - wissel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.34.","schakelaars - kruis ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.35.","schakelaars - timerschakelaars ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.36.","schakelaars - teleruptoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.37.","schakelaars - dimmers ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["71.40.","speciale toebehoren - algemeen"]
["71.41.","speciale toebehoren - bewegingsdetectoren ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Schakelaar Toebehoren ","Stuks",null,1]
["71.42.","speciale toebehoren - foto-elektrisch schakelaar ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Schakelaar Toebehoren ","Stuks",null,1]
["71.43.","speciale toebehoren - schemerschakelaar ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Schakelaar Toebehoren ","Stuks",null,1]
["72.","ELEKTRICITEIT LICHTARMATUREN"]
["72.00.","elektriciteit lichtarmaturen - algemeen"]
["72.10.","binnenarmaturen E27 - algemeen ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.11.","binnenarmaturen E27 - met lenskap ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.12.","binnenarmaturen E27 - andere ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.20.","binnenarmaturen TL - algemeen"]
["72.21.","binnenarmaturen TL - opbouwarmatuur plafond"]
["72.21.10.","binnenarmaturen TL - opbouwarmatuur plafond - T8 ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.21.20.","binnenarmaturen TL - opbouwarmatuur plafond - T5 ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.22.","binnenarmaturen TL - lichtstrip keukenaanrecht ",{"$nulls":7},1]
["72.22.10.","binnenarmaturen TL - lichtstrip keukenaanrecht/T8 ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.22.20.","binnenarmaturen TL - lichtstrip keukenaanrecht/T5 ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.40.","binnenarmaturen halogeen - algemeen"]
["72.41.","binnenarmaturen halogeen - transfo ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.42.","binnenarmaturen halogeen - inbouwspots ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.43.","binnenarmaturen halogeen - opbouwspots ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.50.","veiligheidsverlichting - algemeen"]
["72.51.","veiligheidsverlichting - autonoom niet-permanent ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.52.","veiligheidsverlichting - autonoom permanent ","FH","st","TYPE 5","Object","Lamp","Stuks",null,1]
["72.53.","veiligheidsverlichting - centrale noodvoeding ","SOG",null,"Geen",{"$nulls":4},1]
["72.54.","veiligheidsverlichting - armaturen ","SOG",null,"Geen",{"$nulls":4},1]
["72.55.","veiligheidsverlichting - signalisatie & pictogrammen ","PM",null,"Geen",{"$nulls":4},1]
["72.60.","buitenarmaturen - algemeen"]
["72.70.","armaturen geleverd door het bestuur - algemeen"]
["73.","ELEKTRICITEIT BEL & PARLOFOON"]
["73.00.","elektriciteit bel & parlofoon - algemeen"]
["73.10.","individuele belinstallaties - algemeen"]
["73.11.","individuele belinstallaties - huisbel ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["73.12.","individuele belinstallaties - beldrukknop ","PM",null,"Geen",{"$nulls":4},1]
["73.13.","individuele belinstallaties - beltransfo ","PM",null,"Geen",{"$nulls":4},1]
["73.14.","individuele belinstallaties - bedrading ","PM",null,"Geen",{"$nulls":4},1]
["73.20.","parlofooninstallatie - algemeen"]
["73.21.","parlofooninstallatie - binnenposten ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["73.22.","parlofooninstallatie - deurstation ","PM",null,"Geen",{"$nulls":4},1]
["73.23.","parlofooninstallatie - beltransfo ","PM",null,"Geen",{"$nulls":4},1]
["73.24.","parlofooninstallatie - verdeeldozen ","PM",null,"Geen",{"$nulls":4},1]
["73.25.","parlofooninstallatie - bedrading ","PM",null,"Geen",{"$nulls":4},1]
["73.26.","parlofooninstallatie - elektrisch deurslot ","PM",null,"Geen",{"$nulls":4},1]
["73.30.","toegangscontrolesysteem - algemeen","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"SOG",null,"Geen",{"$nulls":4},1]
["74.","ELEKTRICITEIT TELECOM & DOMOTICA"]
["74.00.","elektriciteit telecom & domotica - algemeen"]
["74.10.","telefoon - algemeen"]
["74.11.","telefoon - buitenbekabeling ","SOG",null,"Geen",{"$nulls":4},1]
["74.12.","telefoon - basis aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.13.","telefoon - extra aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.14.","telefoon - binnenbekabeling ","PM",null,"Geen",{"$nulls":4},1]
["74.20.","kabeldistributie - algemeen"]
["74.21.","kabeldistributie - buitenbekabeling ","SOG",null,"Geen",{"$nulls":4},1]
["74.22.","kabeldistributie - basis aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.23.","kabeldistributie - extra aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.24.","kabeldistributie - binnenbekabeling ","PM",null,"Geen",{"$nulls":4},1]
["74.30.","netwerkbekabeling - algemeen"]
["74.31.","netwerkbekabeling - buitenbekabeling ","SOG",null,"Geen",{"$nulls":4},1]
["74.32.","netwerkbekabeling - basis aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.33.","netwerkbekabeling - extra aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.34.","netwerkbekabeling - binnenbekabeling ","PM",null,"Geen",{"$nulls":4},1]
["74.40.","satelietontvangstsysteem - algemeen"]
["74.41.","satelietontvangstsysteem - centrale schotelantenne ","SOG",null,"Geen",{"$nulls":4},1]
["74.42.","satelietontvangstsysteem - buitenbekabeling ","SOG",null,"Geen",{"$nulls":4},1]
["74.43.","satelietontvangstsysteem - basis aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.44.","satelietontvangstsysteem - extra aansluitpunt ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["74.45.","satelietontvangstsysteem - binnenbekabeling ","PM",null,"Geen",{"$nulls":4},1]
["74.50.","alarmkabel - algemeen"]
["74.60.","luidsprekerkabel - algemeen"]
["74.70.","oproepsystemen ADL - algemeen"]
["74.80.","multimediakast","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":5},"Object",null,"Stuks",null,1]
["75.","ELEKTRICITEIT VERWARMING"]
["75.00.","elektriciteit verwarming - algemeen"]
["75.10.","direct systeem - algemeen"]
["75.11.","direct systeem - gedecentraliseerd"]
["75.11.10.","direct systeem - gedecentraliseerd/wandconvectoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["75.11.20.","direct systeem - gedecentraliseerd/plintconvectoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["75.11.30.","direct systeem - gedecentraliseerd/stralingselementen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["75.20.","accumulatiesysteem - algemeen"]
["75.21.","accumulatiesysteem - gedecentraliseerd"]
["75.21.10.","accumulatiesysteem - gedecentraliseerd/dynamisch gemengd ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["75.30.","meet- & regeltoestellen - algemeen"]
["75.31.","meet- & regeltoestellen - klokthermostaten "]
["75.31.10.","meet- & regeltoestellen - klokthermostaten/direct systeem ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["75.31.20.","meet- & regeltoestellen - klokthermostaten/accumulatie systeem ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
[null,null,"PM",null,"Geen",{"$nulls":4},1]
["76.","ELEKTROMECHANICA LIFTEN"]
["76.00.","elektromechanica liften - algemeen"]
["76.01.","algemeen - grenzen van de aanneming ","PM",null,"Geen",{"$nulls":4},1]
["76.02.","algemeen - controle op afmetingen ","PM",null,"Geen",{"$nulls":4},1]
["76.03.","algemeen - documentatie en studie ","PM",null,"Geen",{"$nulls":4},1]
["76.04.","algemeen - werfinstallatie en -organisatie ","PM",null,"Geen",{"$nulls":4},1]
["76.05.","algemeen - onderhoud tijdens waarborgperiode ","PM",null,"Geen",{"$nulls":4},1]
["76.10.","bestaande installaties - algemeen"]
["76.11.","bestaande installaties - afbraak ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Lift Bestaande installaties","Stuks",null,1]
["76.12.","bestaande installaties - renovatie ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW Lift Bestaande installaties","Stuks",null,1]
["76.20.","elektrische liften - algemeen"]
["76.21.","elektrische liften - met machinekamer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["76.22.","elektrische liften - zonder machinekamer (gearless) ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["76.30.","kooiuitrusting - algemeen"]
["76.31.","kooiuitrusting - personenlift ","PM",null,"Geen",{"$nulls":4},1]
["76.32.","kooiuitrusting - goederenlift ","PM",null,"Geen",{"$nulls":4},1]
["76.33.","kooiuitrusting - vandalismewerend ","PM",null,"Geen",{"$nulls":4},1]
["76.40.","deuren & fronten - algemeen"]
["76.41.","deuren & fronten - personenlift ","PM",null,"Geen",{"$nulls":4},1]
["76.50.","bedienings- & signalisatiepanelen - algemeen"]
["76.51.","bedienings- & signalisatiepanelen - personenlift ","PM",null,"Geen",{"$nulls":4},1]
["77.","BRANDDETECTIE & ALARMSYSTEMEN"]
["77.00.","branddetectie & alarmsystemen - algemeen"]
["77.10.","centrale eenheid - algemeen ","SOG",null,"Geen",{"$nulls":4},1]
["77.20.","energievoorziening - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["77.30.","bekabeling - algemeen ","PM",null,"Geen",{"$nulls":4},1]
["77.40.","brandmelding - algemeen"]
["77.41.","brandmelding - branddetectoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["77.42.","brandmelding - handmelders ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["77.43.","brandmelding - gasdetectoren ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["77.44.","brandmelding - autonome rookmelders ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["77.50.","alarmsirenes - algemeen"]
["77.51.","alarmsirenes - signal fast sweep ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["77.60.","evacuatietoebehoren - algemeen"]
["77.61.","evacuatietoebehoren - deurpomp met magneethouder ","FH","st","TYPE 4","Door","Gebruik ARCHICAD property: VMSW deurpomp","Stuks",null,1]
["77.62.","evacuatietoebehoren - pictogrammen ","PM",null,"Geen",{"$nulls":4},1]
["77.63.","evacuatietoebehoren - brandweersleutelkluis","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[]
["80.","BINNENSCHILDERWERKEN"]
["80.00.","schilderwerken - algemeen"]
["80.10.","binnenschilderwerken op pleisterwerk - algemeen"]
["80.11.","binnenschilderwerken op pleisterwerk - acrylaathars ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.12.","binnenschilderwerken op pleisterwerk - acrylaatdispersie ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.13.","binnenschilderwerken op pleisterwerk - vinyllatex ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.14.","binnenschilderwerken op pleisterwerk - kwartshoudende structuurverf ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.15.","binnenschilderwerken op pleisterwerk - meerkleurige effectverf ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.20.","binnenschilderwerken op gipskartonplaten - algemeen"]
["80.21.","binnenschilderwerken op gipskartonplaten - acrylaathars ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.22.","binnenschilderwerken op gipskartonplaten - acrylaatdispersie ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.23.","binnenschilderwerken op gipskartonplaten - vinyllatex ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.24.","binnenschilderwerken op gipskartonplaten - kwartshoudende structuurverf ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.25.","binnenschilderwerken op gipskartonplaten - meerkleurige effectverf ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.30.","binnenschilderwerken op beton - algemeen"]
["80.31.","binnenschilderwerken op beton - acrylaathars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.32.","binnenschilderwerken op beton - acrylaatdispersie ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.33.","binnenschilderwerken op beton - vinyllatex ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.34.","binnenschilderwerken op beton - kwartshoudende structuurverf ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.35.","binnenschilderwerken op beton - meerkleurig effectverf ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.36.","binnenschilderwerken op beton - epoxyverf ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Zone","Gebruik ARCHICAD property: VMSW binnenschilderwerken",null,null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.40.","binnenschilderwerken op metselwerk - algemeen"]
["80.41.","binnenschilderwerken op metselwerk - acrylaathars ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.42.","binnenschilderwerken op metselwerk - acrylaatdispersie ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.43.","binnenschilderwerken op metselwerkwerk - vinyllatex ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.44.","binnenschilderwerken op metselwerk - kwartshoudende structuurverf ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.45.","binnenschilderwerken op metselwerk - meerkleurige effectverf ","FH","m2","TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.50.","binnenschilderwerken op hout en houtachtige platen - algemeen"]
["80.51.","binnenschilderwerken op hout en houtachtige platen - lak"]
["80.51.10.","op hout en houtachtige platen - lak/acryllaatdispersie ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.51.20.","op hout en houtachtige platen - lak/polyurethaan acrylaathars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.51.30.","op hout en houtachtige platen - lak/alkyd-urethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.51.40.","op hout en houtachtige platen - lak/alkydhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.52.","binnenschilderwerken op hout en houtachtige platen - vernis"]
["80.52.10.","op hout en houtachtige platen - vernis / acrylurethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.52.20.","op hout en houtachtige platen - vernis/polyurethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.52.30.","op hout en houtachtige platen - vernis/alkydurethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.53.","binnenschilderwerken op hout en houtachtige platen - beits ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur binnenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["80.60.","binnenschilderwerken op metaal - algemeen"]
["81.","BEHANGWERKEN"]
["81.00.","behangwerken - algemeen"]
["81.10.","verwijderen van behangpapier - algemeen ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["81.20.","behangen met glasvezeldoek - algemeen"]
["81.21.","behangen met glasvezeldoek - op nieuw pleisterwerk ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["81.22.","behangen met glasvezeldoek - op oud pleisterwerk ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["81.23.","behangen met glasvezeldoek - op gipskartonplaten ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the inside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW behangwerken","Oppervlakte binnendagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.","BUITENSCHILDERWERKEN"]
["82.00.","buitenschilderwerken - algemeen"]
["82.10.","buitenschilderwerken op buitenbepleistering - algemeen"]
["82.11.","buitenschilderwerken op buitenbepleisteringen - acrylaatdispersie ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.12.","buitenschilderwerken op buitenbepleisteringen - siloxaan ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.13.","buitenschilderwerken op buitenbepleisteringen - silicaat ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.20.","buitenschilderwerken op beton - algemeen"]
["82.21.","buitenschilderwerken op beton - acrylaatdispersie ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.22.","buitenschilderwerken op beton - siloxaan ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.23.","buitenschilderwerken op beton - silicaat ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.24.","buitenschilderwerken op beton - kwartshoudende structuurverf ","FH","m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.30.","buitenschilderwerken op gevelmetselwerk - algemeen"]
["82.31.","buitenschilderwerken op gevelmetselwerk - acrylaatdispersie ","FH","m2","TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.32.","buitenschilderwerken op gevelmetselwerk - siloxaan ","FH","m2","TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.33.","buitenschilderwerken op gevelmetselwerk - silicaat ","FH","m2","TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.34.","buitenschilderwerken op gevelmetselwerk - kwartshoudende structuurverf ","FH","m2","TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.40.","buitenschilderwerken op hout en houtachtige platen - algemeen"]
["82.41.","buitenschilderwerken op hout en houtachtige platen - lak"]
["82.41.10.","op hout en houtachtige platen - lak/acryllaatdispersie watergedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.41.20.","op hout en houtachtige platen - lak/alkyd-urethaan watergedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.41.30.","op hout en houtachtige platen - lak/alkydhars solventgedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":5},"Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.41.40.","op hout en houtachtige platen - lak/urethaan-alkyd solventgedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.42.","buitenschilderwerken op hout en houtachtige platen - vernis"]
["82.42.10.","op hout en houtachtige platen - vernis/alkyd-urethaanhars ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.43.","buitenschilderwerken op hout en houtachtige platen - beits"]
["82.43.10.","op hout en houtachtige platen - beits/alkydhars watergedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.43.20.","op hout en houtachtige platen - beits/alkydhars solventgedragen ","FH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"ARCHICAD property: Lengte muur buitenzijde",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW binnenschilderwerken","omtrek dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only","Omtrek ","werkt alleen indien horizontaal geplaatst",1]
[null,null,null,"m2","TYPE 3","Beam",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.50.","nabehandelingen op metselwerk - algemeen"]
["82.51.","nabehandelingen op metselwerk - hydrofobering ","FH","m2","TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.52.","nabehandelingen op metselwerk - antigraffiti ","FH","m2","TYPE 3","Column",null,"Top Surface",null,1]
[{"$nulls":4},"TYPE 3","Wall",null,"Net Surface Area on the outside face",null,1]
[{"$nulls":4},"TYPE 4","Door","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 4","Window","Gebruik ARCHICAD property: VMSW buitenschilderwerken","Oppervlakte dagkanten (2x hoogte + 1x breedte)",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["82.60.","buitenschilderwerken op metaal - algemeen"]
[]
["90.","BUITENVERHARDINGEN"]
["90.00.","buitenverhardingen - algemeen"]
["90.10.","funderingen - algemeen"]
["90.11.","funderingen - steenslag"]
["90.11.10.","funderingen - steenslag/niet-continue korrelverdeling ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.11.20.","funderingen - steenslag/continue korrelverdeling zonder toevoegsels ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.11.30.","funderingen - steenslag/continue korrelverdeling met toevoegsels ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.12.","funderingen - ternair mengsel ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.13.","funderingen - zandcement ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.14.","funderingen - schraal beton"]
["90.14.10.","funderingen - schraal beton/ongewapend ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.14.20.","funderingen - schraal beton/gewapend ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.20.","verhardingen - algemeen"]
["90.21.","verhardingen - in rijen te leggen kasseien ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.22.","verhardingen - mozaïekkeien ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.23.","verhardingen - betonstraatstenen"]
["90.23.10.","verhardingen - betonstraatstenen/kleurvast ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.23.20.","verhardingen - betonstraatstenen/waterdoorlatend ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.24.","verhardingen - gebakken straatstenen ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.25.","verhardingen - betontegels"]
["90.25.10.","verhardingen - betontegels/kleurvast ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.25.20.","verhardingen - betontegels/waterdoorlatend ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.25.30.","verhardingen - betontegels/grasbetontegels ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.25.40.","verhardingen - betontegels/silexbetontegels ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.26.","verhardingen - tegels in natuursteen ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.27.","verhardingen - dolomiet ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.28.","verhardingen - gepolierd beton ","FH of VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["90.29.","verhardingen - tactiele oppervlakken ","FH of VH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["90.30.","lijnvormige elementen - algemeen"]
["90.31.","lijnvormige elementen - boordstenen"]
["90.31.10.","lijnvormige elementen - boordstenen/beton"]
["90.31.11.","lijnvormige elementen - boordstenen/beton - prefab ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["90.31.12.","lijnvormige elementen - boordstenen/beton - ter plaatse gestort ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["90.31.20.","lijnvormige elementen - boordstenen/palissaden ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["90.31.30.","lijnvormige elementen - boordstenen/metaal ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["90.32.","lijnvormige elementen - watergreppels"]
["90.32.10.","lijnvormige elementen - watergreppels/beton"]
["90.32.11.","lijnvormige elementen - watergreppels/beton - prefab ","FH of VH","m","TYPE 3","Beam",null,"ARCHICAD property: Lengte Balk of Hoogte kolom",null,1]
["91.","BUITENCONSTRUCTIES EN AFSLUITINGEN"]
["91.00.","buitenconstructies en afsluitingen - algemeen"]
["91.10.","tuinafsluitingspalen - algemeen"]
["91.11.","tuinafsluitingspalen - staal ","PM",null,"Geen",{"$nulls":4},1]
["91.12.","tuinafsluitingspalen - hout ","PM",null,"Geen",{"$nulls":4},1]
["91.13.","tuinafsluitingspalen - beton ","PM",null,"Geen",{"$nulls":4},1]
["91.20.","draadafsluitingen - algemeen"]
["91.21.","draadafsluitingen - gladde draad ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["91.22.","draadafsluitingen - draadgaas ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["91.30.","tuinschermen - algemeen"]
["91.31.","tuinschermen - schapenhek ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["91.32.","tuinschermen - houtschermen ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["91.33.","tuinschermen - betonplaten ","FH","m","TYPE 3","Wall",null,"Lengte volgens eigen middenas",null,1]
["91.40.","tuinhekken - algemeen"]
["91.41.","tuinhekken - staal ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["91.42.","tuinhekken - hout ","FH","st","TYPE 5","Door",null,"Stuks",null,1]
["91.50.","terrassen tuinhout - algemeen"]
["91.51.","terrassen tuinhout - tegels ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["91.52.","terrassen tuinhout - beplanking ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["91.60.","constructies tuinhout - algemeen"]
["92.","BUITENMEUBILAIR EN UITRUSTINGSELEMENTEN"]
["92.00.","buitenmeubilair en uitrustingselementen - algemeen"]
["92.10.","brievenbussen - algemeen"]
["92.11.","brievenbussen - geleverd door het bestuur ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.12.","brievenbussen - prefab beton ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.13.","brievenbussen - staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.14.","brievenbussen - aluminium ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.20.","vuilnisbakken - algemeen"]
["92.21.","vuilnisbakken - geleverd door het bestuur ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.22.","vuilnisbakken - staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.23.","vuilnisbakken - kunststof ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.30.","fietsrekken - algemeen"]
["92.31.","fietsrekken - blokken beton ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.32.","fietsrekken - modules staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.33.","fietsrekken - aanleunbeugels staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.34.","fietsrekken - ophangelementen staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.35.","fietsrekken - klemmen staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.40.","parkingelementen - algemeen"]
["92.41.","parkingelementen - parkeerpalen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.42.","parkingelementen - parkeerbeugels ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.50.","zitbanken - algemeen"]
["92.51.","zitbanken - geleverd door het bestuur ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.52.","zitbanken - zonder rugleuning ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.53.","zitbanken - met rugleuning ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.60.","boomomrandingen - algemeen"]
["92.61.","boomomrandingen - roosters beton ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.62.","boomomrandingen - roosters gietijzer ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.63.","boomomrandingen - roosters kunststof ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.64.","boomomrandingen - roosters staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.70.","plantbescherming - algemeen"]
["92.71.","plantbescherming - boombeugels staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.73.","plantbescherming - boomkorven staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["92.74.","plantbescherming - plantkorven staal ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["93.","GROENAANLEG EN -ONDERHOUD"]
["93.00.","groenaanleg en -onderhoud - algemeen"]
["93.10.","grondbewerkingen - algemeen"]
["93.11.","grondbewerkingen - diepspitten ","PM",null,"Geen",{"$nulls":4},1]
["93.12.","grondbewerkingen - egaliseren ","PM",null,"Geen",{"$nulls":4},1]
["93.13.","grondbewerkingen - frezen ","PM",null,"Geen",{"$nulls":4},1]
["93.20.","verwerking teelaarde - algemeen"]
["93.21.","verwerking teelaarde - afkomstig van afgraving ","FH/VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["93.22.","verwerking teelaarde - te leveren door de aannemer ","FH/VH","m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":4},"TYPE 5","Morph",null,"Net Volume",null,1]
["93.30.","verwerken van bodemverbeteringsmiddelen - algemeen ","FH/VH","kg","TYPE 4","Slab","vul de ARCHICAD property 'Soortelijk gewicht' in","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Mesh","vul de ARCHICAD property 'Soortelijk gewicht' in","ARCHICAD property: Gewicht materiaal",null,1]
[{"$nulls":4},"TYPE 5","Morph","vul de ARCHICAD property 'Soortelijk gewicht' in","ARCHICAD property: Gewicht materiaal",null,1]
[null,null,null,"m3","TYPE 3","Slab",null,"Net Volume ","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Volume",null,1]
[{"$nulls":5},"Morph",null,"Net Volume",null,1]
["93.40.","aanleg grasmatten - algemeen"]
["93.41.","aanleg grasmatten - door bezaaiing ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["93.42.","aanleg grasmatten - door bezoding ","FH","m2","TYPE 3","Slab",null,"Top Surface","waarden detailmeetstaat correct indien vloer rechthoekig",1]
[{"$nulls":4},"TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":4},"TYPE 5","Morph","Geometry Method: Straight only!","Surface Area",null,1]
["93.50.","aanplanting houtachtige vegetaties - algemeen"]
["93.51.","aanplanting houtachtige vegetaties - bomen ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["93.52.","aanplanting houtachtige gewassen - hagen ","FH","st","TYPE 5","Morph",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
[{"$nulls":4},"TYPE 5","Wall",null,"Stuks",null,1]
["93.53.","aanplanting houtachtige gewassen - heesters ","FH","st","TYPE 5","Object",null,"Stuks",null,1]
["93.60.","hulpmiddelen groenaanleg - algemeen"]
["93.61.","hulpmiddelen groenaanleg - boompaalconstructies ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW hulpmiddelen groenaanleg","Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["93.62.","hulpmiddelen groenaanleg - boomroosters ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW hulpmiddelen groenaanleg","Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["93.63.","hulpmiddelen groenaanleg - ondergrondse verankering van bomen ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW hulpmiddelen groenaanleg","Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["93.64.","hulpmiddelen groenaanleg - groeiplaatsverbetering van bomen (irrigatie) ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW hulpmiddelen groenaanleg","Stuks",null,1]
[{"$nulls":4},"TYPE 5","Object",null,"Stuks",null,1]
["93.65.","hulpmiddelen groenaanleg - haagsteun ","FH","m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
[null,null,null,"m","TYPE 5","Object",null,"Lengte","Let op! Enkel Horizontale lengte wordt gemeten",1]
["93.70.","groenonderhoud - algemeen"]
["93.71.","groenonderhoud - maaien van grasmatten ","FH","m2","TYPE 5","Mesh",null,"Net Area",null,1]
[{"$nulls":5},"Morph","Geometry Method: Straight only!","Surface Area",null,1]
["93.72.","groenonderhoud - bomen snoeien ","FH","st","TYPE 4","Object","Gebruik ARCHICAD property: VMSW bomen snoeien","Stuks",null,1]
["93.73.","groenonderhoud - scheren van hagen en beplantingsmassieven ","FH","m2","TYPE 4","Morph","Gebruik ARCHICAD Property: VMSW_scheren van hagen en beplantingsmassieven","Surface Area",null,1]
[{"$nulls":4},"TYPE 4","Wall","Gebruik ARCHICAD Property: VMSW_scheren van hagen en beplantingsmassieven","Top Surface",null,1]
["93.74.","groenonderhoud - snoeien van heesters ","FH","st","TYPE 5",null,null,"Stuks",null,1]